**If the UE does not support UL on intra-band EN-DC part of a band combination, then the combination is not an intra-band EN-DC combination but it has an intra-band EN-DC component.**