**3GPP TSG-RAN4 Meeting #98-e *R4-2100988***

**Electronic Meeting, 25th Jan - 5th Feb, 2021**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.101-3** | **CR** | **0453** | **rev** | **-** | **Current version:** | **17.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | CR introduction completed band combinations for Dual Connectivity (DC) of 5 bands LTE inter-band CA (5DL/1UL) and 1 NR band (1DL/1UL) | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Samsung | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | DC\_R17\_5BLTE\_1BNR\_6DL2UL-Core | | | | |  | ***Date:*** | | | 2021-1-28 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | |  |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | Completed new DC inter-band combinations for Dual Connectivity (DC) of 5 bands LTE inter-band CA (5DL/1UL) and 1 NR band (1DL/1UL) are introduced into TS 38.101-3 in RAN4 #98e meeting. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | The following EN-DC band combinations completed are added from RAN4 #98-e meeting  DC\_1A-3A-7A-8A-40A\_n78(2A)  DC\_1A-3A-7A-8A-40C\_n78(2A)  Which completed in the following contritbuion:  R4-21000324 | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The requirements for above band combinations are incomplete. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 5.5B.4.5 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | |  | | |
| ***affected:*** | | **X** |  | Test specifications | | | | TS 38.521-3 | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | |  | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

## <Unchanged sections omitted>

#### 5.5B.4.5 Inter-band EN-DC configurations within FR1 (six bands)

Table 5.5B.4.5-1: Inter-band EN-DC configurations within FR1 (six bands)

|  |  |
| --- | --- |
| EN-DC  configuration | Uplink EN-DC  configuration  (NOTE 1) |
| DC\_1A-3A-7A-8A-40A\_n78A  DC\_1A-3A-7A-8A-40A\_n78(2A)  DC\_1A-3A-7A-8A-40C\_n78A  DC\_1A-3A-7A-8A-40C\_n78(2A) | DC\_1A\_n78A  DC\_3A\_n78A  DC\_7A\_n78A  DC\_8A\_n78A  DC\_40A\_n78A |
| DC\_1A-3A-7A-20A\_n28A-n78A2,3 | DC\_1A\_n28A  DC\_1A\_n78A  DC\_3A\_n28A  DC\_3A\_n78A  DC\_7A\_n28A  DC\_7A\_n78A  DC\_20A\_n28A  DC\_20A\_n78A |
| DC\_1A-3A-7A-28A\_n5A-n78A  DC\_1A-3A-7C-28A\_n5A-n78A  DC\_1A-3C-7A-28A\_n5A-n78A  DC\_1A-3C-7C-28A\_n5A-n78A | DC\_1A\_n5A  DC\_1A\_n78A  DC\_3A\_n5A  DC\_3C\_n5A  DC\_3A\_n78A  DC\_3C\_n78A  DC\_7A\_n5A  DC\_7C\_n5A  DC\_7A\_n78A  DC\_7C\_n78A  DC\_28A\_n5A  DC\_28A\_n78A |
| DC\_1A-3A-7A-28A\_n7A-n78A | DC\_1A-n7A  DC\_3A-n7A  DC\_7A-n7A4  DC\_28A\_n7A  DC\_1A\_n78A  DC\_3A\_n78A  DC\_7A\_n78A  DC\_28A\_n78A |
| DC\_1A-3C-7A-28A\_n7A-n78A | DC\_1A-n7A  DC\_3A-n7A  DC\_3C-n7A  DC\_7A-n7A4  DC\_28A\_n7A  DC\_1A\_n78A  DC\_3A\_n78A  DC\_3C\_n78A  DC\_7A\_n78A  DC\_28A\_n78A |
| DC\_1A-3A-7A-28A\_n40A-n78A | DC\_1A\_n40A  DC\_1A\_n78A  DC\_3A\_n40A  DC\_3A\_n78A  DC\_7A\_n40A  DC\_7A\_n78A  DC\_28A\_n40A  DC\_28A\_n78A |
| NOTE 1: Uplink EN-DC configurations are the configurations supported by the present release of specifications.  NOTE 2: Applicable for UE supporting inter-band EN-DC with mandatory simultaneous Rx/Tx capability.  NOTE 3: The frequency range in band n28 is restricted for this band combination to 703-733 MHz for the UL and 758-788 MHz for the DL.  NOTE 4: Only single switched UL is supported. | |

## <Unchanged sections omitted>