**3GPP TSG-RAN WG4 Meeting # 98-bis-e R4-210xxxx**

**Electronic Meeting, Apr. 12-20, 2021**

**Agenda item: 8.6.3**

**Source:** Moderator (CMCC)

**Title:** Email discussion summary for [98-bis-e][321] NR\_HST\_FR1\_Demod

**Document for:** Information

# Introduction

This email discussion focuses on UE demodulation for Rel-17 NR HST, including agenda 8.6.3.1~8.6.3.3. Two topics are included in total, including PDSCH requirements for CA scenarios and enhanced transmission schemes. The agreed way forward in previous meeting is in R4-2103876.

The targets of email discussion for 1st round and 2nd round are:

* 1st round: discuss the open issues and strive to minimize the open issues
* 2nd round: according to 1st round discussion, discuss left open issues for 2nd round, and strive to minimize the open issues, and strive to approve the WF.

# Topic #1: Work Plan

*Agenda 8.6.1*

## Companies’ contributions summary

|  |  |  |  |
| --- | --- | --- | --- |
| **TDoc** | **Title** | **Source** | **Proposals/ Observations** |
| [**R4-2104946**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2104946.zip) | Updated work plan for enhancement for NR high speed train scenario in FR1  (demod part) | CMCC | This contribution provides updated work plan for enhancement for NR high speed train scenario in FR1. |

## Open issues summary

### Work plan for FR1 HST demod part

**Issue 1-1: Work plan (demod part)**

According to the revised WID, the demodulation part shall be finalized by September 2022 (RAN #97).

Companies please check the updated work plan for demodulation part in [**R4-2104946**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2104946.zip)**.**

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | **Comments** |
| **Ericsson** | Issue 1-1:  We are fine with the work plain for the demodulation part. The demodulation part may complete earlier depending on the progress, but it is important to keep the work scope as specified in the current WID. |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
| **Issue 1-1-1: Work plan (demod part)** |  |

# Topic #2 PDSCH requirements for CA scenarios

*Agenda 8.6.3.2*

## Companies’ contributions summary

|  |  |  |  |
| --- | --- | --- | --- |
| **TDoc** | **Title** | **Source** | **Proposals/ Observations** |
| [**R4-2104844**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2104844.zip) | On PDSCH CA Requirements in HST | Apple | Proposal #1: Introduce requirements for CA for HST-DPS with one active TCI state only.  Proposal #2: Define applicability rule for CA requirements in HST scenario as - If UE supports demodulationEnhancement-r16, only HST-SFN JT requirements shall apply, otherwise HST-DPS requirements shall apply for CA.  Proposal #3: Do not introduce requirements in HST for FDD 15KHz + TDD 15KHz CA and TDD 15 kHz + TDD 30 kHz CA.  Proposal #4: Use same applicability rule on CA duplex mode for HST CA as CA CQI requirements.  Channel Model for HST-DPS  *Observation #1: The deployment parameters for HST-SFN JT and HST-DPS are the same, yet HST-DPS doesn’t consider time varying path power or delay.*  *Observation #2: With modified channel model for HST-DPS with time varying path power or delay, we observe 2dB degradation in performance for 2x2.*  *Observation #3: For HST-DPS the visibility is 1 RRH and UE will not be able to measure L1-RSRP or track TRS from next RRH prior to TCI state switch.*  Proposal #5: RAN4 further evaluates if HST-DPS channel model is practical in actual deployment and update the channel model if necessary. |
| [**R4-2104939**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2104939.zip) | Simulation results for HST-SFN joint transmission for CA scenario | CMCC |  |
| [**R4-2104948**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2104948.zip) | Discussion on FR1 HST UE demodulation for CA scenario | CMCC | *Observation 1: HST-SFN joint transmission scheme and DPS transmission scheme are different transmission schemes, it is doubtful to say that passing one test implies also passing the other test.*   * *Based on discussion in Rel-16 NR HST WI, different UE have different implementation on the frequency tracking of these two transmission schemes* * *DPS scheme provides better performance, while HST-SFN joint transmission scheme requires advanced receiver.*   *Proposal 1: considering that HST-SFN joint transmission scheme and DPS transmission scheme are different transmission schemes, not sure whether we can specify the applicability rule between HST-SFN joint transmission scheme and DPS transmission scheme for CA scenario.*  *Proposal 2: for SCS configuration for CA scenario to be considered and applicability rule for SCS configuration, we provide two options to move forward:*   * *Option 1: FDD 15 kHz + TDD 15 kHz CA and TDD 15 kHz + TDD 30 kHz CA are covered, and the applicability rule between CA scenario with TDD 15 kHz SCS and CA scenario with TDD 30 kHz SCS specified in Rel-16 can be reused* * *Option 2: FDD 15 kHz + TDD 15 kHz CA and TDD 15 kHz + TDD 30 kHz CA are precluded, and no applicability rule for FDD 15 kHz + FDD 15 kHz CA, TDD 30 kHz + TDD 30 kHz CA and FDD 15 kHz + TDD 30 kHz CA (i.e. it is not preferred to reuse CA CQI applicability rule to PDSCH CA normal demodulation requirements)*   *Proposal 3: it is proposed that Rel-17 FR1 HST PDSCH CA requirements are release independent from Rel-15.* |
| [**R4-2104976**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2104976.zip) | Views on HST CA tests for FR1 | NTT DOCOMO, INC. | Proposal 1: Target maximum Doppler frequency under DPS transmission scheme are as follows.   * For FDD 15kHz : 870Hz * For TDD 30kHz : 1667Hz   Proposal 2: Apply the following test applicability rules.   * If UE pass Rel-17 DPS CA tests, Rel-17 HST-SFN CA tests can be skipped * If UE pass Rel-17 HST-SFN CA tests, Rel-17 DPS CA tests can be skipped   Observation 1: If there are no technical issues in the future discussion, the HST-SFN CA and DPS CA requirements should be treated as release independent from Rel-15. |
| [**R4-2106431**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2106431.zip) | Views on HST CA PDSCH performance requirements | Intel Corporation | Proposal #1: Define HST CA requirements with DPS Tx scheme.  Proposal #2: Reuse applicability rule from DPS single carrier to CA and define new one as: UE can skip single carrier test case if it has passed corresponding CA test case.  Proposal #3: If UE supports HST JT scheme, it can be tested only with this Tx scheme in CA mode, otherwise CA requirements with DPS Tx scheme should be applied.  Proposal #4: Do not define HST PDSCH CA requirements with TDD 15 kHz duplex mode.  Proposal #5: For HST PDSCH CA tests define the following applicability rule on CA duplex modes for testing: If UE supports both FDD 15 kHz + TDD 30 kHz and FDD 15 kHz + FDD 15 kHz CA duplex modes, apply requirements only to the first one.  Proposal #6: Make HST PDSCH CA requirements release independent from Rel-15.  Proposal #7: Do not define new network assistant signalling and UE capability for HST CA operation. |
| [**R4-2106808**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2106808.zip) | Discussion on PDSCH CA scenarios for NR UE HST FR1 performance requirements | Huawei, HiSilicon | Observation 1: Existing HST network assisted signaling and UE capability can cover CA scenario.  Proposal 1: For HST-DPS, considering DPS with both one and two active TCI(s). Reuse the applicability rule between the two DPS schemes from single carrier.  Proposal 2: Define applicability rule that UE has passed DPS CA requirements can skip SFN CA requirements.  Proposal 3: PDSCH is not scheduled on ‘S’ slots under HST-SFN propagation condition for HST CA requirements.  Proposal 4: Do not consider TDD 15 kHz for HST CA requirements.  Proposal 5: Reuse CA CQI applicability rule on CA duplex modes for testing.  Proposal 6: Not define release independent for HST CA requirements.  Proposal 7: Do not introduce extra UE capability or network-assisted signaling for SCell for HST CA scenario. |
| [**R4-2106809**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2106809.zip) | Simulation results for PDSCH CA scenarios for NR UE HST FR1 performance requirements | Huawei, HiSilicon |  |
| [**R4-2106862**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2106862.zip) | Initial simulation result of PDSCH for CA in HST | Ericsson |  |
| [**R4-2106863**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2106863.zip) | PDSCH demodulation requirements for CA with HST-SFN scenario | Ericsson | Proposal 1: Define PDSCH demodulation requirements for HST-DPS for CA with the applicability rule.  Proposal 2: If UE is capable of HST-SFN advanced receiver (for CA) and UE passes the PDSCH with HST-SFN CA requirements, the UE can skip the PDSCH with HST-DPS CA requirements.  Proposal 3: For PDSCH CA demodulation in HST, RAN4 defines the following combinations only:  • FDD SCS=15kHz + FDD SCS=15kHz  • TDD SCS=30kHz + TDD SCS=30kHz  • FDD SCS=15kHz + TDD SCS=30kHz  Observation 1: highSpeedDemodFlag-r16 can be configured for SCell.  Proposal 4: Not to introduce a new network-assisted signaling to inform HST-SFN deployment for SCell.  Proposal 5: RAN4 confirm Rel-16 UE capability signaling demodulationEnhancement can be applicable for PDSCH CA scenario also.  Proposal 6: RAN4 need to discuss further the new UE demodulation requirements for HST-SFN CA are release independent Rel-15 or not, depending on the applicability of Rel-16 UE capability for HST-SFN advanced receiver.  Proposal 7: RAN4 need to discuss further the new UE demodulation requirements for HST-DPS CA are release independent Rel-15 or not. |
| [**R4-2107041**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2107041.zip) | Views on FR1 HST PDSCH CA Tests | Qualcomm Incorporated | Proposal 1: If UE passes the FR1 HST PDSCH CA tests for HST-SFN scheme, tests with HST-DPS scheme can be skipped.  Proposal 2: Do not define FR1 HST PDSCH CA tests for Duple/SCS combinations involving TDD 15kHz.  Proposal 3: Reuse CA CQI applicability rule on CA duplex modes for testing: If UE supports both FDD 15 kHz + TDD 30 kHz and FDD 15 kHz + FDD 15 kHz CA duplex modes, FDD 15kHz + FDD 15kHz CA tests can be skipped. |
| R4-2104923 | Discussion on PDSCH requirements for CA in FR1 HST | ZTE Corporation | Proposal 1 : It could define CA requirements for DPS scheme.  Proposal 2 : Do not define a new HST network assisted signaling or UE capability for HST CA scenario |

## Open issues summary

### Test parameters for CA scenario

**Issue 2-1-1: Transmission schemes**

* Agreements in RAN4#98e meeting:
* Define HST CA requirements for HST-SFN joint transmission
* FFS whether to define HST CA requirements for DPS transmission scheme (with one active TCI state and/or two active TCI states)
  + It’s RAN4 common understanding DPS scheme can achieve better performance compared to joint transmission schemes and no advanced received required for HST deployment.
  + Candidate option for further discussion:
    - It’s RAN4 recommendation to include DPS scheme into FR1 HST WI, and further discuss whether test cases need to specified or not, and if specified, test applicable rules will be specified to ensure only one scheme will be verified for CA cases for UE.
* Agreements in RAN#91e meeting:
  + Specify the UE demodulation requirements for CA scenario with the same target speed (up to 500km/h) and carrier frequency (up to 3.6 GHz) as Rel-16 NR HST for HST-SFN joint transmission scheme and DPS transmission scheme.
    - Requirements/tests applicability rules should be discussed in order to minimize the testing burden.
* Proposals in RAN4#98bis-e meeting:
  + Option 1 (Apple): Introduce requirements for CA for HST-DPS with one active TCI state only.
  + Option 2 (Huawei, Intel): For HST-DPS, considering DPS with both one and two active TCI(s). Reuse the applicability rule between the two DPS schemes from single carrier.
* Recommended WF
  + More discussion is needed.

**Issue 2-1-2: Special slot configuration**

* Proposals in RAN4#98bis-e meeting:
  + Option 1 (Huawei): PDSCH is not scheduled on ‘S’ slots under HST-SFN propagation condition for HST CA requirements.
* Recommended WF
  + Can we agree that PDSCH is not scheduled on “S” slot under HST-SFN propagation condition?

**Issue 2-1-3: SCS configurations**

* Agreements in RAN4#98e meeting:
* *At least cover following cases:*
  + *FDD 15 kHz + FDD 15 kHz*
  + *TDD 30 kHz + TDD 30 kHz*
  + *FDD 15 kHz + TDD 30 kHz*
* *FFS whether following need to be included or not:*
  + *FDD 15 kHz + TDD 15 kHz CA*
  + *TDD 15 kHz + TDD 30 kHz CA*
* Proposals in RAN4#98bis-e meeting:
  + Option 1 (Apple, Intel, Huawei, Ericsson, Qualcomm): Do not introduce requirements in HST for FDD 15KHz + TDD 15KHz CA and TDD 15 kHz + TDD 30 kHz CA.
  + Option 2 (CMCC): FDD 15 kHz + TDD 15 kHz CA and TDD 15 kHz + TDD 30 kHz CA are covered, and the applicability rule between CA scenario with TDD 15 kHz SCS and CA scenario with TDD 30 kHz SCS specified in Rel-16 can be reused
  + Option 3 (CMCC): FDD 15 kHz + TDD 15 kHz CA and TDD 15 kHz + TDD 30 kHz CA are precluded, and no applicability rule for FDD 15 kHz + FDD 15 kHz CA, TDD 30 kHz + TDD 30 kHz CA and FDD 15 kHz + TDD 30 kHz CA (i.e. it is not preferred to reuse CA CQI applicability rule to PDSCH CA normal demodulation requirements)
* Recommended WF
  + 5 companies support not defining TDD 15KHz for CA scenario. 1 company propose two options and would like to discuss TDD 15KHz together with the applicability rule for SCS configuration (issue 2-2-1). More discussion is needed.

### Applicabiliy rule

**Issue 2-2-1: Applicability rule for SCS configuration**

* Agreements in RAN4#98e meeting:
  + FFS whether reuse CA CQI applicability rule on CA duplex modes for testing: If UE supports both FDD 15 kHz + TDD 30 kHz and FDD 15 kHz + FDD 15 kHz CA duplex modes, apply requirements only to the first one
* Proposals in RAN4#98bis-e meeting:
  + Option 1 (Apple, Intel, Huawei, Qualcomm): Use same applicability rule on CA duplex mode for HST CA as CA CQI requirements.
  + Option 2 (CMCC): Do not reuse CA CQI applicability rule to PDSCH CA normal demodulation requirements
* Recommended WF
  + More discussion is needed.

**Issue 2-2-2: Applicability rule for HST-SFN joint transmission scheme and DPS transmission scheme**

* Agreements in RAN#91e meeting:
  + Specify the UE demodulation requirements for CA scenario with the same target speed (up to 500km/h) and carrier frequency (up to 3.6 GHz) as Rel-16 NR HST for HST-SFN joint transmission scheme and DPS transmission scheme.
    - Requirements/tests applicability rules should be discussed in order to minimize the testing burden.
* Proposals in RAN4#98bis-e meeting:
  + Option 1 (Apple, Intel, Ericsson, Qualcomm): Define applicability rule for CA requirements in HST scenario as - If UE supports demodulationEnhancement-r16, only HST-SFN JT requirements shall apply, otherwise HST-DPS requirements shall apply for CA.
  + Option 2 (CMCC): considering that HST-SFN joint transmission scheme and DPS transmission scheme are different transmission schemes, not sure whether we can specify the applicability rule between HST-SFN joint transmission scheme and DPS transmission scheme for CA scenario.
  + Option 3 (DOCOMO):
    - If UE pass Rel-17 DPS CA tests, Rel-17 HST-SFN CA tests can be skipped
    - If UE pass Rel-17 HST-SFN CA tests, Rel-17 DPS CA tests can be skipped
  + Option 4 (Huawei):
    - Define applicability rule that UE has passed DPS CA requirements can skip SFN CA requirements.
* Recommended WF
  + More discussion is needed.

**Issue 2-2-3: Applicability rule between single carrier and CA**

* Proposals in RAN4#98bis-e meeting:
  + Option 1 (Intel): UE can skip single carrier test case if it has passed corresponding CA test case.
* Recommended WF
  + More discussion is needed.

### Release independent

**Issue 2-3-1: Release independent**

* Agreements in RAN4#98e meeting:
  + FFS whether HST PDSCH CA requirements can be release independent from Rel-15
* Proposals in RAN4#98bis-e meeting:
  + Option 1 (CMCC, DOCOMO, Intel): it is proposed that Rel-17 FR1 HST PDSCH CA requirements are release independent from Rel-15.
  + Option 2 (Huawei): Not define release independent for HST CA requirements.
  + Option 3 (Ericsson):
    - RAN4 need to discuss further the new UE demodulation requirements for HST-SFN CA are release independent Rel-15 or not, depending on the applicability of Rel-16 UE capability for HST-SFN advanced receiver.
    - RAN4 need to discuss further the new UE demodulation requirements for HST-DPS CA are release independent Rel-15 or not.
* Recommended WF
  + More discussion is needed.

### UE capability and network-assisted signalling

**Issue 2-4-1: UE capability and network-assisted signalling**

* Agreements in RAN4#98e meeting:
* FFS whether existing HST network assisted signaling and UE capability can cover CA scenario
* Proposals in RAN4#98bis-e meeting:
  + *Option 1 (Intel, Huawei, Ericsson, ZTE):* Do not define new network assistant signalling and UE capability for HST CA operation
* Recommended WF
  + Do not define new network assistant signalling and UE capability for HST CA operation
  + Rel-16 network assistant signalling and UE capability signalling can be applicable for PDSCH CA scenario

### Channel Model

**Issue 2-5-1: Channel model for HST-DPS**

* Proposals in RAN4#98bise meeting (R4-2104844, Apple):
  + Observation #1: The deployment parameters for HST-SFN JT and HST-DPS are the same, yet HST-DPS doesn’t consider time varying path power or delay.
  + Observation #2: With modified channel model for HST-DPS with time varying path power or delay, we observe 2dB degradation in performance for 2x2.
  + Observation #3: For HST-DPS the visibility is 1 RRH and UE will not be able to measure L1-RSRP or track TRS from next RRH prior to TCI state switch.
  + Proposal #5: RAN4 further evaluates if HST-DPS channel model is practical in actual deployment and update the channel model if necessary.
* Recommended WF
  + Companies please provide your views on the new proposal for HST-DPS channel model.

## Companies views’ collection for 1st round

### Open issues

|  |  |
| --- | --- |
| **Company** | **Comments** |
| **Ericsson** | Issue 2-1-1:  Option 2. We prefer to use the same applicability rule as single carrier case.  Issue 2-1-2:  Support the recommended WF.  Issue 2-1-3:  Option 1. RAN plenary agreed to include DPS for PDSCH CA demodulation requirements, but WID also adds the note the requirements/tests applicability rules should be discussed in order to minimize the testing burden. Since RAN4 has already included TDD 15kHz in Rel-16 PDSCH CA demodulation, we don’t need to repeat it for Rel-17 HST scenario.  Issue 2-2-2:  Option 1 or Option 3. We understand Rel-16 HST does not define the applicability rule between HST-DPS and HST-SFN JT. But we are discussing the CA scenario. We think it is possible to consider the applicability rule between CA HST-SFN JT and CA HST-DPS.  We are also fine with Option 3, because it is more generic, and we think this option includes both Options 1 and 4.  Issue 2-2-3:  We need discuss the applicability of CA case and single carrier case carefully, depending on the conclusion of the applicability between CA HST-SFN and CA HST-DPS.  This is our preference:   * If UE pass Rel-17 DPS CA tests:   + Rel-17 HST-SFN CA tests can be skipped.   + Rel-16 DPS single carrier tests can be skipped.   + Rel-16 HST-SFN single carrier tests should be passed if UE has capability. * IF UE pass Rel-17 HST-SFN CA tests:   + Rel-17 DPS CA tests can be skipped.   + Rel-16 HST-SFN single carrier tests can be skipped.   + Rel-16 DPS single carrier tests should be passed.   We may need to check the impact to other HST test cases such as HST single tap etc.  Issue 2-3-1:  Option 3. First we need to confirm whether the UE capability of HST-SFN advanced receiver can be applicable for CA. If yes, we are fine the HST-SFN CA demodulation requirements are release independent from Rel-15 (or Rel-16 if companies have concern).  Issue 2-4-1:  Support the recommended WF.  Issue 2-5-1:  We agree with the observations by Apple, but we prefer to keep the existing SNR definition for HST-DPS. If RAN4 need to update the HST-DPS according to the actual deployment, we think RAN4 also need to update the existing HST single tap model since this model keeps the same delay and path power.  Also the existing RAN4 UE demodulation requirements use the SNR to achieve 30%/70% of the maximum throughput, so we would like to keep the same signal power level during the tests, if UE receives PDSCH only from one transmission point. |

### CRs/TPs comments collection

|  |  |
| --- | --- |
| **CR tdoc number** | **Comments collection** |
|  |  |
|  |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
|  |  |

*Recommendations on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title** | **Assigned Company,**  **WF or LS lead** |
|  |  |  |

## Discussion on 2nd round (if applicable)

### Open issues summary

### Open issues

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |

## Summary on 2nd round (if applicable)

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation** |
|  |  |

# Topic #3: Enhanced transmisison schemes

*Agenda 8.6.3.3*

## Companies’ contributions summary

|  |  |  |  |
| --- | --- | --- | --- |
| **TDoc** | **Title** | **Source** | **Proposals/ Observations** |
| [**R4-2104845**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2104845.zip) | On Enhanced transmission schemes for HST | Apple | Observation #1: The performance with multi-DCI transmission scheme is comparable to DPS for HST.  Proposal #1: Do not introduce requirements with enhanced transmission scheme for HST.  Proposal #2: RAN4 further discuss the channel model for multi-TRP transmission in HST. |
| [**R4-2106432**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2106432.zip) | Views on HST PDSCH performance requirements for multi-DCI based Tx scheme | Intel Corporation | Observation #1: Propagation conditions for each PDSCH scheduled in multi-DCI based Tx scheme in Rel-16 HST-SFN deployment are determined by two tap channel model with time-variant characteristics.  Observation #2: Propagation conditions with multi-DCI Tx scheme and JT scheme are quite similar.  Proposal #1: Do not define performance requirements for multi-DCI based Tx scheme in HST-SFN scenario. |
| [**R4-2106810**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2106810.zip) | Discussion on enhanced transmission schemes for NR UE HST FR1 performance requirements | Huawei, HiSilicon | Proposal 1: Do not consider full overlapping or partially overlapping cases for multi-DCI based multi-TRP.  Proposal 2: Use changed SNR for different time and different RRH for the non-overlapping case, if multi-DCI based multi-TRP requirements are defined.  Proposal 3: Do not scheduled PDSCH in ‘S’ slot, if multi-DCI based multi-TRP requirements are defined.  Proposal 4: Do not consider extra time/frequency offset or calculate them into the total frequency/time offset to ensure the total frequency/time offset is within the UE capability, if multi-DCI based multi-TRP requirements are defined.  Proposal 5: Use total maximum frequency offset of 870Hz for 15KHz SCS, 1667Hz for 30 KHz SCS respectively, if multi-DCI based multi-TRP requirements are defined.  Proposal 6: Do not define requirements multi-DCI based multi-TRP under HST scenario. |
| [**R4-2106811**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2106811.zip) | Simulation results for evaluations of enhanced transmission schemes for NR UE HST FR1 performance requirements | Huawei, HiSilicon | Observation 1: Bad performance using multi-DCI based multi-TRP when UE near the RRH.  Observation 2: DPS is better than multi-DCI based multi-TRP all the time from the perspective of throughput.  Observation 3: Total frequency offset over than 870Hz for 15 kHz SCS will cause the “frequency wrap” then leads to the significant performance degradation.  Observation 4: Maximum throughput cannot achieved for multi-DCI based multi-TRP with MCS 17 and TDD 30 kHz regardless the value of timing offset. |
| [**R4-2106864**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2106864.zip) | PDSCH demodulation requirements with enhanced transmission schemes in HST scenario | Ericsson | Observation 1: mDCI-based PDSCH transmission cannot achieve the maximum throughput when the HST-SFN channel model is applied.  Observation 2: Larger time difference between two TRPs in HST-SFN channel model degrades the UE demodulation performance for the multi-DCI based transmission.  Observation 3: mDCI-based transmission scheme with HST-SFN deployment scenario shows worse performance compared with HST-SFN JT/HST-DPS scenario.  Proposal: RAN4 need more discussion/study whether to define mDCI-based transmission in HST-SFN deployment scenario. |
| [**R4-2107043**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2107043.zip) | Views on FR1 HST Enhanced Transmission Schemes | Qualcomm Incorporated | Proposal 1: Use HST-DPS scheme as reference for evaluating Multi-DCI scheme for FR1 HST.  Proposal 2: Use SNR at 70% of max achievable throughput as evaluation metric for Multi-DCI scheme.  ~~Proposal 3: Do not consider non-overlapping allocation for evaluation of Multi-DCI scheme for FR1 HST.~~ |
| [**R4-2107092**](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2107092.zip) | Discussion on multi-DCI transmission scheme for FR1 HST | MediaTek inc. | Observation 1: When UE is near one RRH, there is a large power imbalance for two TBs and the received SNR for one of two TBs is very low.  Observation 2: When UE is near one RRH, the maximum reception timing difference from two RRHs for multi-DCI based transmission is close to the CP length for SCS=30kHz.  Proposal 1: Fixed MCS simulation is not proper for performance evaluation and we may need further discussion about the performance evaluation method. |

## Open issues summary

**Issue 2-1: Whether to specify PDSCH requirements for multi-DCI transmission scheme**

* Agreements in RAN4#98e meeting:
  + Firstly, focus on the study and evaluate the performance benefits of transmission scheme 2 in HST-SFN deployment comparing to other transmission schemes.
* Proposals in RAN4#98bis-e meeting:
  + Option 1 (Apple, Intel, Huawei): Do not introduce requirements for multi-DCI based transmission scheme for HST
  + Option 2 (Ericsson): RAN4 need more discussion/study whether to define mDCI-based transmission in HST-SFN deployment scenario
* Recommended WF
  + Suggest following last meeting agreements. More evaluation is needed.

**Issue 2-2: Deployment Parameters**

* Agreements in RAN4#98e meeting:
  + Set Ds=700m and Dmin=150m as baseline
  + Take maximum Doppler frequency “870Hz for 15KHz SCS, 1667Hz for 30KHz SCS” as baseline
    - Further check whether Doppler/timing offset may exceed maximum UE capability with the assumption of Non-ideal synchronization
* Proposals in RAN4#98bis-e meeting:
  + Option 1 (Huawei):
    - Use total maximum frequency offset of 870Hz for 15KHz SCS, 1667Hz for 30 KHz SCS respectively, if multi-DCI based multi-TRP requirements are defined.
    - Do not consider extra time/frequency offset or calculate them into the total frequency/time offset to ensure the total frequency/time offset is within the UE capability, if multi-DCI based multi-TRP requirements are defined
* Recommended WF
  + Can we agree with the following recommended WF?
    - Set Ds=700m and Dmin=150m as baseline
    - Take maximum Doppler frequency “870Hz for 15KHz SCS, 1667Hz for 30KHz SCS” as baseline

**Issue 2-3: Reference performance for comparison**

* Agreements in RAN4#98e meeting:
  + Option 1: mDCI-based transmission vs. HST-SFN joint transmission
  + Option 2: mDCI-based transmission vs. HST-DPS
  + Other options are not precluded
* Proposals in RAN4#98bis-e meeting:
  + Option 1 (Qualcomm): Use HST-DPS scheme as reference for evaluating Multi-DCI scheme for FR1 HST.
* Recommended WF
  + More discussion is needed.

**Issue 2-4: PDSCHs allocations between different RRHs**

* Agreements in RAN4#98-e meeting:
  + Baseline assumption for evaluation: reuse the same PRB allocation as Rel-16 eMIMO multi-DCI based transmission, i.e., overlapped in time domain but not overlapped in frequency domain
  + FFS whether to consider both overlapped and non-overlapped PDSCHs allocations between different RRHs for performance analysis
* Proposals in RAN4#98bis-e meeting:
  + Option 1 (Huawei, Qualcomm): Do not consider full overlapping or partially overlapping cases for multi-DCI based multi-TRP.
  + ~~Option 2 (Qualcomm): Do not consider non-overlapping allocation for evaluation of Multi-DCI scheme for FR1 HST.~~
* Recommended WF
  + More discussion is needed

**Issue 2-5: SNR definition**

* Proposals in RAN4#98bis-e meeting:
  + Option 1 (Huawei): Use changed SNR for different time and different RRH for the non-overlapping case, if multi-DCI based multi-TRP requirements are defined.
* Recommended WF
  + More discussion is needed

**Issue 2-6: MCS**

* Agreements in RAN4#98e meeting:
  + MCS 13 and MCS 17 as baseline assumption for further evaluations
  + For mDCI-based transmission vs. HST-SFN joint transmission, use MCS13
  + For mDCI-based transmission vs. HST-DPS, use MCS 17
  + Note: which MCS is adopted depends on the outcome of the discussion on Reference performance for comparison
* Proposals in RAN4#98bis-e meeting:
  + Option 1 (MTK): Fixed MCS simulation is not proper for performance evaluation and we may need further discussion about the performance evaluation method.
* Recommended WF
  + More discussion is needed

**Issue 2-7: Evaluation Criteria**

* Agreements in RAN4#98e meeting:
* Option 1: Max achievable throughput across all scheduled TB
  + Different train locations and SNR points should be analyzed
* Option 2: SNR at 70% @max achievable throughput
* Option 3: Max supported Doppler frequency
* Other options are not precluded
* Proposals in RAN4#98bis-e meeting:
  + Option 1 (Qualcomm): Use SNR at 70% of max achievable throughput as evaluation metric for Multi-DCI scheme.
* Recommended WF
  + More discussion is needed

**Issue 2-8: Special slot configuration**

* Proposals in RAN4#98bis-e meeting:
  + Option 1 (Huawei): Do not scheduled PDSCH in ‘S’ slot, if multi-DCI based multi-TRP requirements are defined.
* Recommended WF
  + Can we agree with above option1?

**Issue 2-9: Channel model**

* Proposals in RAN4#98bis-e meeting:
  + Option 1 (Apple): Further discuss channel model for mTRP transmission in HST-SFN
* Recommended WF
  + Discuss along with issue 2-5-1.

## Companies views’ collection for 1st round

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Ericsson | Issue 2-1:  According to our evaluation, we don’t see performance benefit with mDCI-based transmission in HST-SFN scenario, compared with Rel-16 HST-SFN JT and DPS.  We support Option 1, not introduce PDCSH demodulation requirements for multi-DCI based transmission scheme for HST. |

### CRs/TPs comments collection

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
|  |  |

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation** |
|  |  |
|  |  |

*Suggestion on WF/LS assignment*

|  |  |  |
| --- | --- | --- |
|  | **WF/LS t-doc Title** | **Assigned Company,**  **WF or LS lead** |
| #1 |  |  |

## Discussion on 2nd round (if applicable)

### Open issues summary

### Open issues

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |

## Summary on 2nd round (if applicable)

|  |  |
| --- | --- |
| **CR/TP/LS/WF number** | **T-doc Status update recommendation** |
|  |  |