**3GPP TSG-RAN WG4 Meeting #99-e *R4-211xxxx***

Electronic meeting, May 19th-27th, 2021

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.141-2** | **CR** | **0327** | **rev** | 1 | **Current version:** | **17.1.0**  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | CR to TS 38.141-2 – Introduction of band n67 |
|  |  |
| ***Source to WG:*** | Ericsson |
| ***Source to TSG:*** | R4 |
|  |  |
| ***Work item code:*** | NR\_n67-Perf |  | ***Date:*** | 2021-05-24 |
|  |  |  |  |  |
| ***Category:*** | B |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Add band n67 |
|  |  |
| ***Summary of change:*** | Specify RF requirements for band n67 |
|  |  |
| ***Consequences if not approved:*** | The band will not be specified and no operation could be done in this band. |
|  |  |
| ***Clauses affected:*** | 6.7.4.5.1.2, 6.7.5.4.5.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **x** |  |  Other core specifications  | TS 38.104  |
| ***affected:*** | **x** |  |  Test specifications | TS 38.141-1 |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |

|  |  |
| --- | --- |
| ***This CR's revision history:*** |  |

###### *<Start**of the change>*

6.7.4.5.1.2 Wide Area BS Category B (Option 1)

For Category B operating band unwanted emissions, there are two options for the limits that may be applied regionally. option 1 is as follows.

For a *RIB* operating in Bands n5, n8, n12, n20, n26, n28, n29, n67, n71, emissions shall not exceed the maximum levels specified in table 6.7.4.5.1.2-1:

Table 6.7.4.5.1.2-1: Wide Area BS operating band unwanted emission limits
(NR bands ≤ 1 GHz) for Category B

|  |  |  |  |
| --- | --- | --- | --- |
| Frequency offset of measurement filter ‑3dB point, Δf | Frequency offset of measurement filter centre frequency, f\_offset | Test requirement (Note 1, 2, 4) | Measurement bandwidth |
| 0 MHz ≤ Δf < 5 MHz | 0.05 MHz ≤ f\_offset < 5.05 MHz | 3.8 dBm-7/5(f\_offset/MHz-0.05)dB | 100 kHz  |
| 5 MHz ≤ Δf <min(10 MHz, Δfmax) | 5.05 MHz ≤ f\_offset <min(10.05 MHz, f\_offsetmax) | -3.2 dBm | 100 kHz  |
| 10 MHz ≤ Δf ≤ Δfmax | 10.05 MHz ≤ f\_offset < f\_offsetmax  | -7 dBm (Note 3) | 100 kHz  |
| NOTE 1: For a BS supporting non-contiguous spectrum operation within any *operating band*, the emission limits within sub-block gaps is calculated as a cumulative sum of contributions from adjacent sub blocks on each side of the sub block gap, where the contribution from the far-end sub-block shall be scaled according to the measurement bandwidth of the near-end sub-block. Exception is f ≥ 10MHz from both adjacent sub blocks on each side of the sub-block gap, where the emission limits within sub-block gaps shall be ‑7 dBm/ 100 kHz.NOTE 2: For a *multi-band RIB* with Inter RF Bandwidth gap < 2\*ΔfOBUE the emission limits within the Inter RF Bandwidth gaps is calculated as a cumulative sum of contributions from adjacent sub-blocks or RF Bandwidth on each side of the Inter RF Bandwidth gap, where the contribution from the far-end sub-block or RF Bandwidth shall be scaled according to the measurement bandwidth of the near-end sub-block or RF Bandwidth.NOTE 3: The requirement is not applicable when Δfmax < 10 MHz.NOTE 4: The test requirement is derived from the basic limit a scaling factor of 9 dB and any applicable TT.NOTE 5: Void |

*<End of the change>*

###### *<Start**of the change>*

##### 6.7.5.4.5 Test requirement

6.7.5.4.5.1 Test requirement for *BS type 1-O*

The power of any spurious emission shall not exceed the test limits in table 6.7.5.4.5-1 for a BS where requirements for co-existence with the system listed in the first column apply. For a *multi-band RIB*, the exclusions and conditions in the Note column of table 6.7.5.4.5-1 apply for each supported *operating band*.

Table 6.7.5.4.5-1: BS spurious emissions test limits for BS for co-existence with systems operating in other frequency bands

| System type for NR to co-exist with | Frequency range for co-existence requirement | Test limit | Measurement bandwidth | Notes |
| --- | --- | --- | --- | --- |
| GSM900 | 921 – 960 MHz | -45.4 dBm | 100 kHz | This requirement does not apply to BS operating in band n8. |
|  | 876 – 915 MHz | -49.4 dBm | 100 kHz | For the frequency range 880-915 MHz, this requirement does not apply to BS operating in band n8, since it is already covered by the requirement in clause 6.7.5.3. |
| DCS1800 | 1805 – 1880 MHz | -35.4 dBm | 100 kHz | This requirement does not apply to BS operating in band n3.  |
|  | 1710 – 1785 MHz | -49.4 dBm | 100 kHz | This requirement does not apply to BS operating in band n3, since it is already covered by the requirement in clause 6.7.5.3. |
| PCS1900 | 1930 – 1990 MHz | -35.4 dBm | 100 kHz | This requirement does not apply to BS operating in band n2, n25 or band n70.  |
|  | 1850 – 1910 MHz | -49.4 dBm | 100 kHz | This requirement does not apply to BS operating in band n2 or n25 since it is already covered by the requirement in clause 6.7.5.3.  |
| GSM850 or CDMA850 | 869 – 894 MHz | -45.4 dBm | 100 kHz | This requirement does not apply to BS operating in band n5 or n26.  |
|  | 824 – 849 MHz | -49.4 dBm | 100 kHz | This requirement does not apply to BS operating in band n5 or n26, since it is already covered by the requirement in clause 6.7.5.3. |
| UTRA FDD Band I or | 2110 – 2170 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n1 or n65. |
| E-UTRA Band 1 or NR Band n1 | 1920 – 1980 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n1 or n65, since it is already covered by the requirement in clause 6.7.5.3. |
| UTRA FDD Band II or | 1930 – 1990 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n2 or n70.  |
| E-UTRA Band 2 or NR Band n2 | 1850 – 1910 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n2, since it is already covered by the requirement in clause 6.7.5.3. |
| UTRA FDD Band III or | 1805 – 1880 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n3. |
| E-UTRA Band 3 or NR Band n3 | 1710 – 1785 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n3, since it is already covered by the requirement in clause 6.7.5.3.  |
| UTRA FDD Band IV or | 2110 – 2155 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n66. |
| E-UTRA Band 4 | 1710 – 1755 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n66, since it is already covered by the requirement in clause 6.7.5.3. |
| UTRA FDD Band V or | 869 – 894 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n5 or n26.  |
| E-UTRA Band 5 or NR Band n5 | 824 – 849 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n5 or n26, since it is already covered by the requirement in clause 6.7.5.3. |
| UTRA FDD Band VI, XIX | 860 – 890 MHz  | -40.4 dBm | 1 MHz |  |
| or E-UTRA Band 6, 18, | 815 – 830 MHz  | -37.4 dBm | 1 MHz |  |
| 19 | 830 – 845 MHz | -37.4 dBm | 1 MHz |  |
| UTRA FDD Band VII or | 2620 – 2690 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n7. |
| E-UTRA Band 7 or NR Band n7 | 2500 – 2570 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n7, since it is already covered by the requirement in clause 6.7.5.3. |
| UTRA FDD Band VIII or | 925 – 960 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n8. |
| E-UTRA Band 8 or NR Band n8 | 880 – 915 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n8, since it is already covered by the requirement in clause 6.7.5.3. |
| UTRA FDD Band IX or | 1844.9 – 1879.9 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n3. |
| E-UTRA Band 9 | 1749.9 – 1784.9 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n3, since it is already covered by the requirement in clause 6.7.5.3. |
| UTRA FDD Band X or | 2110 – 2170 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n66 |
| E-UTRA Band 10 | 1710 – 1770 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n66, since it is already covered by the requirement in clause 6.7.5.3. |
| UTRA FDD Band XI or XXI or | 1475.9 – 1510.9 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n74 or n75. |
| E-UTRA Band 11 or | 1427.9 – 1447.9 MHz  | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75 or n76. |
| 21 | 1447.9 – 1462.9 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n74 or n75. |
| UTRA FDD Band XII or | 729 – 746 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n12. |
| E-UTRA Band 12 or NR Band n12 | 699 – 716 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n12, since it is already covered by the requirement in clause 6.7.5.3.For NR BS operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
| UTRA FDD Band XIII or | 746 – 756 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n13. |
| E-UTRA Band 13 or NR Band n13 | 777 – 787 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n13, since it is already covered by the requirement in clause 6.7.5.3. |
| UTRA FDD Band XIV or | 758 – 768 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n14. |
| E-UTRA Band 14 or NR Band n14 | 788 – 798 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n14, since it is already covered by the requirement in clause 6.7.5.3. |
| E-UTRA Band 17 | 734 – 746 MHz | -40.4 dBm | 1 MHz |  |
|  | 704 – 716 MHz | -37.4 dBm | 1 MHz | For NR BS operating in n29, it applies 1 MHz below the Band n29 downlink operating band (Note 5). |
| UTRA FDD Band XX or | 791 – 821 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n20 or n28. |
| E-UTRA Band 20 or NR Band n20 | 832 – 862 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n20, since it is already covered by the requirement in clause 6.7.5.3. |
| UTRA FDD Band XXII or | 3510 – 3590 MHz | -40 dBm | 1 MHz | This requirement does not apply to BS operating in Band n77 or n78. |
| E-UTRA Band 22 | 3410 – 3490 MHz | -37 dBm | 1 MHz | This requirement does not apply to BS operating in Band n77 or n78. |
| E-UTRA Band 24 or NR Band n24 | 1525 – 1559 MHz | -40.4 dBm | 1 MHz |  |
|  | 1626.5 – 1660.5 MHz | -37.4 dBm | 1 MHz |  |
| UTRA FDD Band XXV or | 1930 – 1995 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n2, n25 or n70. |
| E-UTRA Band 25 or NR band n25 | 1850 – 1915 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n25 since it is already covered by the requirement in clause 6.7.5.3. For BS operating in Band n2, it applies for 1910 MHz to 1915 MHz, while the rest is covered in clause 6.7.5.3. |
| UTRA FDD Band XXVI or | 859 – 894 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n5 or n26.  |
| E-UTRA Band 26 or NR Band n26 | 814 – 849 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n26 since it is already covered by the requirement in clause 6.7.5.3. For BS operating in Band n5, it applies for 814 MHz to 824 MHz, while the rest is covered in clause 6.7.5.3. |
| E-UTRA Band 27 | 852 – 869 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n5. |
|  | 807 – 824 MHz | -37.4 dBm | 1 MHz | This requirement also applies to BS operating in Band n28, starting 4 MHz above the Band n28 downlink *operating band* (Note 5). |
| E-UTRA Band 28 or | 758 – 803 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n20, n67 or n28. |
| NR Band n28 | 703 – 748 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n28, since it is already covered by the requirement in clause 6.7.5.3. For BS operating in band n67, it applies for 703 MHz to 736 MHz. |
| E-UTRA Band 29 or NR Band n29 | 717 – 728 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n29. |
| E-UTRA Band 30 or | 2350 – 2360 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n30. |
| NR Band n30 | 2305 – 2315 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n30, since it is already covered by the requirement in clause 6.7.5.3. |
| E-UTRA Band 31 | 462.5 -467.5 MHz | -40.4 dBm | 1 MHz |  |
|  | 452.5 -457.5 MHz | -37.4 dBm | 1 MHz |  |
| UTRA FDD band XXXII or E-UTRA band 32 | 1452 – 1496 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n74 or n75. |
| UTRA TDD Band a) or E-UTRA Band 33 | 1900 – 1920 MHz | -40.4 dBm | 1 MHz |  |
| UTRA TDD Band a) or E-UTRA Band 34 or NR band n34 | 2010 – 2025 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n34. |
| UTRA TDD Band b) or E-UTRA Band 35 | 1850 – 1910 MHz | -40.4 dBm | 1 MHz |  |
| UTRA TDD Band b) or E-UTRA Band 36 | 1930 – 1990 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n2 or n25. |
| UTRA TDD Band c) or E-UTRA Band 37 | 1910 – 1930 MHz | -40.4 dBm | 1 MHz |  |
| UTRA TDD Band d) or E-UTRA Band 38 or NR Band n38 | 2570 – 2620 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n38.  |
| UTRA TDD Band f) or E-UTRA Band 39 or NR band n39 | 1880 – 1920MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n39. |
| UTRA TDD Band e) or E-UTRA Band 40 or NR Band n40 | 2300 – 2400MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Bands n30 or n40. |
| E-UTRA Band 41 or NR Band n41 | 2496 – 2690 MHz | -40.4 dBm | 1 MHz | This is not applicable to BS operating in Band n41. |
| E-UTRA Band 42 | 3400 – 3600 MHz | -40 dBm | 1 MHz | This requirement does not apply to BS operating in Band n77 or n78. |
| E-UTRA Band 43 | 3600 – 3800 MHz | -40 dBm | 1 MHz | This requirement does not apply to BS operating in Band n77 or n78. |
| E-UTRA Band 44 | 703 – 803 MHz | -40.4 dBm | 1 MHz | This is not applicable to BS operating in Band n28. |
| E-UTRA Band 45 | 1447 – 1467 MHz | -40.4 dBm | 1 MHz |  |
| E-UTRA Band 46 | 5150 – 5925 MHz | -39.5 dBm | 1 MHz |  |
| E-UTRA Band 47 | 5855 – 5925 MHz | -39.5 dBm | 1 MHz |  |
| E-UTRA Band 48 | 3550 – 3700 MHz | -40 dBm | 1 MHz | This requirement does not apply to BS operating in Band n77 or n78. |
| E-UTRA Band 50 or NR Band n50 | 1432 – 1517 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75 or n76. |
| E-UTRA Band 51 or NR Band n51 | 1427 – 1432 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n75 or n76. |
| E-UTRA Band 53 or NR Band n53 | 2483.5 - 2495 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n41 or n90. |
| E-UTRA Band 65 or | 2110 – 2200 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n1 or n65.  |
| NR Band n65 | 1920 – 2010 MHz | -37.4 dBm | 1 MHz | For BS operating in Band n1, it applies for 1980 MHz to 2010 MHz, while the rest is covered in clause 6.7.5.3.This requirement does not apply to BS operating in band n65, since it is already covered by the requirement in clause 6.7.5.3. |
| E-UTRA Band 66 or | 2110 – 2200 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n66. |
| NR Band n66 | 1710 – 1780 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n66, since it is already covered by the requirement in clause 6.7.5.3. |
| E-UTRA Band 67 or NR Band n67 | 738 – 758 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n28 or n67. |
| E-UTRA Band 68 | 753 -783 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n28. |
|  | 698-728 MHz | -37.4 dBm | 1 MHz | For BS operating in Band n28, this requirement applies between 698 MHz and 703 MHz, while the rest is covered in clause 6.7.5.3. |
| E-UTRA Band 69 | 2570 – 2620 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n38. |
| E-UTRA Band 70 or | 1995 – 2020 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n2, n25 or n70 |
| NR Band n70 | 1695 – 1710 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n70, since it is already covered by the requirement in clause 6.7.5.3. |
| E-UTRA Band 71 or | 617 – 652 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n71 |
| NR Band n71 | 663 – 698 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n71, since it is already covered by the requirement in clause 6.7.5.3. |
| E-UTRA Band 72 | 461 – 466 MHz | -40.4 dBm | 1 MHz |  |
|  | 451 – 456 MHz | -37.4 dBm | 1 MHz |  |
| E-UTRA Band 74 or | 1475 – 1518 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n74 or n75. |
| NR Band n74 | 1427 – 1470 MHz | -37.4 dBm | 1MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75 or n76. |
| E-UTRA Band 75 or NR Band n75 | 1432 – 1517 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n74, n75 or n76. |
| E-UTRA Band 76 or NR Band n76 | 1427 – 1432 MHz | -40.4 dBm | 1 MHz | This requirement does not apply to BS operating in Band n50, n51, n75 or n76. |
| NR Band n77 | 3.3 – 4.2 GHz | -40 dBm | 1 MHz | This requirement does not apply to BS operating in Band n77 or n78 |
| NR Band n78 | 3.3 – 3.8 GHz | -40 dBm | 1 MHz | This requirement does not apply to BS operating in Band n77 or n78 |
| NR Band n79 | 4.4 – 5.0 GHz | -39.5 dBm | 1 MHz | This requirement does not apply to BS operating in Band n79 |
| NR Band n89 | 824 – 849 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n5, since it is already covered by the requirement in clause 6.7.5.3. |
| NR Band n95 | 2010 – 2025 MHz | -40.4 dBm | 1 MHz |  |
| NR Band n97 | 2300 – 2400MHz | -40.4 dBm | 1 MHz | NR Band n97 |
| NR Band n98 | 1880 – 1920MHz | -40.4 dBm | 1 MHz |  |
| NR Band n99 | 1626.5 – 1660.5 MHz | -37.4 dBm | 1 MHz | This requirement does not apply to BS operating in band n24, since it is already covered by the requirement in subclause 6.7.5.3. |

NOTE 1: As defined in the scope for spurious emissions in this clause, except for the cases where the noted requirements apply to a BS operating in Band n28, the co-existence requirements in 6.7.5.4.5-1 do not apply for the ΔfOBUE frequency range immediately outside the downlink *operating band* (see TS 38.104 [2], table 5.2-1). Emission limits for this excluded frequency range may be covered by local or regional requirements.

NOTE 2: Table 6.7.5.4.5-1 assumes that two *operating bands*, where the frequency ranges in TS 38.104 [2] table 5.2-1 would be overlapping, are not deployed in the same geographical area. For such a case of operation with overlapping frequency arrangements in the same geographical area, special co-existence requirements may apply that are not covered by the 3GPP specifications.

NOTE 3: TDD base stations deployed in the same geographical area, that are synchronized and use the same or adjacent *operating bands* can transmit without additional co-existence requirements. For unsynchronized base stations, special co-existence requirements may apply that are not covered by the 3GPP specifications.

NOTE 4: For NR Band n28 BS, specific solutions may be required to fulfil the spurious emissions limits for BS for co-existence with E-UTRA Band 27 UL *operating band*.

NOTE 5: For NR Band n29 BS, specific solutions may be required to fulfil the spurious emissions limits for NR BS for co-existence with UTRA Band XII, E-UTRA Band 12 or NR Band n12 UL operating band, E-UTRA Band 17 UL operating band.

*<End of the change>*