**3GPP TSG RAN WG1#100bis R1-2002753**

**e-Meeting, April 20th – 30th, 2020**

**Agenda item:** 7.2.6.1

**Source:** Moderator (Samsung)

**Title:** Feature lead summary for MU-MIMO CSI topic #2 (joint TP)

**Document for:** Discussion and Decision

1. Summary

Based on the discussion during the preparation phase summarized in [1], the following TP has been confirmed agreeable and can be endorsed:

TP for TS 38.214 V16.1.0

|  |  |  |
| --- | --- | --- |
| 5.2.2.2.5 Enhanced Type II Codebook**<**Unchanged text is omitted>- When :- For each subband in *csi-ReportingBand* that is not the first or last subband of a BWP, two precoding matrices are indicated by the PMI: the first precoding matrix corresponds to the first PRBs of the subband and the second precoding matrix corresponds to the last PRBs of the subband.- For each subband in *csi-ReportingBand* that is the first or last subband of a BWP- If , one precoding matrix is indicated by the PMI corresponding to the first subband. If , two precoding matrices are indicated by the PMI corresponding to the first subband: the first precoding matrix corresponds to the first PRBs of the first subband and the second precoding matrix corresponds to the last PRBs of the first subband.- If , one precoding matrix is indicated by the PMI corresponding to the last subband. If , two precoding matrices are indicated by the PMI corresponding to the last subband: the first precoding matrix corresponds to the first PRBs of the last subband and the second precoding matrix corresponds to the last PRBs of the last subband.**<**Unchanged text is omitted> vectors, , , are identified by (for ) and wherewhich are indicated by means of the indices (for ) and ( and ), , where**<**Unchanged text is omitted>For all values of , for . If , the nonzero elements of , identified by are found from , for , and from and , for , using as defined in Table 5.2.2.2.5-4 and the algorithm:**<**Unchanged text is omitted>When and are known, and are found as follows:- If , and is not reported. If , , for , and is not reported. If , , where is given in Table 5.2.2.2.5-4 and where the indices are assigned such that increases as increases.**<**Unchanged text is omitted>The codebooks for 1-4 layers are given in Table 5.2.2.2.5-5, where , , for are obtained as in clause 5.2.2.2.3, and the quantities and are given by**<**Unchanged text is omitted>**Table 5.2.2.2.5-5: Codebook for 1-layer. 2-layer, 3-layer and 4-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI‑RS****<**Unchanged text is omitted>

|  |
| --- |
| Where and the mappings from to , , , , , , , , and from to , , , , , and , , , and are as described above, including the ranges of the constituent indices of and .  |

**<**Unchanged text is omitted>5.2.2.2.6 Enhanced Type II Port Selection Codebook**<**Unchanged text is omitted>**Table 5.2.2.2.6-2: Codebook for 1-layer. 2-layer, 3-layer and 4-layer CSI reporting using antenna ports 3000 to 2999+*P*CSI‑RS****<**Unchanged text is omitted>

|  |
| --- |
| Where ,and the mappings from to, , , , , and from to , , , , , and , , , and are as described above, including the ranges of the constituent indices of and .  |

**<**Unchanged text is omitted> |

# References

1. R1-2002717 Feature lead summary for MU-MIMO CSI Moderator (Samsung)