**3GPP TSG RAN WG1 Meeting #100bis-E R1-200xxxx**

**e-Meeting, April 20 – 30, 2020**

**Source: Moderator (Intel Corporation)**

**Title: Summary of email discussions for NR Mobility Enhancements**

**Agenda item: 7.2.9**

**Document for: Discussion**

# Introduction

In this contribution, we summarize the email discussion approved for discussion during RAN1 #100bis-E. Chairman has approved three email discussion threads for RAN1 #100bis-E. The following are the approved email discussions:

* [100b-e-NR-Mob-Enh-01] Email discussion/approval on UL cancellation in UL DAPS-HO by 4/24; if necessary, followed by endorsing the corresponding TP by 4/30 – Daewon (Intel)
* [100b-e-NR-Mob-Enh-02] Email discussion/approval on power sharing mode for UL DAPS-HO by 4/23; if necessary, followed by endorsing the corresponding TP by 4/29 – Daewon (Intel)
* [100b-e-NR-Mob-Enh-03] Email discussion/approval on PDCCH/PDSCH restrictions for DL DAPS-HO by 4/22; if necessary, followed by endorsing the corresponding TP by 4/28 – Daewon (Intel)

# Email Discussion [100b-e-NR-Mob-Enh-01]

[Copy discussion from the document for email thread-01]

# Email Discussion [100b-e-NR-Mob-Enh-02]

[Copy discussion from the document for email thread-02]

# Email Discussion [100b-e-NR-Mob-Enh-03]

This discussion is regarding the PDCCH/PDSCH restrictions for DL DAPS-HO (Issue #1 from [11]).

**Issue and Proposal Summary:**

Proposal from [1] is to define a separate capability for UE that can process overlapping resources from source and target cell in intra-frequency DAPS HO. The motivation for introducing a new capability is not force certain UEs to be able to process DL signals that overlap in time and frequency resources, which can be difficult in some scenarios without SIC techniques. The following are the proposals made:

* Proposal by Huawei [1]: Restrict the minimum UE capability of DAPS-HO to FDMed simultaneous reception from source and target cells on overlapping OFDM symbols.
* Proposal by Huawei [1]: Introduce additional UE feature simultaneousRxOnOverlappedfreqAndtime to indicate the support of simultaneous reception from source and target cells on overlapped time and frequency resources.
* Adopt the following TP [1]:

|  |
| --- |
| **15 Dual active protocol stack based handover**If a UE indicates a capability for dual active protocol stack based handover (DAPS HO), the UE can be provided with a source MCG and a target MCG. The UE may expect to receive one PDCCH associated to one MCG to schedule one PDSCH, where the full scheduling information for receiving a PDSCH is indicated and carried only by the corresponding PDCCH.If a UE does not indicate a capability *simultaneousRxOnOverlappedfreqAndtime* for simultaneous reception on overlapped frequency resources and is configured with a source MCG and a target MCG, the UE does not expect:* the set of frequency resources provided by higher layer parameter *frequencyDomainResources* in a *ControlResourceSet* in a source MCG to overlap with the set of frequency resources provided by *frequencyDomainResources* in a *ControlResourceSet* in a target MCG and,
* to receive a PDSCH scheduled by a corresponding PDCCH sent by the source MCG to be located in frequency resources overlapping with a PDSCH scheduled by a corresponding PDCCH sent by the target MCG.

If the PDCCHs that schedule corresponding PDSCHs are associated to different MCGs, the UE procedure for receiving the PDSCH upon detection of a PDCCH follows Clause 5.1 in [5, TS 38.214]. |

**Discussion Summary:**

Companies are encouraged to provide comments on the proposal above. Comments should include views on whether proposals by Huawei [1] are acceptable or not. Also, if companies have a modified/reformulated proposal based on proposals from above companies, please do provide them below as well.

|  |  |
| --- | --- |
| Company Name | Comments/Views |
| Huawei/HiSilicon | We support this proposal.  |
| Ericsson | We would like to understand the motivation for the proposal. On one hand, less complex UE implementations are beneficial, but this proposal would lead to increased signaling load on the NW side.We understand that demodulating PDCCH/PDSCH in overlapping time/frequency resources would impact performance, but that is always the case on the cell border. To avoid the performance degradation, the NW may choose to configure non-overlapping frequency resources, but we do not see why the specification should prevent overlapping allocations from a performance point of view.From a complexity point of view, the UE would still have to perform two channel estimations, and two decodes even when the transmissions are non-overlapping, so we do not directly see the impact on complexity.Based on the information at hand, we are not supportive of the proposal. |
| MTK | We support this proposal.To our understanding, demodulating two PDCCHs/PDSCHs simultaneously in overlapping time/frequency resources is different from the case of cell border. On cell border, UE only demodulates the data from the source cell before the handover, and only demodulates the data from the target cell after the handover. UE is not required to demodulate two PDCCHs/PDSCHs simultaneously on cell border. To demodulate two PDCCHs/PDSCHs simultaneously on cell border in overlapping time/frequency resources, in additional to performing two channel estimations, UE also has to handle severe interference between source and target cells. The complexity falls on the interference cancellation rather than the channel estimation. To my understanding, this is discussed in multi-TRP session and some related techniques are discussed there to solve this problem. For a UE supporting DAPS HO, it may not support multi-TRP and demodulating two PDCCHs/PDSCHs simultaneously in overlapping time/frequency resources can impose prohibitively high complexity in UE implementation. NW may choose to configure non-overlapping frequency resources to help UE, but if this is not guaranteed, UE still needs to take the worst case into consideration for implementation. |
| Intel | We would like to get some clarification from the supporting companies on the matter.From our understanding, the receiver complexity between receiving and processing two PDCCH/PDSCH that are not overlapping in frequency but overlapping in time for the intra-frequency DAPS and receiving and processing two PDCCH/PDSCH that are overlapping in time/frequency for the intra-frequency DAPS are more or less the same.Unless successive interference cancellation processing is involved in both cases, UE need to perform channel estimation twice, equalization and demodulation twice, and decoding twice. Of course there will be implementation challenges to process both signals simultaneously, but as long they are to be processed at the same time (i.e. overlapping in time domain), the complexity should be comparable (if not the same).From our opinion, RAN4 will not define minimum performance requirement for this case with the understanding the UE need to implement a SIC receiver. This would be far from the baseline requirements needed for intra-frequency DAPS.Of course, we acknowledge that with SIC, the performance for intra-frequency DAPS would be bad. However, this would not be any better any regular HO, where UEs need to decode signals at cell-edge in the presence of interference from neighbor cells. The NW would need to ensure that lower code rates and modulation schemes are used such that it can combat the interference in such scenario.With this said, assuming RAN4 does not use SIC as the requirements for intra-frequency DAPS, what is the motivation to separate out capability for cases where UE needs to handle signals that overlap in time but not in frequency vs UE needs to handle signals that overlap in time and in frequency in the same carrier frequency (i.e. intra-frequency DAPS)? |
|  |  |
|  |  |

# Reference

1. R1-2001530, “Remaining issues on DAPS-HO,” Huawei, HiSilicon
2. R1-2001624, “Remaining issues on NR mobility enhancements in physical layer,” ZTE
3. R1-2002011, “Corrections to Physical layer aspects of NR mobility enhancement,” Intel Corporation
4. R1-2002148, “Remaining issues for NR Mobility Enhancement,” Samsung
5. R1-2002221, “Remaining physical layer aspects of dual active protocol stack based HO,” Nokia, Nokia Shanghai Bell
6. R1-2002344, “On remaining issues on NR mobility enhancements,” Apple
7. R1-2002490, “Correction to UL power sharing for DAPS HO,” Ericsson
8. R1-2002558, “Maintenance for NR mobility enhancements,” Qualcomm Incorporated
9. R1-2001531, “Remaining PHY aspects for CHO,” Huawei, HiSilicon
10. R1-2001625, “Discussion on FR2 mobility interruption enhancements,” ZTE
11. R1-2002010, “Issue Summary for NR Mobility Enhancements,” Moderator (Intel Corporation)