**3GPP TSG RAN WG1 #101 R1-200xxxx**

**e-Meeting, May 25th – June 5th, 2020**

Source: moderator (vivo)

Title: Feature lead summary on [101-e-NR-eMIMO-ULFPTx-02]

Agenda Item: 7.2.6.4

Document for: Discussion and Decision

1. Introduction

Per guidance from Mr. Chairman, this is to kick-off following email discussion, please provide your views below..

[101-e-NR-eMIMO-ULFPTx-02] TPs for correction on power scaling by 5/29 – Rakesh (vivo)

* TP 1, 2, 8 under Issues 2 of the FL summary

1. Remaining issues
   1. Issue 2 : TPs for correction on power scaling

TP#1

if *ul-FullPowerTransmission* in *PUSCH-Config* is provided and *codebookSubset* in *PUSCH-Config* is set to 'nonCoherent' or 'partialAndNonCoherent', the UE scales by where:

- if *ul-FullPowerTransmission* in *PUSCH-Config* is set to *fullpowerMode1*, and each SRS resource in the *SRS-ResourceSet* with *usage* set to 'codebook' has more than one SRS port, is the ratio of a number of antenna ports with non-zero PUSCH transmission power over the maximum number of SRS ports supported by the UE in one SRS resource

- if *ul-FullPowerTransmission* in *PUSCH-Config* is set to *fullpowerMode2*

- for full power TPMIs reported by the UE [16, TS 38.306], and is the ratio of a number of antenna ports with non-zero PUSCH transmission power over a number of SRS ports for remaining TPMIs, where the number of SRS ports is associated with a SRS resource indicated by a SRI field in a DCI format scheduling the PUSCH transmission if more than one SRS resource is configured in the *SRS-ResourceSet* with *usage* set to 'codebook', or the number of SRS ports is associated with the SRS resource if only one SRS resource is configured in the *SRS-ResourceSet* with *usage* set to 'codebook',

- if *ul-FullPowerTransmission* in PUSCH-Config is set to *fullpower*,

- if a SRS resource with a single port is indicated by a SRI field in a DCI format scheduling the PUSCH transmission when more than one SRS resource is provided in the *SRS-ResourceSet* with *usage* set to 'codebook', or if only one SRS resource with a single port is provided in the *SRS-ResourceSet* with *usage* set to 'codebook',

TP#2

if *ul-FullPowerTransmission* in *PUSCH-Config* is set to *fullpowerMode2*

- for full power TPMIs reported by the UE [16, TS 38.306], and is the ratio of a number of antenna ports with non-zero PUSCH transmission power over a number of SRS ports for remaining TPMIs, where the number of SRS ports is associated with a SRS resource indicated by a SRI field in a DCI format scheduling the PUSCH transmission if more than one SRS resource is configured in the *SRS-ResourceSet* with *usage* set to 'codebook', or the number of SRS ports is associated with the SRS resource if only one SRS resource is configured in the *SRS-ResourceSet* with *usage* set to 'codebook',

- , if a SRS resource with a single port is indicated by a SRI field in a DCI format scheduling the PUSCH transmission when more than one SRS resource is provided in the *SRS-ResourceSet* with *usage* set to 'codebook', or if only one SRS resource with a single port is provided in the *SRS-ResourceSet* with *usage* set to 'codebook', ~~and~~

- , if the SRS resource with 2 ports is indicated by SRI when *codebookSubset* in *PUSCH-Config* is set to 'partialAndNonCoherent' and one SRS resource with 4 ports and one SRS resource with 2 ports are configured in the *SRS-ResourceSet* with *usage* set to 'codebook', and

- if *ul-FullPowerTransmission* in PUSCH-Config is set to *fullpower*,

TP#8

if *ul-FullPowerTransmission* in *PUSCH-Config* is set to *fullpowerMode2*

- for full power TPMIs reported by the UE [16, TS 38.306], and is the ratio of a number of antenna ports with non-zero PUSCH transmission power over a number of SRS ports for remaining TPMIs, where the number of SRS ports is associated with a SRS resource indicated by a SRI field in a DCI format scheduling the PUSCH transmission if more than one SRS resource is configured in the *SRS-ResourceSet* with *usage* set to 'codebook', or indicated by Type 1 configured grant, or the number of SRS ports is associated with the SRS resource if only one SRS resource is configured in the *SRS-ResourceSet* with *usage* set to 'codebook',

- , if a SRS resource with a single port is indicated by a SRI field in a DCI format scheduling the PUSCH transmission when more than one SRS resource is provided in the *SRS-ResourceSet* with *usage* set to 'codebook', or indicated by Type 1 configured grant, or if only one SRS resource with a single port is provided in the *SRS-ResourceSet* with *usage* set to 'codebook', and

- if *ul-FullPowerTransmission* in PUSCH-Config is set to *fullpower*,

|  |  |
| --- | --- |
| Company | Comment |
| Intel | TP #1  The modification is not necessary. For Mode 1, there is no single port operation.  TP #2  The TP is not necessary. In Mode 2, for antenna virtualization to 2-port, the UE needs to report which 2-port TPMI could support full power transmission so that the gNB knows for which TPMI, power scaling factor of 1 should be applied.  TP #8  Fine with the proposal |
| Apple | TP #1: Not necessary. But we think this TP is also correct. Just different ways of specifying the same UE behaviour.  TP #2: Not needed. Isn’t this TP in conflict with the first sub-bullet in which s = #NZP ports/#ports indicated by SRI  TP #8: Fine with the proposal |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# References

[1] R1-2003402, “Feature lead summary on ULFPTx”, vivo, RAN1#101-e