**3GPP TSG RAN WG1 #105-e R1-210xxxx**

**e-Meeting, May 10th – 27th, 2021**

**Agenda item:** 7.2.11

**Source:** Moderator (NTT DOCOMO, INC.)

**Title:** Summary on [105-e-NR-UEFeature-Others-01]

**Document for:** Discussion and Decision

1. Introduction

This contribution summarizes the following email discussion.

[105-e-NR-UEFeature-Others-01] Email discussion/approval on UE features that are not dedicated to specific Rel-16 WI/TEI, till 5/24 (Hiroki, NTT DOCOMO)

* For FG22-10, add below sentence to the note.
  + For *pdcch-MonitoringAnyOccasionsWithSpanGap*, the supported set (set1, set2 or set 3) for cross-carrier scheduling with the different SCSs in the scheduling cell and the scheduled cell is still based on the indicated value for the band of the scheduling cell.

1. Discussion on New FGs that are not dedicated to a specific Rel-16 work item/TEI
   1. FG 22-10

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 22. NR Others | 22-10 | Support of pdcch-MonitoringAnyOccasionsWithSpanGap in case of cross-carrier scheduling with different SCSs in the scheduling cell and the scheduled cell | Support of pdcch-MonitoringAnyOccasionsWithSpanGap in case of cross-carrier scheduling with different SCSs in the scheduling cell and the scheduled cell   * Candidate values: {Interpretation2, Interpretation3} | 3-5b, 18-5 | Yes | N/A |  | Per UE | No | No | N/A | Candidate values: {Interpretation2, Interpretation3}  If UE indicates Interpretation2, it supports 22-10 as long as pdcch-MonitoringAnyOccasionsWithSpanGap is supported for the band of the scheduling/triggering/indicating cell.  If UE indicates Interpretation3, it supports 22-10 as long as pdcch-MonitoringAnyOccasionsWithSpanGap is supported in both the band of the scheduled/triggered/indicated cell and the band of the scheduling/triggering/indicating cell. | Optional with capability signalling |

Following proposal is made in a contribution.

|  |  |
| --- | --- |
| [1] | Below agreements were made in RAN1#104-e meeting.  ***Agreement***  *Regarding the interpretation of UE capabilities in case of cross-carrier operation, for cross-carrier scheduling with the same SCS in the scheduling cell and the scheduled cell, RAN1 clarifies that support of* pdcch-MonitoringAnyOccasionsWithSpanGap *is based on both the support of this capability for the band of the scheduled/triggered/indicated cell and the support of this capability for the band of the scheduling/triggering/indicating cell.*   * *Note: For pdcch-MonitoringAnyOccasionsWithSpanGap, the supported set (set1, set2 or set 3) for cross-carrier scheduling with the same SCS in the scheduling cell and the scheduled cell is still based on the indicated value for the band of the scheduling cell.*   ***Agreement***  *For cross-carrier scheduling with different SCSs in the scheduling cell and the scheduled cell, RAN1 introduces new Rel-16 UE capability to clarify the interpretation of* pdcch-MonitoringAnyOccasionsWithSpanGap *in case of cross-carrier operation.*   * *The detailed design of this new Rel-16 UE capability is to be discussed under Rel-16 UE feature session.*   ***Agreement***  *LS to RAN2 on interpretation of UE features in case of cross-carrier operation is endorsed in* [*R1-2102085*](https://www.3gpp.org/ftp/tsg_ran/TSG_RAN/TSGR_91e/Docs/R1-2102085.zip)  FG 22-10 was introduced to reflect the second agreement listed above. However, one minor issue to clarify for the FG is whether the number of spans/span-gap follow those of the scheduling cell or scheduled cell. We propose to follow the same principle as CCS with same SCS case (like the note in first agreement above).  **Proposal : For FG 22-10, add below sentence to the note column:**  **For *pdcch-MonitoringAnyOccasionsWithSpanGap*, the supported set (set1, set2 or set 3) for cross-carrier scheduling with the different SCSs in the scheduling cell and the scheduled cell is still based on the indicated value for the band of the scheduling cell.** |

Based on the above, following proposal can be discussed in RAN1#105-e meeting.

### **FL proposal #1**

* **For FG22-10, add below sentence to the note.**
  + **For *pdcch-MonitoringAnyOccasionsWithSpanGap*, the supported set (set1, set2 or set 3) for cross-carrier scheduling with the different SCSs in the scheduling cell and the scheduled cell is still based on the indicated value for the band of the scheduling cell.**

Companies are encouraged to check above FL proposal and to provide feedback if any in below. If you cannot accept the FL proposals, please put your company name after “Cannot accept the proposals” below and please provide your alternative proposal (in your comment) which could be acceptable to all in your consideration.

Cannot accept the proposal:

|  |  |
| --- | --- |
| Company | Comment |
| ZTE | Ok with the above FL proposal. |
|  |  |
|  |  |

1. Conclusion

TBD

Reference

[1] R1-2105790 Remaining details of Rel-16 NR UE features Ericsson

[2] R1-2105814 Remaining issues on NR Rel-16 UE features Nokia, Nokia Shanghai Bell

[3] R1-2104120 Updated RAN1 UE features list for Rel-16 NR after RAN1#104bis-e Moderators (AT&T, NTT DOCOMO, INC.)