Companies please share their inputs on the excel spreadsheet in ‘/tsg\_ran/WG1\_RL1/TSGR1\_106-e/Inbox/drafts/8.12.3/RRC Parameters/’.

## Inputs on version-000

Please share your inputs, if any, in the following table

|  |  |
| --- | --- |
| **Company** | **Input** |
| Qualcomm | For locationAndBandwidth-Broadcast,  The parameter is configured in a CFR for broadcast. It should be per CFR instead of per cell.  For pdsch-ConfigCommon-Broadcast,  We think it should be *pdsch-Config-Broadcast*, aligned with *pdsch-Config-Multicast* in a *CFR-Config-Multicast*. The parameters in *pdsch-Config-Broadcast* can be FFS. It is misleading to use *pdsch-ConfigCommon* with TDRA only for broadcast GC-PDSCH.  The parameter is configured in a CFR for broadcast. It should be per CFR instead of per cell.  For pcsch-ConfigCommon-Broadcast,  We think it should be *pdcch-Config-Broadcast*, aligned with *pdcch-Config-Multicast* in a *CFR-Config-Multicast*. The parameters in *pdcch-Config-Broadcast* can be FFS. It is misleading to use *pdcch-ConfigCommon* with CORESET/SS of RA/paging/SIB1 for broadcast GC-PDCCH.  The parameter is configured in a CFR for broadcast. It should be per CFR instead of per cell.  For searchSpaceBroadcast,  The parameter is configured in a CFR for broadcast. It should be per CFR instead of per cell. |
|  |  |

## Inputs on version-001

Please share your inputs, if any, in the following table

…