**3GPP TSG RAN WG1 Meeting #106-e R1-2108207**

**e-Meeting, August 16 – 27, 2021**

**Source: Moderator (Intel Corporation)**

**Title: Summary #1 of email discussion on initial access aspect of NR extension up to 71 GHz**

**Agenda item: 8.2.1**

**Document for: Discussion**

# Introduction

In this contribution, we discuss aspects related to initial access for extending NR up to 71 GHz based on submitted contributions to RAN1 #106-e. The main issues discussed in the following section for initial access are detailed design for synchronization signal block (SSB), CORESET#0, PRACH related issues, and discovery reference signal (DRS) related operations.

During the last RAN Plenary, the WID has been updated to reflect the approved numerologies for initial access. The following is copy of the WID objectives relevant for initial access.

|  |
| --- |
| * Physical layer aspects including [RAN1]:   + Support of up to 64 SSB beams for licensed and unlicensed operation in this frequency range.   + Supports 120kHz SCS for SSB and 120kHz SCS for initial access related signals/channels in an initial BWP.     - Study and specify, if needed, additional SCS (480kHz, 960kHz) for SSB for cases other than initial access.     - Note: coverage enhancement for SSB is not pursued.   + In addition to 120kHz, support 480 kHz SSB for initial access with support of CORESET#0/Type0-PDCCH configuration in the MIB with following constraints:     - Limited sync raster entry numbers       * It is assumed that RAN4 supports a channelization design which results in the total number of synchronization raster entries considering both licensed and unlicensed operation in a 52.6 – 71 GHz band no larger than 665 (Note: the total number of synchronization raster entries in FR2 for band n259 + n257 is 599). If the assumption cannot be satisfied, it’s up to RAN4 to decide its applicability to bands in 52.6 – 71 GHz.     - only 480kHz CORESET#0/Type0-PDCCH SCS supported for 480 kHz SSB SCS.     - Prioritize support SSB-CORESET#0 multiplexing pattern 1. Other patterns discussed on a best effort basis.     - 960 kHz numerology for the SSB is not supported by the UE for initial access in Rel-17.     - Note: Strive to minimize specification impact by reusing tables for CORESET#0 and type0-PDCCH CSS set configuration defined for FR2 in Rel-15, as much as possible     - Note: 480 kHz is an optional SSB numerology for initial access for the UE. A UE supporting a band in 52.6-71 GHz must at least support 120 kHz SCS (for initial access and after initial access)     - Note: Dependency or lack thereof for a UE supporting 480kHz and/or 960kHz numerology for data and control to also support 480kHz SSB numerology for initial access is to be tackled as part of UE capability discussion.   + Support ANR and PCI confusion detection for 120, 480 and 960kHz SCS based SSB, support CORESET#0/Type0-PDCCH configuration in MIB of 120, 480 and 960kHz SSB     - FFS: additional method(s) to enable support to obtain neighbour cell SIB1 contents related to CGI reporting     - Only 1 CORESET#0/Type0-PDCCH SCS supported for each SSB SCS, i.e., (120, 120), (480, 480) and (960, 960).     - Prioritize support SSB-CORESET#0 multiplexing pattern 1. Other patterns discussed on a best effort basis.     - Note: Strive to minimize specification impact by reusing tables for CORESET#0 and type0-PDCCH CSS set configuration defined for FR2 in Rel-15, as much as possible     - Note: From UE perspective, ANR detection for 480/960kHz SCS based SSB is not supported if the UE does not support 480/960 SCS for SSB.     - Note: for ANR, when reading the MIB, the cell containing the SSB is known to the UE, as defined in 38.133 specification.   + Specify support for PRACH sequence lengths (i.e. L=139, L=571 and L=1151) and study, if needed, specify support for RO configuration for non-consecutive RACH occasions (RO) in time domain for operation in shared spectrum |

# Summary of issues

## 2.1 SSB Aspects

### 2.1.1 DRS Related Aspects (and other MIB design other than CORESET#0/Type0-PDCCH)

* From [1] Huawei/HiSilicon:
  + For operation with shared spectrum and for 480 kHz and 960 kHz SSBs, indicate the 7th bit of the candidate SSB index by borrowing the 4th LSB of SFN in the PBCH payload. Indicate the 4th LSB of SFB in MIB payload.
  + Support discovery burst transmission window for all numerologies in shared spectrum in 52.6GHz to 71GHz.
  + If LBT on/off indication is deemed required to determine the size of DCI 1\_0 whose CRC scrambled with SI-RNTI, such an indication may be performed using one of the following methods:
    - Using one bit in MIB
    - Implicitly using the synch raster entry of the associated SSB used for initial access
  + Similar to Rel-16 NR-U, use the following method to implicitly indicate in SIB1 that DBTW is enabled/disabled:
    - If DBTW length is equal to or smaller than the time duration from the beginning of the half frame to the end of the slot containing the candidate SSB index N\_SSB^QCL-1, DBTW is disabled.
    - If DBTW length is larger than the time duration from the beginning of the half frame to the end of the slot containing the candidate SSB index N\_SSB^QCL -1, DBTW is enabled.
    - Note 1: DBTW is configured in SIB1 and N\_SSB^QCL is acquired from the MIB payload.
    - Note 2: Prior to reading SIB1, UE assumes that DBTW includes all candidate SSB positions in a half frame.
  + Values {8, 16, 32, 64} should be supported for N\_{SSB}^{QCL}\ in operation with shared spectrum above 52.6GHz.
  + Configure DBTW length in SIB1 for operation with shared spectrum in 52.6GHz to 71GHz with the following values:
    - 120 kHz SCS: {40, 32, 24, 16, 8, 4} slots = {5, 4, 3, 2, 1} ms
    - 480 kHz SCS: {72, 32, 24, 16, 8, 4} slots = {2.25, 1, 0.75, 0.5, 0.25, 0.125} ms
    - 960 kHz SCS: {64, 32, 24, 16, 8, 4} slots = {1, 0.5, 0.375, 0.25, 0.125, 0.0625} ms
  + In operation with shared spectrum in 60 GHz, for MSB k, k≥1, of inOneGroup and MSB m, m≥1, of groupPresense of ssb-PositionsInBurst:
    - if MSB k of inOneGroup and MSB m of groupPresense are set to 1, the UE assumes that SSB(s) within DBTW with candidate SSB index(es) corresponding to SSB index equal to k-1+(m-1)×8 may be transmitted;
    - if MSB k of inOneGroup or MSB m of groupPresense are set to 0, the UE assumes that the SSB(s) are not transmitted.
  + Regardless of the value of the MSB k of inOneGroup and MSB m of groupPresense in ssb-PositionsInBurst configured in SIB1, if , UE assumes that candidate SSB index(es) corresponding to SSB index equal to are not transmitted.
* From [2] vivo:
  + The following fields could be considered to indicate the value of Q in PBCH:
    - subCarrierSpacingCommon
    - LSB of ssb-SubcarrierOffset
    - Coreset#0 and Type#0 PDCCH indication
  + When DBTW is enabled with indicated value of Q, how to interpret the meaning of ssbPositionsInBurst should be studied.
  + More number of candidate SSBs should be specified for LBT case to alleviate LBT failure than non-LBT case.
  + Support DBTW in un-licensed band/LBT case from 52.6 GHz to 71 GHz for SSB with all supported SCSs.
  + The following methods could be considered to determine whether there is DBTW:
    - Alt. 1: GSCN (licensed or un-licensed);
    - Alt. 2: The indicator in PBCH;
  + Supported DBTW length as the same in NR-U, which is 0.5, 1, 2, 3, 4, 5 msec.
  + The number of candidate SSB positions for SCS 120 kHz and SCS 480 kHz should be 64 and 128 respectively.
  + LBT on/off is not indicated in MIB.
* From [3] Spreadtrum:
  + Confirm that DBTW is supported at least for 120kHz SCS.
* From [4] Interdigital:
  + Enhance the initial access operation to support Discovery Burst (DB) and Discovery Burst Transmission Window (DBTW) in unlicensed spectrum operations that require LBT in beyond 52.6GHz spectrum.
  + Consider indicating enable/disable of DBTW in initial access operations based on a sync raster offset used by SS/PBCH block.
  + Consider the enhancements to indicate the mode of operation regarding the enable/disable of the DBTW, on/off of the LBT, and the license regime based on the combination of Sync. raster offset and MSB of controlResourceSetZero.
  + Support enhancements on the reference tables in indication of Q parameter for up to 64 SSB beams in initial access operations for unlicensed spectrum in beyond 52.6GHz, e.g., subsamples of the Q parameter.
    - Support Alt A, for the total number of options for the Q parameter to not exceed 4.
* From [5] Sony:
  + Discovery Burst Transmission Window should be supported.
  + Enabling/disabling DBTW and should be signalled in MIB
    - Indication of disabling DBTW should be jointly coded with
      * Parameter to signal disabling DBTW and indicates {16, 32, 64, or disabling DBTW} if the number of candidate SSB position is more than 64
      * Parameter to signal disabling DBTW and indicates {8, 16, 32, or disabling DBTW} if the number of candidate SSB position is 64
  + Candidate SSB positions should be extended when DBTW is enabled.
    - For 120 kHz SCS,
      * The number of candidate SSB positions should be 80
      * additional n values (4, 9, 14, 19) should be supported when DBTW is enabled
    - For 480/960 kHz SCS,
      * The number of candidate SSB positions should be 128
      * First symbols of the candidate SSB have index {4, 8, 16,20} + 28\*n, where index 0 corresponds to the first symbol of the first slot in a half-frame
      * n = {0, 1, 2, 3, 5, 6, 7, 8, 10, 11, 12, 13, 15, 16, 17, 18} when DBTW is disabled.
      * n = 0 - 31 when DBTW is enabled
  + For indication of candidate SSB indices, QCL relation, and disabling DBTW, subCarrierSpacingCommon and reserved state of pdcchConfig-SIB1 should be used.
* From [6] Lenovo/Motorola Mobility
  + For NR operation in unlicensed bands between 52.6 GHz and 71 GHz, potential enhancements related to periodic transmission of DRS such as SSB/PBCH/CORESET#0 are needed including:
    - performing directional LBT prior to the transmission of SSB according to the ssb-PositionsInBurst
    - directional LBT on multiple beams at the same time at the beginning of the DRS window
    - Cat 2 LBT (depending on the gap) before actual transmission
* From [7] Samsung:
  + For 480 kHz and 960 kHz,
    - Support the same SS/PBCH block pattern in a slot, and the same pattern is given by Case A/C (i.e., Alt 1 with X=2 and Y=8).
    - Support larger number of slots including candidate SS/PBCH block, when DBTW is enabled.
  + Support discovery burst transmission window for all SCSs on the 60 GHz unlicensed spectrum.
    - The indication of Q can be in MIB for a best effort, and if not possible, in SIB1;
    - The indication of DBTW disabling can be joint coded with the indication of Q, if Q is indicated in MIB; and the indication can use 1 bit in MIB, if Q is not indicated in MIB;
    - The case of an unlicensed operation with DBTW disabled can be supported implicitly, by comparing the Q value and the DBTW window size;
    - Support more than 64 candidate SS/PBCH block locations within a half frame;
      * Current PBCH payload can support timing indication of up to 128 candidate SS/PBCH block candidate locations;
      * Use one PHY bit to indicate the extra candidate SS/PBCH block index (e.g. 7th LSB);
    - For initial access, different synchronization raster entries are applied for licensed and unlicensed operations; for non-initial access, support an explicit indication of licensed or licensed operation when configuring a cell.
* From [8] CATT:
  + The subCarrierSpacingCommon field in MIB can be saved and repurposed.
  + More than 64 SSB transmission opportunities shall be defined within a 5ms SSB burst set to support up to 64 beams for SSB beam sweeping in case of LBT failure. The issue of supporting additional bit(s) for the indicating SSB candidate index needs further study.
  + For no-LBT operation or licensed spectrum operation, value “n” can keep the same value as for the 120KHz SCS case.
  + Additional n value such as #4, #9, #14, and #19 can be used for new SSB candidates if LBT/DBTW is needed for SSB transmission.
  + For up to 71GHz operation and at least for NO-LBT operation, some values of ‘n’ can be reserved for uplink grant scheduling.
  + For NR operation in 60 GHz unlicensed spectrum, the discovery burst transmission window (DBTW) shall be supported for 120 KHz SSB at least when gNB configures more than 56 SSB transmissions.
  + DBTW is not needed for SSB with 480 KHz/960 KHz SCS since the duty cycle is less than 10% over the 100 ms observation window for the short control signaling transmissions.
  + For supporting DBTW of 120KHz SCS SSB, more than 64 SSB (up to a total of 80 ) positions are needed. A total of 7 bits of information is needed to indicate more than 64 SSB candidate locations.
  + For indication of （if needed at for 120kHz SSB）， legacy mechanism can be reused.
  + Considering Contention Exempt Short Control Signalling rules can be applicable to the transmission of SS/PBCH for most cases , only 5ms duration for DBTW operation is supported .
  + For 120 kHz SSB, signaling in MIB can indicate enable/disable of DBTW.
  + If LBT ON/OFF state is indicated in MIB/PBCH, joint coding can be used for indication of LBT ON/OFF, DBTW enabling/disabling and one bit information for candidate SSB index.
  + If LBT ON/OFF state is not indicated in MIB/PBCH, it can be indicated in DCI 1\_0 scrambled by SI-RNTI.
* From [9] ZTE/Sanechips:
  + Discovery burst transmission window (DBTW) should be supported for 120 kHz SSB SCS and other SSB SCSs.
  + In order to reduce the impact of standardization caused by indicating candidate SSB indices, the maximum number of candidate SSB defined in the half-frame can be kept unchanged (maintain 64) or limited to 128 for 480/960 kHz SSB SCS.
  + Four candidate values {8,16,32,64} for are preferred.
  + For 120 kHz SSB, enable/disable of DBTW can be indicated by comparing the value of  in MIB and DBTW length, and explicit signaling is not needed for this purpose.
* From [11] Ericsson:
  + Before RAN1 can agree that DBTW is supported, the following two aspects need to be jointly decided:
    - If and how additional candidate SSB positions are to be supported, and
    - How to signal the following: Q and DBTW on/off
  + Conclude that a DBTW is not supported for the 52.6 – 71 GHz band and that the size of DCI 1\_0 is the same regardless of channel access mode (Option 1). LBT on/off is signaled in SIB1.
* From [12] Futurewei:
  + For 480/960 kHz SS/PBCH DBTW should not be supported.
  + Support enabling and disabling LBT for channel access in shared spectrum, with LBT mode default enabled. Signal LBT disabled in the MIB.
  + For 480/960 kHz SS/PBCH SCS use the field subCarrierSpacingCommon to indicate LBT disabled.
  + For 120 kHz SS/PBCH SCS use the field subCarrierSpacingCommon and the LSB of ssb-SubcarrierOffset to indicate the N\_SSB^QCL, where one of the values indicates LBT disabled.



* + Use the following DBTW lengths values 0.5, 1, 2, 3, 4, 5 msec.
  + For 120 kHz SS/PBCH SCS use DBTW zero length in SIB1 to indicate that DBTW is disabled.
  + For 120kHz SSB the maximum number of candidate positions is 64.
  + Consider using CSI-RS presence in the discovery burst for possible ways to implement beam refinement during the initial channel access.
* From [13] Nokia/NSB:
  + Support operation with and without DBTW for 120 kHz.
  + Support DBTW also for 480/960 kHz SSB.
  + Provide LBT on/off indication in SIB1.
  + Support Option 2: enable/disable of DBTW is indicated by distinct GSCN used by the SSB.
  + Support Alt B) Explicit indication of SSB index and/or SSB candidate location.
  + Support 80 candidate positions for SSB when DBTW is enabled with 120 kHz.
  + Support also 80 candidate positions for SSB when DBTW is enabled with 480/960 kHz (if DBTW is supported for 480/960 kHz).
  + Group additional SSB locations and associate each group to set of regular SSB positions, e.g. after each block of 16 regular SSB positions there is associated group of up to four additional positions that can be used to retransmit any of the associated actual SSBs.
  + Use subCarrierSpacingCommon to indicate whether or not the SSB is in additional SSB position. Use kSSB bits in the SSB located in the additional position (based on subCarrierSpacingCommon) together with SSB index (PBCH DMRS and MSBs in PBCH payload) to provide UE information about the slot timing and actual SSB index transmitted.
  + Supported values for discoveryBurstWindowLength are same as used for Rel-16 NR-U
    - 0.5, 1, 2, 3, 4, 5 ms
  + It is possible to apply SCSe to one part of actually transmitted SSBs and LBT procedure for other/rest of the SSBs.
  + Consider semi-static or predetermined mechanism to determine which SSBs are under SCSe and which under LBT in certain time windows.
  + For 120kHz SSB pattern, introduce additional candidate locations for SSB transmission support for 𝑛 = 4, 9, 14, 19, where n is the slot index in half-frame.
    - The first symbols of the additional candidate SS/PBCH blocks have indexes {4, 8,16, 20} + 28×n.
  + For 480kHz and 960kHz SSB pattern, introduce additional candidate locations for SSB transmission support for 𝑛 = [{8, 9, 10, 11} ,{32,33,34,35}], where n is the slot index in half-frame.
* From [14] Charter:
  + DBTW is not introduced for 120 kHz, 480 kHz, and 960 kHz SCS SSB, including the non-initial access case.
  + If DBTW is introduced, supported DBTW lengths follow Alt 1) 0.5, 1, 2, 3, 4, 5 msec. Number of candidate positions when DBTW is enabled is 64.
* From [15] NEC:
  + DBTW should be supported for SSB transmission with 120 kHz and 480/960 kHz SCS.
  + The long term sensing could be considered as an approach to enabling/disabling DBTW.
  + DBTW indication for SSB transmission could be indicated per SSB/beam.
  + When LBT is used on unlicensed spectrum, enabling/disabling DBTW and LBT on/off indication could be jointly indicated in MIB.
  + At least for 120 kHz SCS SSB, the candidate SSB indication in NR-U should be reused with enhancement to indicate DBTW enabling/disabling and Q value jointly in MIB.
  + Additional discovery burst transmission window in the adjacent frame could be considered as a method of cycling SSB transmission.
  + With concurrent spatial multiplexing DBTWs, all SSBs could be transmitted in a cycling transmission fashion.
  + Additional n values of 4, 9, 14 and 19 should be supported to indicate 80 candidate SSBs in DBTW at least for 120 kHz SCS SSB pattern.
  + The indication of additional candidate SSBs based on additional n values should be investigated.
  + If DBTW is additionally supported for 480/960kHz SCS SSB transmission, 128 SSB candidates should be supported.
* From [16] Panasonic:
  + DBTW is supported regardless of SCS.
  + The number of candidate SSB positions is 64.
  + For enabling/disabling DBTW, Option 1-1 (disabling DBTW is jointly coded with ) with SIB indication of no-LBT mode is supported.
* From [18] Qualcomm:
  + do not support discovery burst transmission window (DBTW) for SSB for SCS 480 and 960 kHz
  + for an unlicensed band that requires LBT, if DBTW for SSB is adopted for 120 kHz SSB:
    - MIB signaling to support indication of for 120 kHz SSB
    - Minimize the number of bits needed to signal (1 or 2 bits) and thus the values (2 or 4 values)
    - Enabling/disabling DBTW can be implicit in the value
    - Consider getting the bits needed from one or more of the following: controlResourceSetZero, searchSpaceZero, ssb-SubcarrierOffset, subCarrierSpacingCommon
    - Number of candidate positions when DBTW is enabled = 64 for 120 kHz SSB
    - Consider having a subset of the SSBs (< 64) transmitted under the short control signal assumption while another subset can be best effort or have multiple positions per beam (have a within the subset)
  + consider increasing the size of the DCI 0\_0 and 1\_0 for NR licensed, by adding a field, to align with the size of the corresponding DCIs for the NR-U
* From [19] LG Electronics:
  + Adopt the following methods to indicate enabled/disabled DBTW for idle and/or connected mode UEs.
    - Separate two sets of GSCN values where one set corresponds to the case of disabled DBTW while the other set corresponds to the case of enabled DBTW
    - Signalling via system information (e.g., measObject)
    - UE-specific RRC signaling (e.g., for SCell addition)
  + Consider all or some of the following bits to indicate candidate values.
    - subCarrierSpacingCommon
    - LSB(s) of ssb-SubcarrierOffset
    - dmrs-TypeA-Position
  + Do not indicate LBT on/off in PBCH. DCI format 1\_0 size should be aligned regardless of LBT on or off.
  + Support of additional n values for the time domain pattern of SS/PBCH block with 120 kHz SCS can be considered to increase SS/PBCH block’s transmission opportunities, only if PBCH payload is sufficient to indicate the increased number of candidate SS/PBCH block indexes.
  + For 480/960 kHz SSB, first symbols of the candidate SSB have index are {4, 8, 16, 20} + 28\*n, where index 0 corresponds to the first symbol of the first slot in a half-frame (i.e., Alt 2 in previous agreement), and values of ‘n’ are consecutive integers (i.e., n = 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15).
* From [20] ETRI:
  + Propose to support DBTW for all SSB SCSs and the same DBTW lengths with Rel-16 NR-U.
  + Propose to support joint coding for LBT, DBTW, and , and study which bits can be used for reinterpretation for the joint coding.
* From [22] Intel:
  + Support DBTW for SSB with SCS 120 kHz
    - The max number of candidate SSB is
    - Support additional values of , such as 4, 9, 14, 19, in the equation defining the first symbols of candidate SS/PBCH blocks
    - Additional candidate SSBs (i.e., with index greater or equal to 64) are indexed in non-ascending order in time
      * An example relationship between candidate SSB index and SSB slot parameter can be specified in a closed form as follows:
  + Support DBTW for SSB with SCS 480 kHz/960 kHz
    - The max number of candidate SSB is
    - All candidate SSBs are indexed in ascending order in time
  + DBTW length is 5 ms.
  + For QCL relationship indication across SSBs, reuse Rel-16 NR-U mechanism by introducing parameter.
  + Explicitly indicate candidate SSB index for and in MIB.
    - No changes to MIB payload size. Further discuss and consider reinterpreting bits from some bit fields within MIB to extend candidate SSB index and provide information
    - FFS:
      * Two or four values of , e.g., or ;
      * Whether the set of values depends on SSB SCS, e.g., for SCS 120 kHz and for SCS 480 kHz/960 kHz.
  + Distinguishing between channel access cases is not needed during reception of DRS based on SS burst.
  + No need to indicate DBTW enabling. The network can configure parameter value to operate as if no DBTW is used.
  + For unlicensed operation, LBT on/off indication is within DCI scheduling SIB1.
  + Indication of licensed vs. unlicensed operation could be done based on SSB raster position. If this is not possible due to future compatibility issues, indicate licensed vs. unlicensed operation in DCI scheduling SIB1
    - To avoid DCI size ambiguity issue for licensed case, apply bit padding to DCI scheduling SIB, i.e., increase the number of reserved bits for DCI 1\_0 scrambled with SI-RNTI.
* From [23] Apple:
  + If DBTW is introduced, for above 52.6GHz frequency band, consider the following:
    - Re-purposing the 1-bit 'subCarrierSpacingCommon'
    - If more than one bit is needed, re-purposing 1-bit MSB of controlResourceSetZero in MIB or providing one more bit information by selecting one sequence from two candidates to scramble CRC bits of PBCH payload.
    - Support joint encoding Q value and licensed/unlicensed band indication.
      * If joint encoding is not possible, licensed/unlicensed band can be signaled in SIB1 and UE monitors the DCI 1\_0 for SIB1 scheduling assuming two different sizes.
* From [24] Sharp:
  + Adopt DBTW for SSB with 120 kHz SCS in above 52.6GHz.
* From [25] NTT Docomo:
  + With 120 kHz SCS, ‘n’ value(s) which can be added on top of the ones agreed already are limited, i.e., ‘n’ = {4, 9, 14, 19} only
  + With 120 kHz SCS, no significant need to support additional ‘n’ values on top of the ones agreed already
  + With 480/960 kHz SCS, not support more than 64 candidate SSB positions
  + DBTW should be supported irrespective of SCS.
    - In a certain region, e.g., Japan, sensing needs to be performed for initiating any transmission by any device in 60 GHz.
  + For DBTW to be supported in Rel-17 NR 52.6 – 71 GHz, similar to DBTW in Rel-16 NR-U, subCarrierSpacingCommon field in MIB should indicate QCL parameter, which is up to 64.
    - Following information can be implicitly indicated via subCarrierSpacingCommon
    - Enabling/disabling of DBTW
    - Licensed/unlicensed band
    - LBT on/off
* From [26] Xiaomi:
  + Alt1 (same as Rel-16 FR1 NR-U) is supported.
  + The number of candidate positions when DBTW is enabled is 64.
* From [27] Convida:
  + Increasing the number of SSB candidate positions to above 64 to increase transmission opportunities to cope with LBT failure should be considered.
  + The number of values for ‘n’ should be dependent on LBT operation and the actual values of ‘n’ for each SCS 480 GHz/960 GHz can be further studied.
* From [28] WILUS:
  + We propose to support discovery burst transmission window (DBTW) for at least 120kHz SCS which makes it possible to define candidate SSB positions within the DBTW with support of DB which was already agreed.
  + It should be further considered that the additional candidate SS/PBCH block locations within a DBTW can be set to the closest slot locations after LBT failure at candidate SS/PBCH blocks locations as defined in FR2.

#### Summary of Discussions

The following are previous agreements on DRS aspects.

|  |
| --- |
| **Agreement:**  For an unlicensed band that requires LBT, further study whether/how to support discovery burst (DB) and discovery burst transmission window (DBTW) at least for 120 kHz SSB SCS   * If DB supported   + FFS: What signals/channels are included in DB other than SS/PBCH block * If DBTW is supported   + Support mechanism to indicate or inform that DBTW is enabled/disabled for both IDLE and CONNECTED mode UEs     - FFS: how to support UEs performing initial access that do not have any prior information on DBTW.   + PBCH payload size is no greater than that for FR2   + Duration of DBTW is no greater than 5 ms   + Number of PBCH DMRS sequences is the same as for FR2 * The following points are additionally FFS:   + How to indicate candidate SSB indices and QCL relation without exceeding limit on PBCH payload size   + Details of the mechanism for enabling/disabling DBTW considering LBT exempt operation and overlapping licensed/unlicensed bands * Whether or not to support DBTW for SSB SCS(s) other than 120 kHz if other SSB SCS(s) are supported   **Agreement:**   * For operation with shared spectrum channel access of NR 52.6 – 71 GHz, support discovery burst (DB) and define the DB same as in Rel-16 37.213 Section 4.0 * FFS: Support discovery burst transmission window (DBTW) at least for SSB with 120 kHz SCS with the following requirements   + PBCH payload size is no greater than that for FR2   + Duration of DBTW is no greater than 5 ms   + Number of PBCH DMRS sequences is the same as for FR2   + FFS: applicability of DBTW design for 120kHz to SSB with 480kHz and 960kHz SCS   + Support mechanism to indicate or inform that DBTW is enabled/disabled for both IDLE and CONNECTED mode UEs     - FFS: how to support UEs performing initial access that do not have any prior information on DBTW.     - FFS: details of the mechanism for enabling/disabling DBTW considering LBT exempt operation and overlapping licensed/unlicensed bands     - FFS: details of how to inform UEs of the configuration of DBTW   **Agreement:**  FFS: Support DBTW at least for 120kHz   * FFS whether DBTW will be applicable for 480/960 kHz SSB SCS   + If DBTW is supported for 480/960kHz SSB:     - For the case agreed in RAN1 #104bis-e where 480/960 kHz SSB location and SCS are explicitly provided to the UE (non-initial access), indication of DBTW configuration (e.g. enable/disable of DBTW,  , and DBTW length) are supported by dedicated signaling.  * For 120kHz SSB, support mechanism to distinguish at least the following scenarios:   + Case 1) (Unlicensed with LBT off) + DBTW disabled   + Case 2) (Unlicensed with LBT on) + DBTW enabled   + Case 3) (Unlicensed with LBT on) + DBTW disabled   + Case 4) (Licensed) + DBTW disabled   + FFS: Whether/how LBT on/off is indicated in MIB     - If not indicated in MIB, then FFS whether/how the UE determines different sizes of DCI 1\_0 with CRC scrambled by SI-RNTI   + FFS: whether any case(s) can be combined for DBTW signaling design and how to handle implications to DCI 1\_0 size ambiguity if is not distinguished in signaling   + FFS: whether all above cases need an explicit indication   + FFS: Whether a single indication can be used for combination of more than one cases * For 120 kHz SSB, enable/disable of DBTW is indicated by one or more of the following methods:   + Option 1) signaling in MIB     - Option 1-1) disabling DBTW is jointly coded with  * + - Option 1-2) indicated by other bit fields in MIB     - FFS: among options 1-1 and 1-2   + Option 2) distinct GSCN used by the SSB   + Option 3) By comparing the value of  in MIB and DBTW length after UE reads SIB1 or by comparing the value of  in MIB and default DBTW length of 5 ms before UE reads SIB1.  * + FFS: whether to support option 1, 2, 3, or any combination of the options.   + Note: enable/disable signaling of DBTW by MIB or GSCN does not preclude other signaling methods   **Agreement:**  If DBTW is supported,   * Working assumption: MIB signaling to support   + Alt A) indication of at least for 120kHz SSB  * + - In this case, the total number of values of to not exceed 4  * + Alt B) Explicit indication of SSB index and/or SSB candidate location     - FFS on the details of signaling   + FFS betweenAlt A, or B, or supporting both * Supported DBTW lengths   + Alt 1) 0.5, 1, 2, 3, 4, 5 msec     - Note: same as Rel-16 FR1 NR-U   + Alt 2) maximum 5 msec     - FFS other values   + FFS between Alt 1 and 2 * Number of candidate positions when DBTW is enabled   + For 120kHz SSB     - FFS between 64 or 80   + If DBTW is additionally supported for 480/960kHz SSB     - FFS between 64 or 128 |

The following is a summary of company position of various aspects of DRS.

* Supporting DBTW
  + Support: Huawei/HiSilicon, vivo, Spreadtrum (for 120kHz), Interdigital, Sony, Samsung, CATT(if more than 56 SSB with 120kHz), ZTE/Sanechips, Futurewei (for 120kHz), Nokia, NEC, Panasonic, ETRI, Intel, Sharp (for 120kHz), NTT Docomo, WILUS (for 120kHz), OPPO, LGE, Xiaomi, Lenovo/Motorola Mobility
  + Do not support: Ericsson, CATT (for 480/960kHz) Futurewei (for 480/960kHz), Charter, Qualcomm (for 480/960kHz)
* Indication of licensed and unlicensed operation:
  + Raster: Samsung, OPPO, Interdigital
  + No distinction: Intel, Qualcomm, ZTE/Sanechips, Ericsson, Huawei/HiSilicon
* Indication of LBT
  + MIB: Huawei/HiSilicon, Interdigital, CATT, Futurewei, OPPO, Xiaomi
  + Other than MIB (e.g. SIB1): vivo, CATT, Ericsson, Nokia/NSB, Intel, Qualcomm, MTK, LGE, Lenovo/Motorola Mobility, Huawei/HiSilicon (Raster)
* Indication of DBTW (for initial access)
  + Implicit:
    - MIB: ~~Huawei/HiSilicon~~, vivo, Interdigital, Samsung, Intel, ZTE/Sanechips, NEC, Qualcomm, NTT Docomo, Panasonic, Lenovo/Motorola Mobility
    - raster: Interdigital, vivo, Nokia/NSB, LGE
    - NR-U solution: Huawei/HiSilicon
      * Comparison of Q in MIB and DBTW length in SIB1. Assume DBTW enabled before reading SIB1.
  + Explicit:
    - Sony (jointly coded with ), Futuerwei, Samsung (jointly coded with ), Ericsson (if DBTW supported, then DBTW on/off jointly coded with )
* Supporting means of conveying candidate SSB location & SSB beams
  + Supported values:
    - 2 values: Qualcomm, NTT Docomo (64 and smaller), OPPO, Xiaomi, Ericsson (if DBTW supported)
    - {8,64}: Intel
    - 4 values: Huawei/HiSilicon, Interdigital, Sony, Qualcomm, Intel, Xiaomi, Futurewei
    - {4,8,16,64}: Intel
    - {8,16,32,64}: Huawei/HiSilicon, ZTE/Sanechips, LGE, Lenovo/Motorola Mobility, Sony (if indication of DBTW is not jointly coded with )
    - {16, 32,64,reserved}: Sony (if indication of DBTW is jointly coded with and number of candidate is >64)
    - {8, 16,32,reserved}: Sony (if indication of DBTW is jointly coded with and number of candidate is 64)
  + Support explicit indication of SSB index and/or SSB candidate location
    - Nokia
* Supported DBTW lengths
  + {0.5, 1, 2, 3, 4, 5}msec for all SCS (as in NR-U)
    - vivo, Futurewei, Nokia, Charter (if DBTW is supported), Xiaomi, Qualcomm (120 kHz), NTT Docomo, ZTE/Sanechips, LGE, NEC, Lenovo/Motorola Mobility, Ericsson (if DBTW supported), Sony
  + 5 msec
    - Intel, CATT
  + 120 kHz SCS: {40, 32, 24, 16, 8, 4} slots = {5, 4, 3, 2, 1} ms
    - Huawei/HiSilicon
  + 480 kHz SCS: {72, 32, 24, 16, 8, 4} slots = {2.25, 1, 0.75, 0.5, 0.25, 0.125} ms
    - Huawei/HiSilicon
  + 960 kHz SCS: {64, 32, 24, 16, 8, 4} slots = {1, 0.5, 0.375, 0.25, 0.125, 0.0625} ms
    - Huawei/HiSilicon
* Number of SSB candidates for DBTW
  + For 120kHz:
    - 64: vivo, CATT(for no LBT/no DBTW cases), Futurewei. Charter (if DBTW is supported), NTT Docomo, Xiaomi, Qualcomm, Panasonic, MTK, LGE, Ericsson (if DBTW supported), Huawei/HiSilicon
    - > 64: Convida
    - 80: Intel, Sony, CATT (for LBT/DBTW cases), Nokia, NEC, ZTE/Sanechips, OPPO
  + For 480kHz:
    - 64: Charter (if DBTW is supported), NTT Docomo, Xiaomi, Qualcomm, Panasonic, MTK, LGE, Lenovo/Motorola Mobility, Futurewei
    - > 64: Convida
    - 80: Nokia
    - 128: vivo, Intel, Sony, Samsung, ZTE/Sanechips, Nokia, NEC, Huawei/HiSilicon
  + For 960kHz:
    - 64: LGE
    - 80: Nokia
    - 128: Nokia, NEC, Lenovo/Motorola Mobility, Huawei/HiSilicon
* DCI sizes between licensed and unlicensed
  + Same size for DCI 1\_0: Ericsson, Qualcomm, LGE, Intel (for SI-RNTI)
  + Same size for DCI 0\_0: Qualcomm
  + Different size for DCI 1\_0: Apple (if joint encoding of Q and licensed/unlicensed band indication is not possible)

#### **1st Round Discussion:**

Please provide comments on the above summary (including aspects that are missing, aspects captured incorrectly, etc). Moderator will provide a suggested proposal once the summary captures all company opinion correctly.

If the above summary is directly edited (please use a color to highlight changes, e.g. RED) and mention the changes/additions in the comment below.

|  |  |
| --- | --- |
| Company | Comments |
| Samsung | * For the number of candidate SSBs, we have a question on the motivation to support at most 64 candidate SSBs when DBTW is on. In our understanding, for FR2-2, there is no strong motivation to support a small number of SSB beams, and very likely in implementation, the number of SSB beams will be larger than 32, then the utilization of DBTW with only 64 candidate SSB locations is indeed limited, and that’s the reason we support more than 64 candidate SSB locations when DBTW is on. * For the SCS applicable to DBTW, we want to address that short control signaling is not globally applicable to all the regions, and there are regions requiring LBT as mandatory procedure for channel access, so the application of DBTW should be for all supported SCSs. Also, some companies mentioned the duty cycle of SSB when using 480/960 is small than the requirement of short control signaling, but it’s not a correct observation. The 20 ms periodicity of SSB is only for initial access and from the UE perspective, but the calculation of duty cycle should be from the cell perspective (i.e., channel utilization). In this sense, if gNB configures a 5 ms periodicity for SSB, there are lots of scenarios for 480/960 kHz SCS cannot satisfy the short control signaling duty cycle. * For the indication of Q, we are not sure whether current MIB can have sufficient number of bits that can be re-interpreted for this purpose. I believe we can utilize similar approach as NR-U: using MIB as the best effort, otherwise use SIB1. * For the DCI 1\_0 size issue, one way is aligning the DCI 1\_0 size for operation with/without shared spectrum channel access, and another way could be indicating operation with/without shared spectrum channel access in MIB (no need to know the value of Q). * We also want a clarification on the proposal of using sync raster to indicate DBTW on/off. In our understanding, DBTW on/off is a semi-static configuration, but sync raster is fixed, so we are not sure how to utilize sync raster to indicate DBTW on/off. Our proposal is to use sync raster to indicate licensed/unlicensed, since it’s a fixed information. |
| Qualcomm | Please see our added support above using “Qualcomm” |
| Panasonic | Please see our added support above using “Panasonic” |
| Mediatek | Please see our added support above using “MTK” |
| Docomo | * For # of candidate SSB positions, the reason why we propose up to 64, which is same as FR2, is because we see remaining MIB fields and PBCH payload are quite limited. We do not strongly prefer to have a significant change on the interpretation of these fields either. On the other hand, we can understand Samsung’s first point. Since DBTW functionality is important from our perspective, we are relatively open to whether 64 or more about # of candidate SSB positions. We would like to hear more views from companies. * We would like to echo Samsung’s 2nd point regarding DBTW per SCS. Since short control signaling is not global rule, “treated as short control signaling” would not justify not to support DBTW. * For Q value indication, of course more variety gives us more flexibility on operation, while we doubt the feasibility in terms of the remaining MIB/PBCH payload available. *subCarrierSpacingCommon* can clearly repurposed for Q as well as Rel-16 NR-U since same SCS is assumed between SSB and CORESET#0. Otherwise use SIB for Q is fine for us. * For the indication of licensed/unlicensed and LBT on/off, our preference is to combine them with Q value single all of them are associated with same aspect and Q value is something already supported in NR. |
| ZTE/Sanechips | Please see our added support above using “ZTE/Sanechips” |
| Nokia | As there are regions where LBT is required, and short control signaling may not be applied (either by rule or due to limitations e.g. in case of 120kHz). Hence DBTW support would seem preferable. If DBTW is supported, our concern is that especially with 120 kHz SCS, there is limited number of available additional candidate location for all SSBs when more than 32 SSBs are used (i.e. =80). It’s expected that at the frequency range of interest the system should be designed to have 64 SSBs. Thus, limiting the DBTW operation only to low number of beams seems counter-intuitive. Hence, if, based on majority view, the based approach is selected, we would like to see also =64 supported.  For the number of candidate locations, we updated the FL summary above to account also the 960kHz case. In terms of total number of SSB candidate locations, we would be fine to assume 128 for 480kHz and 960kHz, but if we want to align with 120kHz sub-carrier spacings, also 80 could be considered.  For the DCI size, we were considering that as the double hypothesis applies only in cell selection phase, assuming two different sizes only in the initial phase would not be overly complex. |
| ZTE/Sanechips | Please see our added support above using “OPPO” |
| LG Electronics | Our views are added above.  Regarding DBTW enabling/disabling, we’d like to clarify how it can be implicitly indicated by using MIB. Does it mean that if MIB indicates Q less than 64, DBTW is enabled, otherwise DBTW is disabled?  Our main concern for more than 64 SSB candidate positions is whether PBCH payload can indicate 7 digits for more than 64 SSB candidate positions. If it will be resolved, we can consider more than 64 SSB candidate positions. |
| NEC | Please see our added support above using “NEC” |
| Xiaomi | Please see our added support above using “Xiaomi” |
| Lenovo, Motorola Mobility | Please see our added support above using “Lenovo/Motorola Mobility” |
| Futurewei | Please see our added support above using “Futurewei” |
| Ericsson | Please see our added support above using "Ericsson"  Our strong view is that we cannot agree to support DBTW for any SCS unless a conclusion is reached on the following two aspects since they directly affect the number of bits in MIB that can be repurposed. So far we have not seen a complete solution, and we are skeptical that enough bits can be found. We have trouble agreeing until a complete solution is on the table (including resolved dependencies to other working groups, e.g., RAN4):   1. If and how additional candidate SSB positions (>64) are to be supported, and 2. How to signal the following: Q and DBTW on/off   Our view on the above two aspects is:   * 64 candidate SSB positions in order to reuse the FR2-based signaling of SSB index * DBTW on/off needs to be provided in MIB which is aligned with previous agreement saying the following:   + If DBTW is supported     - Support mechanism to indicate or inform that DBTW is enabled/disabled for both IDLE and CONNECTED mode UEs * LBT on/off can be signaled in SIB1 * DCI 1\_0 size is the same for both licensed and unlicensed. Alternatively, if it is desired to maintain different DCI 1\_0 sizes (as in Rel-16 NR-U) and it is acceptable for the UE to perform two blind decodes on DCI 1\_0 with CRC scrambled by SI-RNTI, that is okay too. * Any MIB bits that are repurposed for signaling of Q and DBTW on/off must be unused for both licensed and unlicensed operation in order for the UE to correctly determine the MIB for both licensed or unlicensed   + One such bit that can be repurposed for sure is *subCarrierSpacingCommon* since only (120,120), (480,480), and (960,960) combinations are supported |
| CATT | Please see our added support above using “CATT” |
| InterDigital | Please see our added support above using “Interdigital”.  For the indication of licensed/unlicensed, DBTW enable/disable, and LBT on/off, we propose to jointly indicate the mode of operation based on the combination of sync. raster offset and MSB of controlResourceSetZero. |
| Sony | Please see our added support above using “Sony”  As for values, it should depend on whether indication of DBTW is jointly or not jointly coded with . Although our 1st preference is that indication of DBTW is jointly coded with , we added our 2nd preference in the case that indication of DBTW is not jointly coded with . |
| Huawei/HiSilicon | * Regarding the issues addressed in the above summary: We have made some addition/modifications using “Huawei/HiSilicon”   + **Supporting DBTW:** We would like to echo the views of some other companies that short control signaling exemption is not supported in all regions and may not be used to justify that DBTW is not required for 480/960 kHz. Also, as Samsung has mentioned above, assuming that 480/960 kHz SSB burst satisfies the max 10% channel occupation every 100 ms is not accurate. 10% channel occupation should be satisfied from the transmitting equipment perspective (gNB) and is not based on the receiving equipment assumption (UE).   + **Indication of licensed and unlicensed operation:** We would like to have some clarification as to why such an indication is important during initial access. In our view, what may be important for the UE during initial access is to know whether LBT is on or off to resolve the ambiguity in the size of DCI 1\_0 scrambled with SI-RNTI. If LBT on/off is indicated to the UE or the ambiguity in DCI 1\_0 size is resolved by other means, we do not see why UE further need to know if it is operating in shared or unshared spectrum during initial access.   + **Indication of LBT:** During initial access, it is required for resolving the ambiguity in the size of DCI 1\_0 scrambled with SI-RNTI. We suggest indication using synch raster. If ambiguity in the size of DCI 1\_0 scrambled with SI-RNTI is resolved using above solution or any other means, we do not see a strong motivation to indicate LBT/no-LBT to UE before UE reads SIB1.   + **Indication of DBTW:** DBTW enabled/disabled is never explicitly indicated to the UE in Rel-16 NR-U. In Rel-16, UE can infer whether DBTW is enabled/disabled only after reading SIB1 by comparing the maximum number of transmitted SSB indexes (acquired from MIB payload) with the DBTW length (*DiscoveryBurst-WindowLength* provided in SIB1). If DBTW length that is configured in SIB1 is such that DBTW can include more than candidate SSB indexes, UE can infer that DBTW is enabled. In turn, if DBTW length that is configured in SIB1 is such that DBTW cannot include more than candidate SSB indexes, UE can infer that DBTW is disabled. Before reading SIB1, UE assumes that DBTW length is a half frame (includes all candidate SSB positions), and, as such, DBTW is enabled.   It is unclear for us why above mechanism is not also usable in 60 GHz. As such, we added the option of using NR-U solution in above summary.   * + **Supported DBTW lengths:** As discussed above, supported DBTW lengths should be such that, when compared to the values of , UE can infer whether it is enabled or disabled. As we explained in our tdoc in details, since the time interval containing SSB indexes are different in 120, 480, 960 kHz, it is preferable to support different sets of DBTW for different SCSs.   + **Number of SSB candidates for DBTW:** For 120 kHz, we prefer not to change Case D SSB pattern. DBTW is still useful if the number of transmitted SSB indexes is less than 64. For 480 and 960 kHz, up to 128 candidate SSB indexes can be supported by indicating the 7th bit of the candidate SSB index by borrowing the 4th LSB of SFN in the PBCH payload and indicating the 4th LSB of SFN in MIB payload. Note that this does not reduce the periodicity of MIB payload below the current 80 ms. * In addition, we find it important that the following two issues to be discussed in this meeting:   + How to indicate additional Candidate SSB indexes if   How to interpret ssb-PositionsInBurst configured in SIB1 in relation to the indicated value of . |

#### **1st Round Discussion Summary:**

**Issue 1)** On the support of DBTW, there is clear majority for at least 120kHz cases (see below). Suggest discussing further on Proposal 1.1-1 and if possible, agree to it or some modification of it.

|  |
| --- |
| * Supporting DBTW   + Support: Huawei/HiSilicon, vivo, Spreadtrum (for 120kHz), Interdigital, Sony, Samsung, CATT(if more than 56 SSB with 120kHz), ZTE/Sanechips, Futurewei (for 120kHz), Nokia, NEC, Panasonic, ETRI, Intel, Sharp (for 120kHz), NTT Docomo, WILUS (for 120kHz), OPPO, LGE, Xiaomi, Lenovo/Motorola Mobility   + Do not support: Ericsson, CATT (for 480/960kHz) Futurewei (for 480/960kHz), Charter, Qualcomm (for 480/960kHz) |

##### **Proposal 1.1-1)**

* Support DBTW at least for 120kHz
  + FFS whether DBTW will be applicable for 480/960 kHz SSB SCS

**Issue 2)** For indication of licensed/unlicensed, LBT/no LBT, and DBTW/no DBTW cases. Companies are somewhat split, but there are certain options that have greater support. The DCI size handling for licensed and unlicensed seems to related to the same issue as well. Suggest discussing further on Proposal 1.1-2 and if possible, agree to it or some modification of it.

|  |
| --- |
| * Indication of licensed and unlicensed operation:   + Raster: Samsung, OPPO, Interdigital   + No distinction: Intel, Qualcomm, ZTE/Sanechips, Ericsson, Huawei/HiSilicon * Indication of LBT   + MIB: Huawei/HiSilicon, Interdigital, CATT, Futurewei, OPPO, Xiaomi   + Other than MIB (e.g. SIB1): vivo, CATT, Ericsson, Nokia/NSB, Intel, Qualcomm, MTK, LGE, Lenovo/Motorola Mobility, Huawei/HiSilicon (Raster) * Indication of DBTW (for initial access)   + Implicit:     - MIB: ~~Huawei/HiSilicon~~, vivo, Interdigital, Samsung, Intel, ZTE/Sanechips, NEC, Qualcomm, NTT Docomo, Panasonic, Lenovo/Motorola Mobility     - raster: Interdigital, vivo, Nokia/NSB, LGE     - NR-U solution: Huawei/HiSilicon       * Comparison of Q in MIB and DBTW length in SIB1. Assume DBTW enabled before reading SIB1.   + Explicit:     - Sony (jointly coded with ), Futuerwei, Samsung (jointly coded with ), Ericsson (if DBTW supported, then DBTW on/off jointly coded with ) * DCI sizes between licensed and unlicensed   + Same size for DCI 1\_0: Ericsson, Qualcomm, LGE, Intel (for SI-RNTI)   + Same size for DCI 0\_0: Qualcomm   + Different size for DCI 1\_0: Apple (if joint encoding of Q and licensed/unlicensed band indication is not possible) |

##### **Proposal 1.1-2)**

* No indication for licensed and unlicensed operation will be performed in SSB (including MIB)
* Use of LBT by the cell and UEs connected to the cell is not indicated MIB.
  + FFS where and how this is indicated, e.g. SIB1
* For supported SCS cases of DBTW, the indication of use or no use of DBTW will be implicitly indicated (deriving that DBTW is used or not used via configuration of MIB (and SIB1) parameter(s) in certain combinations) in MIB.
  + FFS details of implicit indication in MIB (and in SIB1)
* For both licensed or unlicensed operation and with or without LBT, support the same DCI size for:
  + DCI format 1\_0 scrambled with SI-RNTI
  + FFS for DCI format 1\_0 scrambled with other RNTI, and other DCI formats

**Issue 3)** For means of conveying candidate SSB location & SSB beams, majority of the companies seem to prefer NR-U based approach. Suggest discussing further on Proposal 1.1-3 and if possible, agree to it or some modification of it.

|  |
| --- |
| * Supporting means of conveying candidate SSB location & SSB beams   + Supported values:     - 2 values: Qualcomm, NTT Docomo (64 and smaller), OPPO, Xiaomi, Ericsson (if DBTW supported)     - {8,64}: Intel     - 4 values: Huawei/HiSilicon, Interdigital, Sony, Qualcomm, Intel, Xiaomi, Futurewei     - {4,8,16,64}: Intel     - {8,16,32,64}: Huawei/HiSilicon, ZTE/Sanechips, LGE, Lenovo/Motorola Mobility, Sony (if indication of DBTW is not jointly coded with )     - {16, 32,64,reserved}: Sony (if indication of DBTW is jointly coded with and number of candidate is >64)     - {8, 16,32,reserved}: Sony (if indication of DBTW is jointly coded with and number of candidate is 64)   + Support explicit indication of SSB index and/or SSB candidate location     - Nokia |

##### **Proposal 1.1-3)**

* For supported SCS cases of DBTW, support configuration of in MIB, with following {8,16,32,64} values

**Issue 4)** For Supported DBTW lengths clear majority supports the same lengths as in NR-U. Suggest discussing further on Proposal 1.1-4 and if possible, agree to it or some modification of it.

##### **Proposal 1.1-4)**

* For supported SCS cases of DBTW, support DBTW lengths {0.5, 1, 2, 3, 4, 5} msec
  + Note: this should be the same as Rel-16 NR-U DBTW lengths.

**Issue 5)** For number of SSB candidates for DBTW, support of DBTW for 480/960kHz is pending, but we could further discuss for the 120kHz case. There is larger support for 64 candidates for 120kHz, compared to 80 candidates (10 companies vs 7 companies). Moderator thinks some further discussion would be helpful. Maybe companies can elaborate bit further the concerning aspect of the proposal not supported (so that we get better understanding where the core issues lie). Suggest discussing further on Proposal 1.1-5 and if possible, down-select between alt 1 and 2.

|  |
| --- |
| * Number of SSB candidates for DBTW   + For 120kHz:     - 64: vivo, CATT(for no LBT/no DBTW cases), Futurewei. Charter (if DBTW is supported), NTT Docomo, Xiaomi, Qualcomm, Panasonic, MTK, LGE, Ericsson (if DBTW supported), Huawei/HiSilicon     - > 64: Convida     - 80: Intel, Sony, CATT (for LBT/DBTW cases), Nokia, NEC, ZTE/Sanechips, OPPO   + For 480kHz:     - 64: Charter (if DBTW is supported), NTT Docomo, Xiaomi, Qualcomm, Panasonic, MTK, LGE, Lenovo/Motorola Mobility, Futurewei     - > 64: Convida     - 80: Nokia     - 128: vivo, Intel, Sony, Samsung, ZTE/Sanechips, Nokia, NEC, Huawei/HiSilicon   + For 960kHz:     - 64: LGE     - 80: Nokia     - 128: Nokia, NEC, Lenovo/Motorola Mobility, Huawei/HiSilicon |

##### **Proposal 1.1-5)**

* For 120kHz SSB, the number of candidates for DBTW is:
  + Alt 1) 64
  + Alt 2) 80

#### **2nd Round Discussion:**

Please provide comments for Proposals 1.1-1 ~ 1.5 (copied below for convenience).

##### **Proposal 1.1-1)**

* Support DBTW at least for 120kHz
  + FFS whether DBTW will be applicable for 480/960 kHz SSB SCS

##### **Proposal 1.1-2)**

* No indication for licensed and unlicensed operation will be performed in SSB (including MIB)
* Use of LBT by the cell and UEs connected to the cell is not indicated MIB.
  + FFS where and how this is indicated, e.g. SIB1
* For supported SCS cases of DBTW, the indication of use or no use of DBTW will be implicitly indicated (deriving that DBTW is used or not used via configuration of MIB (and SIB1) parameter(s) in certain combinations) in MIB.
  + FFS details of implicit indication in MIB (and in SIB1)
* For both licensed or unlicensed operation and with or without LBT, support the same DCI size for:
  + DCI format 1\_0 scrambled with SI-RNTI
  + FFS for DCI format 1\_0 scrambled with other RNTI, and other DCI formats

##### **Proposal 1.1-3)**

* For supported SCS cases of DBTW, support configuration of in MIB, with following {8,16,32,64} values

##### **Proposal 1.1-4)**

* For supported SCS cases of DBTW, support DBTW lengths {0.5, 1, 2, 3, 4, 5} msec
  + Note: this should be the same as Rel-16 NR-U DBTW lengths.

##### **Proposal 1.1-5)**

* For 120kHz SSB, the number of candidates for DBTW is:
  + Alt 1) 64
  + Alt 2) 80

|  |  |
| --- | --- |
| Company | Comments |
| vivo | **Proposal 1.1-1**: Support. As mentioned by several companies, short control signaling is not available in all regions. We prefer to support DBTW for all SCSs.  **Proposal 1.1-2**: Partially support  On licensed/unlicensed indication, we think it is too early to conclude this since it is unknown that we could achieve a totally common design for licensed and unlicensed operation;  On LBT indication, we support the proposal;  On DBTW on/off indication, we support the proposal;  On DCI 1\_0 size, whether to have the same size for licensed and unlicensed depends on whether to have licensed/unlicensed indication in SSB, which is preferred to be determined later. We support the same DCI 1\_0 size for unlicensed operation with or without LBT. One more comment is that DCI 1\_0 size is not bundled with RNTI but CSS or USS. So we suggest to change “DCI format 1\_0 scrambled with SI-RNTI” to “DCI format 0\_0 monitored in a common search space”.  **Proposal 1.1-3:** Support  **Proposal 1.1-4:** Support  **Proposal 1.1-5:** Support |
| DOCOMO | **Proposal 1.1-1**: ok to support for 120k SCS at first. We also prefer to support DBTW for all SCSs.  **Proposal 1.1-2**:  On licensed/unlicensed indication, we are fine with not indicating in MIB;  On LBT indication, we are open since it may be implicitly indicated in a certain MIB field;  On DBTW on/off indication, we support the proposal;  On DCI 1\_0 size, open to further discuss  **Proposal 1.1-3:** Support  **Proposal 1.1-4:** Support  **Proposal 1.1-5:** Support Alt 1. |
| Spreadtrum | * + 1. Support     2. FFS. It is related to in MIB, since we don’t know whether there is a bit reserved for the indication of disable/enable DBTW or LBT     3. Support configuration of in MIB. FFS the values.     4. Support multiple candidates of DBTW length. FFS the values.   Support 64 |
| Nokia | Proposal 1.1-1: We would be fine with this proposal.  Proposal 1.1-2: (Assuming that this proposal would be packet with 1.1-1). Regarding the DCI format 1\_0, we don’t see it necessary to align the sizes. The dual hypothesis exists only for the first SIB1 reception. Beyond that we can take this proposal to progress the work.  Proposal 1.1-3: This is evidently majority view, but we would prefer to take this as a working assumption as we need to further consider how the method can be made to operate if Alt 2 of Proposal 1.1-5 is adopted.  Proposal 1.1-4: OK.  Proposal 1.1-5: Our preference would be alt 2. As expressed earlier, as the short control signal exemption cannot always be used and does not cover all SSBs in case of 120kHz, thus supporting DBTW in case of higher number of beams would be preferred. |
| LG Electronics | Proposal 1.1-1) Support but prefer to introduce DBTW for 480/960 kHz SCS as well  Proposal 1.1-2) We still fail to understand how DBTW enabling/disabling can be implicitly indicated by MIB. According to explanation from Huawei, we could understand how UE can infer whether DBTW is enabled/disabled by using SIB1 configuration. However, implicit mechanism by using MIB should be clarified first.  Proposal 1.1-3) Support  Proposal 1.1-4) Support  Proposal 1.1-5) Prefer Alt 1, considering additional 1 bit is need to indicated increased SSB candidate positions |
| ZTE, Sanechips | **Proposal 1.1-1**: Support. We prefer to support DBTW for 480/960 kHz as well.  **Proposal 1.1-2**: Support.  **Proposal 1.1-3:** Support  **Proposal 1.1-4:** Support  **Proposal 1.1-5:** Support. Further, we prefer Alt 2. |
| Samsung | Proposal 1.1-1) We are ok with the proposal, and we support it for 480/960 kHz SCS as well.  Proposal 1.1-2)   * For unlicensed/licensed indication, we are ok with no using MIB to indicate such information, but RAN1 shall not add any intention to prevent RAN4 on the sync raster design. So the wording can be changed to “No indication for licensed and unlicensed operation ~~will be performed in SSB (including MIB)~~ in MIB” * For the indication of LBT, we are ok with the proposal. * For the indication of DBTW, we don’t agree with the proposal. The key issue is, a UE should be able to know whether DBTW is on or off before monitoring Type0-PDCCH, since the monitoring behavior is not the same (e.g. whether to apply Q). Any approach needing the information from SIB1 cannot achieve the purpose. Q is only applicable when DBTW is on, so we don’t understand why we need to indicate Q in MIB even without knowing whether the DBTW is on or off. We still support the proposal of joint coding DBTW off and Q values. * For DCI size, we are ok.   Proposal 1.1-3) As mentioned in the comment in Proposal 1.1-2), Q value is only applicable when DBTW is on, so we don’t think Proposal 1.1-3) is compatible with Proposal 1.1-2). Also, the value of Q depends on the decision of the number of candidate SSB locations, e.g. if the max is 64, and Q doesn’t need to take a value of 64.  Proposal 1.1-4) We are ok with the proposal.  Proposal 1.1-5) We are ok with the proposal, but we wonder what’s the different from the FFS in the last meeting’s agreement “FFS between 64 and 80”? Also this new proposal didn’t include proposal for 480 and 960, then it seems weaker than the agreement of last meeting.  Other than above, we also want to address companies’ concern on supporting larger than 64 number of candidate locations. TTI of MIB is 80 ms, so the 4th LSB of SFN can be re-interpreted for indicating the extra MSB of candidate SSB index and use a MIB bit to indicate the 4th LSB of SFN. This doesn’t impact other indication of timing in PBCH payload and using DMRS of PBCH. |
| Intel | **Proposal 1.1-1)** - agree  **Proposal 1.1-2)** - agree  **Proposal 1.1-3)** – don’t agree. Our first preference is the set of 2 values for as its indication in MIB would require only 1 bit.  The set of 2 values for would assume a small number of beams and a large number of beams. All cases in between could be configured by SSB presence pattern. It’s straightforward to put the large number for equal to the max, i.e., 64 for all SSB SCS. Regarding the small value, we think it should depend on the SCS. For example, in case of SSB SCS 480 kHz/960 kHz, there are no strong reasons to operate with a number of beams 8 (the current max for NR-U Rel-16). Therefore, we propose for SSB SCS 480 kHz/960 kHz. For SSB SCS 120 kHz, the smaller value could be lowered, i.e., .  **Proposal 1.1-4)** – don’t agree. In our understanding, the support of multiple DBTW lengths would require some kind of indication of exact value of DBTW length from the set. This what we try to avoid by proposing a single fixed DBTW length equal to 5 ms.  **Proposal 1.1-5)** – agree. Our preference is Alt.2.  As we showed in our tdoc, it is possible to provide additional SSB candidates for SSB SCS 120 kHz (i.e., with indices 64~79) without affecting the ordering of legacy SSB candidates (i.e., with indices 0~63). One additional bit would be required in the MIB to indicate an index of the larger number of candidate SSBs. This could be done via repurposing the *subCarrierSpacingCommon* bit as SCS for SSB and CORESET#0 has been agreed to always the same for NR in FR2-2. |
| NEC | Proposal 1.1-1) Support, and prefer to support DBTW for all SCSs  Proposal 1.1-2) Support except the indication of DBTW. We share the similar views on joint coding DBTW indication and Q values.  Proposal 1.1-3) Support and FFS the values of Q.  Proposal 1.1-4) Support.  Proposal 1.1-5) Support and prefer Alt 2. |
| Apple | **Proposal 1.1-1: Ok for us.**  **Proposal 1.1-2:** We shared the concern raised by LGe. Our recommendation is to discuss implicit indication solution together with explicit indication directly, instead of agreeing with it and keep FFS on how it works.  **Proposal 1.1-3:** Support. Meanwhile, our understanding is that this proposal has impact on Proposal 1.1-2. Proposal 1.1-2 is reasonable if we conclude to not support explicit indication of DBTW window present using joint coding approach.  **Proposal 1.1-4:** Support.  **Proposal 1.1-5:** Our preference is Alt.1, 64. |
| Convida Wireless | Proposal 1.1-1: We are ok with the proposal.  Proposal 1.1-2: We are ok with the proposal.  Proposal 1.1-3: We are ok with the proposal.  Proposal 1.1-4: We are ok with the proposal.  Proposal 1.1-5: We are ok with the proposal. Our preference is Alt.2, 80. |
| Qualcomm | Proposal 1.1-1: fine for sake of progress  Proposal 1.1-2: generally fine with the proposal, however, implicit DBTW ON/OFF may make sense for MIB but may need further considerations for SIB1, hence we prefer the following:   * *For supported SCS cases of DBTW, the indication of use or no use of DBTW will be implicitly indicated (deriving that DBTW is used or not used via configuration of MIB ~~(and SIB1)~~ parameter(s) in certain combinations) in MIB.*   + *FFS for SIB1*   Proposal 1.1-3: since Proposal 1.1-2 assumes DBTW enable disable may be implicit in MIB (Q value), the maximum need to be similar to the number of candidate SSB locations (to disable) which depends on status of Proposal 1.1-5. Suggest we treat this proposal after we treat Proposal 1.1-2 and Proposal 1.1-5. In addition, we may need to conclude on the number of available MIB signaling bits first, since we may only have 1 bit and that leave 2 values only.  Proposal 1.1-4: fine with the proposal  Proposal 1.1-5: We still need gaps for UL/DL switching and other URLLC data. Hence prefer Alt 1. |
| Futurewei | **Proposal 1.1-1**: Support. On DCI 1\_0 size, open to further discuss  **Proposal 1.1-2**: Support.  **Proposal 1.1-3:** Support  **Proposal 1.1-4:** Support  **Proposal 1.1-5:** Support. We prefer Alt 1 (64). |
| Ericsson | **Proposal 1.1-1**  As we commented in the 1st round, we object to supporting DBTW for any SCS until a full solution is available, including exactly which MIB bits are repurposed and/or resolution of potential dependencies to RAN4  The solution must include:   1. If and how additional candidate SSB positions (>64) are to be supported, and 2. How to signal the following: Q and DBTW on/off   We are certainly open to continuing the discussion on the solution for 1 and 2, but until there is convergence, we cannot agree to support DBTW  **Proposal 1.1-2**  We support the proposal (wiht, except for the following:   * ~~For supported SCS cases of DBTW, the indication of use or no use of DBTW will be implicitly indicated (deriving that DBTW is used or not used via configuration of MIB (and SIB1) parameter(s) in certain combinations) in MIB.~~   + ~~FFS details of implicit indication in MIB (and in SIB1)~~   As we commented in the first round, this reverts the following part of the agreement from RAN#104, and the reason for this agreement is that even for unlicensed operation, it allows the DBTW to be disabled for deployments that don't need it.   * If DBTW is supported   + Support mechanism to indicate or inform that DBTW is enabled/disabled for both IDLE and CONNECTED mode UEs     - FFS: how to support UEs performing initial access that do not have any prior information on DBTW.   During initial access, IDLE mode UEs have not yet read SIB1, so the above solution does not work. In our view, the preferred solution is to indicate DBTW on/off using a MIB bit. Some companies have suggested using a different sync raster positions for indicating DBTW on/off, but clearly there is a RAN4 dependency, and we cannot assume that RAN4 follows that design.  Furthermore, we think there is a different understanding amongst companies of what "implicit" means. Some companies refer to implicit as using a particular value of Q to indicate DBTW off, e.g., Q = 64. We support such a mechanism.  **Proposal 1.1-3**  We cannot agree to this proposal until it is identified which bits in MIB can be repurposed . For signaling 4 values of Q, 2 bits needed. So far, we have only seen that there is 1 bit available, namely *subCarrierSpacingCommon*  **Proposal 1.1-4**  We support this proposal with the following modification:  For supported SCS cases of DBTW (if supported), support DBTW lengths {0.5, 1, 2, 3, 4, 5} msec  **Proposal 1.1-5**  This proposal has already been agreed in the prior meeting |
| Huawei, HiSilicon | **Proposal 1.1-1:** Support. Although we believe that DBTW should be supported for all numerologies.  **Proposal 1.1-2:**   * First bullet: We can support this with the clarification that indication of licensed/unlicensed and indication of LBT/No-LBT are two different issues as a system in unlicensed spectrum may or may not use LBT. Therefore, we propose the following clarification:   + No indication for licensed and unlicensed operation will be performed in SSB (including MIB)     - Whether and/or how LBT/No-LBT is indicated is separately discussed. * Second bullet: Support * Third bullet: Support with the following change:   + For supported SCS cases of DBTW, the indication of use or no use of DBTW will be implicitly indicated (~~deriving that~~ DBTW is used or not used is derived via configuration of MIB (and SIB1) parameter(s) in certain combinations) ~~in MIB~~.     - UE assumes DBTW is used prior to deriving implicit indication (Rel-16 NR-U behavior)     - FFS details of implicit indication in MIB (and in SIB1) * Fourth bullet: We can support it for the sake of progress.   **Proposal 1.1-3:** Support  **Proposal 1.1-4:** We cannot support it.  We believe that a similar method as in Rel-16 NR-U should be used to implicitly indicate whether DBTW is enabled or disabled and, if DBTW lengths {0.5, 1, 2, 3, 4, 5} msec is used for all SCSs, such implicit indication would be completely dysfunctional.  Rel-16 NR-U behavior: As explained before in the first round, DBTW enabled/disabled is never explicitly indicated to the UE in Rel-16 NR-U. In Rel-16, UE can infer whether DBTW is enabled/disabled only after reading SIB1 by comparing the maximum number of transmitted SSB indexes (acquired from MIB payload) with the DBTW length (*DiscoveryBurst-WindowLength* provided in SIB1). If DBTW length that is configured in SIB1 is such that DBTW can include more than candidate SSB indexes, UE can infer that DBTW is enabled. In turn, if DBTW length that is configured in SIB1 is such that DBTW cannot include more than candidate SSB indexes, UE can infer that DBTW is disabled. Before reading SIB1, UE assumes that DBTW length is a half frame (includes all candidate SSB positions), and, as such, DBTW is enabled.  Now, assume that DBTW is supported for 960 kHz and = {8,16,32,64} are supported as in Proposal 1.1-3. This means that the first (=8,16,32,64) can be mapped to the first (4, 8, 16, 32) slots where, for the sake of simplicity of the discussion, we assumed that no UL slots are reserved in the first 32 slots. (4, 8, 16, 32) slots in 960 kHz are (*0.0625, 0.125, 0.25, 0.5) ms.*This simply shows that if DBTW lengths {0.5, 1, 2, 3, 4, 5} msec are supported as in Rel-16, since the smallest supported DBTW value is 0.5 ms, UE assumes that DBTW is always enabled if is configured to be any value less than 64.  Other than above, there is also another major problem with supporting {0.5, 1, 2, 3, 4, 5} msec DBTW lengths especially for higher SCSs. Imagine (four slots of SSB) is configured for 960 kHz SCS. Do companies believe that a DBTW length as large as 5 msec is a viable choice for in 960 kHz? We don’t think so. DBTW = 5 msec for in 960 kHz means that UE assumes the pattern of 8 SSBs repeats 80 times!  **Proposal 1.1-5:** Support Alt 1.  A note to **Samsung** and **Qualcomm** regarding implicit indication of DBTW in MIB and SIB1 in Proposal 1.1-2, to our understanding, this is exactly Rel-16 NR-U behavior (please see our above explanation Rel-16 NR-U behavior). We don’t see why such behavior should change in 60 GHz. Please note that, similar to Rel-16 NR-U, UE should assume DBTW is used prior to deriving implicit indication. We suggested adding this UE assumption to the third bullet of Proposal 1.1.-2. |

#### **2nd Round Discussion Summary:**

From the comments companies Proposal 1.1-1 and 1.1-4 seem generally acceptable. Proposal 1.1-2, 1.1-3, and 1.1-5 seem connected in sense that depending on how many SSB candidates are supported, companies have slight different preferences on how to handle the implicit indication for DBTW enable/disable (including whether this is at all needed).

Moderator suggests to first tackle Proposal 1.1-1 and 1.1-4. Next discuss on the actual number of candidates Proposal 1.1-5, then further discuss how to narrow down the proposal even further based on Proposal 1.1-2 and 1.1-3.

##### **Proposal 1.1-1)**

* Support DBTW at least for 120kHz
  + FFS whether DBTW will be applicable for 480/960 kHz SSB SCS
* Ok: vivo, Docomo (apply to all SCS ), Spreadtrum, Nokia, LGE (apply to all SCS), ZTE/Sanechips (apply to all SCS), Samsung, Intel, NEC, Convida, Qualcomm, Futurewei
* Not ok:

##### **Proposal 1.1-4)**

* For supported SCS cases of DBTW, support DBTW lengths {0.5, 1, 2, 3, 4, 5} msec
  + Note: this should be the same as Rel-16 NR-U DBTW lengths.
* Ok: vivo, Spreadtrum, Nokia, LGE, ZTE, Samsung, NEC, Convida, Qualcomm, Futurewei
* Not ok: Intel (only support 5msec)

Down-Select among Alt 1 and Alt 2 during GTW (if possible)

##### **Proposal 1.1-5)**

* For 120kHz SSB, the number of candidates for DBTW is:
  + Alt 1) 64
  + Alt 2) 80
* Alt 1: Docomo, Spreadtrum, LGE, NEC, Convida, Qualcomm, Futurewei
* Alt 2: Nokia, ZTE/Sanechips, Intel

Based on comments received Proposal 1.1-2 and 1.1-3 were updated to 1.1-2A and 1.1-3A.

##### **Proposal 1.1-2A)**

* No indication for licensed and unlicensed operation in MIB ~~will be performed in SSB (including MIB)~~
  + Not ok: vivo
* Use of LBT by the cell and UEs connected to the cell is not indicated MIB.
  + FFS where and how this is indicated, e.g. SIB1
* For supported SCS cases of DBTW, the indication of use or no use of DBTW will be implicitly indicated (deriving that DBTW is used or not used via configuration of MIB ~~(and SIB1)~~ parameter(s) in certain combinations) in MIB.
  + FFS details of implicit indication in MIB ~~(and in SIB1)~~
  + FFS whether information in SIB1 can be utilized to determine whether DBTW is enabled or disabled
* For both licensed or unlicensed operation and with or without LBT, support the same DCI size for:
  + ~~DCI format 1\_0 scrambled with SI-RNTI~~
  + DCI format 0\_0 monitored in a common search space
  + FFS for DCI format 1\_0 scrambled with other RNTI, and other DCI formats

Below are company preferences based on original proposal.

* Ok: vivo, ZTE/Sanechips, Intel, Convida, Qualcomm, Futurewei
* Maybe: Spreadtrum
* Not ok: NEC, Nokia (concern on DCI size aspect), LGE (concern on DBTW enable/disable), Samsung (concern on DBTW enable/disable), NEC (concern on DBTW enable/disable)

##### **Proposal 1.1-3A)**

* For supported SCS cases of DBTW, support configuration of in MIB, with at least {16, 64}~~following~~ ~~{8,16,32,64}~~ values
  + FFS whether 64 can be replaced with disable of DBTW indication
  + No more than 4 states of value are to be supported.

Below are company preferences based on original proposal.

* Ok: vivo, Spreadtrum, Nokia (for alt 2 of proposal 5), LGE, ZTE/Sanechips, NEC, Convida, Futurewei
* Not ok: Samsung (only applicable with DBTW enabled), Intel (support only 2 values), Qualcomm (need to jointly assess proposal 1.1-2 and 1.1-3)

### 2.1.2 SSB Resource Pattern

* From [1] Huawei/HiSilicon:
  + Support following patterns for SSB with 480 kHz and 960 kHz SCS:
    - For operations without shared spectrum:
      * {2,9}+14n, (n=0,1,2,…,31) for both 480 kHz and 960 kHz SCS.
    - For operations with shared spectrum:
      * {2,9}+14n, (n=0,1,2,…,31,40,…,71) for 480 kHz SCS;
      * {2,9}+14n, (n=0,1,2,…,63) for 960 kHz SCS.
* From [2] vivo:
  + For initial cell search in 52.6-71GHz, a UE may assume that half frames with SSB occur with smaller period than FR2 (e.g. 5ms), or lower RAN4 requirement for the cell search time.
  + If CP length of at least one SCS (e.g. 960K) can’t afford beam switching time that is finally determined in RAN4, the following way could be considered for ALT1 and ALT2 respectively:
    - For ALT1, leave enough time gap between any consecutive candidate SSBs by specifying proper value of X and Y;
    - For ALT2, the same QCL (i.e. the same beam) for contiguous candidate SSBs is assumed to achieve time gap for any consecutive candidate SSBs with different QCL assumption.
  + The exact value of ‘n’ should be determined after RAN4 concludes the exact DL-UL switching time for NR operation in FR2-2.
* From [3] Spreadtrum:
  + The SSB pattern for SSB with 480/960kHz SCS can reuse Case A/C in the current spec, i.e. ALT 1) with X=2 and Y=8.
* From [4] Interdigital:
  + Support Alt 1 for the SSB resource patterns for 480/960kHz SCS SSB blocks.
    - First symbols of the candidate SSB have index {X, Y} + 14\*n, where index 0 corresponds to the first symbol of the first slot in a half-frame. value of X and Y are identical for 480kHz and 960kHz
* From [5] Sony:
  + Candidate SSB positions should be extended when DBTW is enabled.
    - For 120 kHz SCS,
      * The number of candidate SSB positions should be 80
      * additional n values (4, 9, 14, 19) should be supported when DBTW is enabled
    - For 480/960 kHz SCS,
      * The number of candidate SSB positions should be 128
      * First symbols of the candidate SSB have index {4, 8, 16,20} + 28\*n, where index 0 corresponds to the first symbol of the first slot in a half-frame
      * n = {0, 1, 2, 3, 5, 6, 7, 8, 10, 11, 12, 13, 15, 16, 17, 18} when DBTW is disabled.
      * n = 0 - 31 when DBTW is enabled
* From [6] Lenovo/Motorola Mobility
  + For supporting NR from 52.6 GHz to 71 GHz in Rel. 17, for higher subcarrier spacings (numerologies) such as 960kHz for SSB, to allow the beam switching between contiguous SSBs, a gap (for example a symbol gap or post-fix) should be supported before beam switching at least for 960kHz
* From [7] Samsung:
  + For 480 kHz and 960 kHz,
    - Support the same SS/PBCH block pattern in a slot, and the same pattern is given by Case A/C (i.e., Alt 1 with X=2 and Y=8).
    - Support larger number of slots including candidate SS/PBCH block, when DBTW is enabled.
* From [8] CATT:
  + For SSB pattern, considering SCS= 960KHz SSB is not supported for initial access，ALT-2 is preferred.
    - ALT 2) First symbols of the candidate SSB have index {4, 8, 16,20} + 28\*n, where index 0 corresponds to the first symbol of the first slot in a half-frame
  + More than 64 SSB transmission opportunities shall be defined within a 5ms SSB burst set to support up to 64 beams for SSB beam sweeping in case of LBT failure. The issue of supporting additional bit(s) for the indicating SSB candidate index needs further study.
  + For no-LBT operation or licensed spectrum operation, value “n” can keep the same value as for the 120KHz SCS case.
  + Additional n value such as #4, #9, #14, and #19 can be used for new SSB candidates if LBT/DBTW is needed for SSB transmission.
  + For up to 71GHz operation and at least for NO-LBT operation, some values of ‘n’ can be reserved for uplink grant scheduling.
* From [9] ZTE/Sanechips:
  + For SSB with 120kHz SCS for NR 52.6 GHz to 71 GHz: the first symbols of the candidate SS/PBCH blocks have indexes {4, 8,16, 20} + 28×n, where index 0 corresponds to the first symbol of the first slot in a half-frame. For carrier frequencies within 52.6 GHz to 71GHz,
    - if DBTW is not supported or disabled, 𝑛 = 0, 1, 2, 3, 5, 6, 7, 8, 10, 11, 12, 13, 15, 16, 17, 18
    - if DBTW is enabled, the additional n values can be equal to 4, 9, 14, 19 to define 16 additional candidate SSB positions
  + For 480kHz/960kHz SSB, the following alternatives can be considered:
    - Alt 1: First symbols of the candidate SSB have index {X, Y} + 14\*n, where index 0 corresponds to the first symbol of the first slot in a half-frame
      * value of X and Y are identical for 480kHz and 960kHz
        + X=2, Y=8
      * if DBTW is not supported or DBTW is disabled
        + For 480kHz SCS, the 64 candidate SSBs are located in 32 slots, with 2 slots spacing between every 8 consecutive slots to avoid prolonged occupation, i.e. n=0, 1, 2, 3, 4, 5, 6, 7, 10, 11, 12, 13, 14, 15, 16, 17, 20, 21, 22, 23, 24, 25, 26, 27, 30, 31, 32, 33, 34, 35, 36, 37
        + For 960kHz SCS, the 64 candidate SSBs are located in 32 slots, with 4 slots spacing between every 16 consecutive slots to avoid prolonged occupation, i.e. n=0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15, 20, 21, 22, 23, 24, 25, 26, 27, 28, 29, 30, 31, 32, 33, 34, 35
      * if DBTW is supported and it is enabled
        + Additional 64 candidate SSB can be defined after the above original 64 candidate SSB in the half frame
    - Alt 2: First symbols of the candidate SSB have index {4, 8, 16, 20} + 28\*n, where index 0 corresponds to the first symbol of the first slot in a half-frame
      * if DBTW is not supported or DBTW is disabled
        + For 480kHz SCS, the 64 candidate SSBs are located in 32 slots (i.e. 16 slot pairs, where 1 slot pair = 2 slots), with 2 slots spacing between every 4 consecutive slot pairs to avoid prolonged occupation, i.e n=0, 1, 2, 3, 5, 6, 7, 8, 10, 11, 12, 13, 15, 16, 17, 18
        + For 960kHz SCS, the 64 candidate SSBs are located in 32 slots (i.e. 16 slot pairs, where 1 slot pair = 2 slots), with 4 slots spacing between every 8 consecutive slot pairs to avoid prolonged occupation, i.e n=0, 1, 2, 3, 4, 5, 6, 7, 10, 11, 12, 13, 14, 15, 16, 17
      * if DBTW is supported and it is enabled
        + Additional 64 candidate SSB can be defined after the above original 64 candidate SSB in the half frame
  + The following options can be considered for supporting beam switching for SSB with SCS 480 kHz and 960 kHz if the CP cannot cover beam switching and other functions simultaneously.
    - Option 1: In a half-frame, any two candidate SSBs are discontinuous in the time domain
    - Option 1-1: SSB pattern with SCS 480/960 kHz can adopt the existing pattern of Case A and Case C in one or two slots defined in Rel-15 NR
    - Option 1-2: SSB pattern with SCS 480/960 kHz should be re-designed to reserve at least one symbol between any two candidate SSBs, e.g. only defining one candidate SSB per slot, or shift the existing SSB by one or more symbols
    - Option 2: Multiple adjacent candidate SSBs are defined to have a same SSB index or QCL assumption
  + In order to reduce the impact of standardization caused by indicating candidate SSB indices, the maximum number of candidate SSB defined in the half-frame can be kept unchanged (maintain 64) or limited to 128 for 480/960 kHz SSB SCS.
* From [11] Ericsson:
  + For SS/PBCH block with 120 kHz SCS, support Case D pattern as defined in Rel-15. No new values of n are supported.
  + Pending confirmation from RAN4 on 59 ns beam switching times, support the FR2 Case D pattern (ALT 2) for time domain pattern for SSB transmissions with 480 kHz and 960 kHz SCS.
  + Conclude that no additional (compared to the already supported 64) candidate SS/PBCH block positions are introduced.
* From [13] Nokia/NSB:
  + Make a working assumption that no beam switching gap need to be assumed between consecutive SSBs at 480kHz and 960kHz sub-carrier spacing.
  + Support in for 480kHz and 960kHz SSB pattern design empty slots without SSB candidate locations at 0.25ms.
  + Define SSB slot patter for 480kHz and 960kHz sub-carrier spacing so that 8 consecutive slots are contain SSB candidate locations, followed by 4 slots are left unoccupied (by SSBs), until all SSBs locations are accounted
    - The slot indexes n={0,1,2,3,4,5,6,7,
      * 12,13,14,15,16,17,18,19,
      * 24,25,26,27,28,29,30,31,
      * 36,37,38,39,40,41,42,43}
    - Note: The additional candidate locations for DBTW are not accounted above.
  + Define SSB symbol level pattern for 480kHz and 960kHz so that first symbols of the candidate SSB locations are {2,8}+14\*n
    - where index 0 corresponds to the first symbol of the first slot in a half-frame, and n is the corresponding SSB slot index
  + For 120kHz SSB pattern, introduce additional candidate locations for SSB transmission support for 𝑛 = 4, 9, 14, 19, where n is the slot index in half-frame.
    - The first symbols of the additional candidate SS/PBCH blocks have indexes {4, 8,16, 20} + 28×n.
  + For 480kHz and 960kHz SSB pattern, introduce additional candidate locations for SSB transmission support for 𝑛 = [{8, 9, 10, 11} ,{32,33,34,35}], where n is the slot index in half-frame.
* From [14] Charter:
  + Support Alt-1 for 480/960 kHz SSB with first symbols of the candidate SSB have index {X, Y} + 14\*n, where index 0 corresponds to the first symbol of the first slot in a half-frame. The value of n is the same for LBT and no-LBT operation.
* From [16] Panasonic:
  + For SSB symbol position, Case D SSB pattern is reused (i.e., Alt 2).
  + For SSB slot position, Case D SSB patten is reused (i.e., n = 0, 1, 2, 3, 5, 6, 7, 8, 10, 11, 12, 13, 15, 16, 17, 18).
* From [17] OPPO:
  + for SSB pattern design, support Alt-1 {X,Y}+14\*n, with X=1, Y=8.
  + for SSB candidate number within half frame, support the followings
    - For 480kHz, SSB candidate index {1,8}+14\*n, with n=0~63
    - For 120kHz, SSB candidate index {4, 8,16, 20} + 28\*n, with n=0~19
* From [18] Qualcomm:
  + for 480kHz/960kHz SSB, select the following alternative:
    - ALT 1) First symbols of the candidate SSB have index {X, Y} + 14\*n, where index 0 corresponds to the first symbol of the first slot in a half-frame
      * value of X and Y are identical for 480kHz and 960kHz
      * X = 2 and Y = 9
      * Values of ‘n’ shall not be all consecutive integer values (i.e. non-candidate SSB slots are positioned every few candidate SSB slots)
* From [19] LG Electronics:
  + Support of additional n values for the time domain pattern of SS/PBCH block with 120 kHz SCS can be considered to increase SS/PBCH block’s transmission opportunities, only if PBCH payload is sufficient to indicate the increased number of candidate SS/PBCH block indexes.
  + For 480/960 kHz SSB, first symbols of the candidate SSB have index are {4, 8, 16, 20} + 28\*n, where index 0 corresponds to the first symbol of the first slot in a half-frame (i.e., Alt 2 in previous agreement), and values of ‘n’ are consecutive integers (i.e., n = 0, 1, 2, 3, 4, 5, 6, 7, 8, 9, 10, 11, 12, 13, 14, 15).
* From [20] ETRI:
  + Prefer to keep the current 64 SSB candidate positions for 120kHz.
  + Propose to support ALT 1 as SSB patterns for 480kHz and 960kHz SSB.
    - Details on values for X, Y, and n should be further studied.
* From [21] Mediatek:
  + For SSB SCS=120 kHz, additional SSB candidate positions is not needed.
  + For SSB SCS=480/960 kHz, Alt 2 should be supported as the baseline scheme.
* From [22] Intel:
  + Consider at least 1 symbol gap between consecutive SSBs within a slot.
  + Consider at least 1 symbol gap between SSB and the start of the next slot, where PDCCH could be transmitted.
  + Consider SSB pattern in a slot with 3 SSB containing slots, each slot with 2 SSB position, followed by 1 non-SSB carrying slot for 480 kHz and 6 SSB carrying slots followed by 2 non-SSB carrying slots for 960kHz, to accommodate Rx-Tx switching gap.
    - For 480kHz and 960kHz SCS based SSB, first symbols of the candidate SSB have indexes {2,9} + 14×n, where index 0 corresponds to the first symbol of the first slot in a half-frame.
    - For 480kHz, n = {0,1,2, 4,5,6, 8,9,10, 12,13,14, 16,17,18, 20,21,22, 24,25,26, 28,29,30, 32,33,34, 36,37,38, 40,41}, {42, 44,45,46, 48,49,50, 52,53,54, 56,57,58, 60,61,62, 64,65,66, 68,69,70, 72,73,74, 76,77,78, 80}.
      * The second set of n values could be used to enable larger number of candidate SSBs, i.e.,
    - For 960kHz, n = {0,1,2,3,4,5, 8,9,10,11,12,13, 16,17,18,19,20,21, 24,25,26,27,28,29, 32,33,34,35,36,37, 40,41}, {42,43,44,45, 48,49,50,51,52,53, 56,57,58,59,60,61, 64,65,66,67,68,69, 72,73,74,75,76,77, 80,81,82,83}.
      * The second set of n values could be used to enable larger number of candidate SSBs, i.e.,
* From [23] Apple:
  + Support to introduce a unified SSB Pattern for 480kHz SCS and 960kHz SCS (if supported):
    - The first symbol of candidate SSB have indexes {2,9,16,23} within each SSB burst.
    - Reserve 2 slots for DL/UL and UL/DL switching to allow for fast UL transmission between two SSB bursts.
* From [24] Sharp:
  + Based on SSB resource pattern Case D of FR2, other values of n (e.g., 4, 9, 14, 19) should be added for the SSB with 120kHz SCS in above 52.6GHz.
* From [25] NTT Docomo:
  + On down-selection regarding SSB symbol definition, whether to reuse Case D should be discussed considering whether to practically support SSB-CORESET#0 multiplexing within the same slot
  + With 120 kHz SCS, ‘n’ value(s) which can be added on top of the ones agreed already are limited, i.e., ‘n’ = {4, 9, 14, 19} only
  + With 120 kHz SCS, no significant need to support additional ‘n’ values on top of the ones agreed already
  + With 480/960 kHz SCS, non-consecutive SSB slots should be defined to e.g., make UL transmissions possible in the middle of SSB burst.
    - Larger number of consecutive non-SSB slots can be defined during SSB burst can be defined to obtain scheduling flexibility of a DCI (e.g., with repetition and/or multi-PDSCH/PUSCH scheduling)
  + With 480/960 kHz SCS, not support more than 64 candidate SSB positions
* From [26] Xiaomi:
  + For 480 kHz SSB design, we support the option 1 and the n should be no difference for LBT/no LBT operation.
    - [Moderator Note: This might be Alt 1, instead of option 1]
* From [28] WILUS:
  + At least one symbol gap in time domain between SS/PBCH blocks with different SSB indices should be considered for higher subcarrier spacing by taking a beam switching gap into account due to a RF interruption time of Tx/Rx beams and/or LBT gap in unlicensed spectrum.
  + We prefer to have Alt-1 of two alternatives for SS/PBCH block pattern in time domain
    - ALT 1) First symbols of the candidate SSB have index {X, Y} + 14\*n, where index 0 corresponds to the first symbol of the first slot in a half-frame
    - value of X and Y are identical for 480kHz and 960kHz
      * FFS: exact value of X and Y

#### Summary of Discussions

In RAN1 #105e the following agreement was made.

|  |
| --- |
| **Agreement:**  For 480kHz/960kHz SSB, select one of the following alternatives:   * ALT 1) First symbols of the candidate SSB have index {X, Y} + 14\*n, where index 0 corresponds to the first symbol of the first slot in a half-frame   + value of X and Y are identical for 480kHz and 960kHz     - FFS: exact value of X and Y * ALT 2) First symbols of the candidate SSB have index {4, 8, 16,20} + 28\*n, where index 0 corresponds to the first symbol of the first slot in a half-frame * Values of n for 480kHz and 960kHz for ALT 1 and 2   + FFS: whether number of values for ‘n’ depend on LBT operation (i.e. LBT vs no-LBT)   + FFS: exact values of ‘n’ for each SCS   + Values of ‘n’ for one mode of operation shall be strictly a subset of values for another mode of operation, if two mode of operation exist for number of candidate SSBs   + FFS: whether values of ‘n’ shall not be all consecutive integer values (i.e. non-candidate SSB slots are positioned every few candidate SSB slots) |

* SSB pattern for 480/960kHz
  + ALT 1)
    - {X, Y} + 14\*n
      * Interdigital, [Lenovo/Motorola Mobility], Charter, ETRI, [Xiaomi], WILUS, Futurewei
    - (Alt 1-A) {2, 9} + 14\*n



* + - * Huawei/HiSilicon, Qualcomm, Intel, [Apple], Samsung, ZTE/Sanechips
    - (Alt 1-B) {1,8} + 14\*n, Futurewei



* + - * OPPO, Samsung, Futurewei
    - (Alt 1-C) {2, 8} + 14\*n



* + - * Spreadtrum, Samsung, ZTE/Sanechips, Nokia/NSB
  + ALT 2) Case D {4, 8, 16,20} + 28\*n



* + - Sony, CATT, ZTE/Sanechips, Ericsson, Panasonic, LGE, Sharp, MTK
* Supported values of ‘n’
  + Several companies suggested to have few slots that does not have SSB candidates every few slots that have SSB candidates.
  + Moderator notes that supported values of ‘n’ seems to be heavily dependent on DBTW discussion, and therefore suggest to discuss in Section 2.1.1.

#### **1st Round Discussion:**

Moderator suggest to discuss further based on the alternatives presented (above). Also moderator asks if companies who expressed opinion on ALT 1, can support one of the patterns suggested by companies or not.

|  |  |
| --- | --- |
| Company | Comments |
| Samsung | * We support Alt 1-C since it’s one of the supported pattern in Rel-15. We are also supporting Alt 1-A or Alt 1-C if any of them can get consensus. Comparing the three alternatives in Alt 1, Alt 1-A is the best, but we discussed this issue before in Rel-16 NR-U… * For Alt 2, our concern is this pattern is not compatible with the Type0-PDCCH configuration in MIB, i.e., a Type0-PDCCH starting from symbol 7 has collision with the SSB symbol. Also, we want to point out that this pattern is mainly for mixed numerology multiplexing, but this is not a design target in FR2-2. |
| Qualcomm | We are supportive of Alt 1-A ({2, 9} + 14\*n) for the following reasons:   * Allow for gNB beam switching gaps (for slower gNBs)   Allow for possibility of back-to-back multiplexing of CORESET0 + SSB of the same beam (2 symb CORESET0 beam 1 + 4 symb SSB beam 1 + GAP + 2 symb CORESET0 beam 2 + 4 symb SSB beam 2) |
| Panasonic | We think the necessity of a gap symbol due to beam switching time needs to be clarified. According to agreed LS in RAN4(R4-2107985), RAN4 tentatively agreed [59 ns] for gNB beam switching time. “59 ns” fulfils the condition where no explicit switching gap is needed between consecutive SSBs for 960 kHz SCS according to TR38.808 section 4.2.2.4. Thus, we support Alt 2 because potential specification works can be reduced. If a gap symbol is needed due to other factors (e.g., UE Rx beam switching time), we slightly prefer Alt 1-A taking into account allocating a gap symbol and PDCCH between SSBs. |
| Mediatek | Our view was missed in the above summary. We share similar view with Panasonic. Currently RAN 4 has a tentative agreement for beam switching gap, which does not exceed the CP length when SSB SCS is 960 kHz. We are open for further discussion, but we don’t see strong motivation to reserve additional symbol gap for other reasons except for beam switching gap. |
| Sharp | Our original preference is Alt 2 for the minor spec effort, but we could also support Alt 1-A. |
| NTT Docomo | * Maybe good to have a consensus on how to interpret RAN4 LS reply, which says smaller value than CP with 960 kHz SCS is agreed although it is “tentative”. Since it is an important factor to decide the direction here, it would be worth discussing how to treat the tentative value in RAN1 in our view. * Once the tentative value is treated as something we should follow, then we fail to see the motivation to change SSB symbols from case D, which is already supported in 120 kHz SCS. * Otherwise we agree to consider something other than case D. among them, our best preference is {2, 9} since “reuse of the existing NR” is no longer a justification in this case. We believe we can pursue a kind of optimized spec here. |
| ZTE, Sanechips | From the perspective of reducing the impact of standardization, Alt 1-C and Alt 2 are better. However, since RAN4 does not fully determine the value of beam switching time at gNB/UE sides, we can not guarantee that case D can work for beam switching at this stage. Therefore, at least one symbol interval between any two neighbor SSBs should be reserved. So Alt 1-A and Alt 1-C seem more appropriate. Compared with Alt 1-A and Alt 1-C, Alt 1-A is a half-slot symmetric structure, which has many advantages e.g. reduced beam switching times and low detection complexity, so we slightly prefer Alt 1-A.  Please see our added support above using “ZTE/Sanechips” |
| Nokia | In our understanding RAN4 has not concluded that there is a need to assume gap for the gNB beam switching. That being said, while our preference would be alt 1-C, we could also consider alt 1-A.  We do not prefer Alt 1-B as it would limit the PDCCH transmission to single symbol at the start of the slot. |
| OPPO | We support Alt-1B, the design principle is similar to QC’s suggestion, i.e. back-to-back multiplexing. With Alt-1B, the network can also multiplex RMSI with SSB and CORESET for 480kHz SCS. |
| LG Electronics | We strongly support ALT 2. It should be noted that we accepted the introduction of new SCS SSB by adding a NOTE below.  Agreement:  For the case where SSB location and SCS are explicitly provided to the UE (non-initial access) and SSB does not configure Type-0 PDCCH, support 480 kHz and 960 kHz numerologies for the SSB   * Note: Strive to minimize specification impact due to the new SCS for SSB   If we go with Alt 1-A or Alt 1-B, it is a totally different design compared to legacy SSB pattern. Furthermore, based on RAN4 LS, RAN4 tentatively agreed 59 ns for gNB beam switching time and this value is not a problem even for 960 kHz SCS since it is less than 80 % of CP portion. Regarding the back-to-back transmission of SSB and CORESET#0, this issue was extensively discussed in NR-U but was not adopted since how to multiplex SSB and CORESET#0 is up to gNB’s implementation. |
| NEC | Considering the pending requirement from RAN4 for the beam switching gap, we still cannot conclude Alt 2 is applicable now, although it has the less impact on specification. As to the other alternatives, we prefer Alt 1-A with a structure convenient for implement and detection, and considering the beam switching gap as well. |
| Xiaomi | We support Alt1, and Alt 1-A is preferred for one symbol switching time can be supported. |
| Lenovo, Motorola Mobility | We support ALT1 and within that we prefer Alt 1-A, but we are also fine with Alt 1-C if majority of companies support it. |
| Intel | We don’t support Alt2 and we could discuss the variant of Alt1 though our preference is Alt1-A.  We do see strong necessity in time gaps in the DL not because of beam switching only but also because of MIMO TAE. As we tried to explain in our tdoc, MIMO TAE in combination with beam switching together may cause signal distortion if no gaps are placed as illustrated below for 2 Tx port at gNB:    To accommodate MIMO TAE and beam switching some large time interval is needed than just a CP because whether MIMO TAE is late or early is not known at the Tx. This could be illustrated as follows for late and early MIMO TAE:    To be safe, the time interval between symbols should cover 2 times MIMO TAE plus beam switching transient period. Considering current MIMO TAE for gNB of 65 ns, neither CP of SCS 480 kHz nor CP of SCS 960 kHz is suitable. We also need to consider Rx beam switching that could occur at the UE. UE may need to use different beams for different SSB measurements, and we know UE beam switching is expected to be larger than gNB beam switching, especially if it is inter-panel beam switching. Therefore, we support SSB patterns with gaps between consecutive SSBs. |
| Futurewei | Please see our added support above using “Futurewei”. We support ALT 1, more precisely we prefer Alt 1-C, however we are OK with the other options in ALT 1 if they get consensus |
| Ericsson | We share a similar view as LGE, and we would like to maintain similar design as FR2, i.e., Case D pattern (Alt-2). We also agree with the comments on RAN4's discussion on beam switching time – 59 ns (even if still unconfirmed) is less than the CP for both 480 kHz and 960 kHz. We don't think that MIMO TAE is a correct argument given that that requirement is left over from 3G days, and it is not clear that it is relevant for modern active antenna systems. Regarding multiplexing of RMSI and SSB, considering the minimum bandwidth channels for 120 and 480 kHz (100 and 400 MHz), it is not clear that there is sufficient number of RBs available for carrying typical RMSI payloads (~700 or more bits) if one wants to configure 2 SSBs per slot. So, we don't think that optimizing an SSB pattern to fit two Type0-PDCCH monitoring locations, two SSBs, and two RMSI PDSCHs is the correct design goal. |
| CATT | Similar view with LGE and Ericsson. ALT2 because this bring the least impact for specification. |
| Sony | Our 1st preference is Alt 2 because of small specification impact. If there is critical issue on gNB beam switching time, we are fine with Alt 1-C as 2nd preference. |
| Huawei, HiSilicon | We support Alt 1-A. We prefer two have three symbols gap between SSBs in a slot:   * One symbol as a beam switching gap given the fact that, according to ongoing discussions in RAN4, UE’s beam switching time can be in the order of 100-200 ns. Even if the beam switching delay at the UE and gNB are the same (tentatively [59ns]), 72 ns CP for 960 kHz SSB may not be able to absorb DL asynchrony, channel spread, and beam switching time.   Two more symbols to facilitate configuration of up to a two-symbol CORESET#0 prior to the second SSB in the slot. |

#### **1st Round Discussion Summary:**

Companies supportive of Alt 1 generally seems to be ok with Alt 1-A. Other than Alt 1-A, Alt 2 seems to also have some support. The WID explicitly stated to minimize specification impact therefore suggest that we take Alt 2 unless problems are identified for Alt 2. At the same time, companies pointed out the beam switching gap information from RAN4 is currently incomplete so there is risk Alt 2 could have problems later. One company pointed out issues with beam switching gap in conjunction with MIMO TAE which may pose problems if there is no gap between SSBs. Between Alt 1-A and Alt 2, the company split is 14 versus 9. Moderator suggests to see if we can converge to Alt 1-A.

|  |
| --- |
| * SSB pattern for 480/960kHz   + ALT 1)     - {X, Y} + 14\*n       * Interdigital, [Lenovo/Motorola Mobility], Charter, ETRI, [Xiaomi], WILUS, Futurewei     - (Alt 1-A) {2, 9} + 14\*n       * Huawei/HiSilicon, Qualcomm, Intel, [Apple], Samsung, ZTE/Sanechips, [Panasonic (if gap is needed)], Sharp (2nd preference), [NTT Docomo (2nd preference)], Nokia (2nd preference), NEC, Xioami, Lenovo/Motorola Mobility, Futurewei     - (Alt 1-B) {1,8} + 14\*n,       * OPPO, Samsung, Futurewei     - (Alt 1-C) {2, 8} + 14\*n       * Spreadtrum, Samsung, ZTE/Sanechips, Nokia/NSB, Lenovo/Motorola Mobility (2nd preference), Futurewei   + ALT 2) Case D {4, 8, 16,20} + 28\*n     - Sony, CATT, ZTE/Sanechips, Ericsson, Panasonic, LGE, Sharp, MTK, [NTT Docomo] |

##### **Proposal 1.2-1)**

* First symbols of the candidate SSB have index {2, 9} + 14\*n, where index 0 corresponds to the first symbol of the first slot in a half-frame.



#### **2nd Round Discussion:**

Please provide further comments on Proposal 1.2-1.

|  |  |
| --- | --- |
| Company | Comments |
| vivo | We suggest to defer the discussion when RAN4 has a clear conclusion. An important factor to impact the SSB time pattern design is the actually required beam switching time, which is still under discussion in RAN 4. Thus, we think it is better to discuss the SSB time pattern design after RAN4 has a clear-out conclusion. |
| DOCOMO | We tend to agree with Ericsson – may still not be well justified why we need to have beam switching gap. |
| Spreadtrum | Alt 1-C is our preference. |
| Nokia | Proposal 1.2-1: We are OK with this proposal with a minor edit that we indicate that this applies to both, 480kHz and 960kHz sub-carrier spacing, e.g.:   * For 480kHz and 960kHz sub-carrier spacing, first symbols of the candidate SSB have index {2, 9} + 14\*n, where index 0 corresponds to the first symbol of the first slot in a half-frame |
| LG Electronics | We do not support Proposal 1.2-1, which is not aligned with previous RAN1 agreement. |
| ZTE, Sanechips | We support Proposal 1.2-1 as it is the best choice before RAN4 makes a final decision. In addition, even if RAN4 finally conclude that beam switching gap is not needed, Alt 1-A can still work well. |
| Samsung | We are ok with the proposal and Nokia’s modification. We are also ok with Alt 1-C.  For the beam sweeping gap, we believe supporting any of Alt 1 can be independent of RAN4’s decision – no matter beam sweeping gap is needed or not, Alt 1 always works.  Also, we really don’t understand the reasoning why 120 kHz SCS SSB pattern is a baseline for 480 kHz and 960 kHz. If 240 kHz SSB pattern is scaled from 120 kHz, we can accept this argument, but obviously it’s not the case.  For multiplexing 2 Type0-PDCCH and 2 SSB in a slot, we believe this is the most fundamental scenario to be supported for FR2, especially for unlicensed band. Please note that a Type0-PDCCH starting from symbol 7 is in particularly supported for FR2 ONLY, and Alt 2 is not compatible with such configuration. |
| Intel | Support Proposal 1.2-1.  As mentioned previously, RAN4 LS only tentatively concludes on simple beam switching gap, but we need to factor into account MIMO TAE + beam switching (both intra-panel and inter-panel), and also beam switching at the UE (both intra-panel and inter-panel). While the LS from RAN4 is not conclusive, we think it has ample evidence that 74ns CP for 960kHz will not be enough for inter-panel beam switching and once we consider MIMO TAE.  We ask companies, who think gap is not needed, on what their understand is regarding inter-panel beam switching values for gNB and UE. |
| NEC | We support the Proposal 1.2-1, namely Alt 1-A, and share the similar view as ZTE. |
| Apple | We support Proposal 1.2-1.  It should be noted that 59ns beam switching gap is defined for gNB, instead of UE side as clearly written in LS. |
| Qualcomm | We support Proposal 1.2-1 (also with Nokia’s edits).  As for previous RAN1 agreement “*Note: Strive to minimize specification impact due to the new SCS for SSB*”, we agree that specification impact should be minimized as long as we maintain the same level of performance/functionality, which Alt2 may not be able to for some gNB implementations. |
| Sharp | We are fine with Proposal 1.2-1 and Nokia’s modifications. |
| Futurewei | We are fine with the Proposal 1.2-1. |
| Ericsson | We prefer Alt-2 for the reasons already stated. If companies are really worried about beam switching gap, we can wait for RAN4 to confirm the [59 ns] gNB beam switching time. |
| Huawei, HiSilicon | We support the proposal with Nokia’s modification.  As we pointed out in the first round of discussion and by multiple other companies, according to ongoing discussions in RAN4, UE’s beam switching time can be in the order of 100-200 ns. Even if the beam switching delay at the UE and gNB would be the same (tentatively [59ns]), 72 ns CP for 960 kHz SSB may not be able to absorb DL asynchrony, channel spread, beam switching time, and MIMO TAE. Please note that SSB design should also take into account UE beam switching time and not only the gNB bema switching time.  Also, we agree with ZTE that even if it turns out that beam switching gap is not required, the design in Proposal 1.2-1 would still works perfectly. |

#### **2nd Round Discussion Summary:**

Moderator suggests to further discuss based on Proposal 1.2-1A (minor edit of Proposal 1.2-1). Below is a summary of company preferences.

##### **Proposal 1.2-1A)**

* For 480kHz and 960kHz sub-carrier spacing, f~~F~~irst symbols of the candidate SSB have index {2, 9} + 14\*n, where index 0 corresponds to the first symbol of the first slot in a half-frame.



Ok: ZTE/Sanechips, Samsung, Intel, NEC, Apple, Qualcomm, Sharp, Futurewei

Not Ok: Docomo, LGE

Defer discussion: vivo

### 2.1.3 CORESET#0 Configuration

* From [1] Huawei/HiSilicon:
  + For CORESET for Type0-PDCCH in 52.6GHz to 71GHz spectrum, support the following:
    - For {SS/PBCH Block, CORESET for Type0-PDCCH} SCS equal to {120, 120} kHz, support multiplexing pattern 1 and multiplexing pattern 3 as per Agreement in RAN1 104-e.
    - For {SS/PBCH Block, CORESET for Type0-PDCCH} SCS equal to {480, 480} kHz, support multiplexing pattern 1 only.
    - For {SS/PBCH Block, CORESET for Type0-PDCCH} SCS equal to {960, 960} kHz, support multiplexing pattern 1 only.
  + For {SS/PBCH Block, CORESET for Type0-PDCCH} SCS equal to {120, 120} kHz, in addition to the supported values of (, ) from Rel-15, support with .
  + Support the following CORESET#0 RB offsets values for {SSB, CORESET#0} SCS={120, 120} kHz:
    - For CORESET#0 with 24 RBs and 48 RBs: the same as supported values in Table 13-8 of 38.213.
    - For CORESET#0 with 96 RBs: 0, 38, 76 RBs for multiplexing pattern 1 and -20 (-21) RBs when for multiplexing pattern 3.
    - Note: All above RB offsets are nominal and may need to be modified after finalizing synch raster and channel raster design in FR2-2.
  + Support at least the following combinations in 52.6GHz to 71GHz spectrum:
    - for {SSB, CORESET#0} ={480, 480} kHz with multiplexing pattern 1, , ={1,2};
    - for {SSB, CORESET#0} ={960, 960} kHz with multiplexing pattern 1, , ={1,2}.
  + To find the offset between an off-synch raster SSB and the corresponding CORESET#0 in 60GHz unlicensed spectrum, RAN1 should uniquely determine the hypothetical on-synch raster SSB that serves as the reference for the offset to the off-synch raster SSB in case more than one synch rasters are included in a channel bandwidth.
* From [2] vivo:
  + Dedicated signalling can’t be used for conveying the Type-0 PDCCH configuration to read the SIB1.
  + The following SSB-Coreset 0 multiplexing patterns are supported for each SCS pair when operation in FR2-2 (52.6-71GHz):
    - (120K, 120K): Pattern 1, Pattern 3
    - (480K, 480K): Pattern 1, Pattern 3
    - (960K, 960K): Pattern 1, Pattern 3
  + For {SSB, PDCCH} SCS {120, 120} kHz, {480, 480} kHz and {960, 960} kHz in licensed band, the tables for CORESET#0 and type0-PDCCH CSS set configuration defined for FR2-1 in Rel-15 can be reused.
  + For the un-licensed band operation from 52.6GHz to 71GHz, the CORESET design principle should consider two aspects: 1. Occupy as much bandwidth as possible; 2. Use as few bits as possible in the CORESET configuration.
  + For {SSB, PDCCH} SCS {120, 120} kHz, {480, 480} kHz and {960, 960} kHz, the tables for PDCCH monitoring occasions for type0-PDCCH CSS set configuration defined for FR2-1 in Rel-15 can be reused with little adjustment.
* From [3] Spreadtrum:
  + The mechanism of two offsets in MIB defined for NR-U, i.e. Alt 2 (use configuration in MIB to support CORESET#0/Type0-PDCCH), can be reused for UE to determine CORESET#0/Type0-PDCCH.
* From [4] Interdigital:
  + Support Alt 2 on using the CORESET#0/Type0-PDCCH configuration in MIB.
  + Introduce the enhancements on SS/PBCH block transmission patterns to deliberately include the CORESET#0 and SIB1 in fixed time locations along with the corresponding SS/PBCH block to ensure the channel occupancy as much as possible, in the initial access operations for unlicensed spectrum in beyond 52.6GHz.
* From [7] Samsung:
  + For SS/PBCH block with 120 kHz SCS,
    - only support CORESET#0 SCS as 120 kHz;
    - additional CORESET#0 RB offsets are needed;
    - support 96 RB as the number of RBs for CORESET#0.
  + For SS/PBCH block with 480 kHz SCS and 960 kHz,
    - only support CORESET#0 SCS same as SS/PBCH block SCS;
    - support at least the same SS/PBCH block and CORESET#0 multiplexing patterns, number of RBs for CORESET#0, and number of symbols as in 120 kHz SCS;
    - support 96 RB as the number of RBs for CORESET#0;
    - Further study the RB offset based on RAN4 design of channel and synchronization rasters.
* From [8] CATT:
  + Multiplexing pattern 2 or 3 can be used for further multiplexing SSB/CORSET#0 with periodic CSI-RS/paging PDCCH&PDSCH in frequency.
  + For SSB and CORESET#0/Type0-PDCCH with 120 KHz SCS, support the following combinations of SSB/CORESET multiplexing pattern, number of RB and symbols for CORESET.
    - {mux pattern 1, 48 PRB CORESET, 1 symbol CORESET}
    - {mux pattern 1, 48 PRB CORESET, 2 symbol CORESET}
    - {mux pattern 3, 48 PRB CORESET, 2 symbol CORESET}
* From [9] ZTE/Sanechips:
  + The multiplexing pattern 1 and 3 for three approved SCS combinations of SSB and Type0-PDCCH can be considered for Rel-17 NR above 52.6 GHz.
    - (SSB, Type0-PDCCH): SCS (120 kHz, 120 kHz)
    - (SSB, Type0-PDCCH): SCS (480 kHz, 480 kHz)
    - (SSB, Type0-PDCCH): SCS (960 kHz, 960 kHz)
  + For {SSB, CORESET#0 for Type0-PDCCH} SCS = {120, 120} kHz, even though RAN4 has agreed the minimum CBW is increased to 100 MHz, at least SSB and CORESET#0 multiplexing patterns, number of RBs for CORESET#0, number of symbols (duration of CORESET#0) that are supported in Rel-15/16 should still be supported.
* From [11] Ericsson:
  + RAN1 should strive to design a common CORESET0 configuration table for use for all 3 supported SCS combinations (120,120), (480,480), and (960, 960).
  + Reuse existing Table 13-12 in 38.213 for operation with 480 and 960 kHz SCS. For subcarrier spacings 480 and 960 kHz. Use and , respectively, instead of when determining the PDCCH monitoring occasions using offset values from the table.
* From [12] Futurewei:
  + In FR2-2 CORESET#0, PDCCH SIB1 support the same SCS as the SCS for SS/PBCH.
* From [13] Nokia/NSB:
  + Consider also SSB and CORESET#0 multiplexing pattern 3 for 120kHz SSB.
  + Pending on the UE minimum BW capability, consider also SSB and CORESET#0 multiplexing pattern 3 for 480kHz SSB.
  + For CORESET#0 with 120kHz sub-carrier spacing, consider supporting also ={96} for multiplexing pattern 1.
  + For SSB and CORESET#0 with 480kHz sub-carrier spacing with SSB and CORESET#0 multiplexing pattern 1, support following options:
    - ={[1],2, 3}
    - ={24, 48}.
  + For SSB and CORESET#0 with 480kHz sub-carrier spacing with SSB and CORESET#0 multiplexing pattern 3, following configuration options could be considered:
    - ={1,2}
    - ={24, 48}.
  + For SSB and CORESET#0 with 960kHz sub-carrier spacing, with SSB and CORESET#0 multiplexing pattern 1 support
    - ={2, 3}.
    - ={24}.
* From [18] Qualcomm:
  + for FR2-2, CORESET0 SCS = SSB SCS for all SCSs
  + consider minimizing the overhead of beam switching gaps by:
    - Supporting multiplexing pattern 3
    - Introducing an SSB/CORESET0 multiplexing pattern for higher SCS SSB (480 and 960 kHz), where TDM grouping of the SSB and the corresponding CORESET0 is considered
* From [19] LG Electronics:
  + Reuse Table 13-8 in TS 38.213 specification for CORESET#0 configuration with 120/480/960 kHz, except for RB offset values.
  + Reuse Table 13-12 in TS 38.213 specification for type0-PDCCH CSS set configuration with 120/480/960 kHz, except for O values for 480/960 kHz.
* From [21] Mediatek:
  + Support only 1 SCS for CORESET#0/Type0-PDCCH for a given SSB SCS.
* From [22] Intel:
  + Consider using Type0-PDCCH search space in symbols {0,1} and {7, 8} for each SSB.
* From [23] Apple:
  + In addition to 24 and 48 PRBs, 96 PRBs can be considered for CORESET#0 BW with 120kHz SCS.
* From [25] NTT Docomo:
  + On down-selection regarding SSB symbol definition, whether to reuse Case D should be discussed considering whether to practically support SSB-CORESET#0 multiplexing within the same slot
  + With all SCSs supported in 52.6 – 71 GHz and with the restriction agreed in RAN#91-e, the existing SSB-CORESET#0 multiplexing pattern 1 specified in 38.213 with Table 13-8 and 13-12 works as it is.
    - Feasibility of a certain case, where e.g., 2 pairs of {Type0-PDCCH, SIB1 PDSCH} are allocated in a slot, is not clear
    - With 960 kHz SCS, smaller ’O’ value can be added considering shorter time duration SSB beam sweeping
* From [26] Xiaomi:
  + It should be clarified that {480,120} kHz combination of SSB with CORESET#0/Type0-PDCCH SCS is not supported.
* From [28] WILUS:
  + We propose that SS/PBCH block and CORESET#0/RMSI can be multiplexed in TDM/FDM within a slot considering multi-beam operation and it can be closely located without the gap between SSB and CORESET#0/RMSI for not allowing any in-between channel access operation in the unlicensed band.

#### Summary of Discussions

The following are a summary of company views on CORESET#0 configuration aspects.

* For {SSB, CORESET#0/Type0-PDCCH} = {120, 120} kHz
  + controlResourceSetZero
    - Addition of 96 PRB CORESET#0
      * Support: Huawei/HiSilicon, Samsung, Nokia/NSB, Apple
      * Do not support: Ericsson
* For {SSB, CORESET#0/Type0-PDCCH} = {480, 480} kHz
  + controlResourceSetZero
    - Support {24, 48} PRB with {1,2} symbol durations
      * Huawei/HiSilicon
    - Use Table 13-8 (originally intended for {120,120} kHz) except RB offset
      * {mux pattern 1, 24 PRB, 2 symbol}
      * {mux pattern 1, 48 PRB, 1 symbol}
      * {mux pattern 1, 48 PRB, 2 symbol}
      * {mux pattern 3, 24 PRB, 2 symbol}
      * {mux pattern 3, 48 PRB, 2 symbol}
      * [vivo], ~~[~~Samsung (with 96 RB as well)~~]~~, ~~[~~Ericsson~~]~~, LGE, NTT Docomo, Qualcomm
    - Support mux pattern 1 with {24, 48} PRB and {[1],2,3} symbol duration
      * Nokia/NSB
    - Support mux pattern 3 with {24, 48} PRB and {1,2} symbol duration
      * Nokia/NSB, Samsung
    - Support mux pattern 3
      * Qualcomm, Samsung
  + searchSpaceZero
    - Use Table 13-12 (originally intended for {120,120} kHz)
      * NTT Docomo, Ericsson
    - Use Table 13-12 (originally intended for {120,120} kHz) except O values
      * LGE, Samsung, Huawei/HiSilicon
    - Use symbols {0,1} and {7,8} for Type0-PDCCH for each SSB
      * Intel, Qualcomm, Huawei/HiSilicon
* For {SSB, CORESET#0/Type0-PDCCH} = {960, 960} kHz
  + controlResourceSetZero
    - Support {24} PRB with {1,2} symbol durations
      * Huawei/HiSilicon
    - Use Table 13-8 (originally intended for {120,120} kHz) except RB offset
      * {mux pattern 1, 24 PRB, 2 symbol}
      * {mux pattern 1, 48 PRB, 1 symbol}
      * {mux pattern 1, 48 PRB, 2 symbol}
      * {mux pattern 3, 24 PRB, 2 symbol}
      * {mux pattern 3, 48 PRB, 2 symbol}
      * [vivo], ~~[~~Samsung (with 96 RB as well)~~]~~, ~~[~~Ericsson~~]~~, LGE, NTT Docomo, Qualcomm [24 RB only]
    - Support mux pattern 1 with {24~~8~~} PRB and {2,3} symbol duration
      * Nokia/NSB, Samsung
    - Support mux pattern 3
      * Qualcomm, Samsung
  + searchSpaceZero
    - Use Table 13-12 (originally intended for {120,120} kHz)
      * NTT Docomo, Ericsson,
    - Use Table 13-12 (originally intended for {120,120} kHz) except O values
      * LGE, Samsung, Huawei/HiSilicon
    - Use symbols {0,1} and {7,8} for Type0-PDCCH for each SSB
      * Intel, Qualcomm, Huawei/HiSilicon

#### **1st Round Discussion:**

There were some suggestions on mux pattern 3 support. Since the updated WID explicitly mentions to prioritize mux pattern 1, moderator suggests it is suggested to discuss mux pattern 1 aspects first and once concluded continue further discussion mux pattern 3 aspects.

Companies are asked to comment further on the following issues:

Q1) addition of 96 PRB CORESET#0 for {120kHz, 120kHz}={SSB, PDCCH} pair to ‘controlResourceSetZero’ field

Q2) Supported PRB and symbol duration with mux pattern 1 for {480kHz, 480kHz}={SSB, PDCCH} pair and {960kHz, 960kHz}={SSB, PDCCH} pair

Q3) supported search space configurations for {480kHz, 480kHz}={SSB, PDCCH} pair and {960kHz, 960kHz}={SSB, PDCCH} pair. For example, whether Table 13-12 can be used with little or no modifications.

|  |  |
| --- | --- |
| Company | Comments |
| Samsung | Q1) We support adding 96 RB CORESET#0 for better coverage.  Q2) The same RB and symbol duration with Pattern 1 for {120, 120} can be supported for {480, 480} and {960, 960}.  Q3) Table 13-12 can be used as a baseline with necessary modifications, e.g. the O value. |
| Qualcomm | Q1: we do not think there is a strong need to introduce 96 RB option, however, it can be considered if needed  Q2:   * For 480 + 480 kHz: support the same combinations as for 120 + 120 kHz   + 24 RB + 2 symbols   + 48 RB + 1 or 2 symbols * For 960 + 960 kHz: due to min UE BW constraint (400 MHz) and to compensate for coverage,   + 24 RB + 1 or 2 or [3] symbols   Q3: Start with table 13-12 as baseline. However, for the values of “O”, since the SSB beam sweep time for 480 and 960 kHz is short (1 and 0.5 ms), the values of “O” of 2.5, 5, and 7.5 ms may be too long and we may to consider some reduction factor.  In addition, we can also support “Use symbols {0,1} and {7,8} for Type0-PDCCH for each SSB” as indicated above using “Qualcomm” |
| Sharp | Q1: we consider adding 96 PRB as optimization rather than necessity.  Q2: Firstly reuse Table 13-8 with multiplexing pattern 1 as baseline. Limited modifications could be further discussed.  Q3: Firstly reuse Table 13-12 as baseline. Further discuss necessary modifications to accommodate higher SCS. |
| Docomo | Q1) support for better coverage.  Q2) generally fine.  Q3) O value can be revisited. |
| ZTE, Sanechips | Q1) It can be introduced only when there is a strong demand.  Q2) The same RB and symbol duration with Pattern 1 for {120, 120} in Table 13-8 in TS 38.213 can be supported for {480, 480} and {960, 960}.  Q3) Table 13-12 can be used as a baseline with necessary enhancements. Except the O value mentioned by Samsung and Qualcomm, DRS/SSB pattern design discussed in 2.1.2 may also have impacts on search space configurations. |
| Nokia | Q1) We would support adding 96PRB option for 120kHz.  Q2) We would propose to support for {SSB, CORESET#0}={480kHz, 480kHz} multiplexing pattern 1 {,} configurations (in order of priority):   * {48,2} * {24,2}, {48,1} * {24,3}   For {SSB, CORESET#0}={960kHz, 960kHz} multiplexing pattern 1 {,} configurations (in order of priority):   * {24,2} * {24,3}   Q3) Enabling scheduling SIB1 in the same slot as SSB could be considered. Thus PDCCH monitoring occasion option with PDCCH first symbol indexes corresponding to the free symbols in the slot with SSBs should be considered i.e. with Alt 1-C {0,6} or with Alt 1-A {0,7}. In respect to Table 13-12, smaller ‘O’ values could be considered for the 480kHz and 960kHz sub-carrier spacing.  Note minor correction in above summary:  “Support mux pattern 1 with {24~~8~~} PRB and {2,3} symbol duration” |
| LG Electronics | Q1) We don’t think 96 PRB CORESET#0 is additionally needed.  Q2) Same as in NR Rel-15, i.e., 24 RB + 2 symbols or 48 RB + 1 or 2 symbols  Q3) Table 13-12 can be reused with some modifications to O values. |
| Lenovo, Motorola Mobility | Q1) We do not see a need for 96 PRB for 120 kHz.  Q2) We are fine with it.  Q3) The table 13-12 cab be used as a baseline with necessary modifications for O value for 480 and 960 kHz. |
| Intel | Q1) We support adding 96 RB CORESET#0.  For SCS 120 kHz, 96 RBs occupy bandwidth of 138.24 MHz which is larger than 100 MHz that can achieve the conducted power limit of 27 dBm according to US regulation. Without support of 96 PR, we are penalizing the conducted power for all US deployments with 120kHz.  Also, for {120, 120} we would like to suggest removing configurations with 24 RB because there is no more limitation on the min channel bandwidth  Q2) The same RB and symbol duration with Pattern 1 for the current configuration of {120, 120} can be supported for {480, 480} and {960, 960}.  Q3) Table 13-12 can be used as a baseline with necessary modifications. |
| Futurewei | Q1) We are OK with adding 96 PRB CORESET#0 (even we do not think that is a necessity) if the majority wants it.  Q2) The same Pattern 1 for {120, 120} Table 13-8 in TS 38.213 can be supported for {480, 480} and {960, 960} as baseline.  Q3) Use Table 13-12 as a baseline with necessary modifications |
| Ericsson | Please see our added support above using "Ericsson"  Q1) We don't think 96 RB CORESET0 it is needed. Based on link budget analysis, we have found that in terms of coverage, it is not Type0-PDCCH that is limiting; rather, it is RMSI PDSCH. Hence, we don't see a coverage improvement for RMSI by enabling 96 RB CORESET0.  Q2) We think a common table design should be used for 120/480/960 kHz SCS, and that Table 13-8 is the right starting point. It may be necessary to add a new SSB-CORESET0 offset for the 48 RB case (based on RAN4 channelization design) to fully enable use of the minimum bandwidth channels.  Q3) We think that Table 13-12 can be used without modification. For 480 and 960 kHz, additional specification text can be added to re-interpret the offset values (the O values) if it is desired to enable a RMSI beam sweep to start soon after the SSB beam sweep. The proposal in our paper is as follows:   1. Reuse existing Table 13-12 in 38.213 for operation with 480 and 960 kHz SCS. For subcarrier spacings 480 and 960 kHz. Use and , respectively, instead of when determining the PDCCH monitoring occasions using offset values from the table. |
| CATT | Q1) We don’t think 96 PRB CORESET#0 need to be needed.  Q2) Same as in legacy specification TS 38.213  Q3) Table 13-12 can be reused . |
| Sony | Q1) We don’t see strong demand to add 96 PRB CORESET#0 for 120 kHz SCS.  Q2) The same RB and symbol duration with Pattern 1 in Table 13-8 should be considered as baseline.  Q3) Table 13-12 can be reused as baseline. |
| Huawe/HiSilicon | Q1) Support. To maximize Tx power given PSD constraint.  Q2) Support. It is OK to support (PRB, symbol) ={(24,2), (48, 1), (48, 2)} for Mux 1 as in Rel-15 for 120 kHz.  Q3) Support with the following change  “supported search space configurations with mux pattern 1 for {480kHz, 480kHz}={SSB, PDCCH} pair and {960kHz, 960kHz}={SSB, PDCCH} pair. For example, whether Table 13-12 can be used ~~with little or no modifications~~ as a starting point.  In our view, Table 13-12 may be used only as a starting point. However, larger O values can be removed to avoid unnecessary large latency during initial access. We also believe that larger O values are not useful for 120 kHz in FR2-2 and may be removed to “free up” a bit which may be used toward indicating other values such as .  We also agree to use symbols {0,1} and {7,8} for Type0-PDCCH as discussed in Section 2.1.2. We have added our support in the Summary. |

#### **1st Round Discussion Summary:**

**Issue 1)** On whether or not to additionally support 96 PRB for CORESET#0 for {120, 120} = {SSB, PDCCH} case. Few companies mentioned that addition of this is more of optimization rather than necessity. Many companies commented they can consider if it is needed, and several companies expressed support for this. Four company explicitly mentioned they do not think it is needed. Moderator suggest to continue discussion on this topic, at the same time it is suggested that it to be treated with lower priority compared to other proposals during GTW. Continue discussion on Proposal 1.3-1.

|  |
| --- |
| * For {SSB, CORESET#0/Type0-PDCCH} = {120, 120} kHz   + controlResourceSetZero     - Addition of 96 PRB CORESET#0       * Support: Huawei/HiSilicon, Samsung, Nokia/NSB, Apple, NTT Docomo, Lenovo/Motorola Mobility, Intel       * Do not support: Sharp (optimization), LGE, Ericsson, CATT, Sony       * Maybe: Qualcomm, ZTE/Sanechips, Futurewei |

##### **Proposal 1.3-1)**

* Support inclusion of 96 PRB CORESET#0 with appropriate RB offset for {120 kHz, 120 kHz} = {SSB,PDCCH} case to ‘controlResourceSetZero’ field of MIB

**Issue 2)** For the CORESET#0 and Type0-PDCCH SS configurations, companies views are summarized as below. There is good support in using existing Table 13-8 and 13-12 as much as possible. Some companies mentioned certain parameters such as ‘O’ in 13-12 will need to be revisited. Since the RB offset values are pending RAN4 channelization discussion, moderator has formulate a proposal for further discussion in Proposal 1.3-2 and 1.3-3.

|  |
| --- |
| * For {SSB, CORESET#0/Type0-PDCCH} = {480, 480} kHz   + controlResourceSetZero     - Support {24, 48} PRB with {1,2} symbol durations       * Huawei/HiSilicon     - Use Table 13-8 (originally intended for {120,120} kHz) except RB offset       * {mux pattern 1, 24 PRB, 2 symbol}       * {mux pattern 1, 48 PRB, 1 symbol}       * {mux pattern 1, 48 PRB, 2 symbol}       * {mux pattern 3, 24 PRB, 2 symbol}       * {mux pattern 3, 48 PRB, 2 symbol}       * [vivo], ~~[~~Samsung (with 96 RB as well)~~]~~, ~~[~~Ericsson~~]~~, LGE, NTT Docomo, Qualcomm, ZTE/Sanechips, Sharp, CATT, Sony (baseline)     - Support mux pattern 1 with {24, 48} PRB and {[1],2,3} symbol duration       * Nokia/NSB     - Support mux pattern 3 with {24, 48} PRB and {1,2} symbol duration       * Nokia/NSB, Samsung     - Support mux pattern 3       * Qualcomm, Samsung   + searchSpaceZero     - Use Table 13-12 (originally intended for {120,120} kHz)       * NTT Docomo, Ericsson     - Use Table 13-12 (originally intended for {120,120} kHz) except O values       * LGE, Samsung, Huawei/HiSilicon     - Use symbols {0,1} and {7,8} for Type0-PDCCH for each SSB       * Intel, Qualcomm, Huawei/HiSilicon |

For reference, the following is Table 13-8 and 13-12 from TS38.213

Table 13-8: Set of resource blocks and slot symbols of CORESET for Type0-PDCCH search space set when {SS/PBCH block, PDCCH} SCS is {120, 120} kHz

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Index | SS/PBCH block and CORESET multiplexing pattern | Number of RBs | Number of Symbols | Offset (RBs) |
| 0 | 1 | 24 | 2 | 0 |
| 1 | 1 | 24 | 2 | 4 |
| 2 | 1 | 48 | 1 | 14 |
| 3 | 1 | 48 | 2 | 14 |
| 4 | 3 | 24 | 2 | -20 if  -21 if |
| 5 | 3 | 24 | 2 | 24 |
| 6 | 3 | 48 | 2 | -20 if  -21 if |
| 7 | 3 | 48 | 2 | 48 |
| 8 | Reserved | | | |
| 9 | Reserved | | | |
| 10 | Reserved | | | |
| 11 | Reserved | | | |
| 12 | Reserved | | | |
| 13 | Reserved | | | |
| 14 | Reserved | | | |
| 15 | Reserved | | | |

Table 13-12: Parameters for PDCCH monitoring occasions for Type0-PDCCH CSS set - SS/PBCH block and CORESET multiplexing pattern 1 and FR2

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Index |  | Number of search space sets per slot |  | **First symbol index** |
| 0 | 0 | 1 | 1 | 0 |
| 1 | 0 | 2 | 1/2 | {0, if  is even}, {7, if  is odd} |
| 2 | 2.5 | 1 | 1 | 0 |
| 3 | 2.5 | 2 | 1/2 | {0, if  is even}, {7, if  is odd} |
| 4 | 5 | 1 | 1 | 0 |
| 5 | 5 | 2 | 1/2 | {0, if  is even}, {7, if  is odd} |
| 6 | 0 | 2 | 1/2 | {0, if  is even}, {, if  is odd} |
| 7 | 2.5 | 2 | 1/2 | {0, if  is even}, {, if  is odd} |
| 8 | 5 | 2 | 1/2 | {0, if  is even}, {, if  is odd} |
| 9 | 7.5 | 1 | 1 | 0 |
| 10 | 7.5 | 2 | 1/2 | {0, if  is even}, {7, if  is odd} |
| 11 | 7.5 | 2 | 1/2 | {0, if  is even}, {, if  is odd} |
| 12 | 0 | 1 | 2 | 0 |
| 13 | 5 | 1 | 2 | 0 |
| 14 | Reserved | | | |
| 15 | Reserved | | | |

##### **Proposal 1.3-2)**

* For ‘controlResourceSetZero’ configuration for {SSB, CORESET#0/Type0-PDCCH} = {480, 480} kHz and {960, 960} kHz,
  + Support the following set of parameters.

|  |  |  |
| --- | --- | --- |
| SS/PBCH block and CORESET multiplexing pattern | Number of RBs | Number of Symbols |
| 1 | 24 | 2 |
| 1 | 48 | 1 |
| 1 | 48 | 2 |
| 3 | 24 | 2 |
| 3 | 48 | 2 |

* + - Note: the number of entries corresponding the same {mux pattern, number of RB, number of symbol} tuple (listed above) will depend on required RB offsets that needs to be supported based on channel and sync raster design.
  + FFS: addition of any the following set of parameters

|  |  |  |
| --- | --- | --- |
| SS/PBCH block and CORESET multiplexing pattern | Number of RBs | Number of Symbols |
| 1 | 24 | 3 |
| 1 | 96 | 1 |
| 1 | 96 | 2 |
| 3 | 96 | 2 |

##### **Proposal 1.3-3)**

* For ‘searchSpaceZero’ configuration for {SSB, CORESET#0/Type0-PDCCH} = {480, 480} kHz and {960, 960} kHz,
  + Support the following set of parameters are supported for SS/PBCH block and CORESET multiplexing pattern 1:

|  |  |  |
| --- | --- | --- |
| Number of search space sets per slot |  | **First symbol index** |
| 1 | 1 | 0 |
| 2 | 1/2 | {0, if  is even}, {7, if  is odd} |
| 2 | 1/2 | {0, if  is even}, {, if  is odd} |
| 1 | 2 | 0 |

* + - Note: the number of entries corresponding the same {number of SS per slot, M, first symbol index} tuple (listed above) will depend on supported ‘O’ for each tuple.
    - FFS: Values of supported ‘O’ and supported combination of ‘O’ and number of SS per slot, M, first symbol index} tuple.

#### **2nd Round Discussion:**

Please provide further comments for Proposal 1.3-1 ~ 1.3-3. Proposal 1.3-1 is copied below for convenience.

##### **Proposal 1.3-1)**

* Support inclusion of 96 PRB CORESET#0 with appropriate RB offset for {120 kHz, 120 kHz} = {SSB,PDCCH} case to ‘controlResourceSetZero’ field of MIB

|  |  |
| --- | --- |
| Company | Comments |
| vivo | Support the proposal for better coverage and OCB requirement for unlicensed band. |
| DOCOMO | Support the proposal. |
| Spreadtrum | Fine |
| Nokia | Proposal 1.3-1: Still OK  Proposal 1.3-2: In principle OK, not sure if we need the table for the FFS combinations.  Proposal 1.3-3: OK with the proposal with the assumption that Proposal 1.2-1 for SSB resource pattern is agreed. |
| LG Electronics | Proposal 1.3-1) Still we don’t think support of 96 PRBs is essential for FR2-2. Without clear majority support, we cannot accept this proposal.  Proposal 1.3-2) We prefer to reuse all of indexes as in Rel-15, with some modification for RB offset values, if deemed necessary.  Proposal 1.3-3) We prefer to reuse all of indexes as in Rel-15, with some modification for O values. |
| ZTE, Sanechips | For Proposal 1.3-1, we can accept it if most companies think it is necessary.  For Proposal 1.3-2, we are fine with it.  For Proposal 1.3-3, we suggest to defer the discussion as the first symbol index of CORESET#0 is also depending on SSB pattern design discussed in 2.1.2. |
| Samsung | Proposal 1.3-1) Support.  Proposal 1.3-2) Support.  Proposal 1.3-3) We are ok with the proposal, and want to clarify that this proposal is same as reusing Rel-15 table with possible medication on O values right? |
| Intel | **Proposal 1.3-1)** – agree  **Proposal 1.3-2)** – agree  **Proposal 1.3-3) –** agree  For 1.3-1, we would like to comment that, while Ericsson mentioned that RMSI/SIB1 PDSCH is the real bottleneck, the CORESET#0 bandwidth essentially also dictates the maximum bandwidth usage for SIB1 PDSCH, as CORESET#0 bandwidth is the initial BWP. So, we fail to understand why it is ok not to support maximum conducted power transmission for important channels such as PDCCH for SIB1 and PDSCH for SIB1. Both PDCCH and PDSCH get impacted from CORESET#0 bandwidth. |
| Apple | Proposal 1.3-1: Support  Proposal 1.3-2: Ok.  Proposal 1.3-3: Support. |
| Qualcomm | Proposal 1.3-1: fine  Proposal 1.3-2: for 960 kHz, mux pattern 1 with 48 RB and mux pattern 3 with 24 RB exceed the 400 MHz minimum BW capability.  Proposal 1.3-3: fine |
| Sharp | Proposal 1.3-1: Ok if this proposal presents the majority view.  Proposal 1.3-2: Support.  Proposal 1.3-3: Support. |
| Futurewei | Proposal 1.3-1: Not essential but we are OK if the majority wants.  Proposal 1.3-2: OK.  Proposal 1.3-3: OK. |
| Ericsson | Proposal 1.3-1: We still don't see the benefit of this optimization, and it seems like there is not a clear majority.  Proposal 1.3-2: The 96 RBs in the FFS are dependendent on Proposal 1.3-1  Proposal 1.3-3: We think a much simpler solution is to use the existing table 13-12 "as is" and simplify modify the associated procedure text that says :  the UE determines an index of slot  as  that is in a frame with system frame number  by replacing /mu with /mu – 2 for 480 kHz and by /mu – 3 for 960 kHz. This preserves the relative timing of the SSB beam sweep and the Type0-PDCCH monitoring locations for 120 kHz. |
| Huawei, HiSilicon | **Proposal 1.3-1)** Support.  **Proposal 1.3-2)** At this stage, we prefer to support only the first three rows of the Table  (mux pattern, number of RB, number of symbol) = {(1, 24, 2), (1, 48, 1), (1, 48, 2)}. First, according to WID, “Prioritize support SSB-CORESET#0 multiplexing pattern 1. Other patterns discussed on a best effort basis”. So, we don’t see the urgency of supporting Mux 3 combinations when many other aspects of initial access design are not agreed yet. Note that, if possible, we should avoid supporting unnecessary (mux pattern, number of RB, number of symbol) tuples which results in using all four bits of ‘controlResourceSetZero’ while, in other initial access discussion, a major challenge is how to repurpose a bit in MIB for shared spectrum access purposes. |

#### **2nd Round Discussion Summary:**

The following is a summary of company preference for Proposal 1.3-1, 1.3-2A, and 1.3-3. Proposal 1.3-2 has been edited to reformulate the FFS.

##### **Proposal 1.3-1)**

* Support inclusion of 96 PRB CORESET#0 with appropriate RB offset for {120 kHz, 120 kHz} = {SSB,PDCCH} case to ‘controlResourceSetZero’ field of MIB
* Ok: vivo, Docomo, Spreadtrum, Nokia, Samsung, Intel, Apple, Qualcomm, Sharp, Samsung, Intel, Apple, Qualcomm, Sharp, Futurewei
* Not ok: LGE
* Maybe: ZTE/Sanechips

##### **Proposal 1.3-2A)**

* For ‘controlResourceSetZero’ configuration for {SSB, CORESET#0/Type0-PDCCH} = {480, 480} kHz and {960, 960} kHz,
  + Support the following set of parameters.

|  |  |  |
| --- | --- | --- |
| SS/PBCH block and CORESET multiplexing pattern | Number of RBs | Number of Symbols |
| 1 | 24 | 2 |
| 1 | 48 | 1 |
| 1 | 48 | 2 |
| 3 | 24 | 2 |
| 3 | 48 | 2 |

* + - Note: the number of entries corresponding the same {mux pattern, number of RB, number of symbol} tuple (listed above) will depend on required RB offsets that needs to be supported based on channel and sync raster design.
  + FFS: addition of any the following set of parameters
    - {mux pattern, number of RB, number of symbol} = {1, 24, 3}
    - {mux pattern, number of RB, number of symbol} = {1, 96, 1}
    - {mux pattern, number of RB, number of symbol} = {1, 96, 2}
    - {mux pattern, number of RB, number of symbol} = {3, 96, 2}
* Ok: vivo, Docomo, Spreadtrum, ZTE/Sanechips, Samsung, Intel, Apple, Sharp, Futurewei
* Maybe: Nokia (reformulate FFS?), [LGE?], [Qualcomm (commented some config will exceed 400MHz)?]
* Not ok:

##### **Proposal 1.3-3)**

* For ‘searchSpaceZero’ configuration for {SSB, CORESET#0/Type0-PDCCH} = {480, 480} kHz and {960, 960} kHz,
  + Support the following set of parameters are supported for SS/PBCH block and CORESET multiplexing pattern 1:

|  |  |  |
| --- | --- | --- |
| Number of search space sets per slot |  | **First symbol index** |
| 1 | 1 | 0 |
| 2 | 1/2 | {0, if  is even}, {7, if  is odd} |
| 2 | 1/2 | {0, if  is even}, {, if  is odd} |
| 1 | 2 | 0 |

* + - Note: the number of entries corresponding the same {number of SS per slot, M, first symbol index} tuple (listed above) will depend on supported ‘O’ for each tuple.
    - FFS: Values of supported ‘O’ and supported combination of ‘O’ and number of SS per slot, M, first symbol index} tuple.
* Ok: vivo, Docomo, Spreadtrum, Nokia, Samsung, Intel, Apple, Sharp, Futurewei
* Maybe: [LGE?]
* Not ok:
* Defer: ZTE/Sanechips (discuss together with SSB pattern)

### 2.14 ANR/CGI Reporting Aspects

* From [4] Interdigital:
  + Consider introducing the parameters for the neighbor cell SIB1 related to CGI reporting, where the time and frequency allocations and the multiplexing patterns are (pre)configured in fixed settings.
* From [7] Samsung:
  + No need to support extra method for providing the CORESET#0/Type0-PDCCH configuration for ANR purpose.
* From [8] CATT:
  + There is no need to study additional method(s) to enable support to obtain neighbor cell SIB1 contents related to CGI reporting in Rel-17.
* From [17] OPPO:
  + For ANR design, RAN1 considers one of the two options
    - Option 1: RAN1 holds ANR discussion until RAN4 concludes the channelization, LBT bandwidth and sync raster relationship.
    - Option 2: RAN1 does not follow R16 baseline solution and redesign ANR.
* From [18] Qualcomm:
  + for ANR, do not consider additional methods (compared to current NR) to signal the NCGI

#### Summary of Discussions

The updated WID contains FFS on additional method(s) to enable support to obtain neighbor cell SIB1 contents related to CGI reporting.

Three companies mentioned there is no need to consider further, and two companies mentioned methods to support CGI reporting.

#### **1st Round Discussion:**

Further discuss on “FFS: additional method(s) to enable support to obtain neighbour cell SIB1 contents related to CGI reporting”.

|  |  |
| --- | --- |
| Company | Comments |
| Samsung | We don’t think additional method for CGI reporting is needed.   * First, in the CGI reporting scenario, the serving operator may not have information on the configuration of CORESET#0/Type0-PDCCH of a neighboring operator, so the feasibility of the additional method (e.g. dedicated signaling) is concerned. * Secondly, even if the serving operator knows such CORESET#0/Type0-PDCCH configuration, the dedicated signaling can only provide the same information as the indication in the MIB, otherwise such SSB cannot be used as cell-defining SSB for the neighboring operator. * Lastly, the UE anyway needs to read MIB of the SSB from the neighboring cell, e.g. to acquire timing and other information in MIB, so there is no need to have an additional method to provide the CORESET#0/Type0-PDCCH configuration. |
| Qualcomm | Current NR support is enough and there may not be a need to have any additional methods to support signaling the NCGI |
| Fujitsu | We share the views that no additional signaling on top of MIB is needed for providing CORESET#0/Type0-PDCCH configuration. However, some enhancements on providing CORESET#0/Type0-PDCCH configuration by MIB of off-sync SSB may be needed.  In NR-U, the MIB of an off-sync SSB provides CORESET#0/Type0-PDCCH CSS set configuration based on a nominal SSB on the sync raster in the channel where the off-sync SSB is transmitted. It is feasible since each channel includes one and only one sync raster. But for FR2-2, the relation between channels and sync rasters may be different and thus enhancement for off-sync SSB may be needed. Considering that channels and sync rasters are still under discussion, this discussion point could be deprioritized at the current stage. |
| Mediatek | We don’t see the need for additional mechanism for CGI reporting. |
| Sharp | No need to further discuss additional methods. |
| Docomo | Agree no need to support additional functionality for CGI reporting. |
| ZTE, Sanechips | We do not think it is necessary to study additional method(s) (e.g. using dedicated signaling) to enable support to obtain neighbor cell SIB1 contents related to CGI reporting. But we agree that channelization and sync raster defined in Rel-17 above 52.6GHz may have some impact on the current supported method (i.e. using MIB configuration). RAN1 can discuss if some enhancements are needed after RAN4’s work on channelization and sync raster is completed. |
| Nokia | We don’t see a need for any additional methods related to CGI reporting |
| OPPO | We agree with no additional mechanism is needed. But we see an issue to use the R16 method in FR2.2 ANR. The main issue is that there is no 20MHz LBT bandwidth and a unique GSCN in the 20MHz LBT bandwidth. Thus, it is not clear how the UE can obtain the second offset as defined in TS 38.213. |
| LG Electronics | Current NR specification is enough to support ANR/CGI reporting and we don’t see the need to support additional methods for ANR/CGI reporting. |
| NEC | Agree no need to support additional functionality for CGI reporting. |
| Xiaomi | We don’t see the need for additional mechanism for CGI reporting. |
| Lenovo, Motorola Mobility | We also don’t see any need for additional mechanism for CGI reporting |
| Intel | Additional methods of CGI reporting seem to be optimization which could be de-prioritized at this moment |
| Futurewei | We do not see the need to support additional functionality for CGI reporting. |
| Ericsson | We don't see a need to introduce additional methods; the Rel-15 approach is sufficient.  One observation though: the special solution introduced in Rel-16 NR-U to allow an off-sync raster SSB will not work for Rel-17, since the Rel-16 approach required only a single sync raster point per channel, and a channel was well defined as 20 MHz. |
| CATT | We don’t see the need for additional mechanism. |
| Huawei/HiSilicon | Given the agreements reached in RAN 92-e, there is no need for any additional method. |

#### **1st Round Discussion Summary:**

Majority of the companies seems to think no further discussion is necessary.

#### **2nd Round Discussion:**

Moderator suggest to conclude to not discuss further in RAN1 #106-e. Please provide comments if you different suggestion on this issue.

|  |  |
| --- | --- |
| Company | Comments |
| vivo | Support Moderator’s suggestion. |
| DOCOMO | Agree with Moderator’s suggestion. |
| Spreadtrum | We are fine for Moderator’s suggestion |
| LG Electronics | Agree with Moderator’s suggestion |
| ZTE, Sanechips | Support Moderator’s suggestion. |
| Samsung | Agree with Moderator’s assessment.  One further comment on the Rel-16 approach to be used for 60 GHz unlicensed band. Our understanding is, in Rel-16 NR-U band, the sync raster is sparse and CORESET#0 BW is close to channel bandwidth such that using default configuration in MIB could not allow flexible allocation of SSB in the channel, such that we designed the special mechanism of using a second offset to address this issue. If any of such restrictions does not hold, i.e., sync raster is not as sparse as single one in the channel, or CORESET#0 bandwidth is much smaller than channel bandwidth, Rel-15 mechanism (i.e. using default configuration in MIB) is sufficient. |
| Intel | Support the conclusion not to discuss. |
| NEC | Support Moderator’s suggestion. |
| Apple | Agree. |
| Qualcomm | Agree with Moderator’s suggestion. |
| Sharp | Agree. |
| Futurewei | Agree |
| Huawei, HiSilicon | Support. |

#### **2nd Round Discussion Summary:**

TBD

### 2.1.5 Various other aspects on SSB Design

* From [3] Spreadtrum:
  + SSB with 240kHz SCS can be down-prioritized.
  + Supporting initial cell selection with 480kHz SSB should be an optional UE capability separately from supporting other processing with 480/960kHz SCS.
* From [6] Lenovo/Motorola Mobility
  + For supporting NR from 52.6 GHz to 71 GHz in Rel. 17, with higher subcarrier spacings (numerologies), coverage enhancement of channels and signals used for initial access should be considered for NR beyond 52.6 GHz
* From [17] OPPO:
  + The raster step size for 120kHz and 480kHz are 3\*17.28MHz and 15\*17.28MHz, respectively, leading to a total number of raster entries 428.
* From [19] LG Electronics:
  + Discuss how to signal actually transmitted SSBs via ssb-PositionsInBurst when can be indicated to be less than 64 in MIB.
* From [27] Convida:
  + SSB coverage enhancement should be studied for higher SCS.

#### Summary of Discussions

* Companies have provided the following issues
  + Capability
    - Supporting initial cell selection with 480kHz SSB should be an optional UE capability separately from supporting other processing with 480/960kHz SCS.
  + Coverage enhancement
    - For supporting NR from 52.6 GHz to 71 GHz in Rel. 17, with higher subcarrier spacings (numerologies), coverage enhancement of channels and signals used for initial access should be considered for NR beyond 52.6 GHz
    - SSB coverage enhancement should be studied for higher SCS.
    - Note from Moderator: WID explicitly mentions “Note: coverage enhancement for SSB is not pursued.”, therefore not sure if this needs to be further discussed.
  + Raster
    - The raster step size for 120kHz and 480kHz are 3\*17.28MHz and 15\*17.28MHz, respectively, leading to a total number of raster entries 428.
  + ssb-PositionsInBurst
    - Discuss how to signal actually transmitted SSBs via ssb-PositionsInBurst when can be indicated to be less than 64 in MIB

#### **1st Round Discussion:**

Among the additional issues brought up, Moderator assumes that coverage aspects are excluded by the WID and raster issues are for discussion in RAN4 domain. Moderator suggest to further discuss on the two issues brought up.

* Initial cell selection capability for 480kHz
* Signaling for ssb-PositionsInBurst when is indicated.

If there are other issues that require further discussion, please comment here as well.

|  |  |
| --- | --- |
| Company | Comments |
| Samsung | * The capability of 480 kHz for initial access can be discussed in a later phase of the WI (anyway do not impact RAN1 progress). * The indication and interpretation of ssb-PositionsInBurst can be discussed later when the DBTW is finalized. |
| ZTE, Sanechips | We share same views as Samsung on above two issues. |
| Nokia | In our understanding the initial cell selection capability (if any) should be handled as a part of the UE capability discussions as per WID:  “Note: Dependency or lack thereof for a UE supporting 480kHz and/or 960kHz numerology for data and control to also support 480kHz SSB numerology for initial access is to be tackled as part of UE capability discussion.” |
| OPPO | Agree with Samsung |
| LG Electronics | Same view with Samsung |
| Lenovo, Motorola Mobility | Similar view as of Samsung |
| Intel | Defer the discussion on these points |
| Futurewei | We agree that these points can be discuss later. |
| Ericsson | Defer |
| CATT | Ok to defer |
| InterDigital | Fine to defer |
| Huawei/HiSilicon | * As Nokia pointed out, given the referred note from RAN 92-e, “Initial cell selection capability for 480kHz” should be discussed as a part of UE capability discussion.   In our view, interpretation of *ssb-PositionsInBurst* when is indicated can be discussed in this meeting. |
| Convida Wireless | We are ok to defer the discussions for this. |

#### **1st Round Discussion Summary:**

Several companies think the issues are with lower priority compared to other issues. Suggestion to continue discussion but treat the issue with lower priority during GTW sessions.

#### **2nd Round Discussion:**

Please continue to provide comments as in 1st round discussions.

|  |  |
| --- | --- |
| Company | Comments |
| vivo | Fine to defer |
| Intel | Support moderator’s suggestions after the 1st round of discussions. |
| Qualcomm | Fine to defer |
| Futurewei | Agree to defer. |

#### **2nd Round Discussion Summary:**

TBD

## 2.2 PRACH Aspects

### 2.2.1 PRACH Sequence and Format

* From [2] vivo:
  + Support 120KHz and 480KHz as candidate SCS of initial UL BWP.
  + Support 480KHz and 960KHz SCS in addition to 120KHz SCS for PRACH.
* From [7] Samsung:
  + Support short PRACH format for all PRACH sequence lengths and all SCSs , and don’t support long PRACH format.
* From [8] CATT:
  + Consider supporting increasing symbols in time domain to enhance PRACH coverage.
  + Consider repeating and concatenating the PRACH preamble sequence to enhance PRACH coverage for unlicensed spectrum operation.
* From [9] ZTE/Sanechips:
  + Support PRACH with additional SCSs (480 kHz and/or 960 kHz) for both initial and non-initial access cases.
  + For 480kHz and 960kHz, reuse the same RO configuration table as in Rel-15/16 with the same RO density for 120kHz PRACH.
* From [11] Ericsson:
  + For PRACH with 960 kHz SCS for non-initial access use cases, L = 139 is supported, and L = 571 and 1151 are not supported.
  + For 480 kHz SCS for both initial access and non-initial access use cases, L = 139 is supported, and L = 1151 is not supported. It can be further discussed whether or not L = 571 is supported.
* From [12] Futurewei:
  + For initial access and non-initial access use cases, support 120kHz PRACH SCS with sequence length L=571, 1151 (in addition to L=139) for PRACH Formats A1~A3, B1~B4, C0, and C2.
  + For non-initial access use cases, support 480 and 960 kHz PRACH SCS with sequence length L=139 for PRACH Formats A1~A3, B1~B4, C0, and C2, respectively.
* From [13] Nokia/NSB:
  + Support L=571 for PRACH with 480kHz.
* From [18] Qualcomm:
  + consider only using PRACH sequence length = 139 for SCS = 480 kHz and 960 kHz
* From [19] LG Electronics:
  + The 120 kHz PRACH SCS with sequence lengths L=571 and L=1151 are not required for the licensed spectrum where the regulatory requirements are not defined on PSD limit.
  + PRACH only with sequence length L=139 is supported for the 480 kHz SCS for initial/non-initial access and 960 kHz SCS for non-initial access.
* From [21] Mediatek:
  + Support only sequence length L=139 when PRACH SCS=480 kHz and 960 kHz.
* From [22] Intel:
  + Support PRACH formats A1~A3, B1~B4, C0, C2 for with SCS 480 kHz, i.e., .
* From [23] Apple:
  + If 480kHz and 960kHz SCS are used for PRACH transmission, support L=139 only.
* From [24] Sharp:
  + Only support L = 139 for PRACH with 480kHz and 960 kHz SSB SCS.

#### Summary of Discussions

The following are previous agreements on PRACH sequence and formats.

|  |
| --- |
| **Agreement:**   * For initial access and non-initial access use cases, support 120kHz PRACH SCS with sequence length L=571, 1151 (in addition to L=139) for PRACH Formats A1~A3, B1~B4, C0, and C2. * For non-initial access use cases,   + if 480kHz and/or 960 kHz SSB SCS is agreed to be supported, support 480 and/or 960 kHz PRACH SCS with sequence length L=139 for PRACH Formats A1~A3, B1~B4, C0, and C2, respectively.     - FFS: support of sequence length L = 571, 1151 * FFS: Support of 480 and/or 960 kHz PRACH SCS for initial access use cases, if 480 and/or 960 kHz SSB SCS is agreed to be supported for initial access |

* Supported sequence lengths
  + Support PRACH lengths L=571, 1151 for 480kHz, and 960kHz PRACH
    - Samsung
  + Support PRACH length L=571 for 480kHz PRACH
    - Intel, Nokia/NSB, Huawei/HiSilicon
  + Do not support PRACH lengths L=571, 1151 for 960kHz PRACH
    - Ericsson, Qualcomm, Apple, Sharp, OPPO, Huawei/HiSilicon
  + Do not support PRACH lengths L=1151 for 480kHz PRACH
    - Ericsson
  + Do not support PRACH lengths L=571, 1151 for 480kHz PRACH
    - Qualcomm, Apple, Sharp, OPPO
* Consideration of additional formats/PRACH repetition lengths
  + CATT

#### **1st Round Discussion:**

Based on previous agreements and updated WID, moderator assume the following can be confirmed.

* Confirm agreement:
  + Support 480 PRACH SCS with sequence length L=139 for PRACH Formats A1~A3, B1~B4, C0, and C2, respectively for initial and non-initial access cases
  + Support 960 PRACH SCS with sequence length L=139 for PRACH Formats A1~A3, B1~B4, C0, and C2, respectively for non-initial access cases

Also two companies has suggested to support L=571 for 480kHz, while a number of companies suggested not to support L=571 and L=~~1191~~1151 for 480 and 960kHz.

Moderator suggest to discuss on the following options:

* Option 1) Support PRACH length L=571, ~~1191~~1151for 480 and 960 kHz PRACH
* Option 2) Support PRACH length L=571 for 480kHz PRACH, do not support PRACH length L=571, 1191 for 960kHz PRACH and L=~~1191~~1151for 480kHz PRACH.
* Option 3) Do not support PRACH length L=571, ~~1191~~1151for 480 and 960kHz PRACH

|  |  |
| --- | --- |
| Company | Comments |
| Qualcomm | Support option 3, since SCS = 480/960 kHz with sequence length = 139 is enough to achieve the desired BW requirement for the maximum EIRP allowed |
| LG Electronics | Support Option 3 considering the regulatory requirements (e.g., PSD) and the bandwidth occupied by the PRACH. In detail, the 480 kHz PRACH sequence with length L=571 occupies bandwidth of 275 MHz which is larger than 100 MHz that can achieve the conducted power limit of 27 dBm according to US regulation. |
| Fujitsu | 1. Considering BW of PRACH, we slightly prefer Option 3).  2. To confirm the definition of initial access case in the previous agreements:  As discussed in previous meetings, the definition of initial access case for PRACH is ambiguous and confusing. To avoid misunderstanding, could we confirm that initial access case implies that the corresponding ROs are configured by SIB1? |
| Mediatek | Support option 3. We are open for further discussion. However, we don’t see any advantages that can justify the price of excessive bandwidth. |
| Sharp | We prefer option 3, considering PRACH length L=571 for 480kHz PRACH as optimization. |
| Docomo | Support Option 3. |
| ZTE, Sanechips | In these options, 1191 should be changed by 1151.  We prefer Option 2, since 139 long sequence for 480kHz cannot achieve 100MHz emission bandwidth which may lead to limited max peak conducted output power of {500mW × emission-BW / 100MHz} according to US regulation. |
| Nokia | We could consider support for Option 2). Accounting the slightly increased transmission power and processing gain (139 s 571), supporting L=571 for 480kHz, could provide some benefit. |
| OPPO | Support Option 3. |
| Xiaomi | Option 3 is fine for us. |
| Samsung | First, we would like to restate that we don’t think there should be separate design for initial and non-initial access case, because from all the time, the same RACH resource could be used in UE before and after RRC connected mode; NR only introduce there could be additional RACH resource configured for Uplink BWP, but not any specific consideration for initial access or non-initial access.  Then for the SCS and sequence length combination, we believe as long as the channel bandwidth allows, the full flexibility should be supported and the configuration will be up to gNB configuration, so we prefer Option 1. |
| Lenovo, Motorola Mobility | We prefer option 3. |
| Intel | Support Option 2 for the reasons very well explained by LGE |
| Futurewei | Support Option 3. |
| Ericsson | Support Option 3.  Object to Option 1. |
| CATT | We support option 3 |
| InterDigital | Support Option 3. |
| Sony | We support option 3. |
| Huawei/HiSilicon | * Regarding “confirm Agreement”   As Fujitsu also pointed out, which PRACH applications fall into the category of initial access and which RACH applications fall into the category non-initial access has been a subject of lengthy discussions in RAN1 104 and RAN1 104b without any progress. As such, RAN1 could not make an agreement whether or not 480 kHz and/or 960 kHz SCS RACH is supported for initial access. In our view, here are the facts regarding this matter:   * + 480 kHz and 960 kHz SCS PRACH are supported (in an agreement in RAN1 104 at least for “non-initial access” although the definition of “non-initial access” was never fully clarified)   + 960 kHz SSB is not supported for initial access.   + RAN1 specifies PRACH without making distinction between initial access or non-initial access use cases. (This seems to be a general consensus without any formal agreement. At least, to our understanding, Section 6.3.3 of 38.211 does not make such a distinction).   Given above, we cannot “confirm agreement” proposed by FL. Instead, we suggest the following course of action:   * + Continue developing PRACH design for 480/960 kHz in RAN1 without any distinction between initial access and non-initial access use cases.   + In our view, as 960 kHz SSB is not supported for initial access, configuring 960 kHz PRACH in SIB1 for 960 kHz SSB is not required. We are open to further discuss this issue in RAN1 or leave to RAN2 decision. * Regarding supported RACH sequence lengths:   We support Option 2. We do not see any use case for a RACH BW larger than 100 MHz and can’t support Option 1. |

#### **1st Round Discussion Summary:**

There were also two companies who commented that there is no need to distinguish initial and non-initial access for development of physical layer specification. With this moderator assumes that all companies are aligned that

* 480/960 kHz PRACH SCS with sequence length L=139 for PRACH Formats A1~A3, B1~B4, C0, and C2 is supported.

If so no further conclusion and agreement will be needed for the above bullet.

The following is a summary of company views on other PRACH sequence lengths.

* Option 1) Support PRACH length L=571, 1191 for 480 and 960 kHz PRACH
  + Samsung
* Option 2) Support PRACH length L=571 for 480kHz PRACH, do not support PRACH length L=571, 1151 for 960kHz PRACH and L=1151 for 480kHz PRACH.
  + ZTE, Sanechips, Nokia/NSB, Intel
* Option 3) Do not support PRACH length L=571, 1151 for 480 and 960kHz PRACH
  + Qualcomm, LGE, Fujitsu, Mediatek, Sharp, NTT Docomo, OPPO, Xiaomi, Ericsson, Interdigital, Sony

Clear majority of the company think L=139 is sufficient and no further consideration for L=571 and 1151 is needed for 480/960kHz PRACH cases.

#### **2nd Round Discussion:**

Please provide comments on Proposal 1.3-3.

##### **Proposal 2.1-1)**

* Suggested Conclusion:
  + Do not support PRACH length L=571, 1151 for 480 and 960kHz PRACH

|  |  |
| --- | --- |
| Company | Comments |
| vivo | Support the proposal |
| DOCOMO | Support |
| Nokia | Like noted, we saw some merit in supporting L=571 for 480kHz, but don’t have a strong view. |
| ZTE, Sanechips | There is benefit to support L=571 for 480kHz at least in US region, and we don’t see additional spec effort since L=571 is already supported for 30kHz in Rel-16 NRU. Besides, longer PRACH sequence could also be used in licensed band, we tend to spend limited spec effort to achieve such benefits. |
| Samsung | We are not convinced by the discussion that PRACH is also split by intitial access and non-initial access, and also use the impact of SSB, even though SSB and RACH are belong to initial access, but they are separate design.  There are SSB for initial access (cell defining SSB), and SSB for measurement (non-cell defining SSB); but PRACH, there is only SIB1 configured RACH, no matter whether UE is in initial access or non-initial access, UE performs the RACH using same set of configurations. Even UE can be configured by UE specific signaling for a RACH in a non-initial access BWP, but it requires gNB to ensure it’s cell specific configuration;  Why due to SSB did not support 960khz, then RACH cannot support?  RACH support 1.25khz, 5khz in NR FR1, does SSB support?  SSB support 240khz, does RACH support?  SSB numerology and RACH numerology are independent issue. RACH SCS is independently configured from SSB SCS or even UL BWP SCS.  Again, is there any fundamental concern on supporting the preamble lengths in all SCS regardless of the initial access and non-initial access. |
| Intel | Do not support Proposal 2.1-1.  It seems strange to support 96 RBs for CORESET#0 configuration with SCS 120 kHz and not support L=571 for SCS 480 kHz as both means try to address the same issue, i.e., to provide a bandwidth larger than 100 MHz to avoid power reduction in the US.  For those companies, who do not think this is needed, we would like to understand why supporting the highest conducted power for critical channel such as PRACH which is not only used for initial access but for various other functions (e.g. BFR) somehow not important. |
| Apple | Support the proposal. |
| Qualcomm | Support the proposal |
| Sharp | Support the proposal. |
| Futurewei | Agree with the proposal |
| Ericsson | Support |
| Huawei, HiSilicon | We prefer a more conservative approach and leave it open to support the sequence size of 571 for 480 kHz in next meetings. Therefore, we suggest the following which seems to have a stronger majority: **Proposal 2.1-1)**  * Suggested Conclusion:   + Do not support PRACH length L=571, 1151 for ~~480 and~~ 960kHz PRACH and at least L =1151 for 480kHz PRACH. |

#### **2nd Round Discussion Summary:**

The following is a summary of company preferences and discussion. One company asked what main issue would be to support the different SCS for PRACH, as PRACH SCS is inherently not tied to SCS of SSB in NR. One company commented that support of larger PRACH stems from the same reason larger CORESET bandwidth is proposed, and suggested that it should be considered together.

##### **Proposal 2.1-1)**

* Suggested Conclusion:
  + Do not support PRACH length L=571, 1151 for 480 and 960kHz PRACH
* Ok: vivo, Docomo, Apple, Qualcomm, Sharp, Futurewei
* Not ok: ZTE/Sanechips, Samsung, Intel
* Maybe: Nokia

### 2.2.2 RACH Occasion Resources

* From [1] Huawei/HiSilicon:
  + For 480kHz and 960kHz PRACH, support the reference slot duration corresponding to 60 kHz SCS (Option 1 in RAN1 105-e Agreement).
  + Support a gap symbol between consecutive ROs for 480kHz and 960kHz PRACH configurations.
  + For 480kHz and 960kHz PRACH, at least the same RO density (i.e. number of RO per reference slot) as for 120kHz PRACH configuration in FR2 should be supported (Alt 2 in RAN1 105-e Agreement).
  + For 480kHz and 960kHz PRACH configuration, support 1, 2, and 4 PRACH slots per 60kHz reference slot with the following PRACH slot indexes:
    - For 1 PRACH slot per 60kHz reference slot: for 480kHz and for 960kHz PRACH
    - For 2 PRACH slots per 60kHz reference slot: for 480kHz and for 960kHz PRACH.
    - For 4 PRACH slots per 60kHz reference slot: supported values are FFS.
* From [2] vivo:
  + For RO configuration for PRACH with 480/960kHz SCS:
  + Reuse the exiting FR2 RACH configuration table and the location of duration containing PRACH slot pattern within 10ms is same as FR2.
  + How to determine the RACH slot index:
    - Alt.1: Reuse the same reference slot as FR2 and maintain the same number of PRACH slots per reference slot.
    - Alt.2: Reuse the same reference slot as FR2 and increase the number of PRACH slots to more than 2 per reference slot.
  + If gaps between consecutive ROs are needed for LBT and or beam switching, at least the same RO density (i.e. number of RO per reference slot) as for 120kHz PRACH in FR2 is supported.
* From [4] Interdigital:
  + In PRACH configuration, we support Option 1 as it is in compliance with NR Rel.16.
    - Option 1) The reference slot duration corresponds to 60 kHz SCS. A PRACH slot index, , corresponds to one of the starting 480/960 kHz PRACH slots within the reference slot.
  + In PRACH density configuration, support Alt 2 with the same RO density as 120kHz PRACH. Moreover, support further study for higher PRACH slot density for 480kHz and 960kHz PRACH, compared to the 120kHz PRACH.
    - ALT 2) at least the same RO density (i.e. number of RO per reference slot) as for 120kHz PRACH in FR2 is supported
  + For 52.6 – 71 GHz with 120kHz, 480kHz, and 960kHz PRACH, inserting gaps to achieve non-consecutive RACH occasions is not supported.
  + For 52.6 – 71 GHz, support sharing and extending the COT for LBT-free PRACH transmission in the consecutive ROs.
* From [7] Samsung:
  + Using the RO pattern for SCS = 120 kHz derived from the PRACH configuration table as the reference for larger SCS cases.
  + Option 2 for RO pattern determination should be supported.
    - Option 2) Each 120kHz RO corresponds to 4 and 8 candidate RO positions for 480kHz and 960kHz PRACH, respectively. Information about the number and locations of 480/960kHz candidate RO(s) are configured or pre-selected within each 120kHz RO. The reference 120kHz RO is determined by the current PRACH configuration method in Rel-15/16 specification.
  + Support non-consecutive RO configuration to alleviate the RACH LBT failure.
* From [8] CATT:
  + The reference slot duration corresponds to 60 kHz SCS. PRACH slot index corresponds to one of the starting 480/960 kHz PRACH slots within the reference slot.
  + For 480/960 kHz PRACH slots configuration, higher PRACH slot density or higher RO density in time domain can be supported to compensate the impact from MSGS –FDM decreasing and LBT/beam switching GAP.
* From [9] ZTE/Sanechips
  + For 480kHz and 960kHz, reuse the same RO configuration table as in Rel-15/16 with the same RO density for 120kHz PRACH.
  + Proposal 12: Support 60kHz for reference slot as in FR2 with the less spec effort in beyond 52.6GHz.
* From [10] Fujitsu:
  + For 480kHz and 960kHz PRACH, support gaps between consecutive ROs in time domain.
    - If Option 1) supports gaps between consecutive ROs, it is preferred because it is more aligned with the legacy PRACH configuration framework than Option 2).
    - If Option 1) does not support gaps between consecutive ROs, Option 2) is preferred because it supports the gaps by nature.
  + For PRACH density, if gaps between consecutive ROs are supported (by Option 1) or Option 2)), adopt Alt 2) for further discussion on higher density. Otherwise, it is fine to adopt Alt 1) or Alt 2), because there would be no difference between the baseline of the two alternatives.
* From [11] Ericsson:
  + For 480/960 kHz PRACH, support PRACH configurations that allow maintaining the same PRACH processing load (operations/unit time) as for 120 kHz PRACH configurations.
  + For 480/960 kHz PRACH, reuse the current PRACH configuration table in 38.211 for FR2 "as is." Specify rule for which 1 or 2 480/960 kHz slots within a 60 kHz reference slot are used depending on the value in the existing column "Number of PRACH slots within a 60 kHz slot" in the current PRACH configuration table. The rule should be common for all PRACH configurations in the table.
  + Support Option 1 and Alt 1. Regarding the FFS for Alt-1, do not support higher PRACH slot density (number of PRACH slots per reference slot).
  + It is not necessary to optimize PRACH design to allow for LBT gaps between consecutive PRACH occasions within a PRACH slot, especially since PRACH can be classified as short control signaling transmissions consistent with EN 302 567 (see [8]).
  + UE beam switching gaps between consecutive PRACH occasions within a PRACH slot are not needed, since the UE is allowed to send only one PRACH preamble before the end of the RAR window, and will hence not need to transmit in back-to-back PRACH occasions in a slot.
* From [12] Futurewei:
  + For the reference slot duration support Option 1.
  + For PRACH slot density use the same density (i.e. number of PRACH slots per reference slot) as for 120kHz PRACH in FR2-1 is supported (ALT 1).
* From [13] Nokia:
  + Adopt Option 1) The reference slot duration corresponds to 60 kHz SCS. A PRACH slot index, , corresponds to one of the starting 480/960 kHz PRACH slots within the reference slot. FFS: to have LBT gaps between ROs
  + Adopt ALT 2) i.e. the number of ROs per reference slot is the same as for 120kHz PRACH in FR2.
  + If LBT gaps are needed between ROs, it would be better to define fixed LBT gap time between valid ROs that do not depend on the time domain allocation of the PRACH. In that case the LBT gap length would not depend on the used PRACH format.
* From [18] Qualcomm:
  + a maximum of 4 and 2 FD multiplexed ROs for SCS = 120 kHz and sequence length = 571 and 1151, respectively
  + for SCS = 120 kHz, if the maximum number of FD ROs are reduced, consider ways to increase the TD ROs (to maintain the same capacity) with minimal specification impact
  + for higher RACH SCS (480 and 960 kHz), the gap and CP length may not be long enough to absorb the gNB beam switching delay requirement
  + for higher RACH SCS (480 and 960 kHz), consider including a symbol-level gap between ROs to allow for gNB beam switching delay
  + for 480kHz and 960kHz PRACH:
    - The reference slot duration corresponds to 60 kHz SCS. A PRACH slot index, , corresponds to one of the starting 480/960 kHz PRACH slots within the reference slot
    - ROs for a given PRACH configuration can span more than one PRACH slot if gaps between consecutive ROs are supported for LBT and/or beam switching purposes
    - The same RO density (i.e. number of RO per reference slot) as for 120kHz PRACH in FR2 is supported
* From [19] LG Electronics:
  + If the reference slot SCS is kept as 60 kHz and the density of PRACH occasion is the same as in 120 kHz in the time-domain (e.g., 2 slots out of 8 slots for 480 kHz), the PRACH slot index for 480 and 960 kHz SCS can be determined based on the selected two values of with the pre-configured rule or based on the configured/indicated value(s) of by the gNB.
  + If the reference slot SCS is kept as 60 kHz and the density of PRACH occasion is increased compared to 120 kHz in the time-domain, the additional PRACH slots for 480 and 960 kHz SCS can be indicated/configured by the parameter X to allocate the consecutive X slots before the last slot given by (e.g., for 480 and 960 kHz SCS, respectively).
  + When LBT is used to transmit the PRACH preamble, consider to insert CCA gap between adjacent RACH occasions in time domain (e.g. X usec or Y symbol) to avoid inter-UE LBT blocking due to the propagation delay of PRACH transmitted in an earlier RO.
  + Considering the potential gap to account for LBT is needed to be inserted between the adjacent RACH occasions, at least the same RO density (i.e. number of RO per reference slot) as for 120 kHz PRACH in FR2-2 is supported for the PRACH density.
* From [20] ETRI:
  + Support Option 1 and ALT 2 for 480kHz and 960kHz PRACH slot configurations.
* From [22] Intel:
  + For 480kHz and 960kHz PRACH, select Option 1) The reference slot duration corresponds to 60 kHz SCS. A PRACH slot index, , corresponds to one of the starting 480/960 kHz PRACH slots within the reference slot.
  + For PRACH SCS 480 kHz and 960 kHz, introduce optional time gaps between consecutive ROs;
  + Modify equation defining the first OFDM symbol of PRACH RO given Section 5.3.2 from TS 38.211 as follows:
    - ,
    - where is the gap duration (number of OFDM symbols) and for no gap.
  + On PRACH density for 480kHz and 960kHz PRACH, select ALT 2) at least the same RO density (i.e. number of RO per reference slot) as for 120kHz PRACH in FR2 is supported.
* From [23] Apple:
  + Maximum 4 PRACH ROs can be configured for 120kHz SCS with .
  + Maximum 2 PRACH ROs can be configured for 120kHz SCS with .
  + Reuse the existing FR2 PRACH configuration Table to indicate the time-domain PRACH slot location.
  + Support to keep the same PRACH capacity as Rel-16 FR2 for 480kHz and 960kHz SCS to minimize the signaling overhead.
  + The configured PRACH slots should be distributed over the 60kHz reference slot.
* From [24] Sharp:
  + Option 1 for RO design is preferred. Reuse Table 6.3.3.2-4 (Random access configurations for FR2 and unpaired spectrum) in Rel-16 38.211 as much as possible. 60kHz reference slot should be also inherited.
  + Regarding PRACH configuration design for 480/960kHz SCS, keep the same RO density and Alt 2 is preferred.
  + Gaps between consecutive ROs are needed at least for beam switching purposes, which should be considered during RO design.
  + A starting symbol index of a PRACH occasion is given by If non-zero duration gaps are configured between consecutive ROs and the ROs would span multiple PRACH slots, for 480 and 960 kHz SCS, respectively. Otherwise, for 480 and 960 kHz SCS, respectively.
* From [25] NTT Docomo:
  + For RO configuration for PRACH with 480/960 kHz SCS,
    - Support Option 1 to specify only 480/960 kHz PRACH slot within a 60 kHz referenced slot in addition to the existing RO configuration in FR2.
    - Only one or two 480/960 kHz PRACH slot(s) within the 60 kHz referenced slot is sufficient.
    - No need to enhance RA-RNTI calculation for NR operation in 52.6 – 71 GHz
    - No need to consider either LBT or beam switching gap for RO design in 52.6 – 71 GHz
* From [26] Xiaomi:
  + Inconsecutive RO time domain configuration should be supported at least for 480 kHz case.

#### Summary of Discussions

The following are previous agreements on PRACH sequence and formats.

|  |
| --- |
| **Agreement:**   * PRACH configuration for 480/960 kHz SCS (if agreed)   + The minimum PRACH configuration period is 10 ms (as in FR2)   + For RO configuration for PRACH with 480/960kHz SCS,     - FFS: details of how to configure the 480/960 kHz PRACH ROs using [60 or 120 kHz] reference slot considering at least:       * location of 480/960 kHz PRACH slot per reference slot       * location of duration containing 480/960khz PRACH slot pattern within 10ms       * potential impact to RA-RNTI calculation   **Agreement:**  For 480kHz and 960kHz PRACH,   * Down-select among option 1 and 2   + Option 1) The reference slot duration corresponds to 60 kHz SCS. A PRACH slot index, , corresponds to one of the starting 480/960 kHz PRACH slots within the reference slot.  * + - FFS: supported values of the starting PRACH slot index within reference slot and whether or not the ROs for a given PRACH configuration can span more than one PRACH slot if gaps between consecutive ROs are supported for LBT and/or beam switching purposes  * + Option 2) Each 120kHz RO corresponds to 4 and 8 candidate RO positions for 480kHz and 960kHz PRACH, respectively. Information about the number and locations of 480/960kHz candidate RO(s) are configured or pre-selected within each 120kHz RO. The reference 120kHz RO is determined by the current PRACH configuration method in Rel-15/16 specification. * Following alternatives are considered on PRACH density   + ALT 1) At least the same density (i.e. number of PRACH slots per reference slot) as for 120kHz PRACH in FR2 is supported     - FFS: support for higher PRACH slot density (number of PRACH slots per reference slot)   + ALT 2) at least the same RO density (i.e. number of RO per reference slot) as for 120kHz PRACH in FR2 is supported     - FFS: support for higher RO density   + An “example” illustration of PRACH slots for 480/960kHz is shown below:      * FFS: whether and how to account for LBT in RO configuration (if needed) * FFS: whether and how to account for beam switching gap in RO configuration (if needed) |

The following is a summary of company views.

* RO definition for 480 and 960kHz
  + Option 1) The reference slot duration corresponds to 60 kHz SCS. A PRACH slot index, , corresponds to one of the starting 480/960 kHz PRACH slots within the reference slot.



* + - Huawei/HiSilicon, Interdigital, Ericsson, Futurewei, Nokia/NSB, [Qualcomm], ETRI, Intel, [Apple], Sharp, NTT Docomo, LGE, Fujitsu (1st preference, with configurable gaps between ROs), ZTE/Sanechips, OPPO, CATT
  + Option 2) Each 120kHz RO corresponds to 4 and 8 candidate RO positions for 480kHz and 960kHz PRACH, respectively. Information about the number and locations of 480/960kHz candidate RO(s) are configured or pre-selected within each 120kHz RO. The reference 120kHz RO is determined by the current PRACH configuration method in Rel-15/16 specification.
    - Samsung, Fujitsu (2nd preference), OPPO
* PRACH density
  + ALT 1) At least the same density (i.e. number of PRACH slots per reference slot) as for 120kHz PRACH in FR2 is supported
    - Ericsson, Futurewei, MTK, ZTE/Sanechips
  + ALT 2) at least the same RO density (i.e. number of RO per reference slot) as for 120kHz PRACH in FR2 is supported
    - Interdigital, Nokia/NSB, ETRI, Intel, Sharp, LGE, Fujitsu, OPPO, CATT, Huawei/HiSilicon
* Gap between consecutive ROs
  + Support: Huawei/HiSilicon, Samsung, Qualcomm, LGE, Intel (Configurable gap between consecutive RO), [Sharp], Fujitsu, OPPO, Xiaomi, Futurewei
  + Do not support: Interdigital, Ericsson, NTT Docomo, MTK, ZTE/Sanechips
* Slot index for 480/960 kHz PRACH
  + for 480kHz and for 960kHz PRACH
    - Huawei/HiSilicon (For 1 PRACH slot per 60kHz reference slot), Sharp (gap not configured)
  + for 480kHz and for 960kHz PRACH.
    - Huawei/HiSilicon (For 2 PRACH slots per 60kHz reference slot)
  + Depends on , i.e., the number of time domain PRACH occaions within a 60 kHz reference slot (1 or 2) as specified in the 2nd last column of Table 6.3.3.2-4 in 38.211.
    - If
      * for 480kHz and for 960kHz PRACH
    - If
      * for 480kHz and for 960kHz PRACH
    - Ericsson, [it seems this is also supported by Huawei/HiSilicon]
  + for 480 and 960 kHz SCS, respectively
    - Sharp (gap configured)
  + The selected two values of with the pre-configured rule or based on the configured/indicated value(s) of by the gNB
    - LGE
* Maximum FDM of ROs
  + 4 FDM and 2 FDM ROs for 120kHz PRACH with L=571 and 1151, respectively
    - Qualcomm, Apple

#### **1st Round Discussion:**

Suggest to continue discussion on the above issues. Moderator asks companies to provide further comments. Moderator will provide a suggested proposal once the summary captures all company opinion correctly.

If the above summary is directly edited (please use a color to highlight changes, e.g. RED) and mention the changes/additions in the comment below.

|  |  |
| --- | --- |
| Company | Comments |
| Qualcomm | RO definition for 480 and 960kHz: Support 60 kHz reference slot in order to minimize the spec changes  PRACH density: Alt 2 |
| LG Electronics | We added our preference for Option 1 and Alt 2 in the above summary.  We prefer to keep the reference slot subcarrier spacing as 60 kHz and if the density of PRACH occasion is the same as in 120 kHz in the time-domain (e.g., 2 slots out of 8 slots for 480 kHz), the PRACH slot index for 480 and 960 kHz SCS can be determined based on the selected two values of with the pre-configured rule or based on the configured/indicated value(s) of by the gNB. For PRACH density, at least the same RO density (i.e. number of RO per reference slot) as for 120 kHz PRACH in FR2-2 is supported considering the potential gap to account for LBT is needed to be inserted between the adjacent RACH occasions. |
| Fujitsu | We added our preferences in the above summary. |
| Mediatek | Our preferences have been added in the above summary |
| Sharp | We support gap between consecutive ROs. |
| Docomo | For gap between Ros, we are struggling to understand its necessity because of the following:   * In terms of LBT, it is something discussed in Rel-16 NR-U but not supported in our understanding. In 52.6 – 71 GHz, given that much narrower beam is likely used, the case where a PRACH at a RO interferes another PRACH at later RO would barely happen. * In terms of beam switching (at gNB reception), this is depending on RAN4 reply regarding beam switching. As discussed in 2.1.2, we would like to hear companies’ views on how to treat it. With the current value RAN4 told us, beam switching time does not need to be considered here in our view. |
| ZTE/Sanechips | Please see our added support above using “ZTE/Sanechips” |
| Nokia | Our preference is Option 1 with 60kHz reference slot and ALT 2 for PRACH density. We don’t currently see that LBT gaps are absolutely mandatory. |
| OPPO | Please see our added support above using “OPPO” |
| Xiaomi | Please see our added support above using “Xiaomi” |
| Samsung | 1. Even though we still believe Option 2 has benefits, it seems the Option 2 is not preferred by companies, thus, we can live with Option 1 for RO definition for 480 and 960kHz;  2. For RACH density, we want to clarify that, it’s for maximum RACH density instead of every RACH density; with this assumption, we prefer Alt.2; suggested change:  ALT 2) at least the same maximum RO density (i.e. number of RO per reference slot) as for 120kHz PRACH in FR2 is supported  3. For slot index, {7,15} for one PRACH slot and {3,7; 7,15} for 2 PRACH slot seem fine.  4. When gap is needed, it should be designed on top of the configured ROs. |
| Intel | Regarding slot index, although we didn’t propose particular values, our requirement is that the slot index should be aligned with the SSB slot patterns in order to avoid systematic overlapping between SSBs and ROs. |
| Futurewei | Please see our added support above using “Futurewei”. |
| Ericsson | Please see our added support above using "Ericsson". For the slot index for 480/960 kHz, I have merged the first two options into a new option. I believe this is also supported by Huawei/HiSilicon. This option aligns with the following diagram from the agreement, i.e., slots 7 or 3+7 are used for 480 kHz, and slots 7 or 7 + 15 are used for 960 kHz.    Regarding gaps, we agree with DOCOMO's view in terms of LBT. In fact, gaps were not introduced in Rel-16 NR-U, and the system is not broken. Gaps are even less motivated for Rel-17. In terms of beam switching, gaps are not needed from a UE perspective since the UE transmits PRACH in only one RO, so no beam switching needed. From a gNB perspective, RAN4 is discussing 59 ns as a beam switching requirement which is less then the CP for 960 kHz. Hence, gaps are not needed.  We observe that if no gaps are introduced, Alt-2 is equivalent to Alt-1 which is our preference. |
| CATT | Please see our added support above using “CATT”. |
| Huawei/HiSilicon | * Reference slot   + We support Option 1 for PRACH reference slot as in Rel-15. * Beam switching gap   + We believe that beam switching gap symbol is required between consecutive ROs for both 480/960 kHz PRACH. Although beam switch time at gNB is tentatively [59ns], up to 200ns beam switch time at the UE side is suggested in ongoing discussions in RAN4. Comparing these values with the 73ns (146ns) CP length of 960kHz (480kHz) OFDM symbols, the introduction of a beam switching gap symbol for PRACH seem required. Although the CP lengths of different PRACH formats are longer than that of the OFDM symbol, such larger CP lengths are mainly devised to additionally cope with the timing uncertainty that can be up to the maximum round-trip delay in the cell. For instance, the CP of Format A1 is 146ns (292ns) in 960kHz (480kHz) and the CP of Format B1 is 110ns (220ns) in 960kHz (480kHz). Such CP lengths are not enough to accommodate up to 200ns of beam switch time in addition to round-trip time delay, DL time synchronization, and channel dispersion effects. * PRACH density   + We support ALT 2 at least the same RO density (i.e. number of RO per reference slot) as for 120kHz PRACH in FR2 * Number of PRACH slots and PRACH slots indexes in a reference slot   + We support keeping at least the same number of ROs per reference slot and, at the same time, propose to use beam switching gap. Therefore, number of PRACH slots within the PRACH reference slot may need to be increased for some PRACH configuration indexes in Table 6.3.3.2-4:     - There are PRACH configuration indexes where starting symbol is symbol 0 and PRACH duration is 6 symbols with 2 ROs per PRACH slots (e.g. PRACH configuration indexes 68 and 69). In these cases, beam switching gap + number of ROs can be supported within the same slot and the number of PRACH slots in a reference slot does not need to increase. For such cases, for 480kHz and for 960kHz PRACH when the number of PRACH slots in a reference slot is 1 and for 480kHz and for 960kHz PRACH when the number of PRACH slots in a reference slot is 2.     - There are PRACH configuration indexes where the same number of ROs per PRACH slot as in Table 6.3.3.2-4 + beam switching gap cannot be accommodated within a single PRACH slot. In such cases, number of PRACH slots per reference slot should increase to e.g. 4. One way to choose the new PRACH slots is to use the slots immediately after the original PRACH slots to let the ROs in the original PRACH slot spill over to the subsequent slot. However, this is not the only solution and any solution that can support keeping the RO density per reference slot at least the same as in Rel-15 without any (or with minimum) change to Table 6.3.3.2-4 can be discussed. |

#### **1st Round Discussion Summary:**

**Issue 1)** RO definition for 480 and 960kHz. Clear majority of the companies prefer option 1. Suggest to continue discussion based on proposal for option 1.

|  |
| --- |
| * RO definition for 480 and 960kHz   + Option 1) The reference slot duration corresponds to 60 kHz SCS. A PRACH slot index, , corresponds to one of the starting 480/960 kHz PRACH slots within the reference slot.  * + - Huawei/HiSilicon, Interdigital, Ericsson, Futurewei, Nokia/NSB, [Qualcomm], ETRI, Intel, [Apple], Sharp, NTT Docomo, LGE, Fujitsu (1st preference, with configurable gaps between ROs), ZTE/Sanechips, OPPO, CATT   + Option 2) Each 120kHz RO corresponds to 4 and 8 candidate RO positions for 480kHz and 960kHz PRACH, respectively. Information about the number and locations of 480/960kHz candidate RO(s) are configured or pre-selected within each 120kHz RO. The reference 120kHz RO is determined by the current PRACH configuration method in Rel-15/16 specification.     - Samsung, Fujitsu (2nd preference), OPPO |

##### **Proposal 2.2-1)**

* For 480 and 960kHz PRACH:
  + The reference slot duration corresponds to 60 kHz SCS. A PRACH slot index, , corresponds to one of the starting 480/960 kHz PRACH slots within the reference slot.



**Issue 2)** Regarding the PRACH density, majority of the companies prefer Alt 2. The distinction between the two alternatives seems to be minor and seems to depend on whether RO can span more than 1 PRACH slot, which is related to RO density.

Regarding whether or not to support gap between consecutive ROs, more companies prefer to define gaps. One company explicitly mentioned that gap should be configurable.

Moderator suggest continuing discussion based on Alt 2 for density and supporting resource gap between consecutive ROs.

|  |
| --- |
| * PRACH density   + ALT 1) At least the same density (i.e. number of PRACH slots per reference slot) as for 120kHz PRACH in FR2 is supported     - Ericsson, Futurewei, MTK, ZTE/Sanechips   + ALT 2) at least the same RO density (i.e. number of RO per reference slot) as for 120kHz PRACH in FR2 is supported     - Interdigital, Nokia/NSB, ETRI, Intel, Sharp, LGE, Fujitsu, OPPO, CATT, Huawei/HiSilicon, vivo |

##### **Proposal 2.2-2)**

* For 480 and 960kHz PRACH:
  + at least the same RO density (i.e. number of RO per reference slot) as for 120kHz PRACH in FR2 is supported
  + Support resource gap between consecutive ROs.
    - FFS whether this gap can be configured by gNB.

**Issue 3)** Regarding the slot index for 480/960 kHz PRACH, further discussion is needed. One company identified that there are some PRACH configuration entries where all ROs and beam switching gap can be accommodated within PRACH slot and there are some PRACH configuration entries where it may not be possible. For the former cases, few companies suggest to use 7, 15 for 480 and 960kHz, respectively, when 1 occasion is defined for a 60kHz reference and {3,7} and {7,15} for 480 and 960kHz, respectively, when \*2 occasion is defined for a 60kHz reference. Hopefully, even for companies who do not think beam switching gap is needed, if the Proposal 2.2-3 would still be ok.

##### **Proposal 2.2-3)**

* For 480 and 960kHz PRACH when number of time domain PRACH occasions and potential beam switching gap can be placed within a PRACH slot,
  + and number of PRACH slots in a reference slot is 1,
    - for 480kHz and for 960kHz PRACH
  + And when the number of PRACH slots in a reference slot is 2,
    - for 480kHz and for 960kHz PRACH
* FFS: values when number of time domain PRACH occasions and potential beam switching gap cannot be placed within a PRACH slot.

#### **2nd Round Discussion:**

Please provide further comments on Proposal 2.2-1 ~ 2.2-3.

|  |  |
| --- | --- |
| Company | Comments |
| vivo | Support the proposal |
| DOCOMO | * Support Proposal 2.2-1 * For Proposal 2.2-2, still not sure why beam switch gap is needed. Maybe the decision can be discussed with 2.1.2 in terms of beam switching gap. Not sure why UE-side beam switching needs to be considered. * Proposal 2.2-3 should be discussed after Proposal 2.2-2. |
| Nokia | Proposal 2.2-1: We are OK with this proposal.  Proposal 2.2-2: We are OK with this proposal.  Proposal 2.2-3: In principle we are OK with this proposal, but maybe the beam switching text could put as FFS or removed. This can be further discussed of course, but based on latest RAN4 feedback on gNB beam switching gap, this would not seem necessary. |
| ZTE, Sanechips | We are fine with Proposal 2.2-1.  For Proposal 2.2-2, we still don’t quite understand the motivation to introduce the gap between ROs. RAN4 has sent an LS about the gNB beam switching time as 59ns, this can be covered by the CP length of PRACH sequence. As for UE beam switching, it should not be considered for gap between ROs since UE will randomly select only one of these ROs and there is no beam switching issue.  We are fine with Proposal 2.2-3. |
| Samsung | For 2.2-1, we expressed the compromise to option1, but however, we see some proponents raised the additional points for extra design on spilling the RO in more slots than configured in order to accommodate the beam switching gap (or other gap). If this is the case, we will insist on the option2, which can solve the problem once for all.  For 2.2-2, as we commented before, we want to clarify that, it’s for maximum RACH density instead of every RACH density; with this assumption, we prefer Alt.2; suggested change:   * For 480 and 960kHz PRACH:   + at least the same maximum RO density (i.e. number of RO per reference slot) as for 120kHz PRACH in FR2 is supported   + Support ~~resource~~ gap between consecutive ROs in time domain.     - FFS the details to derive the gap ~~whether this gap can be configured by gNB.~~   For 2.2.-3, as we commented in above, we did not see the need to separate the cases based on “when number of time domain PRACH occasions and potential beam switching gap can be placed within a PRACH slot”, and there could be multiple ways to create the gap (e.g., odd or even number indication), which needs no additional spec effort. So suggest:   * For 480 and 960kHz PRACH ~~when number of time domain PRACH occasions and potential beam switching gap can be placed within a PRACH slot~~,   + and number of PRACH slots in a reference slot is 1,     - for 480kHz and for 960kHz PRACH   + And when the number of PRACH slots in a reference slot is 2,     - for 480kHz and for 960kHz PRACH * ~~FFS: values when number of time domain PRACH occasions and potential beam switching gap cannot be placed within a PRACH slot.~~ |
| Intel | Proposal 2.2-1) – agree  Proposal 2.2-2) – agree  Proposal 2.2-3) – don’t agree.  We prefer to defer agreement on this proposal until it is clarified whether time gaps between consecutive ROs are needed or not. We prefer to have a single solution which would cover both cases with and without gaps. |
| Apple | Proposal 2.2-1: Support.  Proposal 2.2-2: Support in principle.  Regarding the ‘gap’, our understanding is that it mainly targets to provide flexibility at gNB for Rx beam switching, instead of UE side. Another potential benefit is to reduce the blocking probability for two consecutive ROs for unlicensed operation. If it was defined as ‘configurable’, we do not see strong concern as gNB/operator can disable or configure it as ‘0’ by proper configuration if wants.  Proposal 2.2-3: Support. |
| Qualcomm | Proposal 2.2-1: fine  Proposal 2.2-2: fine  Proposal 2.2-3: This is fine assuming no gaps between ROs, if RO gaps are allowed and the same number of ROs (compared to 120 kHz) is desired, then ROs for some configurations will need more than 1 RA slot, hence, this (Proposal 2.2-3) may not work. Suggest we defer this discussion until the following are concluded: 1) RO gaps need and design, 2) to allow (or not) for ROs to spill into adjacent slots |
| Sharp | Proposal 2.2-1: Support  Proposal 2.2-2: Support  Proposal 2.2-3: We also think that detailed discussion should be after concluding Proposal 2.2-1 and Proposal 2.2-2. |
| Futurewei | Proposal 2.2-1 OK  Proposal 2.2-2 OK  Proposal 2.2-3 Fine to discuss further |
| Ericsson | **Proposal 2.2-1**: Support  **Proposal 2.2-2**: We do not support the 2nd sub-bullet, i.e., we still do not support gaps. If companies are worried about gNB beam switching gap, then we can wait for RAN4 to confirm [59 ns].  We can be open to the first sub-bullet with the following clarification:   * For 480 and 960kHz PRACH:   + For a given configured number of frequency domain ROs, at least the same RO density (i.e. number of RO per reference slot) as for 120kHz PRACH in FR2 is supported   **Proposal 2.2-3**: Support conditioned on the following changes:   * For 480 and 960kHz PRACH when number of time domain PRACH occasions and ~~potential~~ beam switching gap (if supported) can be placed within a PRACH slot,   + and number of time domain PRACH ~~slots~~ occasions in a reference slot is 1,     - for 480kHz and for 960kHz PRACH   + And when the number of time domain PRACH ~~slots~~ occasions in a reference slot is 2,     - for 480kHz and for 960kHz PRACH * FFS: values when number of time domain PRACH occasions and ~~potential~~ beam switching gap (if supported) cannot be placed within a PRACH slot. |
| Huawei, HiSilicon | Proposal 2.2-1: Agree  Proposal 2.2-2: Agree  Proposal 2.2-3: We prefer to support this with the following modification. Otherwise, the time domain PRACH occasions can always be modified (reduced) such that the PRACH occasions and potential beam switching gap can be placed within a PRACH slots **Proposal 2.2-3)**  * For 480 and 960kHz PRACH when number of time domain PRACH occasions corresponding to a PRACH Config. Index in Table 6.3.3.2-4 of 38.211 and potential beam switching gap can be placed within a PRACH slot,   + and number of PRACH slots in a reference slot is 1,     - for 480kHz and for 960kHz PRACH   + And when the number of PRACH slots in a reference slot is 2,     - for 480kHz and for 960kHz PRACH * FFS: values when number of time domain PRACH occasions corresponding to a PRACH Config. Index in Table 6.3.3.2-4 of 38.211 and potential beam switching gap cannot be placed within a PRACH slot. |

#### **2nd Round Discussion Summary:**

Below is a summary of company preferences. Proposal 2.2-2A and 2.2-3A are alternative proposals from Samsung. Moderator suggest to continue discuss based on the proposal listed.

##### **Proposal 2.2-1)**

* For 480 and 960kHz PRACH:
  + The reference slot duration corresponds to 60 kHz SCS. A PRACH slot index, , corresponds to one of the starting 480/960 kHz PRACH slots within the reference slot.



* Ok: vivo, Docomo, Nokia/NSB, ZTE/Sanechips, Intel, Apple, Qualcomm, Sharp, Futurewei
* Not Ok: Samsung (if gaps are needed option 2 would be better design)

##### **Proposal 2.2-2)**

* For 480 and 960kHz PRACH:
  + at least the same RO density (i.e. number of RO per reference slot) as for 120kHz PRACH in FR2 is supported
  + Support resource gap between consecutive ROs.
    - FFS whether this gap can be configured by gNB.
* Ok: vivo, Nokia/NSB, Intel, Apple, Qualcomm, Sharp, Futurewei
* Not Ok: Docomo, ZTE/Sanechips

##### **Proposal 2.2-2A)**

* For 480 and 960kHz PRACH:
  + at least the same maximum RO density (i.e. number of RO per reference slot) as for 120kHz PRACH in FR2 is supported
  + Support ~~resource~~ gap between consecutive ROs in time domain.
    - FFS the details to derive the gap
    - ~~FFS whether this gap can be configured by gNB.~~

##### **Proposal 2.2-3)**

* For 480 and 960kHz PRACH when number of time domain PRACH occasions and potential beam switching gap can be placed within a PRACH slot,
  + and number of PRACH slots in a reference slot is 1,
    - for 480kHz and for 960kHz PRACH
  + And when the number of PRACH slots in a reference slot is 2,
    - for 480kHz and for 960kHz PRACH
* FFS: values when number of time domain PRACH occasions and potential beam switching gap cannot be placed within a PRACH slot.
* Ok: vivo, Apple, Qualcomm
* Maybe: Docomo
* Not Ok: Intel (prefer to defer)
* Defer: Intel, Sharp, Futurewei

##### **Proposal 2.2-3A)**

* For 480 and 960kHz PRACH ~~when number of time domain PRACH occasions and potential beam switching gap can be placed within a PRACH slot,~~
  + and number of PRACH slots in a reference slot is 1,
    - for 480kHz and for 960kHz PRACH
  + And when the number of PRACH slots in a reference slot is 2,
    - for 480kHz and for 960kHz PRACH
* ~~FFS: values when number of time domain PRACH occasions and potential beam switching gap cannot be placed within a PRACH slot.~~

### 2.2.3 RAR Window & RA Preamble ID

* From [1] Huawei/HiSilicon:
  + Introduce additional bits in the DCI scheduling RAR to resolve the issue of RA-RNTI/MsgB-RNTI calculation for 480 kHz and 960 kHz RACH procedure.
  + Support maximum of 40 ms for ra-ResponseWindow for operation with shared spectrum and msgB-ResponseWindow for both operations with and without shared spectrum. Support indicating two LSBs of SFN at which gNB has received msg1 (MsgA) in DCI format 1\_0 with CRC scrambled by RA-RNTI (MsgB-RNTI).
* From [2] vivo:
  + For larger PRACH SCS (480KHz/960KHz), the following options can be considered for RA-RNTI calculation:
    - Alt.1: Modify the RA-RNTI formula as following and introduce some contention resolution mechanism to resolve the conflict.
      * RA-RNTI = (1+s\_id+14×t\_id+14×X×f\_id +14×X×8×ul\_carrier\_id) mod A
    - Alt.2: Reuse the current RA-RNTI formula while introducing additional indicator field to indicate the time-frequency resource together with RA-RNTI.
    - Alt.3: Depending on the RO configuration pattern, reuse/modify the RA-RNTI formula and express the slot indexes t\_id based on a new specific subcarrier spacing.
* From [8] CATT:
  + For supporting Msg1 transmission with 480 KHz/960 KHz SCS, RA-RNTI is divided into two parts. One part of RA-RNTI is carried by DCI, and the remaining 16-bit of RA-RNTI could be used to scramble CRC of the DCI1. Two possible options are:
    - Option A:
      * RA-RNTI = (1 + s\_id + 14 × t\_id + 14 ×× f\_id + 14 × × 8 × ul\_carrier\_id) mod
      * inDCI\_bit = floor ((1 + s\_id + 14 × t\_id + 14 ×× f\_id + 14 × × 8 × ul\_carrier\_id) /)
      * s\_id is the index of the first OFDM symbol of the PRACH occasion (0 ≤ s\_id < 14)
      * t\_id is the index of the first slot of the PRACH occasion in a system frame (0 ≤ t\_id < 640)
    - Option B:
      * RA-RNTI = 1 + s\_id + 14 ×(t\_id mod 80) + 14 × 80 × f\_id + 14 × 80 × 8 × ul\_carrier\_id
      * inDCI\_bit =
      * s\_id is the index of the first OFDM symbol of the PRACH occasion (0 ≤ s\_id < 14)
      * t\_id is the index of the first slot of the PRACH occasion in a system frame (0 ≤ t\_id < 640)
* From [9] ZTE/Sanechips:
  + For higher PRACH SCS (480 and/or 960 kHz), consider the following options for further down-selection of RA-RNTI enhancements:
    - Option 2)
      * Segment the PRACH into N segments
      * Non-overlapping PRACH slot location in each segment(80 slots)
    - Option 3)
      * Segment the PRACH into N segments
      * is the index of the PRACH slot that contains the PRACH occasion in a segment.
      * In DCI: RA-indication = Segment index
    - Option 7)
      * is the index of the first 120kHz slot that contains the PRACH occasion in a system frame.
      * is the index of the first OFDM symbol of the PRACH occasion based on the value of specified in clause 5.3.2 of TS 38.211.
* From [10] Fujitsu:
  + For 480kHz and 960kHz PRACH, the following should be considered to uniquely identify a RO:
    - When calculating RA-RNTI, t\_id is determined in a way that more than one slot can have the same t\_id; and
    - DCI scheduling RAR indicates the local index among the slots having the same t\_id.
* From [11] Ericsson:
  + For 480/960 kHz PRACH, reuse the RA-RNTI expressions from Rel-15/16, with the additional statement that for 480/960 kHz PRACH, t\_id should be determined based on a subcarrier spacing of 120 kHz.
  + Postpone further discussions of RA-RNTI design until the PRACH configuration design is settled.
* From [13] Nokia:
  + Reuse RA-RNTI formula defined for 120 kHz SCS also for the cases PRACH is configured with 480 or 960 kHz SCS where
    - assumes 480/960 kHz SCS
    - assumes 120 kHz SCS
* From [19] LG Electronics:
  + If the reference slot SCS remains as 60 kHz and the density of PRACH occasion is the same as in 120 kHz in the time-domain (e.g., 2 slots out of 8 slots for 480 kHz), the existing RA-RNTI/MSGB-RNTI equation can be reused for 480 and 960 kHz SCS by reinterpreting the slot indexes t\_id based on a new specific subcarrier spacing as the slot indexes of 120 kHz SCS (e.g., floor(t\_id/n) where n=4 for 480 kHz SCS and n=8 for 960 kHz).
  + If the reference slot SCS remains as 60 kHz and the density of PRACH occasion is increased compared to 120 kHz in the time-domain, to calculate RA-RNTI/MSGB-RNTI associated with the PRACH occasion for 480 and 960 kHz SCS using the existing RA-RNTI equation, the following options can be considered:
    - Option 1: Divide the RAR window for RA-RNTI (or msg2 window for MSGB-RNTI) into N sub-periods (where each sub-period is 80 slots using the used SCS) + signal the sub-period index using the DCI that schedules the MSG2/MSGB.
    - Option 2: Divide the frequency index or the symbol index into M subset (if M=4, the subset index 0/1/2/3 can be configured to the frequency index {0, 1}, {2, 3}, {4, 5}, {6, 7}, respectively) + signal the subset index using the DCI that schedules the MSG2/MSGB
* From [20] ETRI:
  + Propose to reuse the current equation with minor modifications for RA preamble ID calculation.
    - RA-RNTI = 1 + s\_id + 14 × t\_id + 14 × 80 × f\_id + 14 × 80 × 8 × ul\_carrier\_id
      * t\_id is the index of 120kHz slot that contains RO in a system frame
      * s\_id is the index of the first OFDM symbol of RO based on the value of specified in clause 5.3.2 of TS 38.211
* From [22] Intel:
  + RA-RNTI computation equation should be adjusted to avoid overflow in case of PRACH SCS 480 kHz and 960 kHz;
  + Support the following modified equation for RA-RNTI computation:
    - ,
    - where t\_id is based on the value of specified in clause 5.3.2 of TS 38.211.
* From [23] Apple:
  + modifying the existing calculation equation or redefine t\_id based on 120kHz SCS to solve the RA-RNTI overflowing problem:
* From [24] Sharp:
  + Assuming RO density per reference slot is unchanged, without modifying the formula and definition of s\_id. Modify the definition of t\_id as the slot index referring to 120kHz SCS.

#### Summary of Discussions

The following list of options are from last meetings discussion.

|  |
| --- |
| * + **Plain Modulus Category**     - Option 1)   + **PRACH Sub-segmentation Method Category**     - Option 2)       * Segment the PRACH into N segment       * Non-overlapping PRACH slot location in each segment(80 slots)       * ~~The same PRACH slot location in each 120kHz slot duration~~     - Option 3)       * Segment the PRACH into N segments       * is the index of the PRACH slot that contains the PRACH occasion in a segment.       * In DCI: RA-indication = Segment index     - Option 4)       * Segment the PRACH into N segments       * In DCI:     - Option 5)       * Segment the PRACH into N segments       * In DCI:     - Option 6)       * In DCI:   + **Compressing some indices Category (may require a matching RO configuration to work properly)**     - Option 7)       * is the index of the first 120kHz slot that contains the PRACH occasion in a system frame.       * is the index of the first OFDM symbol of the PRACH occasion based on the value of specified in clause 5.3.2 of TS 38.211.     - Option 8)       * RA-RNTI = 1 + s\_id + 14 × floor(t\_id / ) + 14 × 80 × f\_id + 14 × 80 × 8 × ul\_carrier\_id,       * t\_id is based on the value of specified in clause 5.3.2 of TS 38.211. |

The following is summary of company views.

* Alt 1) Plain Modulus Category, some example in option 1
  + Vivo, Apple
* Alt 2) PRACH Sub-segmentation Method Category, some examples in option 2 ~ 6
  + Huawei/HiSilicon, vivo, CATT, ZTE/Sanechips, Fujitsu, LGE
* Alt 3) Compressing some indices Category (may require a matching RO configuration to work properly) , some examples in option 7 ~ 8
  + vivo, ZTE/Sanechips, Ericsson, Nokia/NSB, ETRI, Intel, Sharp

#### **1st Round Discussion:**

Moderator suggest to further discuss the three categories and the detailed options.

|  |  |
| --- | --- |
| Company | Comments |
| Qualcomm | Although requires some extra signaling, but we prefer Alt2.  For Alt 1, the RA-RNTI can be more than FFFF and modular operation needs to be applied. Due to the modular operation, some ROs:   * May have the same RA-RNTI * May collide with FFF0–FFFD (reserved) or P-RNTI (FFFE) or SI-RNTI (FFFF)   Hence, some restrictions need to be applied:   * ROs with RA-RNTI conflicting with the pre-allocated RNTIs should not be used. * When multiple ROs have the same RA-RNTI but not conflicting with the pre-allocated RNTIs, only one of the ROs can be used (e.g., the first RO among those ROs with the same RA-RNTI) or rely on the existing contention resolution mechanisms   For Alt3, some restrictions may be needed to the RO design for it to work |
| Fujitsu | 1. For down selection of options for RA-RNTI calculation, the impact on MSBG-RNTI should be considered. For example, if RA-RNTI is calculated by Alt 1), additional method may be needed for handling collision between RA-RNTI and MSBG-RNTI. From this perspective, Alt 1) is not preferred. Then between Alt 2) and Alt 3), considering flexibility, Alt 2) is preferred.  2. It seems that option 2) should belong to Alt 3) rather than Alt 2). |
| Sharp | We prefer Alt 3 which provides a simple solution with minor specification impact. |
| ZTE, Sanechips | Alt 2 and Alt 3 both work for us.  To better align with the category, Option 2 can be modified as   * Option 2)   + Segment the PRACH into N segments   + Non-overlapping PRACH slot location in each segment(80 slots)   Option 2 can be categorized in either Alt 2) or Alt 3), since it also requires some compression and relies on the RO configuration. |
| Nokia | While we prefer Alt 3, it might be best to wait the conclusion in Section 2.2.2 |
| Samsung | Alt. 3 seems fine.  One simple way is actually, the t\_id could be the logical order index of the PRACH slot. Because based on previous design, the PRACH slot density anyway will not be larger than 80 (i.e., the max one in 120khz case); |
| Lenovo, Motorola Mobility | We support Alt 3. |
| Intel | This decision could be made after the agreement on RACH occasion resources configuration as it may impact parameters constituting RA-RNTI calculation formula (e.g., s\_id and t\_id). |
| Futurewei | We prefer Alt 2, Option 6 |
| Ericsson | Defer until agreement on RO configuration is achieved.  Assuming Option-1 + Alt-1 is adopted, then we observe the following:  Similar to Rel‑15/16, a maximum of one PRACH slot can occur within the duration of a 120 kHz slot, thus the expression for computing RA-RNTI in Rel‑15/16 can be directly reused, with the additional statement that for PRACH subcarrier spacings 480/960 kHz, t\_id should be calculated based on a subcarrier spacing of 120 kHz. |
| LG Electronics | This issue depends on the result of the discussion in the RO configuration for PRACH density in the previous section. We support Alt 3 if the density of PRACH occasion is the same as in 120 kHz in the time-domain (e.g., 2 slots out of 8 slots for 480 kHz), and if the higher density of PRACH occasion is supported, then Option 3 in Alt 2 can be considered. |
| Huawei/HiSilicon | We prefer Alt 2 category:   * It is more straightforward at least because it is usable independent of the parallel discussion of PRACH design and it is forward compatible. * If RA-RNTI formula needs to change, the discussion may actually need to be made in RAN2 as RA-RNTI formula is introduced in 38.321. However, if RA-RNTI ambiguity issue is resolved using, eg, segmentation, then, only adding 3 bits in DCI is required. In such a case, the discussion can be made in RAN1.   Finally, note that the issue of extending RAR window length was resolved in NR-U by adding 2 bits in DCI which, conceptually, is similar to Alt 2. |

#### **1st Round Discussion Summary:**

Here is the summary of company views.

* Alt 1) Plain Modulus Category, some example in option 1
  + Vivo, Apple
* Alt 2) PRACH Sub-segmentation Method Category, some examples in option 2 ~ 6
  + Huawei/HiSilicon, vivo, CATT, ZTE/Sanechips, Fujitsu, LGE (if higher density than 2 is supported), Futurewei, Qualcomm
* Alt 3) Compressing some indices Category (may require a matching RO configuration to work properly) , some examples in option 7 ~ 8
  + vivo, ZTE/Sanechips, Ericsson, Nokia/NSB, ETRI, Intel, Sharp, LGE, Lenovo/Motorola Mobility, Samsung

Company views are somewhat split between Alt 2 and 3. Alt 3 has more supporting companies. At the same time several companies commented that this can be discussed once the RO density for PRACH is concluded.

#### **2nd Round Discussion:**

Moderator suggests continuing discussion on RA-RNTI issue and try to conclude after PRACH RO definition and density discussion has been sufficiently resolved. Please continue to provide comments.

|  |  |
| --- | --- |
| Company | Comments |
| vivo | Support moderator’s suggestion |
| ZTE, Sanechips | Fine with moderator’s suggestion. |
| Samsung | We are ok with moderator’s assessment. |
| Intel | Let’s wait for agreements on PRACH Occasions configuration. |
| Apple | Support moderator’s suggestion. |
| Qualcomm | Support moderator’s suggestion |
| Sharp | Agree with moderator’s suggestion. |
| Futurewei | Fine to discuss further. |
| Huawei, HiSilicon | OK with the proposal |

#### **2nd Round Discussion Summary:**

TBD

### 2.2.4 Other aspects on PRACH

* From [12] Futuerwei:
  + If the UE RACH transmission can be LBT exempt under the short control signaling exclusion, support signaling to indicate UE that LBT is disabled or enabled for the RACH procedure.
* From [13] Nokia/NSB:
  + Discuss whether 960 kHz SCS PRACH procedure is supported from IDLE/Inactive state.

#### Summary of Discussions

The following are issues that were mentioned by companies.

* Short control signal exemption applicability for PRACH
* Whether 960kHz PRACH is supported for IDLE/inactive state.

#### **1st Round Discussion:**

Moderator assumes applicability of short control signal exemption will be discussed under channel access agenda. Moderator suggest companies to provide comments on the following issue.

* Whether 960kHz PRACH is supported for IDLE/inactive state

If there are other issues that require further discussion, please comment here as well.

|  |  |
| --- | --- |
| Company | Comments |
| Qualcomm | Initial access SSB (and hence PRACH) is limited to 480 kHz. We think this is outside the RAN1 and RAN agreements so far. |
| Nokia | As the physical layer functionality/design for CBRA will be in place/needed for CONNECTED mode operation, we don’t see reason why this should be excluded. In respect to WID, the definition of initial access was not ever clearly concluded for PRACH, while for DL/SSB it was considered in RAN1#104e as:   |  | | --- | | * + - “SSB in non-initial access” here refers to:       * SSB in Scell, where gNB is able to provide assistance information (e.g. SSB center frequency, SCS, etc)       * SSB for neighbor cell RRM measurements, where information is provided by gNB).     - “SSB in initial access” here refers to       * SSB used for “Cell Selection” defined in TS38.133 Section 4.1, which includes stored information cell selection and initial cell selection. | |
| Futurewei | We agree with Qualcomm, 960 kHz SCS PRACH for IDLE/inactive initial access is not supported. |
| Ericsson | Agree with Qualcomm |
| LG Electronics | We also agree with Qualcomm.  Since the 480 kHz SCS SSB was agreed to be supported for the initial access in RAN#92-e, the 480 kHz SCS PRACH can also be supported for the initial access in addition to the 120kHz SCS PRACH while the 960 kHz SCS PRACH is only supported for the non-initial access case. For use cases of 960 kHz SCS PRACH, the PRACH sequence with L=139 for 960 kHz SCS may not provide enough coverage for the initial access use case because the OFDM symbol duration becomes shorter with larger SCS. In addition, in order to support the RACH procedure of the active bandwidth part after initial access, PRACH SCS aligned with data SCS may be beneficial. Therefore, the 960 kHz SCS PRACH can be used for the cases other than initial access (e.g., for SCell) where the coverage is not a concern. |
| Huawei/HiSilicon | We don’t think this issue needs to be discussed but if this has to be discussed, our view is closer to Qualcomm’s view. |
| Samsung | The agreement of supporting 480 kHz SSB and 480 kHz CORESET#0 is only for the configuration by MIB. We believe it needs clarification on whether 960 kHz can be configured for initial BWP as configured by SIB1, and we don’t think this issue was discussed before. After that, the SCS of PRACH should be clear. |

#### **1st Round Discussion Summary:**

Further discussion seems necessary.

#### **2nd Round Discussion:**

Continue discussion.

|  |  |
| --- | --- |
| Company | Comments |
|  |  |

#### **2nd Round Discussion Summary:**

TBD

## 2.3 Others Aspects

* From [3] Spreadtrum:
  + The SSB-based TRS/CSI-RS validation can be supported.
* From [11] Ericsson:
  + The current RSSI and CO measurement in Rel-16 should be enhanced to support NR unlicensed operation in the spectrum beyond 52.6 GHz in Rel-17. The enhancement at least includes extension of reference SCS and indication of channel bandwidth. The enhancement details of the RRC configuration for RSSI and CO measurement should be decided by RAN2.
* From [12] Futurewei:
  + In 60 GHz shared spectrum band, where the LBT is enabled, allow a COT a gap between consecutive transmissions of at least one slot 480 kHz SCS duration (32us) without LBT.
  + Consider using CSI-RS presence in the discovery burst for possible ways to implement beam refinement during the initial channel access.
* From [13] Nokia:
  + It is proposed that RAN1 discusses whether IDLE mode procedures (camping, reselection) are supported for 960kHz sub-carrier spacing.
* From [7] Samsung:
  + RAN1 clarifies that the configurable SCS for initial BWP configured by SIB1 can be 120 kHz, 480 kHz, and 960 kHz.

#### Summary of Discussions

The following are issues that were mentioned by companies.

* The SSB-based TRS/CSI-RS validation can be supported.
* The current RSSI and CO measurement in Rel-16 should be enhanced to support NR unlicensed operation in the spectrum beyond 52.6 GHz in Rel-17. The enhancement at least includes extension of reference SCS and indication of channel bandwidth. The enhancement details of the RRC configuration for RSSI and CO measurement should be decided by RAN2.
* In 60 GHz shared spectrum band, where the LBT is enabled, allow a COT a gap between consecutive transmissions of at least one slot 480 kHz SCS duration (32us) without LBT.
* Consider using CSI-RS presence in the discovery burst for possible ways to implement beam refinement during the initial channel access.
* It is proposed that RAN1 discusses whether IDLE mode procedures (camping, reselection) are supported for 960kHz sub-carrier spacing.
* RAN1 clarifies that the configurable SCS for initial BWP configured by SIB1 can be 120 kHz, 480 kHz, and 960 kHz.

#### **1st Round Discussion:**

Moderator suggest to continue discussion on the above issues.

If there are other issues that require further discussion, please comment here as well.

|  |  |
| --- | --- |
| Company | Comments |
| Nokia | The consideration related to support of the IDLE mode procedures for 960kHz relates also to the discussion in Section 2.2.4 |
| Samsung | One of our proposals is missing from the summary (added above), which is related to PRACH SCS in IDLE/INACTIVE, but not limited. Actually we want to clarify the SCS of initial DL/UL BWP configured by SIB1 (the one configured by MIB is clear). If this issue is clarified, we believe the applicable SCS for PRACH in IDLE/INACTIVE is also clear. Based on current agreement, we didn’t see 960 kHz cannot be configured for SCS of initial DL/UL BWP configured by SIB1. |
| Futurewei | 960 kHz support in IDLE/INACTIVE. Same as 2.2.4 We do not see it in the scope of the discussions. We should discuss all other items. |

#### **1st Round Discussion Summary:**

Further discussion seems necessary for the other issues listed.

#### **2nd Round Discussion:**

Continue discussion.

|  |  |
| --- | --- |
| Company | Comments |
|  |  |

#### **2nd Round Discussion Summary:**

TBD

# Summary of Proposed Agreements/Conclusions

[To be filled]

# Summary of Agreements/Conclusions from RAN1 #106-e

[To be filled]

# Reference

1. R1-2106442, “Initial access signals and channels for 52-71GHz spectrum,” Huawei, HiSilicon
2. R1-2106579, “Discussions on initial access aspects for NR operation from 52.6GHz to 71GHz,” vivo
3. R1-2106692, “Discussion on initial access aspects for NR for 60GHz,” Spreadtrum Communications
4. R1-2106766, “Discussions on initial access signals and channels for operation in 52.6-71GHz,” InterDigital, Inc.
5. R1-2106795, “Considerations on initial access aspects for NR from 52.6 GHz to 71 GHz,” Sony
6. R1-2106831, “Initial access aspects for NR from 52.6 GHz to 71GHz,” Lenovo, Motorola Mobility
7. R1-2106873, “Initial access aspects for NR from 52.6 GHz to 71 GHz,” Samsung
8. R1-2106956, “Initial access aspects for up to 71GHz operation,” CATT
9. R1-2107000, “Discussion on the initial access aspects for 52.6 to 71GHz,” ZTE, Sanechips
10. R1-2107032, “Considerations on initial access for NR from 52.6GHz to 71 GHz,” Fujitsu
11. R1-2107050, “Initial Access Aspects,” Ericsson
12. R1-2107097, “Initial access for Beyond 52.6GHz,” FUTUREWEI
13. R1-2107104, “Initial access aspects,” Nokia, Nokia Shanghai Bell
14. R1-2107112, “Further discussion of initial access for NR above 52.6 GHz,” Charter Communications
15. R1-2107149, “Discussion on initial access aspects supporting NR from 52.6 to 71 GHz,” NEC
16. R1-2107176, “Initial access aspects for NR from 52.6GHz to 71 GHz,” Panasonic Corporation
17. R1-2107237, “Discusson on initial access aspects,” OPPO
18. R1-2107330, “Initial access aspects for NR in 52.6 to 71GHz band,” Qualcomm Incorporated
19. R1-2107435, “Initial access aspects to support NR above 52.6 GHz,” LG Electronics
20. R1-2107471, “Discussion on initial access aspects for NR from 52.6 to 71GHz,” ETRI
21. R1-2107517, “Discussion on initial access of 52.6-71 GHz NR operation,” MediaTek Inc.
22. R1-2107577, “Discussion on initial access aspects for extending NR up to 71 GHz,” Intel Corporation
23. R1-2107726, “Initial access signals and channels,” Apple
24. R1-2107789, “Initial access aspects,” Sharp
25. R1-2107845, “Initial access aspects for NR from 52.6 to 71 GHz,” NTT DOCOMO, INC.
26. R1-2107912, “On initial access aspects for NR from 52.6GHz to 71 GHz,” Xiaomi
27. R1-2108008, “NR SSB design consideration from 52.6 GHz to 71 GHz,” Convida Wireless
28. R1-2108148, “Discussion on initial access aspects for NR beyond 52.6GHz,” WILUS Inc.