**3GPP TSG RAN WG1 #107-e R1-21xxxxx**

**e-Meeting, November 11th – 19th, 2021**

**Agenda item:** 7.2.6

**Source:** Moderator (Samsung)

**Title:** Summary for Rel.16 NR eMIMO maintenance

**Document for:** Discussion and Decision

1. Introduction

The moderator summary of the maintenance-related issues raised in the submitted contributions for Rel.16 NR\_eMIMO maintenance is given below. The listed maintenance issues are under the usual designations:

* LP: low-PAPR RS
* MB: Multi-beam operation
* MT: Multi-TRP
* MU: Type-II enhancement for MU-CSI
* UL: UL full power transmission
* O: Other

An initial assessment on each of the issues is given (but can be revised based on the outcome of the discussion during the preparation week). The assessment will be used as a basis to select four issues (per chairman instruction) for further discussion in the upcoming weeks.

* *High priority (H):* this includes high-priority item (essential, pending issues, broken spec components) and proposed editorial changes that either enhance the clarity of the specs or correct mistakes
* *Non-essential (N)*: this includes all other purposes such as spec optimization and low priority issues
* *Editorial (E)*: this includes editorial issues that will be handled as editorial CRs (to be communicated to the editors/chairs) and thereby not counted toward the four-thread quota

1. Maintenance issues

The issues are summarized in the following table:

**Table 1 Summary**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **#** | **Issue (summary of CR proposal)** | **Companies** | **Initial assessment** | **Company inputs (if any)** |
| MB.1 | 1. Duplicated description of “in slot n”:  “when the UE would transmit a PUCCH with HARQ-ACK information in slot n corresponding to the PDSCH carrying the activation command ~~is transmitted in slot n~~”  2. Clarify the reference SCS µ:  “…the UE assumptions on updating spatial relation for the SRS resource shall be applied for SRS transmission starting from the first slot that is after slot n+3N\_slot^(subframe,µ) where µ is the SCS configuration for the PUCCH.”  FL: Necessary corrections and they are editorial. | Huawei, HiSilicon | E | Apple: In principle, we are fine with the editorial CR for the first the change, for the second change, we think some discussion should be needed. In general, we think this can be considered as “H”, since the second change defines a new behavior. |
| MB.2 | Clarify that gNB response for SCell-BFR is associated with a PUSCH with a same HARQ process number and a same serving cell as for the PUSCH including the BFR MAC-CE rather than just with a same HARQ process number. (R1-2110966)  FL: It seems to be a good clarification. | ZTE | H | Apple: We agree with FL proposal |
| MB.3 | Clarify the SCS of 28 symbols based on failed serving cell(s). (R1-2110967)  FL: It was discussed twice, but there is no consensus due to concern from Qualcomm. Whether to discuss it again can be up to Qualcomm. | ZTE | H | Apple: Hopefully we can reach consensus for this issue. But if companies’ position does not change, we would suggest not to discuss this issue. |
| MB.4 | Remove an unnecessary change from editor in alignment CR in RAN1 #106b. Clarify that UE can indicate both SSB and CSI-RS for CBD to higher layer. (R1-2111851)  FL: This is an editorial change to remove one unnecessary change. | Apple | E | Apple: We agree to handle it as editorial CR |
|  | | | | |
| MT.1 | Add description of using Table 7.3.1.2.2-1A/2A/3A/4A for NC-JT transmission in DCI 1\_2 in 38.212 (R1-2111672)  FL: necessary editorial change | Ericsson | E | Apple: We agree to handle it as editorial CR |
|  | | | | |
| MU.1 | Correction on RI and LI reporting  FL: Editorial. The 1st bullet may be revised as:  For Type I CSI feedback, Part 1 contains RI (if reported), CRI (if reported), CQI for the first codeword (if reported). Part 2 contains PMI (if reported) , LI (if reported) and contains the CQI for the second codeword (if reported) when RIvalue is larger than 4. | CATT (R1-2111219) | E | Apple: We agree to handle it as editorial CR. Both the LI part and the 2L-1 part. |
| MU.2 | mapping between K^NZ indicator and candidate values  FL: Not critical (may be a good clarification but not needed) | Qualcomm,  Huawei/HiSi | N |  |
| MU.3 | Typo corrections  FL: Editorial | Nokia/NSB (R1-2112355) | E | Apple: We agree to handle it as editorial CR |
| MU.4 | if , the value is negative  FL: This has been discussed in the past. This is a corner case, will not in practice almost surely. | Qualcomm | N |  |
| MU.5 | CSI frequency granularity when Mv=1  A CSI Reporting Setting is said to have a wideband frequency-granularity if  - *reportQuantity* is set to 'cri-RI-PMI-CQI', or 'cri-RI-LI-PMI-CQI', *cqi-FormatIndicator* is set to 'widebandCQI' and *pmi-FormatIndicator* is set to 'widebandPMI', or  *- reportQuantity* is set to 'cri-RI-PMI-CQI', or 'cri-RI-LI-PMI-CQI', *codebookType* is set to 'typeII -r16' or 'typeII-PortSelection-r16' with and *cqi-FormatIndicator* is set to 'widebandCQI', or  - *reportQuantity* is set to 'cri-RI-i1' or  FL: This was agreed in RAN1#106b-e for Rel-17 FDD CSI codebook (for Mv=1). But the need for Rel-16 CB is unclear since with Mv=1 and WB CQI, WB PMI should be implied even without the added condition.  If added, this could be perceived as E. Otherwise N | Samsung | Either N or E | Apple: We are open to discuss. But we have concern since wideband frequency-granularity will impact the low latency AP-CSI reporting, i.e., Table 5.4-1 in 38.214, at least. |
|  | | | | |
| UL.1 | When higher layer parameter *ul-FullPowerTransmission* is set to 'fullpowerMode2',  - the UE can be configured with one SRS resource or multiple SRS resources with same or different number of SRS ports within an SRS resource set with *usage* set to 'codebook', and only one SRS resource in the SRS resource set may be transmitted at a given time instant.  FL: Rel-15 also supports configured 2 SRS resources for usage “codebook”, where SRS is not precoded hence gNB should configure 2 SRS resources in time non-overlapping symbols or slots | Apple | N | Apple: This issue also exists in Rel-15 as FL mentioned. But there is a UE capability on number of SRS resources for CB in Rel-15 and usually UE would report 1 for this UE capability. But for uplink full power mode 2, normally more than 1 SRS resources should be supported, then this issue become critical. |
|  |  |  |  |  |

1. Discussion and proposal

From the inputs shared by participating companies during the preparation phase, the following **observation** can be made:

* The following issues can be handled as E (a part of editorial CR):
* The following issues can be designated as H (requiring discussion and additional agreements/conclusions):

# References

|  |  |  |  |
| --- | --- | --- | --- |
| 1 | R1-2110966 | Draft CR on gNB response for SCell-BFR | ZTE |
| 2 | R1-2110967 | Draft CR on SCS determination of 28 symbols for Rel-16 SCell BFR | ZTE |
| 3 | R1-2111219 | Draft CR on MU-CSI enhancement | CATT |
| 4 | R1-2111672 | Clarification on DCI 1\_2 antenna port determination in TS 38.212 | Ericsson |
| 5 | R1-2111851 | CR on SCell Candidate Beam Detection | Apple |
| 6 | R1-2111852 | CR on SRS Transmission for Uplink Full Power | Apple |
| 7 | R1-2112195 | Discussion on UCI issues for eType II CSI | Qualcomm Incorporated |
| 8 | R1-2112355 | Corrections on eType II codebook tables | Nokia |
| 9 | R1-2112399 | Correction on the description of MAC-CE application time in TS 38.214 | Huawei, HiSilicon |
| 10 | R1-2112412 | Correction of UCI mapping for eType II codebook | Huawei, HiSilicon |
| 11 | R1-2111713 | Correction on frequency granularity of CSI based on Rel.16 Type II codebooks | Samsung |
|  |  |  |  |
|  |  |  |  |