Companies are to share their inputs on the excel spreadsheet in /tsg\_ran/WG1\_RL1/TSGR1\_107-e/Inbox/drafts/8.1.2.4/RRC/.

## Inputs on version 00

Please share your inputs, if any, in the following table

Table 1 Inputs: Initial version

|  |  |
| --- | --- |
| **Company** | **Input** |
| Moderator | 1. I have updated RRC parameter for configuration of TRP-based pre-compensation scheme by removing FR1 only restrcition.  2. I have marked row 5 for RRC parameter ‘twoQclTypeDPdcchSfn’ in red. It has ‘unstable’ status from last RAN1 meeting. Would be great to decide on necessity of this parameter during this meeting. |
| Ericsson | On the row 5, we haven’t yet discussed this during this meeting. The question is weather we need an additional RRC parameter for this QCL assumption. Is there a need for gNB to configure the behaviour or is UE going to support the combination of different configurations? Would it be equavilent to sfnSchemeA or sfnSchemeB is configured for PDCCH? |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

## Inputs on version xx

Please share your inputs, if any, in the following table

....