3GPP TSG RAN WG1 #109-e R1-22xxxxx

e-Meeting, May 9th – 20th, 2022

**Agenda item: 5.1**

**Source: Moderator (Qualcomm)**

**Title: [109-e-AI5-LSs-02] Email discussion for incoming LS on UE capabilities for MBS (R1-2203218)**

**Document for: Discussion**

# Introduction

SA2 has sent an LS to RAN1 on UE capabilities of MBS in [1]. SA2 has requested RAN1 input on the following questions for SA2’s Rel-18 work on MBS enhancements study (FS\_5MBS\_Ph2).

|  |
| --- |
| ***Question 1****: Whether, similarly to eMBMS case for eMTC/NB-IoT, would it be useful for NG-RAN to receive from 5GC information on NR UE capabilities (e.g. RedCap) of the target recipients of MBS data in MBS broadcast mode.* ***Question 2****: If the answer to Question 1 is yes, we would like to ask RAN1 which are the possible targeted NR UE capabilities that should be provided to NG-RAN by the 5GC. SA2 can further study mechanisms in the context of the MBS enhancements study (FS\_5MBS\_Ph2).* |

This contribution is a summary of the following email discussion:

[109-e-AI5-LSs-02] Email discussion for incoming LS on UE capabilities for MBS (R1-2203218) by May 13 – Le (Qualcomm)

optional

# Email discussion

## MBS broadcast for RedCap UEs

**ZTE [3]:**

**Issue#1: Whether Redcap UE is allowed to receive broadcast (and multicast)**

Overall, this issue can be left to the Redcap UE feature discussion. The basic principle should be that if there is any spec impacts or negative impacts for Redcap UEs to receive broadcast (and multicast), then it should NOT be supported, since the RedCap WI is completed currently and no more optimization with spec impacts is persued in the CR stage. More specifically, since Redcap UEs have limited bandwidth, if the Recap UEs and non-Redcap UEs share the same MBS CFR, then network can only configures a small CFR for all UEs, which will definitely impact the efficiency of non-Redcap UEs. Similar as bandwidth limitation, modulation and Rx branches are also reduced, which brings similar impacts on non-RedCap UE. Furthermore, since the CFR should contains CORESET#0, then for RedCap, we need to determine whether separate initial DL BWP for RedCap should be used for MBS, when this separate initial DL BWP contain CORESET#0 or not. Even MBS is only supported in initial DL BWP for non-RedCap, it is still needed to determine how/when to receive the MBS service if separate initial BWP is configured for RedCap UE in idle/inactive mode.

***Observation 1****: RAN1 sees lots of open issues on allowing Redcap UE to support MBS, e.g., reduced bandwidth, modulation order and Rx branches, separate initial DL BWP with/without CORESET#0 and impacts to non-Redcap UEs.*

***Proposal 1****: Before answering questions in* *R1-2203218, RAN1 decides whether to allow Redcap UE to support Rel-17 broadcast (and multicast) in Redcap UE feature discussion.*

***Proposal 2****: Reply to LS R1-2203218/ S2-2203020 that Redcap UE is NOT allowed to support MBS.*

vivo [4]:

Answer: During the RAN1 discussion of Rel-17 NR MBS WI, the issue raised by SA2 LS was not discussed. Per RAN1’s understanding, the Rel-18 WI on enhanced NR MBS (RP-213568) does not has related work scope and RAN1 TU.

CMCC [5]:

However, it should be noted that, whether RedCap UE can support broadcast service reception, i.e., FG 33-1 has not been discussed in RAN1. If RedCap UE cannot support MBS broadcast service, it would be not necessary for NG-RAN to receive from 5GC information on NR UE capabilities (e.g. RedCap) of the target recipients of MBS data in MBS broadcast mode.

Huawei [6]:

From RAN1 perspective, Rel-17 NR MBS UE features can be supported by eMBB UEs or RedCap UEs if there is use case for RedCap UEs to support MBS, e.g., receiving MBS broadcast for firmware update.

Qualcomm [7]:

In NR Rel-17 MBS, there has not been specific consideration on the support of MBS broadcast transmission for different types of UEs, such as RedCap UEs with reduced bandwidth capability.

### 1st round

**FL comments:**

Per FL’s understanding, SA2’s questions are for the MBS broadcast reception of RedCap UEs. Here we don’t need to discuss the MBS multicast reception for RedCap UEs in SA LS reply.

As [Huawei] mentioned, from RAN1 perspective, RedCap UEs are capable of receiving Rel-17 MBS broadcast services if supporting FG33-1 [2]. However, [ZTE, CMCC, vivo, QC] have showed concern that that in NR Rel-17 MBS discussion, there has not been specific consideration on the support of MBS broadcast transmission for different types of UEs, such as RedCap UEs with reduced bandwidth capability. The broadcast CFR with BW size larger than CORESET0 (i.e., Case C and Case E) cannot be supported by RedCap UEs. If RedCap UEs can support MBS broadcast reception in Rel-17 MBS, only CFR with BW size same as CORESET0 (i.e., Case A) can be configured and it limits the transmission of MBS broadcast services targeting to non-RedCap UEs. [vivo] mentioned that the Rel-18 WI on enhanced NR MBS (RP-213568) does not has related work scope and RAN1 TU.

Therefore, companies are encouraged to share comments on the following RAN1 issues:

**Proposal 1:**

**RAN1 to discuss the following:**

* **Confirm that RedCap UEs supporting FG33-1 are capable to receive MBS broadcast services in Rel-17**
* **Discuss whether further enhancement on broadcast CFR for MBS broadcast services targeting RedCap UEs and non-RedCap UEs can be considered in Rel-18 MBS WID**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| MediaTek | **For the 1st sub-bullet:** Not support.From our understanding, the Rel-17 MBS broadcast is designed for eMBB-like UE instead of RedCap UE. For example, for MBS broadcast UE, the modulation order can be up to 64QAM/256QAM, supporting MBS broadcast service reception on SCell or non-serving cell, supporting FDMed b/w unicast PDSCH and group common PDSCH for broadcast PDSCH if agreed, and support the larger common frequency resources (i.g., case C and Case E) for broadcast reception and so on. Besides, considering the FG 33-1 is conditional mandatory FG for MBS broadcast, it means UE needs to support all the components in FG 33-1 if the UE can receive the broadcast services, especially for the RRC IDLE/INACTIVE UEs. Therefore, it is mandatory to support CFR of case C and case E for UE receiving the broadcast services, which against the RedCap UE’s restriction that the maximum bandwidth of an FR1 RedCap UE is 20MHz. To sum up, the two FGs between RedCap and MBS are separately discussed and the MBS broadcast design in whole Rel-17 discussion does not consider for the RedCap UE (e.g., supporting CFR of case C/E, FDMed case, SCell and non-serving cell reception), we suggest making the following conclusion:**Conclusion:** RedCap UE cannot receive the Rel-17 MBS broadcast services.**For the 2nd sub-bullet:** From our understanding, the use case is not clear to use the RedCap UE to receive the MBS broadcast services, especially considering the UE bandwidth reduction to 5MHz in FR1 for Rel-18 RedCap UE. Besides, it needs to discuss the broadcast reception from different operator and UE needs to use shared processing for MBS broadcast and unicast reception as states in the objective of Rel-18 MBS WID, however, RedCap UE only has one CC restriction, it will have larger WID modification and need more discussion for the scope if RedCap UE can receive the Rel-18 MBS services, which is not preferred. Therefore, we suggest following the current RAN plenary’s decision (e.g., the objective of Rel-18 MBS/RedCap WID, TU allocation) and no need to do any change with the following conclusion:**Conclusion:** RedCap UE cannot receive the Rel-18 MBS broadcast services. |
| ZTE | As we analysed in our contribution, at least two aspects need to be considered for MBS reception of Redcap UEs:1. Negative impacts on non-Redcap UEs. Since broadcast is for all UEs under this cell, if we allow Redcap UEs to support MBS, it means the CFR has to be smaller than 20MHz. This will have negative impacts on the MBS deployments.
2. Relationship between CFR for MBS and separate initial BWP for Redcap UEs. The CFR has to contain CORESET#0 based on the MBS previous agreements. However, the separate initial BWP for Redcap UEs is not required to contain CORESET#0/CD-SSB. This issue needs to be addressed.

Considering Rel-17 discussion for MBS and Redcap has been finalized, we suggest to conclude that Redcap UE is not allowed to receive MBS.If companies feel that Rel-18 may have some room for Redcap UE supporting MBS, then it can be discussed in RAN instead of RAN1. Besides, we think it is more appropriate to discuss this issue in the Redcap UE feature session. Because companies have discussed similar issues for other functionalities for Redcap UE there. |
| vivo | **For the first sub-bullet: ok**The two FGs between RedCap and MBS are separate. If RedCap UEs have the capability of supporting FG33-1, it is nature that these UEs are capable to receive MBS broadcast services in Rel-17. There is no limitation from specification perspective.**For the second sub-bullet: not support**RAN1 is not the right group to discuss the scope of the WID scope and it is clear that RAN1 is not involved based on the current Rel-18 MBS WID.  |
| Lenovo | 1. For 1st bullet: Not support.

We don’t think it is a right timing to discuss the support of RedCap UE for MBS reception. As we defined in Rel-17 MBS, the design target is for eMBB UE. With consideration of RedCap UE for receiving MBS, the CFR has to be configured with a narrow bandwidth, which has negative on eMBB UE’s MBS experience. Especially, when Case C or even Case E is configured for idle/inactive UE, RedCap UE can’t be supported.1. For 2nd bullet, it is OK to us if MBS services for RedCap UE and eMBB UEs are separately configured which is supposed no RAN1 impact.
 |
| Apple | For the first sublet, in principle if the RedCap UE has the capability of FG33-1, then RedCap UE could receive the broadcast service. But it will put restrictions on CFR configuration. According to current specification, RedCap UE receiving broadcast service is allowed. For the second bullet, it seems not the enhancement of CFR configuration. If supporting Rel-18 RedCap UE, the CFR is further limited to 5MHz.  |
| Spreadtrum | For the first bullet, in principle it is OK for Redcap UE to receive broadcast service when Redcap UE supporting FG33-1. Indeed, it would restrict CFR configuration and initial DL BWP configuration for Redcap UEs. But following current specification, such configuration, e.g., CORESET#0 as the CFR and no separated initial DL BWP is configured for Redcap UE, is allowed, and it is up to gNB’s implementation.For the second bullet, it can be discussed in RAN, not RAN1. |
| Nokia, NSB | **1st bullet:** In principle, yes. A RedCap UE could indicate support for FG33-1. Whether this makes any practical sense is another question altogether as the network would very unlikely plan for RedCap MBS if that means different BW or different coverage. The debate on forbidding a RedCap UE to indicate FG33-1 should be deferred to RedCap UE features discussion as this question is not a key issue wrt. the LS answer.**2nd bullet:** WID contents discussion is for RAN and not for RAN1 to do. |
| Ericsson | * **Confirm that RedCap UEs supporting FG33-1 are capable to receive MBS broadcast services in Rel-17**

OK with the first bullet. As previously commented by other companies above, the feature groups are separate and if a redcap UE signals MBS support, there is no reason to exclude it. We don’t think it could be a problem for redcap UEs to be integrated in a MBS solution, as in all likelihood they will not share the same MBS service (same G-RNTI) as eMBB UEs. * **Discuss whether further enhancement on broadcast CFR for MBS broadcast services targeting RedCap UEs and non-RedCap UEs can be considered in Rel-18 MBS WID**

This should be discussed in RAN. RAN1 has no TUs for MBS in rel-18. |
| Moderator | Summary:* Whether RedCap UEs supporting FG33-1 are capable to receive MBS broadcast services in Rel-17
	+ Positive: vivo, Apple, Spreadtrum, Nokia/NSB, Ericsson,
	+ Negative: MTK, ZTE, Lenovo
* Discuss whether further enhancement on broadcast CFR for MBS broadcast services targeting RedCap UEs and non-RedCap UEs can be considered in Rel-18 MBS WID
	+ To be discussed in RAN: ZTE, Lenovo, Spreadtrum, Nokia/NSB, Ericsson, vivo
	+ No support in Rel18: MTK

Please continue discussion of Proposal 1a revised based on the comment:**Proposal 1a:** * **Confirm that RedCap UEs supporting FG33-1 are capable to receive MBS broadcast services in Rel-17**
* **Ask RAN to iscuss whether further enhancement on broadcast CFR for MBS broadcast services targeting RedCap UEs and non-RedCap UEs can be considered in Rel-18 MBS WID**
 |
| vivo | Ok with the above proposal 1a. |
| CMCC | We support proposal 1a.We think Redcap UE can indicate support FG 33-1, for some uses cases, e.g., software delivery over wireless in factory. |
| MediaTek | **For the 1st sub-bullet: Confirm that RedCap UEs supporting FG33-1 are capable to receive MBS broadcast services in Rel-17****Not support.**As commented in 1st round, we think Rel-17 MBS broadcast design discussion is targeted for the eMBB-like UE instead of RedCap UE e.g., supporting CFR of case C/E, FDMed case, SCell and non-serving cell reception for MBS broadcast. Especially for the Case C and case E, it is conditional mandatory UE feature for UE supporting FG 33-1, which against the RedCap UE’s restriction that that the maximum bandwidth of an FR1 RedCap UE is 20MHz. So, we still suggest making the following conclusion for this issue.**Conclusion:** RedCap UE cannot receive the Rel-17 MBS broadcast services.Considering the SA2’s LS focus on the Rel-18 work on MBS enhancements study (*FS\_5MBS\_Ph2),* we can deprioritize the discussion related Rel-17 MBS if we cannot achieve the above conclusion.**For the 2nd sub-bullet: Ask RAN to iscuss whether further enhancement on broadcast CFR for MBS broadcast services targeting RedCap UEs and non-RedCap UEs can be considered in Rel-18 MBS WID****Not support.**The use case is not clear for RedCap UE to receive the MBS broadcast on non-serving cell, especially considering only one CC is used for RedCap UE. |
| Huawei, HiSilicon | Our comment in v003 is not included.For the updated proposal: Fine with the 1st bullet, to MediaTek, FG33-1 for broadcast does not preclude redcap UE support it in our opinion technically. 2nd bullet I wonder whether need to bother RAN plenary to discuss it because this SA2 LS seems all the work can be done in CN which does not necessary mean optimization needs to be done in RAN.  |
| ZTE | **For the first bullet:** Still, we don’t support this. It seems our previous concerns have not been addressed by companies. We hope companies can share your understandings on these two aspects. Also, we propose to discuss in Redcap UE feature session because they have been doing similar exercise for other functionalities for Redcap UE.1. Negative impacts on non-Redcap UEs. Since broadcast is for all UEs under this cell, if we allow Redcap UEs to support MBS, it means the CFR has to be smaller than 20MHz. This will have negative impacts on the MBS deployments.
2. Relationship between CFR for MBS and separate initial BWP for Redcap UEs. The CFR has to contain CORESET#0 based on the MBS previous agreements. However, the separate initial BWP for Redcap UEs is not required to contain CORESET#0/CD-SSB. This issue needs to be addressed.

**For the second bullet:** We don’t think it is necessary to have this conclusion in RAN1. It is always contribution driven and companies are free to submit tdocs in RAN. |
| Apple | Ok with proposal 1a. |
| Nokia, NSB | **Proposal 1a 1st bullet:** In principle OK. As per the current spec, a RedCap UE could indicate support for FG33-1. The debate on forbidding a RedCap UE to indicate FG33-1 should be deferred to RedCap UE features discussion, though as similar restrictions for RedCap UEs’ support for other features are also debated there.**Proposal 1a 2nd bullet:** We don’t see the need for asking RAN to do this as RAN1 just because we received an LS from SA2. If companies want to extend the WID scope, they are free to submit their proposal directly to RAN. |
| Moderator2 | Summary:* Confirm RedCap UEs supporting FG33-1 are capable to receive MBS broadcast services in Rel-17
	+ Yes: vivo, Apple, Spreadtrum, Nokia/NSB, Ericsson, CMCC, Huawei/HiSi
	+ No: MTK, ZTE, Lenovo
* Ask RAN to discuss whether further enhancement on broadcast CFR for MBS broadcast services targeting RedCap UEs and non-RedCap UEs can be considered in Rel-18 MBS WID
	+ Yes: CMCC, vivo, Apple
	+ No: MTK, ZTE, Nokia/NSB, Huawei/HiSi

**@MTK:**For broadcast CFR, Case A/C/E is to provide flexible scheduling for gNB. But it does not mean all UEs are required to support all the Cases. I think the reason for SA2 to send LS to RAN1 is that there are broadcast services targeting to RedCap UEs, and RAN should make sure the broadcast services are transmitted within the max bandwidth of RedCap UEs.Regarding “*The use case is not clear for RedCap UE to receive the MBS broadcast on non-serving cell, especially considering only one CC is used for RedCap UE*”, we are not discussing non-serving cell case, so the concern is not relevant. But correct me if I miss something.**@ZTE:** There is negative impact on non-Redcap UEs because of only one CFR for all broadcast services in Rel17. But it is not reasonable to disallow some broadcast services targeting RedCap UEs to be transmitted because of this concern. Optimization of CFR for different broadcast services (for RedCap UEs and non-RedCap UEs) can be further discussed (e.g., in future Release).Regarding “separate initial BWP for Redcap UEs”, my understanding is that it does no impact broadcast CFR. The broadcast CFR will be CORESET0 (Case A) for RedCap UEs supporting broadcast reception.For “discuss in Redcap UE feature session because they have been doing similar exercise for other functionalities for Redcap UE”, it does not matter where to discuss this issue and no need to wait for other session progress. Since the discussion on SA2 LS is related with this issue, companies can share the views here directly. |

### 2nd round

In order to reply SA2 LS, FL suggests focusing on **Proposal 1b**. Companies are encouraged to share the considerations on the broadcast services targeting RedCap UEs, if Option 2 is preferred.

**Proposal 1b: RAN1 to down-select in RAN1#109-e**

* **Option 1: RedCap UEs supporting FG33-1 are capable to receive MBS broadcast services in Rel-17**
* **Option 2: RedCap UEs cannot support FG33-1 in Rel-17**

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Spreadtrum | Option 1. The current specification can support this if Redap UE has capability of FG33-1, although it may set scheduling restriction. |
| ZTE | Our preference is Option2.We are not sure whether there is broadcast service only targeting RedCap UEs because Non-Redcap UEs can receive these service as well. As we commented previously,1. If companies really see the need of allowing RedCap UEs to support broadcast in Rel-17, then we suggest to discuss this issue in RedCap UE feature session so that companies can apply the same criteria (as they have been used for other similar issues for RedCap UEs) to determine whether RedCap UE should support broadcast. Based on our understanding, the criteria they used is that, if there is spec impacts or negative impacts on the Non-RedCap UE, then this should be dropped.
2. If companies want to allow RedCap UEs to support broadcast in Rel-18, companies can provide contributions to RAN or SA.

Regarding how to reply the LS, we can reply that RAN1 has non consensus on whether Rel-17 RedCap UE can support broadcast reception since this is not discussed in RAN1 previously.  |
| MediaTek | Option 2.Thanks for Moderator and Huawei’s explanation to MTK. Regarding the CFR configuration, we have the different understanding. Since CFR of Case A, Case C and Case E are supported for the RRC IDLE/IANCTVIE UEs receiving the MBS broadcast services, the sentence of “support of CFR configuration for broadcast” has been captured in the FG33-1, so, if RedCap UE supporting the FG33-1, it needs to support the capability to process the broadcast services within the CFR of case E. Unfortunately, it is against with the RedCap UE’s restriction that the maximum bandwidth of an FR1 RedCap UE is 20MHz. In addition, please note that SA2’s LS focus on the Rel-18 work on MBS enhancements study (*FS\_5MBS\_Ph2)* as copied following, we can deprioritize the discussion related Rel-17 MBS if we cannot make option 2 (RedCap UEs cannot support FG33-1 in Rel-17) as a conclusion.

|  |
| --- |
| SA2 is working in rel.18 in the MBS enhancements study (FS\_5MBS\_Ph2) to define support for Group Communication (Key Issue #4) and Coexistence with existing power saving mechanisms for capability-limited devices (Key Issue #5) in TR 23.700-47. |

Regarding the moderator’s other comments to us “Regarding “*The use case is not clear for RedCap UE to receive the MBS broadcast on non-serving cell, especially considering only one CC is used for RedCap UE*”, we are not discussing non-serving cell case, so the concern is not relevant. But correct me if I miss something.”, this comment is to reply the 2nd sub-bullet in your previous proposal related with the Rel-18. In the objective of Rel-18 MBS, it needs UE to receive the MBS services on non-serving cell (e.g., other operator) via shared processing with the unicast, e.g., one CC is used for the MBS reception from non-serving cell as discussed in previous RAN plenary. However, the RedCap UE only has one CC, so, at least in current stage, we cannot support RedCap UE (e.g., via some optimization) can receive the Rel-18 MBS since the use case is not clear. Anyway, we agree with other companies’ vives whether to modify the WID is RAN’s scope, which cannot be decided by RAN1, and also there is no need to send an LS to RAN. If some companies are interested with the issue, it can directly submit the contribution to the RAN meeting and trigger the discussion.Mod: thanks for the explanation. The 2nd sub-bullet is not for non-serving cell, which is actually for the serving cell case with possible different CFR for broadcast services targeting to RedCap and non-RedCap UEs.  |
| Huawei, HiSilicon | Option1 RedCap UEs supporting FG33-1 are capable to receive MBS broadcast services in Rel-17 but it is conditioned on NW is aware of it. If NW configures a CFR larger than 20MHz, then even RedCap UEs supporting FG33-1, UE cannot receive MBS broadcast services |
| vivo | Option 1. The max bandwidth for Redcap UE is 20MHz does not mean the UE can’t support case E. For example, the initial BWP is 10MHz and CFR is 20MHz. If CFR is larger than 20MHz, Redcap UE cannot receive MBS broadcast services in this case, but it does not mean Redcap UE can’t receive broadcast in any case. |
| Nokia, NSB | Same view as Huawei/HiSili. We are not so sure RedCap UE with MBS makes sense with CFR > 20 MHz, but there are bands where this is not an issue. The LS response discussion is not really the place to say that this UE capability combination is not allowed, or under which conditions the capability is allowed. Such limitations would need to be discussed within the WI or UE feature agenda items.One possibility is to conclude and respond to SA2 that: **RAN1 has not restricted RedCap UEs from supporting MBS, but at the current stage of Rel-17 dicussions, some companies are voicing an opinion that RedCap UEs should not indicate support for MBS.** |
| Mod | Summary: * **Option 1: RedCap UEs supporting FG33-1 are capable to receive MBS broadcast services in Rel-17**
	+ Spreadtrum, Huawei/Hisi, vivo, Nokia/NSB
* **Option 2: RedCap UEs cannot support FG33-1 in Rel-17**
	+ ZTE, MTK

Based on the observation, I would like to take the suggestion from Nokia with minor modification to try to conclude this issue **Proposal 1c: RAN1 to reply LS from SA2 and CC RAN as:*** **Rel-17 specifications have not restricted RedCap UEs from supporting MBS broadcast, but at the current stage of Rel-17 discussions, some companies think that RedCap UEs should not indicate support for MBS broadcast.**
 |

### 2nd round

**Proposal 1c: RAN1 to reply LS from SA2 and CC RAN as:**

* **Rel-17 specifications have not restricted RedCap UEs from supporting MBS broadcast, but at the current stage of Rel-17 discussions, some companies think that RedCap UEs should not indicate support for MBS broadcast.**

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |

## Question 1 in SA2 LS

|  |
| --- |
| ***Question 1****: Whether, similarly to eMBMS case for eMTC/NB-IoT, would it be useful for NG-RAN to receive from 5GC information on NR UE capabilities (e.g. RedCap) of the target recipients of MBS data in MBS broadcast mode.*  |

ZTE [3]:

**Issue#2: If Recap UE is allowed to receive broadcast, would it be useful for NG-RAN to receive from 5GC information on NR UE capabilities on RedCap of the target recipients of MBS data in MBS broadcast mode?**

If Recap UE is allowed to receive broadcast, then it will be useful/necessary for NG-RAN to receive from 5GC information on NR UE capabilities on RedCap of the target recipients of MBS data in MBS broadcast mode. However, this is also a spec impact for allowing Redcap UEs to support broadcast.

CMCC [5]:

**Proposal 1. Reply the LS to SA2 on Question 1:** **It would be useful for NG-RAN to receive from 5GC information on NR UE capabilities (e.g. RedCap) of the target recipients of MBS data in MBS broadcast mode. However, RAN1 has not discussed whether** **RedCap UE can support broadcast service, e.g., receiving DCI format 4\_0.**

Huawei [6]:

Answer to Q1: If gNB is not aware of whether the MBS services transmission provided by gNB is targeting eMBB or RedCap UE only or both, gNB can configure resources with a smaller bandwidth for reception by all UE types. Nevertheless, it might be useful for NG-RAN to receive from 5GC information on NR UE capabilities, based on which gNB might be able to configure the resources for broadcast transmission more efficiently.

Qualcomm [7]:

Yes, we think it is useful at least for gNB to configure the bandwidth location/size of the common frequency resource for MCCH/MTCH.

### 1st round

**FL comments:**

[ZTE, CMCC, Huawei, QC] share the view that if RedCap UEs are capable of receiving MBS broadcast servicesand gNB is aware of whether the MBS broadcast service is targeting to RedCap UEs, it is useful for NG-RAN to receive from 5GC information on NR UE capabilities (e.g. RedCap) of the target recipients of MBS data in MBS broadcast mode.

**Proposal 2:**

**RAN1 to answer Q1 as follows:**

* **It is useful for NG-RAN to receive from 5GC information on NR UE capabilities (e.g. RedCap) of the target recipients of MBS data in MBS broadcast mode.**

Companies are encouraged to provide comments below:

|  |  |
| --- | --- |
| **Company** | **Comments** |
| MediaTek | Not sppport.As discussed in the Proposal 1, we suggest that RedCap UE cannot receive the MBS broadcast service, so, it naturally does not need to notify the RAN side about the RedCap UE capability for receiving the MBS broadcast services. Besides, the same MBS broadcast service targeted users are not only for RRC CONNECTED state, but also for RRC IDLE/INACTUVE state, however, if UE in RRC IDLE/INACTIVE state, the RAN also does not know which UE to receive the broadcast service, so, it is not useful for the RAN side to know the RedCap UE capability for MBS broadcast reception. |
| ZTE | From our perspective, it would be good to address the issues in proposal1 first and then come back to this question. |
| vivo | Not support.Even if it might be a useful information, it has not been discussed during the discussion of Rel-17 MBS WI and it is quite clear that such information exchange is not in scope of Rel-18 MBS WID.  |
| Lenovo | Agree with MediaTek |
| Apple | Agree with ZTE, this is depending on whether allow RedCap UE to receive the broadcast service. If yes, the information is useful. Otherwise, the information is not needed. |
| Spreadtrum | Agree with ZTE. |
| Nokia, NSB | We do not support this, and do not see the usefulness. When specifically thinking of RedCap, we agree with MediaTek, but the LS cited RedCap as an example UE type, not the UE type.  |
| Ericsson | Agree with ZTE analysis. Moreover, we don’t think RAN1 should decide what is useful for NG-RAN.  |
| Moderator | Summary:* **It is useful for NG-RAN to receive from 5GC information on NR UE capabilities (e.g. RedCap) of the target recipients of MBS data in MBS broadcast mode**
	+ Yes (if RedCap can receive broadcast): ZTE, Apple, Spreadtrum
	+ No: MTK, Lenovo, Nokia/NSB,
	+ FFS: vivo, Ericsson

Please continue discussion of Proposal 2a revised based on the comment:**Proposal 2a:** **RAN1 to answer Q1 as follows:*** **If RedCap UEs are capable of receiving MBS broadcast services, it is useful for NG-RAN to receive from 5GC information on NR UE capabilities (e.g. RedCap) of the target recipients of MBS data in MBS broadcast mode.**
 |
| vivo | Not support above proposal 2a. Agree with other company, we don’t think RAN1 should decide what is useful for NG-RAN. We prefer to discuss this issue in RAN together with that in proposal 1a. |
| CMCC | Support proposal 2a, since this information can assist the broadcast CFR configuration for NG-RAN. |
| MediaTek | **Not support.** We basically hold the similar view as commented in the 1st round, especially considering the UE in RRC IDLE/INACTIVE state, the RAN also does not know which UE to receive the broadcast service, so, it is not useful for the RAN side to know the RedCap UE capability for MBS broadcast reception.  |
| Huawei, HiSilicon | **Our comment in v003 is not included.****Fine with the updated one.**  |
| ZTE | Based on our observation, it seems most companies are fine to focus on proposal 1 first and then come back to this proposal 2a later.We still hold the same view that we should first address the issue in proposal 1. |
| Apple | OK with Proposal 2a. |
| Nokia, NSB | Not OK with the proposal 2a, tend to agree with MediaTek |
| Moderator2 | Summary:* **If RedCap UEs are capable of receiving MBS broadcast services, it is useful for NG-RAN to receive from 5GC information on NR UE capabilities (e.g. RedCap) of the target recipients of MBS data in MBS broadcast mode**
	+ Yes: Apple, CMCC, Huawei/HiSi
	+ No: MTK, Nokia/NSB
	+ FFS: ZTE (deferred after proposal 1), vivo (RAN to discuss)

@MTK:Network can know what broadcast services are targeting to RedCap UEs. gNB who can support RedCap UEs and broadcast transmission will make sure the broadcast services are transmitted within the max bandwidth of RedCap UEs, but gNB does not need to know which RedCap UE is receiving. @vivo:Could you please explain more why “we don’t think RAN1 should decide what is useful for NG-RAN”. SA2 LS is sending to RAN1 and at least we can give the answer from RAN1 perspective.Considering there is no clear consensus, we can focus on Proposal 2b in Sect. 2.1.2 before replying Q1.  |
| vivo | @ ModeratorWe think this issue is also relevant with RAN2, at least RAN2 should be involved to make decision. |

## Question 2 in SA2 LS

|  |
| --- |
| ***Question 2****: If the answer to Question 1 is yes, we would like to ask RAN1 which are the possible targeted NR UE capabilities that should be provided to NG-RAN by the 5GC. SA2 can further study mechanisms in the context of the MBS enhancements study (FS\_5MBS\_Ph2).* |

CMCC [5]:

Proposal 2. Reply the LS to SA2 on Question 2: Whether a UE is a RedCap UE or not should be provided to NG-RAN by the 5GC.

Huawei [6]:

Answer to Q2: It is sufficient for 5GC to provide only an indication that a UE is known to be a RedCap UE.

Qualcomm [7]:

A basic capability of RedCap UEs has been defined as FG28-1, given in Appendix. If an indication of max BW of RedCap UE capability is received from the CN, which is expected to be specified by RAN2 as part of UE capabilities (need to be further confirmed by RAN2), gNB can know that a broadcast service is targeted to RedCap UEs and configure the common frequency resource for the broadcast service accordingly. For instance, the bandwidth of the broadcast service for RedCap UEs is limited to the maximum bandwidth of RedCap UEs (Max FR1 BW is 20MHz and max FR2 BW is 100MHz as in FG28-1). The information of coverage level capability is not specifically needed for RedCap UEs, since similar coverage is supported for NR RedCap UEs and non-RedCap UEs.

Note that, in our understanding, the “capability” referred to in the SA2 LS corresponds to an indication conveyed from the CN to the RAN indicating the target type of UE for a given service, and not an explicit indication from the UE to the CN. From RAN1 perspective, it is beneficial if the gNB has information for a given MBS broadcast service targeted to RedCap UEs, who has limited maximum TBS/bandwidth.

### 1st round

**FL comments:**

[CMCC, Huawei, QC] have similar view that whether a UE is a RedCap UE with the limited max BW capability as defined by FG28-1 [2] should be provided to NG-RAN by the 5GC. As [QC] mentioned, considering similar coverage is supported for NR RedCap UEs and non-RedCap UEs, the coverage level capability is not specifically needed for RedCap UEs (different from coverage level capability required for broadcast services targeting to LTE MTC/NB-IoT), which can be clarified in the reply.

**Proposal 3:**

**RAN1 to answer Q2 as follows:**

* **The only capability information to be provided to NG-RAN is the RedCap UE max BW capability as defined by FG28-1. The information of coverage level capability is not specifically needed for RedCap UEs.**

Companies are encouraged to provide comments below:

|  |  |
| --- | --- |
| **Company** | **Comments** |
| MediaTek | As discussed in the proposal 2, the answer for Q1 is no. So, it does not need to reply this question. |
| ZTE | From our perspective, it would be good to address the issues in proposal1 first and then come back to this question. |
| vivo | As discussed in the proposal 2, the answer for Q1 is out of scope, it does not need to reply this question. |
| Nokia, NSB | Agree with MediaTek and ZTE.  |
| Ericsson | Agree with other that the question is premature.  |
| Moderator | Summary:* + Compares prefer to defer the discussion for Q2 after 2.1.
 |

# Conclusion

# References

1. R1-2203128(S2-2203020), “UE capabilities for MBS”, SA2#150-e, April 6 – 12, 2022
2. R1-2202927, “LS on updated Rel-17 RAN1 UE features list for NR”, RAN1#108-e, Feb. 21 – Mar. 3, 2022.
3. R1-2203246 [Draft] Reply UE capabilities for MBS ZTE
4. R1-2203497 Draft Reply LS on MBS UE capabilities vivo
5. R1-2204273 Discussion on SA2 LS on UE capabilities for MBS CMCC
6. R1-2204928 Discussion on UE capabilities for receiving MBS broadcast Huawei, HiSilicon
7. R1-2204970 Discussion on SA2 LS on UE capabilities of NR MBS broadcast reception Qualcomm Incorporated

# Appendix: UE feature FG28-1 and FG33-1 [2]

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Features** | **Index** | **Feature group** | **Components** | **Prerequisite feature groups** | **Need for the gNB to know if the feature is supported** | **Applicable to the capability signalling exchange between UEs (Sidelink WI only)”.** | **Consequence if the feature is not supported by the UE** | **Type****(the ‘type’ definition from UE features should be based on the granularity of 1) Per UE or 2) Per Band or 3) Per BC or 4) Per FS or 5) Per FSPC)** | **Need of FDD/TDD differentiation** | **Need of FR1/FR2 differentiation** | **Capability interpretation for mixture of FDD/TDD and/or FR1/FR2** | **Note** | **Mandatory/Optional** |
|  28. NR\_redcap | 28-1 | RedCap UE | 1. Maximum FR1 RedCap UE bandwidth is 20 MHz.2. Maximum FR2 RedCap UE bandwidth is 100 MHz.3. Early indication of RedCap UE in Msg.1 for 4-step RACH4. Separate initial UL BWP for RedCap UEs- It includes the configuration(s) needed for RedCap UE to perform random access- Enabling/disabling of frequency hopping for common PUCCH resources5. Separate initial DL BWP for RedCap Ues- It includes CSS/CORESET for random access- FFS: For separate initial DL BWP used for paging, CD-SSB is included- For separate initial DL BWP only used for RACH, SSB may or may not be includedFFS whether to add any other basic features for RedCap UE |  | Yes |   | [Network assumes the UE is not a RedCap UE] | [Per UE] | [No] | [No] |   | [RedCap UEs do not support carrier aggregation or dual connectivity.]It is up to RAN2 whether/how to capture the capabilities for early indication of RedCap UE in Msg 3 and Msg A | Optional with capability signalingRedCap UE must indicate this FG is supported |
| 33. NR\_MBS | 33-1 | Broadcast | * + - 1. Support of group-common PDCCH/PDSCH with CRC scrambled by MCCH-RNTI.
			2. Support of group-common PDCCH/PDSCH with CRC scrambled by G-RNTI.
			3. Support of CFR configuration for broadcast.
			4. Support of CORESET and common search space for broadcast.
			5. Support of DCI format 1\_0 with CRC scrambled with G-RNTI/MCCH-RNTI for broadcast.
			6. Support of inter-slot TDM between unicast PDSCH and group-common PDSCH in different slots.
			7. Support MCCH change notification indication via DCI.
			8. support of higher layer configured slot-level repetition up to 8 for MTCH

DCI indicated slot-level repetition up to 16 for MTCH is defined as another FG, FFS whether to merge with FG 33-3-1 |  | Up to RAN2 |  |  | Up to RAN2 | Up to RAN2 | Up to RAN2 |  |  | Up to RAN2 |