**3GPP TSG RAN WG1 Meeting #109-e R1-22xxxxx**

**9th May *–* 20th May2022**

**Agenda Item:** 8.10

**Source:** Moderator **(**Qualcomm Incorporated)

**Title:** Summary #1 of [109-e-R17-eIAB-03]

**Document for:** Discussion and decision

# Introduction

This contribution provides a summary of the following email discussion:

[109-e-R17-eIAB-03] Issues #6, #7, #9, #10, #13, #14, #16 by May 20 – Luca (Qualcomm)

* This email discussion is to start on May 16

The referenced issues #6, #7, #9, #10, #13, #14, and #16 were identified in the preparation phase [109-e-Prep-AI8.10-eIAB] based on the contributions [1] – [13] and were prioritized as priority 3.

Discussion topics are purple background highlighted.

FL agreements or conclusions from email discussion and/or online sessions are green background highlighted.

Active discussion items for which companies’ input is sought are yellow background highlighted.

Inactive discussion topics are grey highlighted.

New text from the moderator in each round of discussion after the initial revision is highlighted in green.

# Summary

This discussion covers 7 issues identified based on the contributions [1] – [13] submitted for agenda item 8.10.

**Issue #6.** **Handling of multiple DCI format 2\_5 indications with overlapping durations**

* References: [3], [10], [11]
* No upper layer signaling impact – priority 3

**Issue #7.** **Brackets in definition of H/S/NA for RB set**

* References: [6], [7], [10], [13].
* No upper layer signaling impact – priority 3

**Issue #9. Extension of exception for cell-specific/semi-static signals to soft or not available RB sets**

* References: [7], [9], [13]
* No upper layer signaling impact – priority 3

**Issue #10.** **Update to determination of availability in DC scenario**

* References: [13]
* No upper layer signaling impact – priority 3

**Issue #13.** **DL Tx power adjustment MAC-CE**

* References: [13]
* No upper layer signaling impact – priority 3

**Issue #14. Descriptions of MT’s UL MAC-CEs**

* References: [13]
* No upper layer signaling impact – priority 3

**Issue #16. Alignment of parameters names**

* References: [13]
* No upper layer signaling impact – priority 3

# Discussion

## Issue #6. Handling of multiple DCI format 2\_5 indications with overlapping durations

This issue relates to a potential limitation in the current specification for the scenario in which there is a desire to release of Soft resources via DCI Format 2\_5 following different periodicities amongst different DU cells associated with the MT cell

Related input from contributions:

|  |  |
| --- | --- |
| ZTE  [3] | [Proposal 5: For multiple DCI Format 2\_5 indications with overlapping durations, Rel-16 mechanism is reused.](#_Toc4678) |
| Ericsson  ]10] | Proposal 11 One availabilityCombination of the availabilityCombinations table is reserved to signal to the IAB-DU that “No new Availability Indication is provided” in DCI format 2\_5 for slots which receive multiple Availability Indicators. |
| ETRI  [11] | Proposal 3. RAN1 to clarify that with proper configurations there are no potential issues from multiple DCI Format 2\_5 indications with overlapping durations. |

|  |
| --- |
| **Conclusion (RAN1-108e)**  *Defer discussion (contribution driven) of potential issues/solutions for multiple DCI Format 2\_5 indications with overlapping durations until RAN1#109-e.* |

**Summary of views:**

* [3] proposed to reuse Rel-16 mechanism
* [10] proposed to reserve an entry in the availabilityCombinations table to signal to the IAB-DU that “No new Availability Indication is provided” in DCI format 2\_5 for slots which receive multiple Availability Indicators.
* [11] proposed to clarify that there is no issue, with proper configuration.

Based on the input on this issue the FL recommends getting additional input from more companies.

**FL Proposal 3.1a**

**RAN1 to downselect in RAN1#109-e one of the following alternatives:**

* **Alt1: in Rel17 there is no additional specification for handling of multiple DCI Format 2\_5 indications with overlapping durations.**
* **Alt2: One availabilityCombination of the availabilityCombinations table is reserved to signal to the IAB-DU that “No new Availability Indication is provided” in DCI format 2\_5 for slots which receive multiple Availability Indicators.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Do you agree with FL Proposal 3.1a?**  **Views on Alt1 vs. Alt2?** | **Comments** |
|  |  |  |
|  |  |  |

## Issue #7. Brackets in definition of H/S/NA for RB set

This issue relates to…

Related input from contributions:

|  |  |
| --- | --- |
| Samsung  [6] | Proposal 2: In the definition for FDM Hard, remove “[provided it does not impact the IAB-MT’s ability to transmit and receive in any other RB set that is configured as Not Available or configured as Soft and not indicated available]”. |
| NTT DOCOMO  [7] | Proposal 2: Adopt the following TP for TS 38.213 section 14. |
| Ericsson  ]10] | Proposal 6 Remove the brackets in the definition of frequency domain H/S/NA from the agreement of the RAN1#108-e meeting and agree on the following text proposal. |
| Qualcomm  [13] | Proposal 3.2  Adopt to the following text proposal for soft RB sets in 38.213: |

RAN1#108-e achieved the following agreement, in which there are some clauses in the brackets that may need further discussions and clarifications.

|  |
| --- |
| **Agreement (RAN1#108-e)**  Adopt the following definition for H/S/NA configured in an RB set of a symbol:   * FDM Hard: When an RB set of a downlink, uplink, or flexible symbol is configured as hard, the IAB-DU cell can respectively transmit, receive, or either transmit or receive on the RB set in the symbol [provided it does not impact the IAB-MT’s ability to transmit and receive in any other RB set that is configured as *Not Available* or configured as *Soft* and not indicated available]. * FDM Soft: When an RB set of a downlink, uplink, or flexible symbol is configured as soft, the IAB-DU cell can respectively transmit, receive or either transmit or receive on the RB set in the symbol only if   + the IAB-MT does not transmit or receive on the RB set during the symbol of the IAB-DU cell, or   + with respect to all serving cells,     - the IAB-MT would transmit or receive on the RB set during the symbol of the IAB-DU cell, and the transmission or reception on the RB set [or any ~~adjacent~~ RB set that is configured as Not Available or configured as Soft and not indicated available] during the symbol of the IAB-DU cell is not changed due to a use of the RB set in the symbol by the IAB-DU, or   + if the IAB-MT is not configured with SCG     - if the IAB-MT detects a DCI format 2\_5 with an AI index field value indicating the soft RB set as available   + if the IAB-MT is configured with SCG     - the IAB-MT detects two DCI formats 2\_5 with an AI index field value indicating the soft RB set as available from MCG and SCG respectively, or     - the IAB-MT detects a DCI format 2\_5 with an AI index field value indicating the soft ~~symbol~~ RB set as available from one cell group (either MCG or SCG), and, with respect to all serving cells of the other cell group:       * the IAB-MT would transmit or receive on the RB set during the symbol of the IAB-DU cell, and the transmission or reception on the RB set during the symbol of the IAB-DU cell is not changed due to a use of the RB set in the symbol by the IAB-DU. * FDM NA: When an RB set of a downlink, uplink, or flexible symbol is configured as unavailable, the IAB-DU neither transmits nor receives at the RB set in the symbol. |

38.213(V17.1.0) currently has the following related clause.

|  |
| --- |
| When an RB set of a downlink, uplink, or flexible symbol is configured as hard, the IAB-DU cell can respectively transmit, receive, or either transmit or receive on the RB set in the symbol.  When an RB set of a downlink, uplink, or flexible symbol is configured as soft, the IAB-DU cell can respectively transmit, receive or either transmit or receive on the RB set in the symbol only if  - the IAB-MT does not transmit or receive on the RB set during the symbol of the IAB-DU cell, or  - with respect to all serving cells, the IAB-MT would transmit or receive on the RB set during the symbol of the IAB-DU cell, and the transmission or reception on the RB set or any RB set that is configured as unavailable or configured as soft and not indicated as available during the symbol of the IAB-DU cell is not changed due to a use of the RB set in the symbol by the IAB-DU, or  - the IAB-MT detects a DCI format 2\_5 with an AI index field value indicating the soft RB set as available if the IAB-MT is not configured with an SCG, or  - the IAB-MT detects two DCI formats 2\_5 with an AI index field value indicating the soft RB set as available from the MCG and SCG, respectively, or  - the IAB-MT detects a DCI format 2\_5 with an AI index field value indicating the soft RB set as available from one cell group and with respect to all serving cells of the other cell group, the IAB-MT would transmit or receive on the RB set during the symbol of the IAB-DU cell, and the transmission or reception on the RB set during the symbol of the IAB-DU cell does not change due to a use of the RB set in the symbol by the IAB-DU.  When an RB set of a downlink, uplink, or flexible symbol is configured as unavailable, the IAB-DU neither transmits nor receives in the RB set in the symbol. |

**Summary of views:**

* Regarding FDM Hard:
  + Remove *“[provided it does not impact the IAB-MT’s ability to transmit and receive in any other RB set that is configured as Not Available or configured as Soft and not indicated available]”*
    - Supported by [6], [7], [13]
  + Include *“provided it does not impact the IAB-MT’s ability to transmit and receive in any other RB set that is configured as Not Available or configured as Soft and not indicated available”*
    - Supported by [10]
* Regarding FDM Soft:
  + Include *“or any RB set that is configured as Not Available or configured as Soft and not indicated available”*
    - Supported by [6], [7], [10], [13]
* [7], [10], and [13] provided related TPs.

There is consensus amongst the companies that provided input on this issue about removing the square brackets around “or any RB set that is configured as Not Available or configured as Soft and not indicated available” for the FDM Soft definition in the aforementioned RAN1#108-e agreement.

There is a majority amongst the companies that provided input on this issue about removing the text “provided it does not impact the IAB-MT’s ability to transmit and receive in any other RB set that is configured as Not Available or configured as Soft and not indicated available” within square brackets around for the FDM Hard definition in the aforementioned RAN1#108-e agreement. The FL assessment of this aspect is aligned with the majority view because:

a) it keeps the definition of a Hard resource consistent with the Rel16 definition whereby a Hard resource can be used unconditionally by the IAB-DU, and

b) there will ne no guarantee that the cell-specific/semi-static signals for which a protection is desired to be in place as for Rel16 (see issue #9) without further changes to the specification (being equivalent to a Hard resource provides no guarantee of ability to use).

Moreover the FL notes that the potentially impacted specification text is also potentially subject to additional unrelated modifications based on the discussion of other issues, hence it is proposed to agree on an amendment of the related RAN1#108-e agreement and then a TP can be defined later once all issues are (hopefully) closed.

**FL Proposal 3.2a**

**The following RAN1#108-e agreement is amended as:**

|  |
| --- |
| **Agreement (RAN1#108-e)**  Adopt the following definition for H/S/NA configured in an RB set of a symbol:   * FDM Hard: When an RB set of a downlink, uplink, or flexible symbol is configured as hard, the IAB-DU cell can respectively transmit, receive, or either transmit or receive on the RB set in the symbol ~~[provided it does not impact the IAB-MT’s ability to transmit and receive in any other RB set that is configured as~~ *~~Not Available~~* ~~or configured as~~ *~~Soft~~* ~~and not indicated available]~~. * FDM Soft: When an RB set of a downlink, uplink, or flexible symbol is configured as soft, the IAB-DU cell can respectively transmit, receive or either transmit or receive on the RB set in the symbol only if   + the IAB-MT does not transmit or receive on the RB set during the symbol of the IAB-DU cell, or   + with respect to all serving cells,     - the IAB-MT would transmit or receive on the RB set during the symbol of the IAB-DU cell, and the transmission or reception on the RB set ~~[~~or any ~~adjacent~~ RB set that is configured as Not Available or configured as Soft and not indicated available~~]~~ during the symbol of the IAB-DU cell is not changed due to a use of the RB set in the symbol by the IAB-DU, or   + if the IAB-MT is not configured with SCG     - if the IAB-MT detects a DCI format 2\_5 with an AI index field value indicating the soft RB set as available   + if the IAB-MT is configured with SCG     - the IAB-MT detects two DCI formats 2\_5 with an AI index field value indicating the soft RB set as available from MCG and SCG respectively, or     - the IAB-MT detects a DCI format 2\_5 with an AI index field value indicating the soft ~~symbol~~ RB set as available from one cell group (either MCG or SCG), and, with respect to all serving cells of the other cell group:       * the IAB-MT would transmit or receive on the RB set during the symbol of the IAB-DU cell, and the transmission or reception on the RB set during the symbol of the IAB-DU cell is not changed due to a use of the RB set in the symbol by the IAB-DU. * FDM NA: When an RB set of a downlink, uplink, or flexible symbol is configured as unavailable, the IAB-DU neither transmits nor receives at the RB set in the symbol. |

|  |  |  |
| --- | --- | --- |
| **Company** | **Do you agree with FL Proposal 3.2a?** | **Comments** |
|  |  |  |
|  |  |  |

## Issue #9. Extension of exception for cell-specific/semi-static signals to soft or not available RB sets

This issue relates to the TP for the RAN1#104-e agreement on the Extension of exception for cell-specific/semi-static signals to soft or not available RB sets.

Related input from contributions:

|  |  |
| --- | --- |
| NTT DOCOMO  [7] | Proposal 1: Adopt the following TP for TS 38.213 section 14. |
| LG Electronics  [9] | Proposal 1: Capture the following TP for TS 38.213 on frequency resource for cell-specific/semi-static signals and channels. |
| Qualcomm  [13] | Proposal 4.2  Adopt the following text proposal for cell-specific/semi-static signals in the frequency domain in 38.213:   |  | | --- | | An RB set of a symbol is equivalent to being configured as hard if an IAB-DU would transmit a SS/PBCH block, PDCCH for Type0-PDCCH CSS sets configured by *pdcchConfigSIB1*, or a periodic CSI-RS in the RB set of the symbol, or would receive a PRACH or a SR in the RB set of the symbol. | |

RAN1#104-e agreed to the following.

|  |
| --- |
| **Agreement (RAN1-104e)**  Regardless of simultaneous operation, the same cell-specific/semi-static signals and channels of the IAB-DU considered as hard time/frequency resources in Rel-16 are also considered as hard time/frequency resources in Rel-17.  FFS: IAB-MT behavior in case of conflicts between cell-specific signals/channels and other resource configurations of the IAB-MT (e.g., dedicated slot configurations) |

38.213 has the following clause (from Rel-16)

|  |
| --- |
| A symbol of a slot is equivalent to being configured as hard if an IAB-DU would transmit a SS/PBCH block, PDCCH for Type0-PDCCH CSS sets configured by *pdcchConfigSIB1*, or a periodic CSI-RS in the symbol of the slot, or would receive a PRACH or a SR in the symbol of the slot. |

**Summary of views:**

* [7], [9] and [13] have TPs to extend the above 38.213 clause to the RB sets.

The FL has a slight preference for keeping the Rel-16 version of the clause unchanged and adding the same clause in which ‘symbol’ is replaced with ‘RB set of a symbol’.

**FL Proposal 3.3a**

**Adopt the following TP in clause 14 of TS38.213:**

|  |
| --- |
| An RB set of a symbol is equivalent to being configured as hard if an IAB-DU would transmit a SS/PBCH block, PDCCH for Type0-PDCCH CSS sets configured by *pdcchConfigSIB1*, or a periodic CSI-RS in the RB set of the symbol, or would receive a PRACH or a SR in the RB set of the symbol. |

|  |  |  |
| --- | --- | --- |
| **Company** | **Do you agree with FL Proposal 3.3a?** | **Comments** |
|  |  |  |
|  |  |  |

## Issue #10. Update to determination of availability in DC scenario

This issue relates to a correction in the description of the implicit determination of availability of a Soft resource for the DC scenario.

Related input from contributions:

|  |  |
| --- | --- |
| Qualcomm  [13] | Proposal 4.1  Adopt to the following text proposal for soft symbols in 38.213: |

38.213(V17.1.0) currently has the following related clauses:

|  |
| --- |
| When a downlink, uplink, or flexible symbol is configured as soft, the IAB-DU cell can respectively transmit, receive or either transmit or receive in the symbol only if  - the IAB-MT does not transmit or receive during the symbol of the IAB-DU cell, or  - with respect to all serving cells, the IAB-MT would transmit or receive during the symbol of the IAB-DU cell, and the transmission or reception during the symbol of the IAB-DU cell is not changed due to a use of the symbol by the IAB-DU, or  - the IAB-MT detects a DCI format 2\_5 with an AI index field value indicating the soft symbol as available if the IAB-MT is not configured with an SCG, or  - the IAB-MT detects two DCI formats 2\_5 with an AI index field indicating the soft symbol as available from the MCG and SCG, respectively, or  - the IAB-MT detects a DCI format 2\_5 with an AI index field value indicating the soft symbol as available from one cell group and with respect to all serving cells of the other cell group, the IAB-MT would transmit or receive during the symbol of the IAB-DU cell, and the transmission or reception during the symbol of the IAB-DU cell does not change due to a use of the symbol by the IAB-DU. |

**Summary of views:**

* [13] has a TP to correct the case where the availability indication is received from one cell group and not from the other one, and hence the conditions for implicit determination of availability need to be specified for the SCG.

The FL assessment is that this is a required specification correction to reflect RAN1’s intent of the following RAN1#105-e agreement:

|  |
| --- |
| **RAN1#105-e Agreement**  For an IAB-MT with multiple serving cells (including the case with two parent nodes), a per-cell IAB-DU soft resource is considered as available if the resource is either explicitly indicated (via DCI 2\_5), or implicitly determined as available with respect to all serving cells.   * If the IAB-DU per-cell soft resource neither explicitly indicated as Available, nor implicitly determined as Available by the IAB-DU with respect to at least one serving cell   + Alt 1. The IAB-DU per-cell resource is assumed to be not available * This agreement does not necessarily mean the Rel-16 spec does not support what is described in the main bullet |

**FL Proposal 3.4a**

**Adopt the following TP in clause 14 of TS38.213:**

|  |
| --- |
| When a downlink, uplink, or flexible symbol is configured as soft, the IAB-DU cell can respectively transmit, receive or either transmit or receive in the symbol only if  - the IAB-MT does not transmit or receive during the symbol of the IAB-DU cell, or  - with respect to all serving cells, the IAB-MT would transmit or receive during the symbol of the IAB-DU cell, and the transmission or reception during the symbol of the IAB-DU cell is not changed due to a use of the symbol by the IAB-DU, or  - the IAB-MT detects a DCI format 2\_5 with an AI index field value indicating the soft symbol as available if the IAB-MT is not configured with an SCG, or  - the IAB-MT detects two DCI formats 2\_5 with an AI index field indicating the soft symbol as available from the MCG and SCG, respectively, or  - the IAB-MT detects a DCI format 2\_5 with an AI index field value indicating the soft symbol as available from one cell group and with respect to all serving cells of the other cell group,   * the IAB-MT does not transmit or receive during the symbol of the IAB-DU cell, or * the IAB-MT would transmit or receive during the symbol of the IAB-DU cell, and the transmission or reception during the symbol of the IAB-DU cell does not change due to a use of the symbol by the IAB-DU. |

|  |  |  |
| --- | --- | --- |
| **Company** | **Do you agree with FL Proposal 3.4a?** | **Comments** |
|  |  |  |
|  |  |  |

## Issue #13. DL Tx power adjustment MAC-CE

This issue relates to some potential inaccuracies in the current TS38.213 specification in regard to the DL Tx power adjustment MAC-CE.

Related input from contributions:

|  |  |
| --- | --- |
| Qualcomm  [13] | Proposal 4.3  Adopt the following text proposal for DL TX Power Adjustment MAC-CE in 38.213: |

38.213(V17.1.0) has the following description for the DL Tx Power Adjustment MAC CE:

|  |
| --- |
| For a serving cell of an IAB-MT, the IAB-MT can be provided a set of TCI states or a set of RS resource indexes corresponding to a SS/PBCH block or to a CSI-RS resource index for a slot where a PDSCH EPRE adjustment is indicated by DL Tx Power Adjustment MAC CE as described in [11, TS 38.321]. The PDSCH EPRE can be derived from a downlink CSI-RS EPRE as described in [6, TS 38.214] and a PDSCH power offset provided by *powerControlOffsetIAB* as described in [11, TS 38.321]. For a downlink DM-RS and/or PT-RS associated with a PDSCH, the IAB-MT may assume that the ratio of PDSCH EPRE to DM-RS EPRE, and/or PT-RS EPRE to PDSCH EPRE,is obtained as for a "UE" in [6, TS 38.214]. If no TCI state or RS resource index is provided to the IAB-MT, the IAB-MT may assume that a same PDSCH EPRE adjustment applies to all TCI states or RS resource indexes configured for the IAB-MT. A PDSCH EPRE adjustment provided by DL Tx Power Adjustment MAC CE may be restricted to frequency resources of an IAB-node that do not result in simultaneous reception on the same frequency resources by an IAB-MT and IAB-DU in a slot. |

There are two concerns about the above clause:

* it does not capture the fact that the indicated DL TX power adjustment may be associated with a specific multiplexing mode, and
* it does not correctly capture the following RAN1#107-e agreement about the overlapping and non-overlapping frequency resources.

|  |
| --- |
| **RAN1#107-e Agreement**  **The indication of the desired/provided DL TX power adjustment and desired UL PSD range can further include:**   * **An indication of whether a desired/provided power configuration or adjustment is applied on FDM resources where the simultaneous MT’s and DU’s signals are non-overlapping in the frequency-domain and/or on non-FDM resources where the simultaneous MT’s and DU’s signals may overlap in the frequency-domain, for a given (MT CC, DU cell).** |

**Summary of views:**

* [13] has a TP to capture the indication of the associated configurations.

**FL Proposal 3.5a**

**Adopt the following TP in clause 14 of TS38.213:**

|  |
| --- |
| For a serving cell of an IAB-MT, the IAB-MT can be provided a set of TCI states or a set of RS resource indexes corresponding to a SS/PBCH block or to a CSI-RS resource index for a slot where a PDSCH EPRE adjustment is indicated by DL Tx Power Adjustment MAC CE as described in [11, TS 38.321]. The PDSCH EPRE can be derived from a downlink CSI-RS EPRE as described in [6, TS 38.214] and a PDSCH power offset provided by *powerControlOffsetIAB* as described in [11, TS 38.321]. For a downlink DM-RS and/or PT-RS associated with a PDSCH, the IAB-MT may assume that the ratio of PDSCH EPRE to DM-RS EPRE, and/or PT-RS EPRE to PDSCH EPRE,is obtained as for a "UE" in [6, TS 38.214]. If no TCI state or RS resource index is provided to the IAB-MT, the IAB-MT may assume that a same PDSCH EPRE adjustment applies to all TCI states or RS resource indexes configured for the IAB-MT. A PDSCH EPRE adjustment provided by DL Tx Power Adjustment MAC CE may be restricted to   * to an associated multiplexing mode of the IAB-node, if that indication is provided, and/or * when ~~frequency resources of an IAB-node that do not result in~~ simultaneous reception by the IAB-MT and transmission/reception by an IAB-DU cell occur in ~~on the same~~ nonoverlapping frequency resources ~~by an IAB-MT and IAB-DU in a slot~~, or when simultaneous reception by the IAB-MT and transmission/reception by an IAB-DU cell occur in overlapping frequency resources. |

|  |  |  |
| --- | --- | --- |
| **Company** | **Do you agree with FL Proposal 3.5a?** | **Comments** |
|  |  |  |
|  |  |  |

## Issue #14. Descriptions of MT’s UL MAC-CEs

This issue relates to missing descriptions of MT’s UL MAC-CEs in TS38.213.

Related input from contributions:

|  |  |
| --- | --- |
| Qualcomm  [13] | Proposal 4.4  38.213 to capture the descriptions of the following MAC-CE messages:   * IAB-MT Recommended Beam Indication * Desired DL Tx Power Adjustment * Desired IAB-MT PSD Range |

38.213(V17.1.0) has the descriptions of the Child IAB-DU Restricted Beam Indication MAC CE and DL Tx Power Adjustment MAC-CE but does not have any description for IAB-MT Recommended Beam Indication, Desired DL Tx Power Adjustment, and Desired IAB-MT PSD Range.

While 38.321 will have the detailed design and content of these MAC-CE, it will not likely have an informative description of the intention and applicability of these messages. Hence, it seems appropriate to introduce these MAC-CEs in 38.213.

**Summary of views:**

* [13] proposed to capture the descriptions of the following MC-CE messages in 38.213
  + IAB-MT Recommended Beam Indication
  + Desired DL Tx Power Adjustment
  + Desired IAB-MT PSD Range

**FL Proposal 3.6a**

**TS38.213 to capture the descriptions of the following MAC-CE messages:**

* **IAB-MT Recommended Beam Indication**
* **Desired DL Tx Power Adjustment**
* **Desired IAB-MT PSD Range**

|  |  |  |
| --- | --- | --- |
| **Company** | **Do you agree with FL Proposal 3.6a?** | **Comments** |
|  |  |  |
|  |  |  |

## Issue #16. Alignment of parameters names

This issue relates to alignment of parameters names in TS38.213 with upper-layer parameters defined naming.

Related input from contributions:

|  |  |
| --- | --- |
| Qualcomm  [13] | Proposal 4.5  Adopt the following text proposals for 38.213: |

Given the name of some of the related upper-layer messages and parameters are getting finalized, 38.213 should be updated to correctly reflect them.

**Summary of views:**

* [13] has TPs for the following
  + Use “*Frequency-Domain HSNA Configuration List*” instead of “*Rel-17 frequency-domain IAB-DU-Resource-Configuration-H/S/NA-Config*”
  + Reflect the RRC parameters (such as “*availabilityCombinationsRBGroups*”, “*RbSetGroups*”) related to the availability indication.

**FL Proposal 3.7.1a**

**Adopt the following TP in clause 14 of TS38.213:**

|  |
| --- |
| With reference to slots of an IAB-DU cell, the IAB-DU can be provided an indication of hard, soft or unavailable type per RB set for symbols configured as downlink, uplink or flexible in a slot by *~~Rel-17 frequency-domain IAB-DU-Resource-Configuration-H/S/NA-Config~~ Frequency-Domain HSNA Configuration List* [16, TS 38.473]. The RB set size and the number of RB sets are configured by *RB-Set-Configuration* [16, TS 38.473]. If an indication of hard, soft or unavailable type is not provided for an RB set of a symbol in a slot, the IAB-DU applies the configuration of hard, soft or unavailable type provided by *HSNA Slot Configuration List* in *gNB-DU Cell Resource Configuration* [16, TS 38.473] for the RB set of the symbol in the slot. If an indication of hard, soft, or unavailable type is provided for an RB set in a symbol of a slot, the IAB-DU applies the configuration of hard, soft, or unavailable type provided ~~by~~ *~~Rel-17 frequency-domain IAB-DU-Resource-Configuration-H/S/NA-Config~~* *Frequency-Domain HSNA Configuration List* [16, TS 38.473] when the IAB-node uses simultaneous transmission and reception in the slot. |

|  |  |  |
| --- | --- | --- |
| **Company** | **Do you agree with FL Proposal 3.7.1a?** | **Comments** |
|  |  |  |
|  |  |  |

**FL Proposal 3.7.2a**

**Adopt the following TP in clause 14 of TS38.213:**

|  |
| --- |
| For each cell of an IAB-DU in a set of cells of the IAB-DU, the IAB-DU can be provided:  - an identity of the IAB-DU cell by *iab-DU-CellIdentity*  - a location of an availability indicator (AI) index field in DCI format 2\_5 by *positionInDCI-AI*  - a set of availability combinations by *availabilityCombinations or availabilityCombinationsRBGroups*, where each availability combination in the set of availability combinations includes  - *resourceAvailability* indicating availability of soft symbols in one or more slots for the IAB-DU cell, or one or multiple *RbSetGroups* with each *RbSetGroup* indicating *resourceAvailability* ~~with each~~ *~~resourceAvailablity~~* ~~indicating availability of~~ *for* soft resources in one or more slots for the associated *rbSets* ~~one RB set group where one RB set group includes one or multiple RB sets~~, and  - a mapping for the soft symbol, and/or for soft resources, availability combinations provided by *resourceAvailability* to a corresponding AI index field value in DCI format 2\_5 provided by *availabilityCombinationId* |

|  |  |  |
| --- | --- | --- |
| **Company** | **Do you agree with FL Proposal 3.7.2a?** | **Comments** |
|  |  |  |
|  |  |  |

# References

[1] R1-2203078   Remaining issues on R17 IAB enhancements, Huawei, HiSilicon

[2] R1-2203353   Maintenance on Enhancements to Integrated Access and Backhaul, Nokia, Nokia Shanghai Bell

[3] R1-2203359   Maintenance on enhancements to IAB, ZTE, Sanechips

[4] R1-2203523   Maintenance on Enhancements to Integrated Access and Backhaul, vivo

[5] R1-2203763   Discussions on enhancements to resource multiplexing between child and parent links of an IAB node, CEWiT

[6] R1-2203871   Maintenance on Enhancements to NR IAB, Samsung

[7] R1-2204351   Maintenance on Enhancements to Integrated Access and Backhaul, NTT DOCOMO, INC.

[8] R1-2204413   Resource multiplexing in enhanced IAB systems, Lenovo

[9] R1-2204528   Remaining details on enhancements to IAB, LG Electronics

[10] R1-2204640 Maintenance on enhanced IAB, Ericsson

[11] R1-2204648 Discussions on eIAB maintenance, ETRI

[12] R1-2204777 Remaining details on Frequency-domain Resource Multiplexing for IAB, Intel Corporation

[13] R1-2204992 Remaining issues on eIAB, Qualcomm Incorporated

[14] RP-220519, 3GPP TSG RAN Meeting #95e, Electronic Meeting, March, 2022

[15] R2-224093, 3GPP RAN TSG WG2 Meeting #117-e, Electronic Meeting, February-March, 2022