3GPP TSG RAN WG1 #109-e R1-220xxxx

e-Meeting, May 9th – 20th, 2022

Source: Moderator (OPPO)

Title: Discussion summary#1 for other aspects on AI/ML for beam management

Agenda Item: 9.2.3.2

Document for: Discussion and Decision

# Introduction

The Rel-18 WID of AI/ML for NR Air Interface focuses on a subset of three typical use cases:

1. CSI feedback enhancement
2. Beam management
3. Positioning accuracy improvement.

This document focuses on the other aspects of AI/ML for beam managements, including representative sub use cases and potential specification impact. The company proposals are summarized, and offline proposals drafted passed on company contributions.

Regarding the file names, companies are encouraged to follow the guidance of R1-2203012 (Page 16) as below:

|  |
| --- |
| * + - To avoid ending-up with too long file names and downloading/opening issues, the following naming convention is recommended:       * Keep the previous company’s name (only the most recent one) in the filename, e.g.         + 5/Summary-1-v000-Moderator (HW)         + 5/Summary-1-v001-LG         + 5/Summary-1-v002-LG-CATT         + 5/Summary-1-v003-CATT-vivo         + 5/Summary-1-v004-Moderator(HW)       * It helps identifying on which previous version your input is based on and solve any crossing emails issue. Note the use of 3digit version numbers in the file names. |

# Contact Information

Respondents to the email discussion are encouraged to fill in the following table.

|  |  |  |
| --- | --- | --- |
| Company | Name | Email |
| Moderator | Zhihua SHI | szh@oppo.com |
| Apple | Yushu Zhang | yushu\_zhang@apple.com |
| vivo | Peng SUN | sunpeng@vivo.com |
| AT&T | Thomas Novlan | thomas\_novlan@labs.att.com |
| Futurewei | Baoling Sheen | bsheen@futurewei.com |
| Xiaomi | Mingju Li | limingju@xiaomi.com |
| Lenovo | Bingchao LIU | liubc2@lenovo.com |
| Sony | Chen SUN | Chen.sun@sony.com |
| Huawei, HiSilicon | Thorsten Schier | thorsten.schier@huawei.com |
| NEC | Zhen He | he\_zhen@nec.cn |
| LG Electronics | SeongWon Go  Hyungtae Kim | sw.go@lge.com  ht.kim@lge.com |
| Panasonic | Quan Kuang | quan.kuang@eu.panasonic.com |
| Henrik Ryden | Ericsson | Henrik.a.ryden@ericsson.com |
| Nokia, NSB | Keeth Jayasinghe  Mihai Enescu | keeth.jayasinghe@nokia.com, mihai.enescu@nokia.com |
| CATT | Yongqiang FEI | feiyongqiang@catt.cn |
| Fujitsu | Wang Xin | wangxin@fujitsu.com |
| Samsung | Zhe Chen | tom.chenzhe@samsung.com |
| CMCC | Jun ZUO | zuojun@chinamobile.com |
| NVIDIA | Xingqin Lin | xingqinl@nvidia.com |
| CAICT | Xiaofeng Liu | Liuxiaofeng1@caict.ac.cn |
| OPPO | Jianfei Cao | caojianfei@oppo.com |
| MediaTek | Li-Chuan Tseng / Abhishek Roy | Li-Chuan.Tseng@mediatek.com  Abhishek.Roy@mediate.com |

# Summary of Contributions and Offline Proposals

## Sub use cases

The objective on the use case of beam management is captured in R18 SID (RP-213599) as below:

|  |
| --- |
| Use cases to focus on:   * Initial set of use cases includes:   + CSI feedback enhancement, e.g., overhead reduction, improved accuracy, prediction [RAN1]   + **Beam management, e.g., beam prediction in time, and/or spatial domain for overhead and latency reduction, beam selection accuracy improvement [RAN1]**   + Positioning accuracy enhancements for different scenarios including, e.g., those with heavy NLOS conditions [RAN1] * Finalize representative sub use cases for each use case for characterization and baseline performance evaluations by RAN#98   + The AI/ML approaches for the selected sub use cases need to be diverse enough to support various requirements on the gNB-UE collaboration levels |

Following the SID, companies proposed a dozen of sub use cases for AI/ML-based beam management with different inputs, different outputs, different functionalities, different benefits and so on. The detailed observations and proposals are collected in Section 4.

### Categories and typical sub use cases

In order to facilitate the subsequent discussions, we categorize the diverse sub use cases, proposed by all the contributions of RAN1#109e, into the following types:

* Cat1: Spatial-domain DL beam prediction
  + **BM-Case1:** Spatial-domain DL beam prediction for Set A of beams based on measurement results of Set B of beams
* Cat2: Time-domain DL beam prediction
  + **BM-Case2:** Temporal DL beam prediction for Set A of beams based on the historic measurement results of Set B of beams
* Cat3: Others
  + **BM-Case3:** Beam prediction for higher frequency band (e.g., a band in FR2) based on measurement results of lower frequency band(s) (e.g., a band in FR1)
  + **BM-Case4:** Beam prediction based on UE positioning/trajectory
  + **BM-Case5:** Beam prediction in terms of Qos
  + **BM-Case6:** Spatial-domain UL beam prediction for Set A of beams based on measurement results of Set B of beams
  + **BM-Case7:** beam measurement feedback compression
  + **BM-Case8:** Parameter optimization to improve performance of multi-beam system

For **BM-Case1**, the main idea is that AI/ML model is to predict the top-N1 DL beams out of Set A based on the measurement results of Set B of beams. There were different options proposed by contributions for Set A and Set B and companies’ views are as below:

* Set B is a sub set of Set A.
  + Huawei [1], ZTE [2], Ericsson [3], IDC[4], CATT [5], vivo [6], NEC [7], Xiaomi [9], Samsung[10], OPPO[11], Beijing Jiaotong University[12], Panasonic [13], FUTUREWEI[14], CIACT[16], Apple[17], CMCC[18], Lenovo[20], Spreadtrum[21], TCL[22], Nokia[23], Intel[24], NVIDIA[25], Mavenir [27], QC[28], Fujitsu[29]
* Set A consists of narrow beams whereas Set B consists of wide beams
  + CATT [5], vivo [6], DOCOMO[19], Nokia[23], QC[28]

When N1 > 1, a second stage may be needed, i.e., the best beam is further selected based on the sweeping of AI/ML-predicted N1 beams. While most companies discussed the DL Tx beam predictions, there was also some companies discussing the DL Rx beam predictions, e.g., SS[10], Intel[24].

For **BM-Case2**, the main idea is that AL/ML model is to predict the information of DL beam(s) for future time based on historic measurement results. There were different proposals based on the contributions for the information of beam(s):

* Top-N2 beams and the predicted L1-RSRP
  + Huawei [1], ZTE [2], Ericsson [3], IDC[4], CATT [5], vivo [6], NEC [7], Sony[8], Xiaomi [9] (lower priority compared to Case 1), Samsung[10], OPPO[11] (lower priority compared to Case 1), Panasonic [13], FUTUREWEI[14], LGE[15] (high priority), Apple[17], DOCOMO[19], Spreadtrum[21], TCL[22], Nokia[23], Intel[24], NVIDIA[25], Mavenir [27], QC[28]
* Beam dwelling time
  + ZTE[2], NEC [7], Apple[17]
* Beam failure / blockage
  + Panasonic[13], TCL[22], QC[28]
* New candidate beam
  + Panasonic[13], TCL[22]

For **BM-Case3**, the main idea is that AL/ML model is to predict the top-N3 DL beams for a frequency band in FR2 based on the measurement results of a lower frequency band, which can be in FR1. A second stage is usually used to further the best beam by utilizing the sweeping of AI/ML-predicted N3 beams.

For **BM-Case4**, the main idea is that AL/ML model is to predict the best beams based on UE location/trajectory. For this case, new type of UE measurement/reporting, rather than beam management measurement/reporting, will be used.

For **BM-Case5**, the best beam is predicted according to the QoS class and its requirements. The main motivation is that UEs are sometimes scheduled to a beam that is not the strongest (signal strength wise) but a beam that can improve the UEs QoS metrics. Nokia [23] suggested reinforcement learning for this case.

For **BM-Case6**, the main idea is that AI/ML model is to predict the top-N6 UL beams out of Set A based on the measurement results of Set B of beams, where Set B is a subset of Set A. Generally speaking, BM-Case6 is the counterpart of BM-Case1 for the UL beam management.

For **BM-Case7**, the main idea is that UE generates the reported results by using AI/ML-based encoder (for compression) based on the beam measurement results and gNB recovers the beam information by using the corresponding AI/ML-based decoder.

For **BM-Case8**, one example in Mavenir[27] is that AI/ML model is to optimize the beam-specific cell individual offset (CFO) and Time-to-Trigger (TTT) parameters in real time or, near-real time. This would reduce the cases of too early, too late switches, ping-pong effects and switching failures and thus, reduce the latency and the outage rate. In general, it is to improve the beam-based mobility. Another example in Charter[30] is to optimize vector-quantized codebook for beam management on the gNB side.

Companies’ views are summarized in the following table:

Table 1: Sub use cases and categories

|  |  |  |
| --- | --- | --- |
| Category | Sub use case | Supported or mentioned (but doesn’t explicitly say no or low priority) by companies |
| Cat1:  Spatial-domain DL beam prediction | **BM-Case1:** Spatial-domain DL beam prediction for Set A of beams based on measurement results of Set B of beams | 26  Huawei [1], ZTE [2], Ericsson [3], IDC[4], CATT [5], vivo [6], NEC [7], Xiaomi [9], Samsung[10], OPPO[11], Beijing Jiaotong University[12], Panasonic [13], FUTUREWEI[14], CIACT[16], Apple[17], CMCC[18], DOCOMO[19], Lenovo[20], Spreadtrum[21], TCL[22], Nokia[23], Intel[24], NVIDIA[25], Mavenir [27], QC[28], Fujitsu[29] |
| Cat2:  Time-domain DL beam prediction | **BM-Case2:** Temporal DL beam prediction for Set A of beams based on the historic measurement results of Set B of beams | 22  Huawei [1], ZTE [2], Ericsson [3], IDC[4], CATT [5], vivo [6], NEC [7], Sony[8], Samsung[10], OPPO[11], Panasonic [13], FUTUREWEI[14], LGE[15], Apple[17], DOCOMO[19], Spreadtrum[21], TCL[22], Nokia[23], Intel[24], NVIDIA[25], Mavenir [27], QC[28], |
| Cat3: Others | **BM-Case3:** Beam prediction for higher frequency band (e.g., a band in FR2) based on measurement results of lower frequency band(s) (e.g., a band in FR1) | 2  Sony[8], Apple[17], |
| **BM-Case4:** Beam prediction based on UE positioning/trajectory | 2  Sony [8], Lenovo[20], |
| **BM-Case5:** Beam prediction in terms of Qos | 1  Nokia[23] |
| **BM-Case6:** Spatial-domain UL beam prediction for Set A of beams based on measurement results of Set B of beams | 1  Samsung[10], |
| **BM-Case7:** beam measurement feedback compression | 1  Samsung[10], |
| **BM-Case8:** The beam-specific parameter optimization | 2  Mavenir[27], Charter[30] |

Please provide your input with regard to the following aspects:

* Is any sub use case proposed in some tdoc(s) missing? If so, please add the related information including the brief description of the new sub use cases, the corresponding tdoc, and so on
* Is the position of some company misunderstood or wrongly captured? If so, please correct me.
* Descriptions of the above sub use cases
* …

|  |  |
| --- | --- |
| Company | Comments |
| Apple | We are fine to divide all use cases into two categories: 1) spatial domain beam prediction, 2) time domain beam prediction, 3) other. But it seems case 1, 3, 4, 5 are for spatial domain beam prediction, which should be under cat 1.  In addition, if case 2 includes beam dwelling time prediction, we suggest we explicitly mention that. From current formulation, it seems this only includes beam index prediction. |
| Lenovo | We are generally fine with this categorization, and we are also a supporter of case 2.  However, we understand that case 6 should belong to Cat 1 since they target a similar function. |
| SONY | We are fine with above categories but think that it should be clarified that BM-Case1 and BM-Case2 apply to both DL TX beam prediction and DL RX beam prediction. While the moderator has noted that for BM-Case1, “most companies discussed the DL Tx beam predictions, there was also some companies discussing the DL Rx beam predictions, e.g., SS [10], Intel [24]”, this statement is also true for BM-Case2. In [8], we consider the sub use case with DL RX beam prediction at the UE side. Since the movement/rotation of UE can bring larger changes of UE DL Rx beam while there are relatively small changes of gNB DL Tx beam, considering as an input the selected DL Rx beams at the UE side over a period as a beam set into an AI/ML model, UE Rx beam prediction at UE side can be performed to reduce UE measurement in beam maintenance/switching. |
| HW/HiSi | We agree with the categorization |
| LGE | OK with the current categorization. |
| Panasonic | We are not sure about the criterion for such categorization. For example, in current formulation, cases 1 and 2 are already broad to cover different sub use cases already. It is unclear whether some sub use cases can be separately studied. On the other hand, the other cases (cases 3-8) can somehow fit into either case 1 or case 2 (or both). For example, the case4 where AL/ML model is to predict the best beams based on UE location/trajectory. It could belong to either case 1 and case 2. So it seems important to discuss the criterion for categorization. |
| Ericsson | We are fine with the categories, however, 3,4,5,6 should be part of category 1. |
| Nokia, NSB | * *Is any sub use case proposed in some tdoc(s) missing? If so, please add the related information including the brief description of the new sub use cases, the corresponding tdoc, and so on*   No   * *Is the position of some company misunderstood or wrongly captured? If so, please correct me.*   No   * *Descriptions of the above sub use cases*   It would be good to highlight that some sub-use cases are related to each other. As mentioned also by Apple & E///, there are 1) spatial domain beam prediction, 2) time domain beam prediction, 3) other. We think that BM-Case5 can also be with the first category.  With above BM-Case1 definition -i.e., the AI/ML model is to predict the top-N1 DL beams out of Set A based on the measurement results of Set B of beams, top-N1 is not defined as strongest beams (should not be the case as well) and can also be selected based on another objective (QoS, cell throughput, scheduling latency, etc..) and clearly up to ML model used by companies. We should not restrict companies using of different loss functions and study possible directions on beam prediction in spatial domain.  For 1) spatial domain beam prediction, support to study both cases: (1) Set B is a subset of Set A ;and (2) Set A consists of narrow beams whereas Set B consists of wide beams.  For 2) time domain beam prediction, support to study the cases: (1) Top-N2 beams IDs (but NOT predicted L1-RSRP) |
| Samsung | We are fine with the categorization other than case 4. For clarification, we could like to know whether the UE location information in case 4 includes the position information obtained by CSI-RS/PRS measurement. If so, case 4 can be under case 1 and/or case 2, and position information can be regarded as e.g., assistance information. |
| CMCC | Spatial-domain DL beam prediction can be a start point of the study of AI based BM. Case 5,6 should be under cat 1. |
| NVIDIA | This categorization is a good starting point. Whether some case(s) in Cat 3 can be recategorized to Cat 1 or 2 can be FFS. |
| CAICT | Fine with the description. |
| OPPO | We are fine with the categorization. |
| MediaTek | We suggest that **Inter-cell beam management (ICBM)** be included in BM-Case1 and BM-Case2. Instead of beam selection, we care about cell selection (e.g. in time-domain, predicting Cell ID of the best beam in future time slot). We think AI assistance brings more gains for inter-cell BM than intra-cell BM, e.g., more latency/interruption time could be saved.  Note that ICBM introduced in Rel-17 feMIMO WI does not support mobility (i.e., no serving cell change). Therefore, ICBM should be considered in the scope of BM use case in R18 AI SI. |

As shown in the above table, majority companies support both **BM-Case1** and **BM-Case2**. Meanwhile, the other sub use cases are supported by a limited number of companies. Thus, it is suggested to focus on the sub use case **BM-Case1** and **BM-Case2** in the first step, and continue to discuss other sub use cases. The following proposal can be discussed, and further refined based on the inputs:

***Proposal 1-1: For AI/ML-based beam management, support BM-Case1 and BM-Case2 as the representative sub use case for characterization and baseline performance evaluations***

* ***BM-Case1: Spatial-domain DL beam prediction for Set A of beams based on measurement results of Set B of beams***
* ***BM-Case2: Temporal DL beam prediction for Set A of beams based on the historic measurement results of Set B of beams***
* ***FFS: details of BM-Case1 and BM-Case2***
* ***FFS: other sub use cases***

Please provide your input wrt description of the proposal as well as any other potential sub use cases that should be treated with high priority. In addition, please mention any other aspect that should be considered/included.

|  |  |
| --- | --- |
| Company | Comments |
| Apple | OK |
| vivo | Support |
| AT&T | support |
| Futurewei | We are ok to consider prioritizing BM-Case1 and BM-Case2 as 2 sub use cases for BM use case to facilitate the discussion. It is recommended to avoid too many sub use cases per each high level use case. At study/SI level, final set of representative sub use cases should be discussed and agreed across use cases. |
| Xiaomi | Ok |
| Lenovo | We are fine with the proposal. |
| Sony | We are OK with the proposal. We understand that BM-Case1 and BM-Case2 apply to both DL TX beam prediction and DL RX beam prediction. |
| HW/HiSi | We agree for BM-Case1.  For BM-Case2, we are positive to evaluate it, but want to emphasize that spatial consistency reflecting the UE trajectory needs to be defined firstly before being able to proceed.  Therefore, we propose to update the Proposal as follows:    ***Proposal 1-1: For AI/ML-based beam management, support BM-Case1 and BM-Case2 as the representative sub use case for characterization and baseline performance evaluations***   * ***BM-Case1: Spatial-domain DL beam prediction for Set A of beams based on measurement results of Set B of beams*** * ***BM-Case2: Temporal DL beam prediction for Set A of beams based on the historic measurement results of Set B of beams and under consideration of spatial consistency reflecting the UE trajectory*** * ***FFS: details of BM-Case1 and BM-Case2*** * ***FFS: other sub use cases*** |
| NEC | Support |
| LGE | OK |
| Panasonic | We are generally fine to have focused study. However, the definition of BM-Case 1 and BM-Case 2 is not so clear. For example, why two beam sets are needed for the time domain prediction in Case 2? Also, as commented above, other cases (cases 3-8) seemingly can fall into these two cases as well. |
| Ericsson | Agree |
| Nokia, NSB | OK with the direction. But, as we commented before, not with descriptions to separate BM-cases #3-6.  We suggest rewording as below,  ***Proposal 1-1: For AI/ML-based beam management, support ~~BM-Case1 and BM-Case2~~ following ~~as the~~ representative sub use cases for characterization and baseline performance evaluations***   * ***~~BM-~~Case1: Spatial-domain DL beam prediction for Set A of beams based on measurement results of Set B of beams*** * ***~~BM-~~Case2: Temporal DL beam prediction for Set A of beams based on the historic measurement results of Set B of beams*** * ***FFS: details of ~~BM-~~Case1 and ~~BM-~~Case2***   ***FFS: other sub use cases*** |
| CATT | We are fine with the categorization. |
| Fujitsu | Since both BM-case1 and BM-case 2 may be categorized as collaboration level 1, the specification impacts (e.g. beam measurement, beam report, beam indication) are similar. To limit workload, it’s recommended to select case 1 as the only representative sub use case. |
| Samsung | Support the proposal. |
| CMCC | Support. HW’s update is fine to us. |
| NVIDIA | Support |
| CAICT | Support |
| OPPO | Support |
| MediaTek | We are okay with prioritizing BM-Case 1 and BM-Case 2. |

There were only a limited number of contributions to propose other sub use cases (i.e., BM-Case3, BM-Case4, BM-Case5, BM-Case6, BM-Case7, BM-Case8). However, since this is the first meeting, most of companies didn’t touch these sub use cases in their contributions. Thus, it would be good to check companies’ view to facilitate the decision how to proceed with these sub use cases.

***Collection of companies’ view:*** Companies are invited to input views on the following sub use cases and detailed explanation/ reasons are encouraged as well.

|  |  |  |
| --- | --- | --- |
| **Sub use cases for AI/ML based BM** | **Support** | **Not support** |
| BM-Case3 | Sony |  |
| BM-Case4 | Lenovo; Sony, Ericsson, Samsung |  |
| BM-Case5 |  |  |
| BM-Case6 | Samsung |  |
| BM-Case7 | Samsung |  |
| BM-Case8 |  |  |

Detailed explanation/ reasons can be added to the following table

|  |  |
| --- | --- |
| Company | Comments |
| Apple | We support case 3. But since this is the first meeting, do we really need to exclude any use case? We suggest we list all cases for further study and companies can investigate the pros and cons. |
| AT&T | We are interested in Case 4 and Case 8 and agree that down selection is not needed at this phase. Characterization of the cases relative to Case 1 and Case 2 would especially be relevant (especially to the extent that common evaluation assumptions and AI/ML modeling approaches can be applied). |
| Futurewei | For the study in Rel-18, we suggest not considering BM-Case3 to BM-Case8 and focus on BM-Case1 and BM-Case2 only. |
| Lenovo | BM-Case4 should also be supported since beam prediction with side information, e.g., UE positioning/trajectory is more beneficial for HST and highway scenario. andFurther, the UE trajectory is modeled in EVM. |
| Sony | We support both BM-case 3 and BM-case 4. For BM-case 3, since both FR1 and FR2 are supported/discussed in specifications, it is beneficial to develop the relationship between two frequency band by AI for other usages like BM. For BM-case 4, as there is also an objective in this Rel-18 SI on AI positioning, it seems natural to use the positioning information more efficiently to assist beam prediction. |
| HW/HiSi | At first glance, we are skeptical to the support of the BM-Case3 to BM-Case8. But we could give it more time to digest the proposals. If including too many use cases, we might not be able to progress with the other common issues we also need to align on |
| NEC | We support at least BM-Case4. However, before fully evaluating the advantages and disadvantages of each case, it seems that we should not preclude any one case. |
| Ericsson | We support case 4, but it could be part of category 1. This could be part of assistance information for gNB sided beam prediction. Or used directly for UE-sided beam predictions. |
| Nokia, NSB | Please see the comments under description of cases and P 1-1. |
| CATT | We suggest focus on BM-Case1 and BM-Case 2 only. |
| Fujitsu | To make a conclusion, we think the followings should be investigated firstly,   * The benefits of case3-8. * The differences on potential specification impacts between case3-8 and case 1-2. |
| Samsung | As discussed in our paper, both case 6 and case 7 are beneficial to leverage AI prediction. Besides, case 4 (subject to our clarification) is also very attractive since UE positioning information may significantly improve beam prediction accuracy. |
| CMCC | We are interested in case 6,7, and it is better to analyze the necessity, pros and cons of these cases before precluding some cases. |
| NVIDIA | At this early stage of the study item, all inputs are encouraged. |
| CAICT | We are open to study more sub use cases and no strong will to support a special cases for BM-Case 3- Case 8. |
| OPPO | Open to further study these sub use cases |
| MediaTek | BM-Case4 can also be considered. |

### Details of sub use case **BM-Case1**

Where the AL/ML model is deployed is a key issue and has significant impact on the design and specification. Based on the contributions, there are different preferences for the AL/ML model deployment:

* AL/ML model deployed at NW side is preferred
* AL/ML model deployed at UE side is preferred
* both AL/ML model deployed at NW side and AL/ML model deployed at UE side are studied in R18
* Joint AL/ML model at NW and UE size can be studied

Additionally, AT&T[26] proposed to study centralized (e.g., across multiple gNBs) AI/ML operations. For the difference preferences, companies’ views are as below:

Table 2: AI model deployment

|  |  |  |
| --- | --- | --- |
|  | Preferred or mentioned | Not preferred |
| AI model deployed at NW side | Huawei [1], ZTE [2], Ericsson [3], IDC [4], CATT[5], Sony [8], Xiaomi[9], Samsung[10], LGE[15], CIACT[16], CMCC[18], DOCOMO[19], Spreadstrum[21], Nokia[23], AT&T[26], QC[28] |  |
| AI model deployed at UE side | Huawei [1], Ericsson [3], IDC [4], CATT[5], Sony [8], Xiaomi[9], Samsung[10], LGE[15], CAICT[16], CMCC[18], Spreadstrum[21], Nokia[23], AT&T[26], QC[28], Charter[30] | ZTE [2], |
| Joint AI at both NW and UE | Samsung[10], | Ericsson [3], |
| Joint AI across multiple gNB | AT&T[26] |  |
| Note:   * This table doesn’t differentiate the sub use cases. Some companies may prefer one deployment for one sub use case and prefer another deployment for other use cases. | | |

According to the above table, the first two types of AI/ML model deployment were supported or mentioned by most companies. Thus, the following proposal can be discussed, and further refined based on the inputs:

***Proposal 2-1: For the sub use case BM-Case1, down select one of the following AI/ML model deployments:***

* ***Alt.1: AI/ML models deployed at NW side***
* ***Alt.2: AI/ML models deployed at UE side***
* ***Alt.3: Both AI/ML models deployed at NW side and AI/ML models deployed at UE side***

Please provide your input wrt the above alternatives in the above proposal. In addition, feel free to provide other comment/suggestion

|  |  |
| --- | --- |
| Company | Comments |
| Apple | We are not sure whether we understand the definition of “deployed” correctly, especially for Alt3. Does it mean training in one side but inference is in the other side? |
| vivo | We prefer Alt 2, but we are open to study Alt 1 and Alt 3. |
| AT&T | We support Alt. 1 and are open to studying Alt. 2/3 as well |
| Futurewei | Alt.3. It is preferred to be flexible in deployment scenarios at this early stage of the SI. |
| Xiaomi | We want to clarify that deployment including both model training and inference?  For model training we prefer to be deployed at NW side.  For inference, we support either NW side or UE side. |
| Lenovo | We are open to both Alt1 and Alt2.  The AI/ML model for BM-Case1 can be flexibly deployed either at NW or UE side. From the expected performance aspect, Alt2 is preferred for overhead reduction. While considering deployment only at UE would be restrictive, e.g., some of the AI models may need more memory/complex to be executed at UE, we are also fine with Alt1.  Further, more clarification of Alt.3 is needed. Does Alt. 3 mean joint training and inference at both UE and NW sider? |
| SONY | We are OK with Alt 1 and Alt 2, but not support Alt3. Since different deployments on UE side or gNB side could be applied for different scenarios. |
| HW/HiSi | We would like to clarify of the “deployment” at one side, means training and inference at the same side? For Alt3, does it include that training is done on one side and inference on the other side?  We would prefer if model training and inference is performed at the same side. |
| NEC | We would like to clarify that, Alt.3 means that both Alt.1 and Alt.2 can be supported? If so, we support Alt.3. From our point of view, at least until we evaluate the advantages and disadvantages of Alt.1 and Alt.2, we should not preclude either of the two alternatives. |
| LGE | We are open but prefer Alt 1 considering limited computing power of UE side. |
| Panasonic | Same question as Xiaomi. If model training is at NW side and model inference is at UE side, is it the Alt.3 ? |
| Ericsson | Given the amount of companies proposing alt 1 & 2. We think both should be studied. Regarding the term deployed, we should use the terminology from the general aspect discussion. Such as single-sided UE/NW or dual-sided model. |
| Nokia, NSB | We are fine with studying these alternatives, and not required to mention down selecting these yet. Also, suggest rewording (same with the P 1-1),  ***Proposal 2-1: For the sub use case ~~BM-~~Case1, ~~down select one of the~~ further study following AI/ML model deployments:***   * ***Alt.1: AI/ML models deployed at NW side*** * ***Alt.2: AI/ML models deployed at UE side*** * ***Alt.3: Both AI/ML models deployed at NW side and AI/ML models deployed at UE side*** |
| CATT | We are OK with Alt.1 and Alt.2. For Alt.3, it gets less preference but can be discussed. We may end up with more than one deployment options. The proposal can be modified as:  ***For the sub use case BM-Case1, down select one or more of the following AI/ML model deployments:*** |
| Fujitsu | Supports Alt3. |
| Samsung | Support the proposal in principle. It seems that the wording of Alt-3 is confusing. We suggest to change Alt-3 as:  ***Alt.3: Both Alt1 and Alt2*** |
| CMCC | In our understanding, here "deployed" means inference instead of training. We think both Alt1 and Alt 2 can be considered. |
| NVIDIA | It does not appear necessary to make such down selection at this early stage of the study item. |
| CAICT | We think both NW and UE could use AI/ML model to predict the best beams. |
| OPPO | Support Alt.3. Samsung’s version is better |
| MediaTek | Where to “deploy” the AI/ML model depends on the results of our evaluation. Hence, we think at this moment we should keep it open. |

For an AI/ML-based mechanism, two basic factors are the input and output. Thus, in order to finalize a specific sub use case, the input and output should be clearly defined. As we discussed in Section 3.1.1, there are different proposals for the Set A and Set B. Thus, based on the contributions, the following proposal can be discussed, and further refined based on the inputs:

***Proposal 2-2: For the sub use case BM-Case1, down select one of the following alternatives:***

* ***Alt.1: Set B is a subset of Set A***
  + ***FFS: the number of beams in Set A and B***
  + ***FFS: how to determine Set B out of the beams in Set A (e.g., fixed pattern, random pattern, …)***
* ***Alt.2: Set A consists of narrow beams and Set B consists of wide beams***
  + ***FFS: the number of beams in Set A and B***
* ***Alt.3: both Alt1 and Alt.2***

Please provide your input wrt the above alternatives in the above proposal. In addition, feel free to provide other comment/suggestion. Further refinement will be based on the inputs.

|  |  |
| --- | --- |
| Company | Comments |
| Apple | We think Alt3 should be the most straightforward way. Both sub-sampling and hierarchical based approaches should be valid. We failed to see any reason to preclude one.  In addition, we suggest adding the following:   * ***Alt.4: set A and set B beams are in different bands*** |
| vivo | Alt 3 with the understanding that Alt 1 and Alt2 have the same core issue: finding an AI algorithm with good prediction performance gain and also provide sufficient flexibility on AI model deployment. |
| AT&T | We support Alt. 3 |
| Futurewei | Alt.3, be flexible and open to both options at the early stage of the SI. Down selection may be discussed/considered when evaluation results (including overhead) are available. |
| Xiaomi | Prefer Alt 3 |
| Lenovo | From the overhead reduction point of view, both Alt1 and Alt2 can be considered.  Regarding Alt2: suggest to add an FFS to Alt2 to discuss the QCL relation between beams in set A and beams in set B?   * ***Alt.2: Set A consists of narrow beams and Set B consists of wide beams***   + ***FFS: the number of beams in Set A and B***   + ***FFS: QCL relation between beams in Set A and beams in Set B*** |
| HW/HiSi | We prefer Alt3 |
| NEC | We currently support Alt.3. At least from the simulation results provided some companies, significant gains can be obtained by using Alt.1 and Alt.2. However, if the workload is limited, e.g., only one sub use case is finalized for each use case, Alt.1 is our preferred one. |
| LGE | Support Alt 1. |
| Panasonic | We support Alt 3. |
| Ericsson | We think alt 3 should be used, no need to down select and prohibit studies on both alternatives |
| Nokia, NSB | Please reword “BM”, ok with the proposal otherwise. And support Alt.3. |
| CATT | Alt 3. Final selections can be made based on subsequent evaluation results. We don’t need to make decision now. |
| Fujitsu | Supports Alt3. |
| Samsung | Support the proposal in principle. However, the definition of Set A and Set B is missing in this proposal. Hence, we suggest to add the following note.  ***Note: Set A is for DL beam prediction and Set B is for DL beam measurement.*** |
| CMCC | Prefer Alt3. |
| NVIDIA | It does not appear necessary to make such down selection at this early stage of the study item. Hence, our preference is Alt 3 to explore both. |
| CAICT | We support Alt.3. |
| OPPO | We prefer Alt.1 |
| MediaTek | We support Alt. 3. |

For AI/ML input, there are also different proposals for companies. Thus, based on the contributions, the following proposal can be discussed, and further refined based on the inputs:

***Proposal 2-3: Regarding the sub use case BM-Case1, further study the following alternatives for AI/ML input with potential down-selection:***

* ***Alt.1: Only L1-RSRP measurement based on Set B of DL Tx beams***
* ***Alt.2: L1-RSRP measurement based on Set B of DL Tx beams and the corresponding beam ID***
* ***Alt.3: …***

Please provide your input wrt the above alternatives in the above proposal as well as any other potential alternative that should be treated with high priority. In addition, feel free to provide other comment/suggestion. Further refinement will be based on the inputs.

|  |  |
| --- | --- |
| Company | Comments |
| Apple | We suggest adding the following alternative:   * ***Alt.3: CIR based on Set B of DL Tx beam(s)*** |
| vivo | From our perspective, 3 alternatives can be studies,   * ***Alt 1: Only L1-RSRP measurement based on Set B of DL Tx beams*** * ***Alt 2: L1-RSRP measurement based on Set B of DL Tx beams and assistance information which may include, beam ID, beam angle or position information*** * ***Alt 3: L1-RSRP measurement based on Set B of DL Tx beams, assistance information and expected information which the output of AI model is predicted partial RSRPs corresponding to expected Rx angle in AI input.***   Thus, different assistance information can be discussed in Alt 2 or Alt 3. |
| Futurewei | Regarding the input, we prefer leaving it open to company’s implementation. |
| Xiaomi | As for the corresponding beam ID, we want to clarify that is it only related to Tx beam ID or both Tx and Rx beam ID? |
| Lenovo | More clarification on Alt1 is needed.  Does Alt1 mean that the measured L1-RSRP corresponding to all the beams in Set B are taken as AI/ML input? |
| HW/HiSi | At least Alt 1 can be studied, open to Alt 2 as well |
| NEC | Neither of the two alternatives should be precluded at the beginning of the study. So, we prefer adding the following alternative:   * ***Alt.3: both Alt.1 and Alt.2*** |
| LGE | We think we don’t need to restrict the AI/ML input, Companies can provide their input such as Tx/Rx beam ID, UE position related information, etc. But, Alt 1 or Alt 2 can be the baseline. |
| Ericsson | We don’t think the input should be restricted to RSRP measurements but could also include information such as UE position information. Avoid restricting the input open for now. |
| Nokia, NSB | Agree LGE, inputs consider at the ML model can be proprietary, and there can be other inputs to consider than the ones listed in the proposal. Not sure there is enough evidence to remove different alternatives.  ***Proposal 2-3: Regarding the sub use case ~~BM-~~Case1, further study at least the following alternatives for AI/ML input with potential down-selection:***   * ***Alt.1: Only one input parameter type (e.g., L1-RSRP, CIR) measurementconsidered based on Set B of DL Tx beams*** * ***Alt.2: More than one input parameter types (e.g., L1-RSRP, beam ID, , beam angle) measurementconsideredbased on Set B of DL Tx beams ~~and the corresponding beam ID~~*** * ***Alt.3: One or more input parameter type(s) (e.g., L1-RSRP, beam ID, beam angle) measurement consideredbased on Set B of DL Tx beams with other assistance information.***   ***For each alternative, companies to provide details on any impacts to Air-interface signaling to generate input parameters to ML model.*** |
| CATT | We don’t need to make decision at this early stage. Companies can choose their input for the purpose of study. |
| Fujitsu | We think beside the L1-RSRP measurement based on set B, whether additional inputs are required depends on AI/ML model and its evaluation results. It should be open and not necessary to limit the AI/ML model input in initial stage. |
| Samsung | Support the proposal in general and we are also fine to additionally include Alt 2 provided by vivo. Moreover, L1-RSRP can be considered as baseline, and additional metrics can be considered as potential AI input, but justification is needed, e.g., the gain achieved with or without the additional metrics. |
| CMCC | Alternatives from vivo is fine. The relationship between different alternatives may be not exclusive. The selection of Alt1 or Alt2 may depend on whether sparse beam pattern is fixed or variable. Alt3 intends to make one AI model applicable to UEs with different Rx beam number. |
| NVIDIA | It does not appear necessary to make such down selection at this early stage of the study item. It should be up to companies to explore. Support to further study this. |
| CAICT | We think L1-RSRP should be included and other input could also be considered for performance further enhancement. It may depend on company’s input. |
| OPPO | We prefer Alt.2 and open to other alternatives |
| MediaTek | At this moment we can leave it open, as we believe more discussions and clarifications are required. |

***Proposal 2-4: Regarding the sub use case BM-Case1, further study the following alternatives for AI/ML output with potential down-selection:***

* ***Alt.1: Beam ID(s) and the predicted L1-RSRP of the predicted Top-N1 DL Tx beams*** 
  + ***FFS: N1***
* ***Alt.2: …***

Please provide your input wrt the above alternatives in the above proposal as well as any other potential alternative that should be treated with high priority. In addition, feel free to provide other comment/suggestion. Further refinement will be based on the inputs.

|  |  |
| --- | --- |
| Company | Comments |
| Apple | We suggest adding the following. Compared to predicted L1-RSRP in Alt1, the possibility for the beam to be the best beam could be more important.  ***Alt.2: Beam ID(s) of the predicted Top-N1 DL Tx beams***  ***Alt.3: Beam ID(s) and possibility for the beam to be the best beam of the predicted Top-N1 DL Tx beams*** |
| vivo | This is first meeting. We can make the categories more generic and inclusive.  ***Proposal 2-4: Regarding the sub use case BM-Case1, further study the following alternatives for AI/ML output with potential down-selection:***   * ***Alt.1: L1-RSRP*** * ***Alt.2: Beam information, such as beam ID, beam angle.*** * ***Alt 3: confidence level*** * ***Alt 4:…*** |
| Futurewei | We suggest leaving the output also open to company’s implementation choice as long as we agree on the set of performance evaluation metrics. For example, if companies agree to use Top-1/optimal/best beam prediction accuracy as one of the KPIs, then directly predicting L1-RSRP may not be required. If, however, companies agree to use measured RSRP or RSRP gap as one of the KPIs, then at least the predicted L1-RSRP (for the Top-1 or Top-K beams) has to be available from the output (either directly as a prediction output or not). |
| Xiaomi | We prefer to separate L1-RSRP and beam ID as two alternatives. |
| Lenovo | Suggest to add another Alt.  ***Alt.2: Beam ID(s) of the predicted Top-N1 DL beams with L1-RSRP higher than a threshold.*** |
| HW/HiSi | In this early stage the output can be left to implementation. However, if and alignment across companies is desired, then we prefer Alt 1. |
| NEC | We suggest adding the following alternative:   * ***Alt.2: Beam ID(s) of the predicted Top-N1 DL Tx beams***   + ***FFS: N1*** |
| LGE | Predicted beam ID(s) and predicted RSRP of predicted beam(s) are fine for us. |
| Panasonic | Agree with Apple that best beam ID(s) are more important than predicted L1-RSRP values. Furthermore, we think a new set B (updated from old set B) can also be considered as the output. |
| Ericsson | Agree with Alt2. Note that beam ID is not defined in current standard. However, there are TCI states.  We propose another alternative.  ***Alt.2: TCI states and the predicted L1-RSRP of the predicted Top-N1 TCI states*** |
| Nokia, NSB | As AI/ML models are proprietary, there can be other outputs. In general, it is hard to define outputs at this stage. If the P.2-3 update looks ok, we can consider a similar approach to cover alternatives. |
| CATT | At this early stage, the output shall be open for companies to choose their implementation. For example, the confidence of the predicted beams to be the best beam, or, the confidence of the predicted RSRP higher than a threshold. |
| Fujitsu | To decide the AI/ML output, it needs to clarify if the AI/ML model includes some post-processing or not. For example, the best beam ID can be derived from predicted L1-RSRP with some post-processing. In this case, the basic outputs may select “***the predicted L1-RSRP of the predicted Top-N1 DL Tx beams***”, and other expected outputs are derived from it with some conventional methods. We suggest adding the flowing alternative in initial stage.  Alt2: ***the predicted L1-RSRP of the predicted Top-N1 DL Tx beams*** |
| Samsung | We fine with the Alt-1 in the proposal. Also, Alt-2 provided by Apple is also acceptable to us. |
| CMCC | To predict Top-N1 DL Tx beams, the output of AI model may include RSRP of Top-N1 DL Tx beams, or RSRP of all DL Tx beams and Top-N1 DL Tx beams are selected based on all RSRP. The number of predicted DL Tx beams of AI model does not need to be fixed.  ***Proposal 2-4: Regarding the sub use case BM-Case1, further study the following alternatives for AI/ML output with potential down-selection:***   * ***Alt.1: L1-RSRP*** * ***Alt.2: Beam information, such as beam ID, beam angle.*** * ***Alt 3: L1-RSRP and beam information.***   ***…*** |
| NVIDIA | It does not appear necessary to make such down selection at this early stage of the study item. It should be up to companies to explore. |
| CAICT | We are fine with Alt.1 for BM-Case1 as baseline. |
| OPPO | We are fine with Alt-1 and Alt-2 proposed by Apple |
| MediaTek | L1-RSRP in Alt 1 can be considered as the baseline. However, instead of accurate number of L1-RSRP in future time slots, we may want AI/ML to predict who will be the Top-N1 beams, this can be just a list of beam IDs or associated with some probabilities.  Moreover, in case of inter-cell beam management, we suggest the following:  ***Alt.x: Cell ID(s) which the predicted Top-N1 DL beams belong to.*** |

There may be some other issues for each sub use cases. For example, whether online training or offline training is assumed, which is also related to the discussion/output of AI 9.2.1. We can discuss these issues later.

Please provide your input wrt any other issues that should be discussed with higher priority, any other suggestion/comment, …

|  |  |
| --- | --- |
| Company | Comments |
| CMCC | We suggest that following problems can also be discussed.  1) Which side does AI model perform training, NW side or UE side?  2) Does training performed online or offline?  3) Does model inference procedure of spatial domain beam prediction include P1 or P1 and P2 process? |
|  |  |
|  |  |
|  |  |
|  |  |

### Details of sub use case **BM-Case2**

***Proposal 3-1: For the sub use case BM-Case2, down-select one of the following AI/ML model deployments:***

* ***Alt.1: AI/ML models deployed at NW side***
* ***Alt.2: AI/ML models deployed at UE side***
* ***Alt.3: Both AI/ML models deployed at NW side and AI/ML models deployed at UE side***

Please provide your input wrt the above alternatives in the above proposal. In addition, feel free to provide other comment/suggestion. Further refinement will be based on the inputs.

|  |  |
| --- | --- |
| Company | Comments |
| Apple | Similar to proposal 2-1, we are not sure whether we understand the definition of “deployed” correctly, especially for Alt3. Does it mean training in one side but inference is in the other side? |
| vivo | Similar to proposal 2-1 |
| AT&T | We support Alt. 1 and are open to studying Alt. 2/3 |
| Futurewei | Alt.3. It is preferred to be flexible in deployment scenarios at this early stage of the SI. |
| Xiaomi | Prefer Alt 1 |
| Lenovo | We are open to both Alt1 and Alt2.  The AI/ML model for BM-Case1 can be flexibly deployed either at NW or UE side. From the expected performance aspect, Alt2 is preferred for overhead reduction. While considering deployment only at UE would be restrictive, e.g., some of the AI models may need more memory/complex to be executed at UE, we are also fine with Alt1.  Further, more clarification of Alt.3 is needed. Does Alt. 3 mean joint training and inference at both UE and NW sider? |
| SONY | We are OK with the classification. But for Alt 2 It is better to specify the usage of AI model deployed at UE side either for gNB beam prediction or for UE-beam prediction.  We would prefer to not perform a down selection at this stage, but to study the merits of the three alternatives. |
| HW/HiSi | Similar comment as to proposal 2-1 |
| NEC | As we mentioned in proposal 2-1, we are not sure whether Alt.3 means that both Alt.1 and Alt.2 are supported. If so, we support Alt.3. |
| LGE | We are fine with studying Alt 1 with priority, but not sure down selection is needed given that this is very first meeting. In addition, it is unclear to use how Alt3 works. Does it mean beam prediction at both sides? |
| Panasonic | Both Alt.1 and Alt.2 can be considered. Alt.3 needs more clarification. Does it mean both NW and UE have model inference? Or it means training and inference are split between UE and NW. |
| Ericsson | Alt.3. Both alternative 1 & 2 should be studied. It is unclear which node is the best location for such model at this stage. Regarding the term deployed, we should use the terminology from the general aspect discussion. Such as single-sided UE/NW or dual-sided model. |
| Nokia, NSB | Alt.3.  Suggest removal of “BM” as in earlier comments.  We are fine with studying these alternatives, and not required to mention down selecting yet. |
| CATT | We are ok with Alt.1 and Alt.2. Alt.3 can also be discussed. We may end up with more than one deployment options. The proposal can be modified as:  ***For the sub use case BM-Case1, down select one or more of the following AI/ML model deployments:*** |
| Fujitsu | Support alt.3 |
| Samsung | Support the proposal in principle. Similar to proposal 2-1, it seems that the wording of Alt-3 is confusing. We suggest to change Alt-3 as:  ***Alt.3: Both Alt1 and Alt2*** |
| CMCC | Similar to proposal 2-1 |
| NVIDIA | It does not appear necessary to make such down selection at this early stage of the study item. |
| CAICT | We think BM-Case2 is more gNB specific and Alt.2 should be considered. |
| OPPO | Support Alt.3. Samsung’s version is better. |
| MediaTek | We prefer Alt.3. |

There are different proposals from companies for the Set A and Set B. Thus, based on the contributions, the following proposal can be discussed, and further refined based on the inputs

***Proposal 3-2: For the sub use case BM-Case2, further study the following alternatives with potential down-selection:***

* ***Alt.1: Set B is a subset of Set A***
  + ***FFS: the number of beams in Set A and B***
  + ***FFS: how to determine Set B out of the beams in Set A (e.g., fixed pattern, random pattern, …)***
* ***Alt.2: Set A and Set B are the same***
  + ***FFS: the number of beams in Set A and B***
* ***Alt.3: …***

Please provide your input wrt the above alternatives in the above proposal as well as other potential alternatives should be with high priority. In addition, feel free to provide other comment/suggestion. Further refinement will be based on the inputs.

|  |  |
| --- | --- |
| Company | Comments |
| Apple | For beam prediction, it seems there is no need to define the connection between set A and set B. |
| vivo | Support. |
| AT&T | We support the proposal and prefer Alt. 2 |
| Futurewei | Alt.2 may be a more typical case in time domain beam prediction. Depending on evaluation results, Alt.1 may be ok as well. In summary, we prefer leaving this open at the early stage of SI. |
| Xiaomi | Prefer alt 1 for beam prediction in time domain. |
| Lenovo | If we also consider overhead reduction for BM-Case2, we prefer to Alt1. |
| Sony | We are OK to study both alternatives and do not need to down-select at this stage. |
| HW/HiSi | We agree with the comment from Apple, there is no need to define the connection between set A and B.  Otherwise, we would like a more generic approach:   * Set A and Set B are subset of Set C.   + FFS: the number of beams in Set A, B, and C.   FFS: how to determine Set B out of the beams in Set C (e.g., fixed pattern, by AI/ML model prediction) |
| NEC | It is noted that the main idea of beam prediction in time domain is to predict the information of DL beam(s) for future time based on historic measurement results of some beams. And it is hard for us to see the connection between the future beams (Set A) and the historic beams (Set B). So, we agree with Apple’s comments. |
| LGE | We are fine with study but it is unclear why a FFS point is needed for Alt2 given that set A=set B? From our understanding, number of beam should be the same. |
| Panasonic | For time domain beam prediction, the motivation to define two sets are not so clear to us. |
| Ericsson | Agree with NEC/Apple. We need to clarify the relation between set A & B. |
| Nokia, NSB | OK in general. Agree with Apple, NEC, E///.  Suggest also removing “BM” in the proposal. |
| CATT | Alt.2 seems to be the baseline, while other options can still be considered, e.g., Set A and Set B are different sets of beams with different beam width. |
| Fujitsu | For beam prediction in time domain, the definition of set A and B needs more clarification. It seems no needs to define the relation between set A and set B. |
| Samsung | We think that Alt-1 and Alt-2 can be somehow combined. We suggest the following formulation:   * ***Alt.1: Set B is a subset of Set A***   + ***Note: Set B equals to Set A is a special case.***   + ***FFS: the number of beams in Set A and B***   + ***FFS: how to determine Set B out of the beams in Set A (e.g., fixed pattern, random pattern, …)***   Also, the definition of Set A and Set B is missing in this proposal. Hence, we suggest to add the following note.  ***Note: Set A is for DL beam prediction and Set B is for DL beam measurement.*** |
| CMCC | Support |
| NVIDIA | Support further study. It does not appear necessary to make such down selection at this early stage of the study item. |
| CAICT | We think the prediction in time domain could combine with spatial domain. Alt.1 could be considered. Purely time domain prediction could use more history information and there is no need for the bundling of Set A and B. |
| OPPO | We prefer Alt.2 |
| MediaTek | We prefer Alt.2 |

For the historic measurement results, it is natural to have a window or a number on the past measurement instances. Thus, the following proposal can be discussed, and further refined based on inputs.

***Proposal 3-3: Regarding the sub use case BM-Case2, the measurement results of K (K>=1) past measurement instances are used for AI/ML model input:***

* ***FFS: values of K***

Please provide your input wrt the description of the above proposal. In addition, feel free to provide other comment/suggestion. Further refinement will be based on the inputs.

|  |  |
| --- | --- |
| Company | Comments |
| Apple | OK in principle, but we think the K instances should be with the same interval, right? |
| Vivo | Fine |
| AT&T | Ok |
| Futurewei | We prefer not fixing the K (K>=1)value and leave it to implementation decision. |
| Xiaomi | Ok |
| Lenovo | Generally Fine.  But we are confused with the term of ‘past’, does it correspond to the latest K beam report or beam measurement before the current beam measurement? |
| Sony | We support this proposal in principle. |
| HW/HiSi | We think there is no need to fix this number, it should be left for implementation. Companies can report their selected value, would be our preference. However, if it is really necessary to take one value for calibration, we are open to discuss. But even if we pick a value of K here for calibration, it should not preclude other values for evaluation. |
| NEC | Support |
| LGE | OK |
| Panasonic | OK. Here we do not see a notion of set A and set B. As commented above, it seems not necessary to define two sets. |
| Ericsson | We support this proposal. But it needs clarification. Important to also describe the timestamp assumed for the K past measurements. The amount of historical measurements can limit when the model can start to be used to perform predictions. |
| Nokia, NSB | OK in general. Up to Companies to disclose their measurement patterns and measurement procedure in the observation window.  Suggest removing “BM” in the proposal. |
| CATT | Support. |
| Fujitsu | Support it. But the value of K depends on the evaluation results. |
| Samsung | The intention of this proposal is understandable. But we don’t think there is a need to limit the number of K at this stage unless it is for calibration purpose in the parallel agenda item. |
| CMCC | OK |
| NVIDIA | Support |
| CAICT | Fine with the proposal. |
| OPPO | Support |
| MediaTek | OK in principle |

***Proposal 3-4: Regarding the sub use case BM-Case2, further study the following alternatives of measurement results for AI/ML input (for each past measurement instance) with potential down-selection:***

* ***Alt.1: L1-RSRP measurement based on Set B of DL Tx beams and the corresponding beam ID***
* ***Alt.2: …***

Please provide your input wrt the above alternatives in the above proposal as well as any other potential alternative that should be treated with high priority. In addition, feel free to provide other comment/suggestion. Further refinement will be based on the inputs.

|  |  |
| --- | --- |
| Company | Comments |
| Apple | We are a bit confused with the definition of set B, does it mean the reported beam(s) or the measured beam(s). If it includes reported beam(s), maybe beam index needs to be added as input in addition to L1-RSRP. |
| vivo | Similar to proposal 2-3. And we believe spatial domain beam prediction algorithm is an essential precondition for time domain beam prediction study. Thus, proposal 3-4 should be a supplement with time domain specific parameters on proposal 2-3. |
| Futurewei | Alt.1 is ok while companies are free to decide whether to use both as input to their AI/ML model. |
| Xiaomi | Support Alt 1. In addition, We think that the input of AI/ML model for time domain beam prediction may be the output of the AI/ML model for spatial domain beam prediction. So it is better to discuss it after spatial domain beam prediction. |
| Lenovo | Generally fine with FL proposal. |
| HW/HiSi | Alt.2: L1-RSRP measurement based on Set B of DL Tx beams and/or the corresponding beam ID |
| NEC | We suggest adding the following alternative:   * ***Alt.2: L1-RSRP measurement based on Set B of DL Tx beams, the corresponding beam ID and assistance information*** |
| LGE | UE velocity, orientation, and/or rotation are also useful for beam prediction. In addition, the increase ratio of L1-RSRP for best N beams can be used as AI/ML input. For example, it can be the ratio of L1-RSRP at past T measurement instance and at past T-τ measurement instance for best N beams. So, companies can provide their additional input for AI/ML model. But, Alt 1 can be the baseline. |
| Panasonic | The motivation to define two sets are not so clear to us. |
| Ericsson | Alt 1 can be baseline. But it should be possible to study additional model inputs. |
| Nokia, NSB | Similar concern here as in P 2-3. There are other possibilities. Suggest capturing the variants in general level than defining inputs explicitly. |
| CATT | We’re ok with Alt 1. But as also mentioned by many companies above, the candidate solutions should be open for now. |
| Fujitsu | The comments are like proposal 2-3. It should be open and not necessary to limit the AI/ML model input in initial stage. |
| Samsung | Support the proposal in general. Also, assistance information such as position information can be added as one of the alternatives. Moreover, L1-RSRP can be considered as baseline, and additional metrics can be considered as potential AI input, but justification is needed, e.g., the gain achieved with or without the additional metrics. |
| CMCC | Similar to proposal 2-3. |
| NVIDIA | At this early stage, should be up to companies to explore all possible options. |
| CAICT | We are fine with the proposal. |
| OPPO | Alt.1 can be the baseline. Open to other alternatives. |
| MediaTek | We are fine with Alt. 1. |

***Proposal 3-5: Regarding the sub use case BM-Case1, further study the following alternatives for AI/ML output (one prediction for a future time instance) with potential down-selection:***

* ***Alt.1: Beam ID(s) and the predicted L1-RSRP of the predicted Top-N2 DL Tx beams*** 
  + ***FFS: N1***
* ***Alt.2: Beam ID(s) and the corresponding beam dwelling time***
* ***Alt.3: Predicted Beam failure and the corresponding bream ID(s)***
* ***Alt.4. Predicted new candidate beam(s)***
* ***Alt.5. …***

Please provide your input wrt the above alternatives in the above proposal as well as any other potential alternative that should be treated with high priority. In addition, feel free to provide other comment/suggestion. Further refinement will be based on the inputs.

|  |  |
| --- | --- |
| Company | Comments |
| Apple | We suggest adding Alt 1b/1c as follows and change “Alt1” into “Alt1a”:   * ***Alt.1b: Beam ID(s) of the predicted Top-N2 DL Tx beams*** * ***Alt.1c: Beam ID(s) and possibility for the beam to be the best beam of the predicted Top-N2 DL Tx beams*** |
| vivo | Similar to proposal 2-4, and we suggest following modifications in proposal 3-5:  ***Proposal 3-5: Regarding the sub use case BM-Case2, further study the following alternatives for AI/ML output (one prediction for a future time instance) with potential down-selection:***   * ***Alt.1: L1-RSRP*** * ***Alt.2: Beam information, such as beam ID, beam angle.*** * ***Alt 3: confidence level*** * ***Alt 4: Beam dwelling time*** * ***Alt.5: Predicted Beam failure*** * ***Alt.6. Predicted new candidate beam(s)*** * ***Alt.7. …*** |
| AT&T | Ok the additional alternatives from vivo, although “confidence level” may need a more detailed definition (e.g. absolute, relative?) |
| Futurewei | Per description provided before, this question should be for BM-Case2.  Alt.1 for BM-Case2. However, we suggest modifying the wording a bit to **“*Beam ID(s) and/or the predicted L1-RSRP of the predicted Top-N2 DL Tx beams”***. We may discuss/decide whether both are needed once the EVM discussion is more stable/clearer. |
| Xiaomi | We prefer to separate L1-RSRP and beam ID to two alternatives. |
| Lenovo | Firstly, the main bullet seems should be for ***BM-Case~~1~~2.***  Suggest to add another Alt:  ***Alt 5: Beam ID(s) of the predicted Top-N1 DL beams with L1-RSRP higher than a threshold.*** |
| HW/HiSi | Can you please clarify what “one prediction for a future time instance means” in BM-case. Shouldn’t in then be BM-Case2? |
| NEC | We suggest the following modifications:   * ***Alt.1: Beam ID(s) of the predicted Top-N2 DL Tx beams*** * ***Alt.2: Beam ID(s) and the predicted L1-RSRP of the predicted Top-N2 DL Tx beams*** * ***Alt.3: Beam ID(s) and the corresponding beam dwelling time*** * ***Alt.4: Predicted Beam failure and the corresponding bream ID(s)*** * ***Alt.5. Predicted new candidate beam(s)*** * ***Alt.6. …*** |
| LGE | In our view, beam confidence for predicted beams, and application time information for the predicted beams also can be considered. Beam dwelling time is one example of the time information however we prefer to capture it more generally. |
| Panasonic | We are fine with modification from vivo. |
| Ericsson | Is there a typo in the proposal ? We assume case 2 is meant.  There is no definition of beam ID. We could use the following instead  **Updated Alt 1**. TCI states and the predicted L1-RSRP of the predicted Top-N2 TCI states  Alt 2. No  Alt 3: Agree in principle. We however need to agree on the term beam ID.  Alt 4: This is same as alt 1 in our view. |
| Nokia, NSB | ML outputs can be proprietary. Similar concern here as in P 2-3/2-4. Suggest capturing the variants in general level than defining outputs explicitly. |
| CATT | We are fine with the listed alternatives. We are also open to consider more, but ‘potential down-selection’ may not be needed at this early stage. |
| Fujitsu | The comments are like proposal 2-4. We support “***the predicted L1-RSRP of the predicted Top-N2 DL Tx beams***” and other outputs may be derived from it through some post-processing. We suggest adding the flowing alternative in initial stage  Alt5: ***the predicted L1-RSRP of the predicted Top-N1 DL Tx beams*** |
| Samsung | Support the proposal and also fine with Alt-1b provided by Apple. |
| CMCC | Similar to proposal 2-4, we suggest following alternatives.  ***Proposal 2-4: Regarding the sub use case BM-Case2, further study the following alternatives for AI/ML output with potential down-selection:***   * ***Alt.1: L1-RSRP*** * ***Alt.2: Beam information, such as beam ID, beam angle.*** * ***Alt 3: L1-RSRP and beam information.***   ***…*** |
| NVIDIA | At this early stage, should be up to companies to explore all possible options. |
| CAICT | We support Alt.1. |
| OPPO | Support the proposal with a preference on Alt.1 |
| MediaTek | Beam dwelling time may be considered.  Also, in case of inter-cell beam management, we suggest the following:  ***Alt.x: Cell ID(s) which the predicted Top-N2 DL beams belong to.*** |

As the AI/ML model predicts the beam information for future time, it should be clear how many future time instances the prediction are made. Thus, the following proposal can be discussed, and further refined based on inputs.

***Proposal 3-6: Regarding the sub use case BM-Case2, AI/ML model output should be F predictions for F future time instances, where each prediction is for each time instance.***

* ***At least F = 1***
* ***FFS: other values of F***

Please provide your input wrt the description of the above proposal. In addition, feel free to provide other comment/suggestion. Further refinement will be based on the inputs.

|  |  |
| --- | --- |
| Company | Comments |
| Apple | OK in principle, but should the F instances with the same interval? |
| vivo | Fine |
| AT&T | Ok |
| Futurewei | At least 1 and let companies to decide how many future time instances should be. |
| Xiaomi | Ok |
| Lenovo | Generally fine with FL proposal. |
| HW/HiSi | At least F = 1, other values can be up for companies to report. |
| NEC | Support |
| LGE | OK |
| Panasonic | OK. |
| Ericsson | Ok |
| Nokia, NSB | OK. Up to Companies to disclose the prediction window. |
| CATT | OK. |
| Fujitsu | Support it. |
| Samsung | Support the proposal. |
| CMCC | OK |
| NVIDIA | OK |
| CAICT | Fine with the proposal. |
| OPPO | Ok |
| MediaTek | OK |

There may be some other issues for each sub use cases. For example, whether online training or offline training is assumed, which is also related to the discussion/output of AI 9.2.1. We can discuss these issues later.

Please provide your input wrt any other issues that should be discussed with higher priority, any other suggestion/comment, …

|  |  |
| --- | --- |
| Company | Comments |
| CMCC | We suggest that following problems can also be discussed.  1) Which side does AI model perform training, NW side or UE side?  2) Does training performed online or offline?  3) Does model inference procedure of time domain beam prediction include P1 or P1 and P2 process? |
|  |  |
|  |  |
|  |  |
|  |  |

## Potential spec impacts

Generally speaking, the spec impacts heavily depend on the detailed sub use cases, e.g., some related aspects are as below:

* What type of training: online or offline?
* Where the AI/ML is deployed: at UE side, at NW side, at both UE and NW side?
* What the input is?
* What the output is?
* …

Thus, the spec impacts discussed in contributions are usually targeted to some specific sub use cases and the potential spec enhancements are quite diverse. Considering the group are still discussing what sub use cases should be supported, a brief summary is trying to capture the key aspects of potential spec enhancement, without many details:

* New or enhanced mechanism(s) to facilitate data collection for UE/NW model, e.g., training, fine-tuning, verification, e.g., some examples are mentioned by contributions
  + Enhanced BM procedures (including signalling/configuration, reporting) to facilitate the training data collection
  + Introduction of some new information, e.g., UE positioning, information from sensor (e.g., velocity, orientation, rotation)
  + Other assistance information for training
* New or enhanced mechanism(s) to facilitate AI/ML inference, e.g., some examples are mentioned by contributions
  + Enhanced BM measurement/reporting for AI inference
  + Signaling/configuration for enhanced BM measurement/reporting
  + Assistance information for AI inference
* New or enhanced mechanism(s) to facilitate AI model life cycle management, e.g., some examples are mentioned by contributions
  + Mechanisms/assistance information for AI/ML model activation, deactivation
  + Mechanisms/assistance information for AI model selection
  + Mechanisms/assistance information for Performance monitoring
  + May include the exchange of some assistance information
* AI-related UE capability and reporting
* Interface of AI model, e.g., input, output
* Other enhancements

This brief summary is not a complete list, and is just used for information. Please see Section 4 for more information. More details will be provided and more discussions will proceed according to the progress of sub use case discussion.

Please share your comment/suggestion on the discussion on spec impact.

|  |  |
| --- | --- |
| Company | Comments |
| Apple | We agree with FL that spec impact depends on use cases. This may be discussed after we identified the use cases. |
| Futurewei | We believe the discussions on specification impact can wait till the discussions on sub use cases and deployment options are more stable. |
| Sony | We agree with FL that this can be discussed later according to the progress. |
| NEC | We are fine with the listed potential spec impact. |
| LGE | We prefer to focus on use case first given that spec impacts are diverge depending on use case. |
| Ericsson | Agree that it should be discussed at a later stage. Upon agreeing to the use cases. |
| CATT | The list looks good. We can further discuss this in a later phase. |
| Fujitsu | Specification impact should be discussed after the finalization of the sub use cases. |
| Samsung | Agree with the FL’s assessment. The details of spec impact can be discussed after the representative sub cases are selected. |
| CMCC | Spec impact can be discussed per sub use case. |
| NVIDIA | This can be discussed after sub use case discussion progresses materially. |
| CAICT | We agree with FL’s observations. |
|  |  |

# Detailed Proposals / Observations

|  |  |
| --- | --- |
| Huawei [1] | ***Observation 1: NW-oriented AI/ML beam management with the AI/ML model trained and inferred both at gNB side can operate under the collaboration level without AI/ML model exchange over the air-interface.***  ***Observation 2: UE-oriented AI/ML beam management with the AI/ML model trained and inferred both at UE side may require the NW to train the AI/ML model and deliver to the UE.***  ***Proposal 1****:* ***For AI/ML-based beam management, the following two sub use cases can be studied:***  ***Beam management in spatial domain***  ***Beam prediction in time domain***  ***Proposal 2: Study whether potential specification impact is needed for AI/ML-based beam prediction considering the following aspects:***  ***AI/ML model training procedure***  ***Enhancement for RSRP report and beam ID report***  ***AI/ML model monitoring procedure*** |
| ZTE [2] | ***Observation 1:*** *The traditional beam training method with brute-force sequential beam searching may result in excessive training overhead, measurement power consumption and processing delay.*  ***Observation 2:*** *Compared with the traditional exhaustive search-based beam training method, the learning-based beam prediction methods can significantly reduce the training overhead and processing delay.*  ***Proposal 1:*** *Both the AI/ML-based spatial-domain beam prediction and time-domain beam prediction should be taken into consideration for possible applicability.*  ***Proposal 2:*** *At least the scenario where AI model is deployed at base station should be considered for specification enhancements on beam management.*  ***Proposal 3:*** *Study potential enhancements on receive beam-related information to the base station reported by UE to assist gNB for more accurate beam prediction and improved generalization of the trained AI/ML model.*  ***Proposal 4:*** *Study potential enhancements to support more flexible beam measurement and reporting, in order to adapt to different AI/ML based beam prediction.*  ***Proposal 5:*** *Consider predictable mobility for beam management as an enhancement aspect for improving UE experience in FR2 high mobility scenario (e.g., high-speed train and high-way) in Rel-18 AI-PHY, which at least includes beam-management-related enhancements for predictable mobility, involving beam measurement, beam report and beam indication.* |
| Ericsson [3] | [Observation 1 Proprietary beam management procedures executed on the UE side (resp. NW side) effect NW side (resp. UE side) data quality and, therefore, AI/ML model generation and performance.](#_Toc102160598)  [Observation 2 Single-sided AI/ML models in the UE, which are transparent to the NW, may make beam management and AI/ML model generation more difficult.](#_Toc102160599)  [Observation 3 UE-side beam prediction AI/ML capability signalling can enable improving NW performance.](#_Toc102160600)  [Proposal 1 Study UE-sided AI enhancements for beam management.](#_Toc102160601)  [Proposal 2 Study NW-sided AI enhancements for beam management.](#_Toc102160602)  [Proposal 3 Do not study dual-sided joint AI enhancements for beam management.](#_Toc102160603)  [Proposal 4 Study enhanced beam management procedures to aid data collection for (offline) single-sided UE/NW model generation, for example potential assistance information.](#_Toc102160604)  [Proposal 5 Study specification impacts for beam prediction AI/ML model configuration activation, deactivation, and monitoring.](#_Toc102160605)  [Proposal 6 Study AI/ML model capability reporting associated with beam predictions from UE.](#_Toc102160606)  [Proposal 7 Study the benefit of signalling predicted values and associated confidence levels for beam management.](#_Toc102160607)  [Proposal 8 Quantify the benefits of site-specific beam prediction models AI/ML models trained on site-specific data.](#_Toc102160608)  [Proposal 9 Study requirements and solutions for enabling trained site-specific beam prediction AI/ML models to UEs](#_Toc102160609) |
| IDC [4] | ***Observation 1:*** *The current NR specification supporting UE reporting with up to 4 best CRIs/SSBRIs with L1-RSRP or L1-SINR can be very limited for gNB estimation.*  ***Observation 2:*** *Partial beam measurement which allows beam prediction by measuring only a subset of beams could be beneficial for reducing RS overheads and reporting latency.*  ***Observation 3:*** *For partial beam measurement, both UE side beam prediction and gNB side beam prediction have benefits.*  ***Observation 4:*** *The current NR specification supports measurement restriction to limit UE measurement, however, measurement restriction is to efficiently utilize RS transmissions for multiple beams not to consider time domain characteristics of beam measurement.*  ***Observation 5:*** *For gNB which predicts beams by using AI/ML, time domain characteristics of beam measurements are essential as well as spatial domain characteristics.*  ***Observation 6:*** *The current NR specification does not consider association between beams with different beam widths.*  ***Observation 7:*** *Utilizing association between beams with different beam widths can provide benefits for prediction accuracy e.g., robust estimation/identification of whole spatial characteristics with wide beams and accurate beam identification with narrow beams.*  ***Observation 8:*** *For Rel-15 beam management, actual mapping between DL Tx beam and UE Rx beam is totally based on UE implementation.*  ***Observation 9:*** *The implementation-based UE Rx beam selection works for Rel-15, however, UE Rx beam information is crucial to accurately predict beam qualities for AI/ML based beam prediction.*  ***Proposal 1:*** *Study benefits of simple specification extension of UE reporting such as* *increasing number of possible best CRIs/SSBRIs, introduction of absolute RSRPs for other CRIs/SSBRIs than the best and other possible extensions and other possible extensions*.  ***Proposal 2:*** *Study benefits of partial beam measurement for specification enhancement to reduce RS overheads and UE reporting latency*.  ***Proposal 3:*** *Study benefits of both UE side beam prediction and gNB side beam prediction for partial beam measurement*.  ***Proposal 4:*** *Study benefits of specification enhancements such as UE reporting with associated time slot domain information*.  ***Proposal 5:*** *Study benefits of specification enhancements on association between beams with different beam widths*.  ***Proposal 6:*** *Study benefits of specification enhancements on acquiring UE Rx beam information*. |
| CATT [5] | ***Proposal 1: The following sub use cases can be considered in Rel-18*** ***AI/ML-based beam management:***  ***Narrow beam prediction based on wide beam measurement.***  ***All beam prediction based on partial beam measurement.t***  ***Beam prediction in time domain.***  ***Proposal 2: The following spec impact of AI/ML based beam management can be considered:***  ***Signaling/procedure of AI model training/updating/fallback;***  ***Interface of AI model, i.e. relationship between measured RS and reported information;***  ***New procedure for RS measurement and reporting;***  ***Signaling/procedure design on exchanging AI-related/non-AI-related assistance information.*** |
| Vivo [6] | Two main sub use cases can be considered for spatial domain beam prediction to reduce overhead and/or improve beam searching accuracy.  Fine beam prediction based on coarse beam measurement  Super-resolution beam prediction based on partial beam measurement.  Study different variations for each sub-use case, considering generalization performance for different number of Tx and Rx beams.  The sub use case of time domain prediction is to predict future beam RSRP with historical RSRPs for both of the following purposes,  Time domain beam prediction for overhead reduction  Time domain beam prediction for accurate beam switching time  Spatial domain beam prediction algorithm is an essential precondition for time domain beam prediction study.  Study impact of different beam sweeping patterns for time domain beam prediction.  Study model deployment procedure and specification impact for both cases that beam prediction functionality resides in UE side and the functionality resides in gNB side.  Study sub-use cases from collaboration level 0~ level 3 for beam management cases.  Study configuration method of beam angle with minimum exposures of implementation details.  Study the gains and impact of different beam input orders.  Study the impact of input beam patterns to model performance monitoring for both spatial and time predictions. |
| NEC [7] | ***Observation 1: At least from the perspective of supporting various gNB-UE collaboration levels and having significant potential specification impact, beam prediction in spatial/time domain can be final representative sub use cases, while*** ***beam selection accuracy improvement can’t.***  ***Observation 2: In order to ensure the performance of the AI model in the real environment, verification of dataset including training, validation and testing is essential.***  ***Observation 3: For sub use case, multiple AI models may be arranged or deployed.***  ***Observation 4: For periodic or semi-persistent beam reporting, overhead of beam measurement and reporting resources can be reduced with beam prediction in time domain.***  ***Proposal 1: Support beam prediction in spatial/time domain as the final representative sub use cases.***  ***Proposal 2: Study the mechanism of exchanging information indicting verification results between gNB and UE.***  ***Proposal 3: Study the mechanism of reporting more beams, e.g., K>4.***  ***Proposal 4: Study the mechanism of model selection.***  ***Proposal 5: Study the mechanism of discontinuous reporting in periodic or semi-persistent beam reporting.***  ***Proposal 6: Study the method of indicating the future beam and the application time of beam.*** |
| Sony [8] | **: Support using AI/ML model trained with all locations and directions of UE for beam prediction and selection at gNB.**  **: Support using dynamic/aperiodic CSI-RS resource set to inform UE candidate beams.**  **: Beam prediction at gNB based on UE’s measurement report can be supported.**  **: Support beam prediction at gNB by using multi pieces of prior CSI information at low frequency for model training.**  **: Propagation environment based AI/ML model selections can be considered at gNB.** |
| Xiaomi[9] | ***Proposal 1: Study sub use case of beam prediction in spatial domain with high priority.***  ***Proposal 2: Prefer AI/ML model training at gNB side and the collaboration level Cat.2 since Rx beam information should be included in beam report for data set collection.***  ***Proposal 3: To discuss whether a common AI model or separate AI models will be trained for UE with different number of Rx beam.***  ***Proposal 4: To input beam information associated with each L1-RSRP to AI/ML model and study how to indicate the Tx beam information of gNB to UE for UE side inference.***  ***Proposal 5: To indicate Rx beam ID to UE for obtaining L1-RSRP input to AI/ML model.*** |
| Samsung[10] | **Proposal 1: Study the sub use cases for beam prediction in spatial domain.**  **Consider gNB-side beam prediction as a sub use case, and**  **Consider UE-side beam prediction as a sub use case.**  **Proposal 2: Study the sub use cases for beam prediction in time domain.**  **Consider gNB-side beam prediction as a sub use case, and**  **Consider UE-side beam prediction as a sub use case.**  **Proposal 3: Study the combination of spatial domain beam predication and time domain beam predication.**  **Proposal 4: Study beam measurement feedback compression as a candidate sub use case.** |
| OPPO[11] | ***Collaboration framework 0a and 0b involves no AI/ML-specific signaling nor model exchange, but they can enable AI/ML-based beam prediction with the aid of existing NR mechanism or modified/enhanced NR system;***  ***Collaboration framework 1b involves AI/ML-specific signaling but no model exchange and it facilitates inference at both sides for AI/ML beam prediction.***  ***For overhead and latency reduction, study the sub use case of AI/ML-based beam prediction in spatial domain as a starting point.***  ***Beam prediction in time domain can be studied and evaluated, but not with top priority.***  ***Study the mechanism and necessity of collaboration framework(s) on a per use case basis for AI/ML beam management.*** |
| Beijing Jiaotong University[12] | ***Proposal #1: Study*** ***image-reconstruction-based beam selection scheme as a use case for beam management enhancement.***  ***Proposal #2: Study the necessary specification change to support AI-based beam selection, considering collaboration level between UE and network, and additional signaling enhancement from the side of network for the adaptive beam measurement.*** |
| Panasonic[13] | **Observation 1: Initial beam establishment is one sub use case.**  **Observation 2: For beam tracking and refining, the following can be considered as sub use cases:**  **Adjustment of measurement/reporting interval**  **Predictive beam switching**  **Partial beam set measurement**  **Observation 3: For beam failure recovery, the AI/ML approaches would be similar to beam tracking and refining sub use cases.**  **Observation 4: For sub use case of initial beam establishment, all AI/ML functionalities located at UE can be considered as baseline, and it can be FFS to spread AI/ML functionalities between UE and network.**  **Observation 5: For sub use case of adjustment of measurement/reporting interval, network based AI/ML can be considered as baseline, and it can be FFS to spread AI/ML functionalities between UE and network.**  **Observation 6: For sub use case of predictive beam switching for RRC\_CONNECTED, network based AI/ML can be considered as baseline, and it can be FFS to spread AI/ML functionalities between UE and network.**  **Observation 7: For sub use case of partial beam measurement, both network based and UE based AI/ML can be considered as baseline, and it can be FFS to spread AI/ML functionalities between UE and network.**  The proposals are as follows:  **Proposal 1: AI/ML mapping within the network (such as gNB or OAM) is up to RAN2/3 discussion. RAN1 discussion should focuses network-UE relation.**  **Proposal 2: Consider the following mapping between sub use cases and network-UE collaboration levels for further study:**   |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | | **Sub use cases** | **Cat-1-UE**  (allAI/ML functionalities at UE) | **Cat-1-network**  (allAI/ML functionalities at network) | **Cat-2**  (Data Collection, Model Training and Model Inference at network; Actor at UE) | **Cat-3**  (Date Collection at network; Model Training, Model Inference and Actor at UE) | **Cat-4**  (Date collection and Model training at network; Model Inference and Actor at UE) | **Cat-5**  (Model Training and Model Inference at both network and UE ) | | **Initial beam establishment** | **Baseline** | **Deprioritzed** | **Deprioritized** | **FFS** | **FFS** | **FFS** | | **Adjustment of measurement/reporting interval** | **FFS** | **Baseline** | **Baseline** | **FFS** | **FFS** | **FFS** | | **Predictive beam switching** | **FFS** | **Baseline** | **Baseline** | **FFS** | **FFS** | **FFS** | | **Partial beam set measurement** | **Baseline** | **Baseline** | **Baseline** | **Baseline** | **FFS** | **FFS** | |
| FUTUREWEI[14] | ***Observation 1: AI/ML-based beam prediction in spatial domain and AI/ML-based beam prediction in time domain can potentially reduce the overhead, improve beam selection accuracy, and improve UE experience/performance.***  ***Proposal 1: Support “AI/ML-based beam prediction in spatial domain” and “AI/ML-based beam prediction in time domain” as sub use cases for AI/ML-based Beam Management use case.*** |
| LGE [15] | **Proposal #1: Consider DL Tx beam prediction in time domain with priority for sub-use cases of AI/ML for beam management.**  **Proposal #2: Potential specification impact for DL Tx beam prediction can be additional UE reporting which can include assistant information for gNB side AI/ML or predicted beam information from UE side AI/ML.** |
| CIACT[16] | ***Proposal 1: AI/ML based algorithm could be used to simplify the beam measurement process.***  ***Proposal 2: Both AI/ML model(s) from gNB based solution and preassemble AI/ML model(s) based solution could be considered for further study.*** |
| Apple[17] | ***Proposal 1: Study spatial domain beam prediction with measurement for limited number of beams as well as a flexible beam measurement and report framework to support dynamic activation/deactivation of beam measurement reference signal and beam report.***  ***Proposal 2: Study FR2 spatial domain beam prediction with FR1 measurements as well as CSI enhancement in FR1 to facilitate the beam prediction in FR2***  ***Proposal 3: Study time domain beam prediction based on past measurement results as well as TCI activation/indication to facilitate the beam prediction in time domain.***  ***Proposal 4: Study beam dwelling time prediction based on past measurement results as well as UE power saving schemes for beam measurement with regard to predicted beam dwelling time.***  ***Proposal 5: Since AI based beam prediction cannot provide 100% beam prediction accuracy, it is necessary to study hybrid AI based and non-AI based beam management.***  ***Proposal 6: Study how to management multiple AI processing simultaneously.*** |
| CMCC[18] | **Proposal 1: Spatial domain beam prediction can be a representative sub use case for beam management.**  **Proposal 2: The model inference procedure of spatial domain beam prediction includes P1 and P2 process.**  **Proposal 3: For spatial domain beam prediction, both model inference operated at gNB side and UE side can be studied.**  **Proposal 4: The same sort method of beam pairs is pre-defined so that gNB and UE have the same understanding of index of beam pairs.**  **Proposal 5: For model inference of spatial domain beam prediction at gNB side, CSI report framework and beam indication need further enhancement.**  **Proposal 6: For model inference of spatial domain beam prediction at UE side, CSI report framework and beam indication need further enhancement.** |
| DOCOMO[19] | **Proposal 1: Time-domain beam prediction should be studied as a sub use-case of beam management in Rel-18 AI/ML for AI.**  **Proposal 2: CSI report should be enhanced to improve the performance of time-domain beam prediction, if time-domain beam prediction is supported as sub use-case.**  **Proposal 3: Spatial-domain beam estimation should be studied as a sub use-case of beam management in Rel-18 AI/ML for AI.**  **Observation 1: Enhancements on beam selection policy in CSI reports might be potential specification impacts for spatial-domain beam estimation.** |
| Lenovo[20] | **Beam measurement and beam selection are important for initial beam assignment procedure during initial access in FR2.**  **Beam measurement and beam selection procedure is the key procedure for all beam management procedures.**  **Beam prediction at gNB/TRP side with model management-related collaboration between gNB and UE (i.e., Cat. 2) can be taken as a sub-use case for beam management in predictable trajectory scenario.**  **Beam selection from a larger number of candidate beams based on the measurement of a small number of configured beams at the UE side using AI model can be taken as another sub-use case.**  **Study UE/NW capability related signaling corresponding to AI-based beam management under correspondent network-UE collaboration levels.**  **Study how to signal AI related parameters for a beam measurement procedure.** |
| Spreadtrum[21] | ***Proposal 1: AI/ML based beam selection can be considered as one of the representative sub use cases.***  ***Proposal 2: AI/ML based beam prediction can be considered as one of the representative sub use cases.***  ***Proposal 3: For AI/ML based beam selection, training could be conducted by gNB, while inference could be conducted by UE for better performance.***  ***Proposal 4: For AL/ML based beam selection, support to configure AI model related information to UE.***  ***Proposal 5: For AL/ML based beam selection,***  ***The current CSI framework can be reused as starting point***  ***The 1/2-port CSI-RS resource and SSB can be reused as measurement resource***  ***Define new reporting quantity for beam that was not directly measured***  ***Define new UE processing capability for AI/ML based beam reporting***  ***Proposal 7: For AL/ML based beam prediction, AI model is implemented by gNB and transparent to UE.***  ***Proposal 8: For AL/ML based beam prediction, the Rel-17 TCI framework can be reused, no more enhancement is required.*** |
| TCL[22] | ***Proposal 1: The configuration of SSB beam scanning at initial access stage can be improved by ML.***  ***Proposal 2: The subsets of beams at the gNB side and UE side, can be constructed with an ML model to reduce the beam training overhead.***  ***Proposal 3: The UE position information is not necessary for predictive beam switching.***  ***Proposal 4: The predictive beam switching shall be discussed in sub use cases of inter-cell beam switching and intra-cell beam switching for latency reduction.***  ***Proposal 5: The beam failure detection performance can be enhanced by an AI/ML model based on historical beam measurements.***  ***Proposal 6: The new candidate beam qnew can be jointly determined by an ML model when beam failure occurs.*** |
| Nokia[23] | The potential use cases that can be beneficial from ML spatial domain beam prediction are:  Use wide beam measurements to predict the best refined beam(s).  Use a subset of wide/refined beam measurements to predict the best wide/refined beam(s).  Utilize the QoS metric to assist the beam prediction for improving system throughput and reducing latency.  Supervised learning ML model beam prediction can be used for finding the highest RSRP wide/refined beam(s) by reducing the beam management overhead significantly.  In order to find beam selections that increase the QoS class specific performance metrics, reinforcement learning approaches can be used for searching the beams than the ones with highest RSRP.  For RL based methods, occasional exploration may be needed to train and validate the ML model.  Support RAN1 to further consider spatial beam prediction based on both supervised learning and reinforcement learning for   * + Beam prediction for reducing beam management resource overhead and latency.   + QoS based beam prediction for improving system throughput and reducing latency.   For beam prediction based on supervised learning, the ML model consider the followings:   * + Model input: RSRP measurements of all/subset of Tx beams from gNB GoB#1, extra info can be included.   + Model output: Prediction of beam ranking or beam RSRP for all/subset of Tx beams from gNB GoB#2.   + **Offline training for the ML model generation.**   For beam prediction based on reinforcement learning, the ML model considers the following   * + Model input: Standard CSI measurements and optionally beam usage statistics and scheduling information if available   + Model output: best beam for QoS class or DRB   + Optionally explorative data collection and training   To enable the supervised learning gNB-based beam inference operation, the existing CSI measurement/report framework can be sufficient.  To enable the supervised learning UE-based beam inference operation  Additional gNB-UE collaboration and signaling may be needed for the ML model selection, model input, model validation and model fine-tuning.  Enhanced CSI measurement/report framework may be needed.  For supervised learning spatial beam prediction, support RAN1 to further study both gNB-based and UE-based beam inference, including   * + The necessary collaboration and signal exchange between gNB and UE for ML model input, model validation, model fine-tuning and model version selection.   + The necessary signaling for CSI reporting to enable ML model inference.   To enable gNB-based QoS aware beam prediction, additional signaling could be introduced so that UEs can expect transmissions from a beam that is not with the highest RSRP.  To enable flexibility of beam prediction in spatial domain, it may be required to have control over the ML model on the exact context of beam prediction in the spatial domain.  For spatial beam prediction, support RAN1 to further study UE-based beam inference, where beam predictions are performed according to the required context set by the gNB.  Spatial-temporal domain beam prediction can be used for reducing beam management resource overhead especially for mobile UE.  Both supervised learning and local online learning provide a framework to track the best beam over time with reduced measurement overhead.  Support RAN1 to further consider the spatial-temporal beam prediction with ML methods, including:   * + Further study spatial-temporal beam prediction with supervised learning method   + Further study spatial-temporal beam prediction local online learning method   + Further study the tradeoffs between the supervised learning method and the online learning method.   To enable the supervised learning or local online learning gNB-based spatial-temporal beam inference operation, the existing CSI measurement/report framework can be sufficient.  To enable the supervised learning or local online learning UE-based spatial-temporal beam inference operation  Additional gNB-UE collaboration and signaling may be needed for the ML model input, model validation, model fine-tuning, and model selection.  Enhanced CSI measurement/report framework may be needed.  Framework supporting model reliability may be needed.  For supervised learning or local online learning spatial-temporal beam prediction, support RAN1 to further study both gNB-based and UE-based beam inference, including   * + The necessary collaboration and signal exchange between gNB and UE for ML model input, model validation, model fine-tuning, model-reliability, and model version selection.   + The necessary signaling for reporting the ML model output. |
| Intel[24] | **For AI/ML assisted beam management use-case, consider both spatial and temporal domain beam prediction sub-use cases within the purview of an offline learning framework.**  **The ML model may reside either at UE or gNB**  **One possible area of specification impact for AI/ML model integration may be for triggering of beam measurement reports and reference signal transmissions, as well new L1 reporting formats.** |
| NVIDIA[25] | **Observation 1: AI/ML techniques can be used to predict beam in time and spatial domain, which can reduce the overhead and latency associated with the P1/P2/P3 beam management procedures.**  **Proposal 1: Beam prediction should be selected as one representative sub use case.**  **Proposal 2: Study the signalling support for the training and execution of AI/ML models for beam prediction.**  **Proposal 3: Study the data required by AI/ML models for beam prediction (e.g., data reported by UE to gNB, assistance data from gNB to UE).**  **Proposal 4: Study how to deliver outputs generated by AI/ML models for beam prediction from gNB to UE and from UE to gNB.** |
| AT&T[26] | **Proposal 1: Both centralized (e.g. across multiple gNBs) and decentralized (e.g. a single gNB or UE) approaches for AI/ML based beam management should be evaluated.** |
| Mavenir [27] | **Proposal 1: RAN WG1 should study the application of AI/ML-based algorithms on the following Use Cases to understand if any specification improvement is required:**  **Reducing the P-1 overhead by optimizing the intra/inter TRxP (e.g., gNB) transmit beam-sweeping directions and periodicity.**  **Reducing the P-2 overhead by predicting the best set of P-2 beams.**  **Improving the beam-based mobility by determining beam-specific cell individual offset (CFO) and Time-to-Trigger (TTT).**  **Proposal 2:** **RAN WG1 should consider the following KPIs while studying the application of AI/ML-based algorithms in beam management:**  **Throughput**  **Beam-switching success rate**  **Number of too early beam-switches**  **Number of too late beam-switches**  **Number of ping-pong cases**  **Link failure rate**  **Outage rate** |
| QC[28] | **Proposal 1: RAN1 should study temporal beam prediction and identify aspects of temporal beam prediction where AI/ML-assisted methods are beneficial.**  **Proposal 2: For UE-side training, RAN1 should focus on offline training scenario, in which the development and training of the AI model for temporal beam prediction happens offline without the need to involve 3gpp signaling.**  **Proposal 3: RAN1 should study the signalling aspects related to gNB sending assistance information to help UE with data collection for training, for the purpose of temporal beam prediction.**  **Proposal 4: RAN1 should study and evaluate the benefits of temporal beam prediction at UE and gNB and the associated signalling needed to assist or enable beam prediction at each side.**  **Proposal 5: For temporal beam prediction, RAN1 should study the signalling aspects related to exchanging information about beam prediction quality and a metric for beam prediction quality**  **Proposal 6: For temporal beam prediction, RAN1 should study the signalling aspects related to gNB sending assistance signalling to help UE in comparing predicted measurements with actual measurements.**  **Proposal 7: RAN1 should study codebook-based spatial domain beam prediction and identify aspects of codebook-based spatial domain beam prediction where AI/ML-assisted methods are beneficial.**  **Proposal 8: For UE-side training, RAN1 should focus on offline training scenario for codebook-based spatial domain beam prediction, in which the AI/ML model design and training does not involve 3gpp signalling.**  **Proposal 9: For UE-side training, RAN1 should study the signalling aspects related to gNB sending assistance information to help UE with data collection for training, for the purpose of codebook-based spatial domain beam prediction.**  **Proposal 10: RAN1 should study and evaluate the benefits of codebook-based spatial (+time) domain beam prediction at UE and gNB and the associated signalling needed to assist or enable beam prediction at each side.**  **Proposal 11: For spatial domain beam prediction, RAN1 should study the signalling aspects related to exchanging information about beam prediction quality and a metric for beam prediction quality.**  **Proposal 12: For spatial domain beam prediction, RAN1 should study the signalling aspects related to gNB sending assistance signalling to help UE in comparing predicted measurements with actual measurements.**  **Proposal 13: RAN1 should study methods for non-codebook-based spatial domain beam prediction and study signalling aspects needed to enable such a prediction.** |
| Fujitsu[29] | **Proposals 1: To limit the workload for evaluation, beam predication in spatial domain can be selected as the only sub use case for beam management.**  **Proposal 2: New signaling carrying beam information in spatial domain should be studied.** |
| Charter[30] | **Observation 1**:DFT based codebooks break down when the angular spread increases (correlation decreases); it is possible to train a ML/DL network in order to derive and update a vector-quantized codebook for beam management on the gNB side, using ML/DL.  **Proposal 1:**Consider the option to enhance beam management with a dynamic vector-quantized codebook based on SVD and ML, and have it exchanged with the UE using appropriate interaction mechanisms between gNB and UE(s). |

# Reference

1. R1-2203143 Discussion on AI/ML for beam management Huawei, HiSilicon
2. R1-2203251 Discussion on potential enhancements for AI/ML based beam management ZTE
3. R1-2203284 Discussions on AI-BM Ericsson
4. R1-2203375 Discussion for other aspects on AI/ML for beam management InterDigital, Inc.
5. R1-2203454 Discussion on other aspects on AI/ML for beam management CATT
6. R1-2203553 Other aspects on AI/ML for beam management vivo
7. R1-2203691 Discussion on other aspects on AI/ML for beam management NEC
8. R1-2203730 Consideration on AI/ML for beam management Sony
9. R1-2203811 Other aspects on AI/ML for beam management xiaomi
10. R1-2203900 Representative sub use cases for beam management Samsung
11. R1-2204018 Other aspects of AI/ML for beam management OPPO
12. R1-2204060 Beam management with AI/ML Beijing Jiaotong University
13. R1-2204078 Discussion on sub use cases of beam management Panasonic
14. R1-2204103 Discussion on sub use cases of AI/ML for beam management use case FUTUREWEI
15. R1-2204152 Other aspects on AI/ML for beam management LG Electronics
16. R1-2204183 Discussions on AI-ML for Beam management CAICT
17. R1-2204241 Enhancement on AI based Beam Management Apple
18. R1-2204298 Discussion on other aspects on AI/ML for beam management CMCC
19. R1-2204378 Discussion on other aspects on AI/ML for beam management NTT DOCOMO, INC.
20. R1-2204420 Further aspects of AI/ML for beam management Lenovo
21. R1-2204501 Discussion on other aspects on AI/ML for beam management Spreadtrum Communications
22. R1-2204569 Discussions on Sub-Use Cases in AI/ML for Beam Management TCL Communication
23. R1-2204574 Other aspects on ML for beam management Nokia, Nokia Shanghai Bell
24. R1-2204796 Use-cases and specification for beam management Intel Corporation
25. R1-2204843 On other aspects of AI and ML for beam management NVIDIA
26. R1-2204863 System performance aspects on AI/ML for beam management AT&T
27. R1-2204938 AI/ML for beam management Mavenir
28. R1-2205027 Other aspects on AIML for beam management Qualcomm Incorporated
29. R1-2205079 Sub use cases and Spec impact on AI/ML for beam management Fujitsu Limited
30. R1-2205094 Discussion on Codebook Enhancement with AI/ML Charter Communications, Inc

# Appendix: Previous Agreements

void