3GPP TSG-RAN WG1 Meeting #109-e R1-22xxxxx

e-Meeting, 9th – 20th May 2022

**Agenda Item: 9.6.1**

**Title: FL summary #1 on potential solutions to further reduce RedCap UE complexity**

**Source: Moderator (Ericsson)**

**Document for: Discussion, Decision**

# 1 Introduction

This feature lead (FL) summary (FLS) concerns the Rel-18 study item (SI) on further NR RedCap UE complexity reduction [1, 2, 3]. This Rel-18 study item was preceded by a Rel-17 study item [4, 5] and a Rel-17 work item [6, 7, 8].

This document summarizes contributions [9] – [35] submitted to agenda item 9.6.1 and relevant parts of contributions [36] – [49] submitted to 9.6.2 and 9.6.3 and captures this email discussion on reduced maximum UE bandwidth:

|  |
| --- |
| [109-e-R18-RedCap-02] Email discussion on further UE complexity reduction by May 20 – Johan (Ericsson)   * Check points: May 18 |

The section numbering in this document follows the draft TR skeleton in [3]. The issues in this document are tagged and color coded with High Priority or Medium Priority. The issues that are in the focus of this round of the discussion are furthermore tagged FL1.

Follow the naming convention in this example:

* *eRedCapComplexityFLS1-v000.docx*
* *eRedCapComplexityFLS1-v001-CompanyA.docx*
* *eRedCapComplexityFLS1-v002-CompanyA-CompanyB.docx*
* *eRedCapComplexityFLS1-v003-CompanyB-CompanyC.docx*

If needed, you may “lock” a discussion document for 30 minutes by creating a checkout file, as in this example:

* Assume CompanyC wants to update *eRedCapComplexityFLS1-v002-CompanyA-CompanyB.docx*.
* CompanyC uploads an empty file named *eRedCapComplexityFLS1-v003-CompanyB-CompanyC.checkout*
* CompanyC checks that no one else has created a checkout file simultaneously, and if there is a collision, CompanyC tries to coordinate with the company who made the other checkout (see, e.g., contact list below).
* CompanyC then has 30 minutes to upload *eRedCapComplexityFLS1-v003-CompanyB-CompanyC.docx*
* If no update is uploaded in 30 minutes, other companies can ignore the checkout file.
* Note that the file timestamps on the server are in UTC time.

In file names, please use the hyphen character (not the underline character) and include ‘v’ in front of the version number, as in the examples above and in line with the general recommendation (see slide 16 in [R1-2203012](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203012.zip)), otherwise the sorting of the files will be messed up (which can only be fixed by the RAN1 secretary).

To avoid excessive email load on the RAN1 email reflector, please note that there is NO need to send an info email to the reflector just to inform that you have uploaded a new version of this document. Companies are invited to enter the contact info in the table below.

**FL1 Question 1-1a: Please consider entering contact info below for the points of contact for this email discussion.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Point of contact** | **Email address** |
| FUTUREWEI | Vip Desai | vipul.desai@futurewei.com |
|  |  |  |
|  |  |  |
|  |  |  |

# 6 Evaluation methodology

6.1 Evaluation methodology for UE complexity reduction

According to the Rel-18 study item description (SID) on further NR RedCap UE complexity reduction [1], further UE complexity reduction techniques should be studied based on Rel-17 evaluation methodology in TR 38.875 [4].

Several contributions [9, 10, 11, 12, 13, 14, 19, 20, 21, 25, 27, 32, 38, 42] provide their views on the cost estimate methodology and present some initial results for Rel-18 enhanced RedCap (“eRedCap”). Regarding the cost estimation methodology, these contributions state that the detailed cost breakdown for the reference NR devices (as provided in Table 6.1-1 in TR 38.875 [4]) should be reused, where the RF-to-baseband cost ratio was assumed to be 40:60 for an FR1 UE. Also, [37] mentions that the selection of reference UE needs to be discussed for Rel-18 RedCap UE cost evaluation.

For cost saving evaluations compared to a Rel-17 baseline, contributions present their results with respect to different versions of Rel-17 RedCap UEs. For example, [10, 12, 14, 21, 39, 42] consider the simplest Rel-17 RedCap (with 20 MHz, 1 Rx, 1 layer, DL 64QAM, HD-FDD or TDD) as the baseline. In particular, the potential further UE complexity reduction features in Rel-18 are considered in combination with the mentioned simplest Rel-17 features [10, 36, 39]. One contribution [9] proposes to define a baseline Rel-17 RedCap UE that supports 20 MHz, 1 Rx, 1 layer, DL 64QAM without HD FDD.

* [9]: Define a baseline Rel-17 RedCap UE that supports a maximum 20 MHz bandwidth, one Rx branch, one MIMO layer, and a maximum DL modulation order of 64QAM.
* [10]: The potential gain of further complexity reduction in Rel-18 should be evaluated with respect to the simplest Rel-17 RedCap UEs.
* [21]: The results of the Rel-18 complexity reduction features are compared against a baseline Rel-17 RedCap UE (20 MHz) with 1Tx-1Rx, 64-QAM DL/ UL, HD-FDD or TDD.
* [36]: The cost evaluation for Rel-18 feature(s) should be carried out by comparing to the simplest Rel-17 RedCap.
  + Comparison of ‘all R17 RedCap features’ and ‘all Rel-17 RedCap features + Rel-18 feature(s)’.

Based on the views provided by contributions, the following questions can be considered regarding the evaluation methodology for Rel-18 UE complexity reduction.

**FL1 High Priority Question 6.1-1a: For cost reduction estimation, can the detailed cost breakdown for the Rel-15 reference NR devices (as provided in Table 6.1-1 in TR 38.875 [4]) be reused?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments** |
| FUTUREWEI1 | Y |  |
|  |  |  |
|  |  |  |

**FL1 High Priority Question 6.1-2a: For comparison with a Rel-17 baseline when evaluating the potential Rel-18 UE complexity reduction features, can the simplest Rel-17 RedCap (with 20 MHz, 1 Rx, 1 layer, DL 64QAM, HD-FDD or TDD) be considered as the baseline? If no, please provide your comments with your proposed baseline.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments** |
| FUTUREWEI |  | We support having a Rel-17 baseline when evaluating potential Rel-18 complexity features. In our baseline, we used (20 MHz, 1 Rx, 1 layer, DL 64QAM) while excluding HD-FDD.  In our view, HD-FDD is a limited use case with access restrictions. We should not make a decision about whether to support complexity technique based on HD-FDD, but we could support HD-FDD if a majority of companies want to include it as part of the baseline. |
| Sierra Wireless | Y | We agree with the proposed baseline. We do prefer to include HD-FDD as part of the baseline. |
|  |  |  |

Furthermore, L2 buffer size reduction aspect is mentioned in [9, 12, 14]. In [9], it is argued that it may not be worthwhile to spend time re-discussing L2 buffer size in Rel-18 as it is difficult to estimate its complexity reduction at the physical layer. Contribution [14] states that clarification about L2 buffer size reduction for peak rate reduction is important. Contribution [36] proposes to consider the cost of memory (external to the RF and BB parts) in the study.

**FL1 High Priority Question 6.1-3a: Should the impact on memory size/cost/complexity (external to the RF and BB parts) be studied/evaluated/captured somehow? Please elaborate in the Comments field.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments** |
| FUTUREWEI1 | N | No changes are needed as the SID says the evaluation methodology is based on TR 38.875.  Even considering memory for the L2 buffer size will complicate the analysis:   * The ratio of RF complexity and baseband complexity may change (possibly in the reference model) – making comparisons to very difficult * The L2 buffer is also dependent on implementation, as the memory needed may be slower that the memory for HARQ * Because L2 memory is smaller since units are bits, not LLRs, the overall complexity for memory is smaller than for HARQ. |
| Sierra Wireless | N | Cost savings would be small. |
|  |  |  |

Beyond the cost/complexity reduction evaluations, many contributions provide their initial evaluations on the impacts of different potential complexity reduction features [9, 10, 11, 12, 14, 15, 16, 19, 23, 24, 29, 31, 32, 34, 35]. It seems to be a common understanding that for each potential further UE complexity reduction feature, the performance impacts, coexistence impacts, specification impacts need to be analyzed. Therefore, the following question can be considered.

**FL1 High Priority Question 6.1-4a: For each potential Rel-18 further UE complexity reduction feature, should the performance impacts, coexistence impacts, and specification impacts be evaluated as listed in the draft TR skeleton [3]?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments** |
| FUTUREWEI1 | Partial Y | The question should be formulated to be independent of the ongoing skeleton discussion. We are OK to include subsections for Performance impacts, Network and coexistence impacts, and Specification impacts, but not (for now) any particular structure within Performance impacts. |
| Sierra Wireless | Y |  |
|  |  |  |

# 7 UE complexity reduction features

7.1 Introduction to UE complexity reduction features

According to the SID [1], some further complexity reduction enhancements may be considered to further expand the market for RedCap use cases with relatively low cost, low energy consumption, and low data rate requirements, e.g., industrial wireless sensor network use cases. Rel-18 eRedCap should provide NR support for low-tier devices between existing LPWA UEs and the capabilities of Rel-17 RedCap UEs. The supported peak data rate for Rel-18 eRedCap targets to 10 Mbps and Rel-18 eRedCap should not overlap with existing LPWA solutions.

Specifically, the objectives of this SID are as follows ‎[1]:

|  |
| --- |
| * Study further UE complexity reduction techniques based on Rel-17 evaluation methodology in TR 38.875 [RAN1]   + Consider network impact, coexistence of Rel-17 and Rel-18 RedCap and non-RedCap UEs in a cell, UE impact, specification impact   + Potential solutions, which may complement each other, for reducing device complexity are focusing on:     - UE bandwidth reduction to 5 MHz in FR1,       * Possibly in combination with relaxed UE processing timeline for PDSCH and/or PUSCH and/or CSI     - reduced UE peak data rate in FR1,       * Possibly including restricted bandwidth for PDSCH and/or PUSCH       * Possibly in combination with relaxed UE processing timeline for PDSCH and/or PUSCH and/or CSI * Notes:   + Rel-15 SSB should be reused and L1 changes minimized.   + Operation in BWP with/without SSB and without/with RF retuning should be considered.   + It is not precluded that some solutions for FR1 can be applied to FR2 in WI stage.   + Aim to define a single Rel-18 RedCap UE type for further UE complexity reduction. |

As we can see, the three main potential complexity reduction features are further UE bandwidth reduction, further UE peak rate reduction, and relaxed UE processing timeline. In the following, different aspects of each potential complexity reduction feature and their potential combinations are discussed.

7.2 Further UE bandwidth reduction

This section focuses on different UE bandwidth reduction options which need to be evaluated. In general, the UE bandwidth reduction can be applied to both radio frequency (RF) and baseband (BB) parts or only to BB parts, both data and control channel or only data channels, and DL and/or UL. Contributions discuss different options for further UE bandwidth reduction in FR1 which are summarized below.

* **Option BW1:** Both RF and BB bandwidths are 5 MHz for UL and DL [9, 10, 11, 13, 14, 18, 25, 32, 33, 35]
* **Option BW2:** 5 MHz BB bandwidth for data and control channels with 20 MHz RF bandwidth for UL and DL [14, 18, 32, 33]
* **Option BW3:** 5 MHz BB bandwidth only for data channels with 20 MHz RF bandwidth for UL and DL. The control channels and other reference signals are still allowed to use a BWP up to the 20 MHz maximum UE RF bandwidth [10, 18, 25, 24, 28, 32, 33, 35]
* **Option BW4:** Baseband bandwidths for data channels can be smaller than 5 MHz for further cost saving. For example, 3 MHz baseband bandwidth only for data channels with 20 MHz RF bandwidth for UL and DL [10]
* **Option BW5:** 20 MHz UE bandwidth in idle/inactive state but 5 MHz bandwidth in connected state [9, 20, 31]
* **Option BW6:** 5 MHz BB bandwidth only for data channels only for DL with 20 MHz RF bandwidth [25]
* **Option BW7:** Both RF and BB bandwidths are 5 MHz only for DL while the UL bandwidth is 20 MHz [9]
* **Option BW8:** No RF reduction but BB reduction for all channels except SSB [18]

Clearly, there can be various options for further UE bandwidth reduction which some of them can be similar (or highly correlated). For evaluations, it is beneficial to down-select the most attractive options. In this regard, the following question can be considered.

**FL1 High Priority Question 7.2-1a: Among the different options presented above for further UE bandwidth reduction in FR1, which option(s) should be studied?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option(s)** | **Comments** |
| FUTUREWEI1 | At least BW1, BW3, BW5 | Given the number of options, it is necessary to downselect. But we are open to consider other options.  Note: BW5 is just a dedicated RRC configuration using a 5 MHz BWP (maximum) operating in 20 MHz. |
| Sierra Wireless | BW3, BW8 | In general we need support for 20MHz RF for SSB/CORESET. |
|  |  |  |

It should be noted that bandwidth reduction naturally results in the peak data rate reduction. The peak data rate can be larger than 10 Mbps with 5 MHz UE bandwidth and high modulation orders (e.g., 64QAM) in FDD. However, in TDD 5 MHz UE bandwidth, the peak data rate for UL or DL can be less than 10 Mbps depending on the TDD pattern [10].

Moreover, there can be similarity between bandwidth reduction options and peak data rate reductions. For example, under certain conditions, the option of BB bandwidth reduction for data channels can resemble the option of peak data rate reduction by restriction of number of PRBs for PUSCH/PDSCH discussed in the next section. Here, following TR 36.888, these two options are treated separately, one in the bandwidth reduction section and the other one in the peak reduction section. Meanwhile, the differences between these two options (i.e., in terms of PRB allocation) can be further discussed.

7.3 Further UE peak rate reduction

This section focuses on different UE peak rate reduction options which need to be evaluated. Contributions discuss different options for further UE peak data rate reduction (considering the 10 Mbps peak rate target) which are summarized below.

* **Option PR1:** Relaxation of the constraint for peak data rate reduction [10, 23, 31, 32, 35]
* **Option PR2:** Restriction of maximum TBS for PDSCH and PUSCH [10, 11, 12, 18, 21, 32, 33, 34]
* **Option PR3:** Restriction of maximum number of PRBs (or bandwidth) for PDSCH and PUSCH [10, 11, 12, 19, 24, 32, 33, 34, 35]
* **Option PR4:** Reduction of scaling factor for peak data rate duction [12, 14]
* **Option PR5:** Relaxation of the maximum modulation order from 64QAM to 16QAM [14, 20, 30, 33]

Clearly, there can be various options for further peak data rate reduction which some of them can be similar (or highly correlated). For evaluations, it is beneficial to down-select the most attractive options. In this regard, the following question can be considered.

**FL1 High Priority Question 7.3-1a: Among the different options presented above for further UE peak data rate reduction, which option(s) should be studied?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option(s)** | **Comments** |
| FUTUREWEI | PR5, PR6 | PR6 is not listed above but in this option, data and control are not in same slot   * PR1/PR4: Should not be studied. Already discussed in Rel-17 * PR2: Should not be studied. It will come naturally from other techniques. * PR3: Neutral. It will be similar to some BW reduction option)   (note to FL: typo for PR4: “duction” -> “reduction”) |
| Sierra Wireless | PR2 | Reducing TBS size gives the most flexibility. |
|  |  |  |

7.4 Relaxed UE processing timeline

This section focuses on different relaxed UE processing timeline options which could be evaluated. Contributions discuss two options for relaxed UE processing timeline which are summarized below.

* **Option PT1:** Relaxation of UE processing time for PDSCH/PUSCH in terms of N1 and N2 [9, 10, 11, 12, 14, 15, 16, 18, 19, 20, 21, 23, 25, 26, 28, 30, 31, 32, 33, 35]
* **Option PT2:** Relaxation of UE processing time for CSI in terms of Z and Z’ [9, 10, 11, 12, 15, 18, 20, 23, 25, 30, 35]

As discussed in Rel-17 [4], there is potential cost reduction for relaxed UE processing timeline with option P1 and/or option P2. Meanwhile, the evaluations in [4] assume the relaxation factor of 2, i.e., doubling N1/N2 and Z/Z’. In this regard, the following questions can be considered.

**FL1 High Priority Question 7.4-1a: Which option(s) should be studied? If some other relaxation factor(s) than 2 should be considered, please indicate so in the Comments field.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Option(s)** | **Comments** |
| FUTUREWEI1 | PT1, PT2 | Given the interest during R18 discussions, we should continue examining process relaxation.  Both options have been examined in R17. However, more companies should provide results for CSI relaxation in order to evaluate the technique as the number of results was limited. |
|  |  |  |
|  |  |  |

7.5 Combinations of UE complexity reduction features

This section focuses on identifying potential combinations of further UE complexity reduction features which need to be evaluated. Contributions present various combinations of the potential complexity reduction features/options discussed in the previous sections. Combinations of relaxed processing time with bandwidth reduction and peak data rate reduction options are generally considered in the contributions [9, 10, 12, 14, 25, 27]. However, since the bandwidth reduction techniques naturally result in the peak data rate reduction, combinations of BW reduction and peak data rate reduction techniques are not considered in most of the contributions. Specifically, contribution [12] points out that it is not necessary to combine the UE bandwidth reduction and reduced UE peak data rate in FR1, since a similar effect can be achieved by both solutions.

Meanwhile, one contribution [21] presents the combination of TBS restriction with bandwidth reduction for further peak rate reduction. Also, [39] indicates that whether both UE bandwidth reduction and reduced UE peak data rate can be selected or only one is down selected depends on not only the cost reduction, but also the performance impacts and specification effort.

In this regard, it can be discussed whether combinations of UE bandwidth reduction and UE peak data rate reduction are feasible options. Therefore, the following question can be considered:

**FL1 High Priority Question 7.5-1a: Should any combination(s) of the further UE bandwidth reduction options listed in Section 7.2 and the UE peak data rate reduction options listed in Section 7.3 be studied? Please elaborate in the Comments field.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments** |
| FUTUREWEI1 |  | From initial analysis, the complexity reduction for most individual techniques is generally small. In order to have a meaningful reduction for Rel-18, combinations of techniques will be needed. How to limit the number of combinations to examine is the challenge. |
| Sierra Wireless |  | Number of combinations should be limited. |
|  |  |  |

While the exact sets of combination of techniques depend on the outcome of previous sections regarding the adopted options for evaluations, the two main sets of combinations are as follows:

* **Combination set 1:** Different combinations of UE bandwidth reduction options and relaxed processing time options.
* **Combination set 2:** Different combinations of UE peak data rate reduction options and relaxed processing time options.

**FL1 High Priority Question 7.5-2a: Can the following combination sets of complexity reduction features be considered as a starting point for the Rel-18 evaluations?**

* **Combination set 1: Different combinations of UE bandwidth reduction options and relaxed processing time options.**
* **Combination set 2: Different combinations of UE peak data rate reduction options and relaxed processing time options.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments** |
| FUTUREWEI |  | While it may be easier to discuss sets, the problem is the combination sets are not necessarily exclusive. A peak data rate reduction is possible with a 5 MHz BW. We can also have a combination of BW reduction and peak data rate (like modulation) and processing. Thus, it is somewhat difficult to create meaningful sets. |
|  |  |  |
|  |  |  |

In addition to the main complexity reduction features identified in the SID [1], a few contributions [9, 18, 20, 25, 31, 32, 35] point out other potential complexity reduction features for Rel-18. Specifically, the following aspects are discussed in these contributions:

* Reduced number of HARQ buffer processes [9, 18, 20, 25, 32]
* HD FDD complexity reduction [31, 32, 35]
* PDCCH monitoring reduction [35]

**FL1 High Priority Question 7.5-3a: In addition to the complexity reduction features/options described in previous sections, should RAN1 prioritize a study of any other aspects related to Rel-18 further UE complexity reduction?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Y/N** | **Comments** |
| FUTUREWEI1 | Y | Studying reduction of the complexity for control processing, including PDCCH monitoring reduction. |
|  |  |  |
|  |  |  |

# References

|  |  |  |  |
| --- | --- | --- | --- |
| [1] | [RP-213661](https://www.3gpp.org/ftp/TSG_RAN/TSG_RAN/TSGR_94e/Docs/RP-213661.zip) | New SID on Study on further NR RedCap UE complexity reduction | Ericsson |
| [2] | [R1-2204058](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204058.zip) | Work plan for Study on further NR RedCap UE complexity reduction | Rapporteur (Ericsson) |
| [3] | [R1-2203121](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203121.zip) | Draft skeleton for TR 38.865 Study on further NR RedCap UE complexity reduction | Rapporteur (Ericsson) |
| [4] | [TR 38.875 V17.0.0](https://www.3gpp.org/ftp/Specs/archive/38_series/38.875/38875-h00.zip) | Study on support of reduced capability NR devices (Release 17) | 3GPP |
| [5] | [R1-2009293](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_103-e/Docs/R1-2009293.zip) | FL summary on RedCap evaluation results | Moderator (Ericsson, Apple, Qualcomm) |
| [6] | [RP-220966](https://www.3gpp.org/ftp/TSG_RAN/TSG_RAN/TSGR_95e/Docs/RP-220966.zip) | Revised WID on support of reduced capability NR devices | Ericsson |
| [7] | [R1-2202535](https://www.3gpp.org/ftp/tsg_ran/WG1_RL1/TSGR1_108-e/Docs/R1-2202535.zip) | RAN1 agreements for Rel-17 NR RedCap | Rapporteur (Ericsson) |
| [8] | [R1-2203115](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203115.zip) | Draft summary of WI on support of reduced capability (RedCap) NR devices | Ericsson |
| [9] | [R1-2203054](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203054.zip) | Discussion of complexity reduction techniques for RedCap UEs in Rel-18 | FUTUREWEI |
| [10] | [R1-2203117](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203117.zip) | Potential solutions to further reduce UE complexity | Ericsson |
| [11] | [R1-2203169](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203169.zip) | Discussion on potential solutions to further reduce UE complexity | Huawei, HiSilicon |
| [12] | [R1-2203338](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203338.zip) | Discussion on potential solutions to further reduce UE complexity | Spreadtrum Communications |
| [13] | [R1-2203473](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203473.zip) | Discussion on solutions to further reduce UE complexity in Rel-18 | CATT |
| [14] | [R1-2203572](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203572.zip) | Techniques to further reduce the complexity of RedCap devices | vivo, Guangdong Genius |
| [15] | [R1-2203600](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203600.zip) | Discussion on further RedCap UE complexity reduction | ZTE, Sanechips |
| [16] | [R1-2203661](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203661.zip) | Discussion on potential solutions to further reduce UE complexity | China Telecom |
| [17] | [R1-2203761](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203761.zip) | Further reduce UE complexity for eRedCap | Panasonic |
| [18] | [R1-2203827](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203827.zip) | Discussion on the potential complexity reduction solutions for further UE complexity reduction | Xiaomi |
| [19] | [R1-2203917](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203917.zip) | Further UE complexity reduction for eRedCap | Samsung |
| [20] | [R1-2203995](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203995.zip) | Solution study on further reduced UE complexity | OPPO |
| [21] | [R1-2204038](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204038.zip) | Further UE Complexity Reduction | Nokia, Nokia Shanghai Bell |
| [22] | [R1-2204176](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204176.zip) | Discussions on potential solutions to further reduce UE complexity | Sharp |
| [23] | [R1-2204255](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204255.zip) | On further RedCap UE complexity reduction features | Apple |
| [24] | [R1-2204315](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204315.zip) | Discussion on further reduced UE complexity | CMCC |
| [25] | [R1-2204389](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204389.zip) | Discussion on potential solutions for further UE complexity reduction | NTT DOCOMO, INC. |
| [26] | [R1-2204437](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204437.zip) | Discussion on potential solutions to further reduce UE complexity | NEC |
| [27] | [R1-2204504](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204504.zip) | Potential solutions to further reduce UE complexity | Lenovo |
| [28] | [R1-2204582](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204582.zip) | Discussion on potential solutions to further reduce UE complexity | Transsion Holdings |
| [29] | [R1-2204626](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204626.zip) | Discussion on potential solutions for further UE complexity reduction | LG Electronics |
| [30] | [R1-2204714](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204714.zip) | On potential solutions to further reduce UE complexity | MediaTek Inc. |
| [31] | [R1-2204747](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204747.zip) | On further complexity reduction of NR UE | Nordic Semiconductor ASA |
| [32] | [R1-2204809](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204809.zip) | On solutions to further reduce UE complexity | Intel Corporation |
| [33] | [R1-2204829](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204829.zip) | Potential techniques for further RedCap UE complexity reduction | InterDigital, Inc. |
| [34] | [R1-2204879](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204879.zip) | Considerations for further UE complexity reduction | Sierra Wireless. S.A. |
| [35] | [R1-2205043](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2205043.zip) | Further complexity reduction for eRedCap device | Qualcomm Incorporated |
| [36] | [R1-2203339](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203339.zip) | Discussion on evaluation needs and assumptions for eRedCap | Spreadtrum Communications |
| [37] | [R1-2203601](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203601.zip) | Evaluation requirements for Rel-18 RedCap UE | ZTE, Sanechips |
| [38] | [R1-2203918](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203918.zip) | Evaluations for eRedCap | Samsung |
| [39] | [R1-2204316](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204316.zip) | Discussion on simulation needs and assumptions | CMCC |
| [40] | [R1-2204505](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204505.zip) | Evaluation needs and assumptions for further NR RedCap | Lenovo |
| [41] | [R1-2204583](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204583.zip) | Discussion on simulation needs and assumptions | Transsion Holdings |
| [42] | [R1-2205044](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2205044.zip) | Evaluation for eRedCap SI | Qualcomm Incorporated |
| [43] | [R1-2203119](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203119.zip) | Initial evaluation results for further RedCap UE complexity reduction | Ericsson |
| [44] | [R1-2203475](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203475.zip) | Views on coexistence between Rel-17 and Rel-18 RedCap UE | CATT |
| [45] | [R1-2203602](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203602.zip) | Other aspects for Rel-18 eRedCap UE | ZTE, Sanechips |
| [46] | [R1-2203829](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2203829.zip) | Other aspects on further NR Redcap UE complexity reduction | Xiaomi |
| [47] | [R1-2204040](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204040.zip) | On other aspects for RedCap evolution | Nokia, Nokia Shanghai Bell |
| [48] | [R1-2204317](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204317.zip) | Discussion on other aspects for RedCap UE | CMCC |
| [49] | [R1-2204917](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_109-e/Docs/R1-2204917.zip) | Overall considerations for Rel-18 RedCap | Huawei, HiSilicon |