**3GPP TSG-RAN WG1 # 110bis-eR1-22xxxx**

**e-Meeting, October 10th – 19th, 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.213** | **CR** | **xxxx** | **rev** | **-** | **Current version:** | **17.3.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Draft CR on CFR configuration for multicast to TS 38.213 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Moderator (CMCC), ZTE, CATT | | | | | | | | | |
| ***Source to TSG:*** | R1 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_MBS-Core | | | | |  | ***Date:*** | | | 2022-10-12 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **F** |  | | | | | ***Release:*** | | | Rel-17 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | In NR, at most 4 DL BWPs can be configured for the UE and there is only one active DL BWP for the UE to perform reception at a time. In each DL BWP, a CFR can be configured for MBS. In current TS 38.213, as first part highlighted in red, if *cfr-ConfigMulticast* does not include *locationAndBandwidthMulticast*, the MBS frequency resource is the active DL BWP. However, the agreement is the bandwidth and location of MBS frequency resource should be equal to its associated DL BWP if *cfr-ConfigMulticast* does not include *locationAndBandwidthMulticast.* It is irrelevant to which DL BWP is activated. In addition, the current description seems meaning that the frequency resource of all the 4 CFRs is the active DL BWP if the CFR frequency resource is not configured.   |  | | --- | | A UE can be configured, per DL BWP by *cfr-ConfigMulticast*, an MBS frequency resource within the DL BWP for PDCCH and PDSCH receptions [4, TS 38.211]. If *cfr-ConfigMulticast* does not include *locationAndBandwidthMulticast*, the MBS frequency resource is the active DL BWP. The UE is not required to simultaneously receive PDSCHs on two serving cells. In clauses referring to a higher layer parameter value provided by *PDCCH-Config* or *PDSCH-Config* or *SPS-Config* for a DL BWP, when applicable a corresponding higher layer parameter value for multicast PDCCH, PDSCH, or SPS PDSCH receptions is provided as described in [12, TS 38.331]. |  |  | | --- | | **Agreement**  If *locationAndBandwidth-Multicast* is not configured in a *cfr-Config-Multicast*, the default value is the *locationAndBandwidth* of the DL BWP in which the *cfr-Config-Multicast* is configured. |   Regarding the simultaneous reception PDSCHs for MBS, it was agreed that a UE can only receive PDSCH for MBS on one serving cell. It has been captured in TS 38.331 as below, where *cfr-ConfigMulticast* can only be configured within one serving cell. So, it is impossible for a UE to simultaneously receive PDSCHs for MBS on two serving cells. The description in TS 38.213 seems redundant.   |  | | --- | | ***cfr-ConfigMulticast***  UE specific common frequency resource configuration for MBS multicast for one dedicated BWP. This field can be configured within at most one serving cell. | | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Delete ‘active’ and ‘The UE is not required to simultaneously receive PDSCHs on two serving cells.’ | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Incorrect definition on bandwidth and location of the MBS frequency resource in case that *cfr-ConfigMulticast* does not include *locationAndBandwidthMulticast.* | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 18 | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | **Isolated impact analysis:**  This CR is based on the RAN1 common understanding. | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | This is the first version for this CR. | | | | | | | | |

## **Multicast Broadcast Services**

<Unchanged parts are omitted>

A UE can be configured, per DL BWP by *cfr-ConfigMulticast*, an MBS frequency resource within the DL BWP for PDCCH and PDSCH receptions [4, TS 38.211]. If *cfr-ConfigMulticast* does not include *locationAndBandwidthMulticast*, the MBS frequency resource is the ~~active~~ DL BWP. ~~The UE is not required to simultaneously receive PDSCHs on two serving cells.~~ In clauses referring to a higher layer parameter value provided by *PDCCH-Config* or *PDSCH-Config* or *SPS-Config* for a DL BWP, when applicable a corresponding higher layer parameter value for multicast PDCCH, PDSCH, or SPS PDSCH receptions is provided as described in [12, TS 38.331].

<Unchanged parts are omitted>