**3GPP TSG RAN WG1 #113 R1-230xxxx**

**Incheon, Korea, May 22nd – May 26th, 2023**

**Agenda Item: 9.9**

**Source: CATT**

**Title: Discussion on RAN2 LS reply on unchanged PCI**

**Document for: Discussion and Decision**

# Introduction

RAN1 has received one LS from RAN2 about the unchanged PCI scenario in NTN [1]. With this LS, RAN2 informed the progress on unchanged PCI and ask for the reply from RAN1 on hard satellite switching (non-overlapping satellite coverage at switching time) and soft satellite switching (overlapping satellite coverage at switching time).

|  |
| --- |
| **To** **RAN1****ACTION:** RAN2 kindly requests RAN1 to take into account the above agreement on hard satellite switching without PCI change and provide feedback if RAN1 identifies any major technical issues, and also provide feedback on the feasibility to support soft satellite switching without PCI change. |

# Discussion

##  First question

**Q1: Is there any technical issue from RAN1 perspective on hard satellite switching without PCI change?**

**Moderator observations:**

From the companies’ contributions [2]-[9], for hard satellite switching, UE can switch to target satellite based on existed procedure. There is no technical issue identified from RAN1 perspective.

Companies are encouraged to provide the answers for above question and the conclusion is expected to derive based on company feedback.

|  |  |
| --- | --- |
| **Company** | **Comment** |
| **CMCC** | No. we do not think there is any technical issue for the hard satellite switching without PCI change. Though there is a time gap without connection during the switching, it could be solved by using legacy mechanism, such as beam failure recovery. In addition, with the notification to re-acquire DL/UL synchronization with the serving cell, as mentioned in the LS, UE can access to the upcoming satellite without any issue.So we see no technical issue for this problem. |
|  |  |
|  |  |
|  |  |
|  |  |

## Second question

The second question is about that RAN2 asked for the feasibility check for soft satellite switching without PCI change. Then for the second question, RAN1 is responsible to feed back the feasibility of soft satellite switching for earth fixed cell case.

**Moderator observations:**

Based on the companies’ contributions [2]-[9], there are some discussions on technical issues from RAN1 aspects. VIVO and OPPO raised one issue that there is the interference between signals from 2 different satellites. CMCC thinks there are possible PCI collision and interference issue for two satellites, but they can be resolved by the implementation, which is supported by the ZTE，Huawei and CATT. In addition, CATT, CMCC and Huawei proposed that UE is required to connect only one satellite in soft satellite switching.

In order to make it clear for technical issues, more detailed discussions are needed. RAN1 needs to identity what is issue and if it can be resolved by the implementation or specification enhancement is needed.

**Q2.1: is there any issues identified from RAN1 perspective on soft satellite switching without PCI change?**

 **[If yes, please list possible issues]**

Companies are encouraged to provide the answers for above question and conclusion are expected to derive based on company feedback.

|  |  |
| --- | --- |
| **Company** | **Comment** |
| **CMCC** | No. As we mentioned in our contribution, the PCI collision and the interference between two satellite with unchanged PCI, they could be solved through implementation such as sending different SSB with same PCI but different indexes and UE scheduled separately.  |
|  |  |
|  |  |
|  |  |

**Q2.2: if the answer for Q2.1 is yes, whether the issues can be resolved by implementation or need RAN1 specification enhancement? Other critical comment can be also raised.**

Companies are encouraged to provide the answers for above question and conclusion are expected to derive based on company feedback.

|  |  |
| --- | --- |
| **Company** | **Comment** |
|  |  |
|  |  |
|  |  |
|  |  |

# References

1. R2-2304273, RAN2, LS on unchanged PCI
2. R1-2304449 Discussion on RAN2 LS on unchanged PCI vivo
3. R1-2304756 Discussion on RAN2 LS reply on unchanged PCI CATT
4. R1-2304757 Draft reply LS to RAN2 on unchanged PCI CATT
5. R1-2305075 Discussion on RAN2 LS on unchanged PCI CMCC
6. R1-2305924 Discussion on LS on unchanged PCI Huawei, HiSilicon
7. R1-2305440 Discussion RAN2 LS on unchanged PCI OPPO
8. R1-2305441 Draft reply LS on unchanged PCI OPPO
9. R1-2305565 Discussion on LS on the unchanged PCI ZTE

# Appendix

## RAN2 agreement

In RAN2 #121bis meeting, RAN2 has made the following agreements：

Agreements:

1. In quasi-earth fixed cell case, for hard satellite switch in the same SSB frequency and same gNB (no key change), satellite switching without PCI changing (not requiring L3 mobility) is supported, unless major technical issues are identified by RAN1 (as usual RAN2 will aim at minimizing the specification impact so that it fits in Rel-18)
2. Remove the part in brackets “as usual RAN2 will aim at minimizing the specification impact so that it fits in Rel-18” in the LS to RAN1. The action to RAN1 will also ask for feedback for the hard satellite switch (not only the soft satellite switch case), e.g. action to RAN1 is to see if there are any major technical issues (as in the agreement).

## Companies’ proposals and observations

|  |  |  |
| --- | --- | --- |
| Contributions number  | Company  | Proposal and observations |
| R1-2304449 | VIVO | ***Observations 1 to 2:**** ***Soft satellite switching would introduce interference between signals from 2 different satellites and it’s hard to introduce additional mechanism to mitigate the interference.***
* ***Hard satellite switching can be supported without any RAN1 impact.***

***Proposal 1:**** ***RAN1 sends an LS reply to RAN2 based on the draft reply provided in Table 1.***
 |
| R1-2305075 | CMCC | **Observation 1:****Whether hard satellite switching or soft satellite switching is used is more dependent on the deployment of satellites.****Observation 2:****With the ephemeris information of new satellite, UE can access to the new satellite reusing the legacy mechanisms in the hard satellite switching.****Observation 3:****Both satellites can be observed by UE in the soft satellite switching. Connecting both satellites and compensating the transmission delay and frequency drift from two satellites will increase UE complexity tremendously.****Observation 4:*** **The PCI collision issue can be solved through grouping the SSBs to two sets and different satellite can transmit different set of SSBs, which is an implementation solution.**
* **Or the same SSBs can be transmitted by the two satellites, but different CSI-RS/TRS can be transmitted through each satellite. UE can connect the satellite following one SSB with specific delay and frequency drift.**

**Proposal 1:****From RAN1’s perspective, no major technical issue is observed for the hard satellite switching without PCI change.** **Proposal 2:****In the soft satellite switching, only UE connecting to one satellite should be discussed.** **Proposal 3:****The PCI collision issue in soft satellite switching can be solved through implementation.****Proposal 4:****The ephemeris of two satellites in soft switching can be informed to UE. This can be realized through implementation or discussed by other working groups** **Proposal 5:****The interference between the UEs under different satellites in the soft satellite switch can be solved though the scheduling of gNB.** **Proposal 6:****From RAN1’s perspective, no major technical issue for soft satellite switching without PCI change is observed. The interference issue can be solved through scheduling of gNB.**  |
| R1-2305440 | OPPO | **Proposal 1: For hard satellite switching, it is feasible as long as the UE can determine when to perform DL/UL synchronization to the upcoming satellite.****Proposal 2: For soft satellite switching, there are many issues that may cause interference issue, UE uplink synchronization issue, and ambiguous applicable ephemeris information issue. Thus, it seems not feasible.**  |
| R1-2305565 | ZTE | ***Observation 1:*** *Due to the different location of satellite which provide the same coverage with unchanged PCI, the DL synchronization procedure (e.g., monitoring the DL signal) and updates of UL timing (e.g., re-acquisition SIB for satellite ephemeris, common TA parameters, etc), should be implemented at UE side.****Proposal 1:*** *For the hard switching, it’s feasible from RAN1 perspective to support satellite switching without PCI changing.****Proposal 2:*** *For the soft switching, it’s feasible from RAN1 perspective support satellite switching without PCI changing. And same enhancement for hard switching can be considered.* |
| R1-2305924 | Huawei | ***Observation 1: From RAN1 perspective, there is no issue identified to support hard switching.******Observation 2: The gNB can mitigate the interference between signals of the two satellites by scheduling and transmitting different SSBs in SS burst from different satellites.******Observation 3: UE does not need to maintain the timing and frequency synchronization simultaneously with two satellites, considering only one satellite is used for the UE on a time occasion in the overlapped coverage.*** ***Proposal 1: Inform RAN2 that hard switching is feasible from RAN1 perspective.******Proposal 2: RAN1 informs RAN2 that interference could happen between the signals relayed by the source satellite and the destination satellite, however, it is feasible to resolve/mitigate the interference issue from RAN1 perspective.*** |
| R1-2304756 | CATT | **Observation 1: Inter-satellite coordination for same gNB for PCI unchanged usage is easily implemented.** **Observation 2: The time gap length of signal interruption between two adjacent satellites is up to network implementation and propagation delay, which is less than 10ms in most of cases from UE reception point of view.** **Observation 3: In order to help UE to fast access the upcoming satellite, common TA and ephemeris information can be informed to UE before satellite switching.****Observation 4: Connecting two satellites simultaneously for signal transmission will increase UE complexity.** **Observation 5: When same PCI is used for two adjacent satellites, there exists possible interference for two satellites in DL and UL.** **Observation 6: With resource separation for two neighboring satellites, the interference issue can be resolved through network implementation. For cell specific signal and resource allocation including SSB, SIB and PRACH, TDM based resource isolation can be used for two satellites. For UE specific signal and resource allocation, FDM based resource isolation can be used.****Proposal 1: From RAN1 perspective, no major technical issue is observed for hard satellite switching on unchanged PCI scenario.** **Proposal 2: For sake of UE implementation simplicity, UE can connect to only one satellite during soft satellite switching period.****Proposal 3: From RAN1 perspective, with proper resource coordination between serving satellite and upcoming satellite and no spec change, soft satellite switching without PCI change is feasible.** |