3GPP TSG-RAN WG2 Meeting #109-e R2-200xxxx

Electronic Meeting, 24th February – 6th March 2020

Agenda: x.x.x

Source: Nokia, LG, Ericsson, ZTE

Title: Potential easies II

Document for: Discussion, Decision

# 1 Introduction

This document is to kick-off the following email discussion:

\* **[AT109e][006][NR15] Potential easies II (Nokia, LG, Ericsson, ZTE)**

      Scope: Treat the documents R2-2000858, R2-2000859, R2-2000353, R2-2000879, R2-2000880, R2-2001612

      Intended outcome: Agreed CRs

      Deadline: Feb 27 1200 CET

# 2 Discussion

## 2.1 R2-2000858, SSB-ToMeasure related clarification

|  |
| --- |
| R2-2000858 |
| COMPANY | COMMENT |
|   |   |
|   |   |
|   |   |

## 2.2 R2-2000859, SSB-ToMeasure related clarification (38.331)

|  |
| --- |
| R2-2000859 |
| COMPANY | COMMENT |
|   |   |
|   |   |
|   |   |

## 2.3 R2-2000353, Clarification on the PLMN-IdentityInfoList

|  |
| --- |
| R2-2000353 |
| COMPANY | COMMENT |
|  Samsung |  Agree with the intention of the CR that there should not be duplicated PLMN entry. The ASN.1 for PLMN is as follows:plmn-IdentityList                   PLMN-IdentityInfoList,PLMN-IdentityInfoList ::=               SEQUENCE (SIZE (1..maxPLMN)) OF PLMN-IdentityInfoPLMN-IdentityInfo ::=                   SEQUENCE {    plmn-IdentityList                       SEQUENCE (SIZE (1..maxPLMN)) OF PLMN-Identity,The ASN.1 provides the flexibility to include PLMN identities in the lower plmn-IdentityList:1. Only one entry in the  PLMN-IdentityInfo. ZTE CR clarifies that such entry should not be duplicated.
2. More than one PLMN identities in the  PLMN-IdentityInfo, when the TAC, CI and cellreservedforoperatoruse fields are coordinated to be the same for the PLMNs.

In our understanding regardless of how the PLMN is signalled, it should be only one entry.  On the wording in the CR we prefer “A given PLMN identity is listed only once in PLMN-IdentityInfo” |
|  Ericsson | We agree with the intention of the CR, and comments provided by Samsung above. We would like to propose a following wording: “A PLMN-identity can be included only once, and in only one entry of the *PLMN-IdentityInfoList*”  to more indicated more clearly that a PLMN identity can only be included once (in this list of lists). |
|   |   |

## 2.4 R2-2000879, Correction on p-maxNR-FR1 for NE-DC

|  |
| --- |
| R2-2000879 |
| COMPANY | COMMENT |
|   |   |
|   |   |
|   |   |

## 2.5 R2-2000880, Correction on SFTD frequency list in INM

|  |
| --- |
| R2-2000880 |
| COMPANY | COMMENT |
|   |   |
|   |   |
|   |   |

## 2.6 R2-2001612, Correction on handover preparation message

|  |
| --- |
| R2-2001612 |
| COMPANY | COMMENT |
|   |   |
|   |   |
|   |   |

# 3 Conclusion