3GPP TSG-RAN WG2 Meeting #109-e R2-200xxxx

Electronic Meeting, 24th February – 6th March 2020

Agenda: x.x.x

Source: Nokia, LG, Ericsson, ZTE

Title: Potential easies II

Document for: Discussion, Decision

# 1 Introduction

This document is to kick-off the following email discussion:

 **[AT109e][006][NR15] Potential easies II (Nokia, LG, Ericsson, ZTE)**

      Scope: Treat the documents R2-2000858, R2-2000859, R2-2000353, R2-2000879, R2-2000880, R2-2001612

      Intended outcome: Agreed CRs

      Deadline: Feb 27 1200 CET

# 2 Discussion

## 2.1 R2-2000858, SSB-ToMeasure related clarification

|  |
| --- |
| R2-2000858 |
| COMPANY | COMMENT |
|  ZTE | We agree with the observations in this contribution. And we think this should already be aligned with UE’s current implementation.  |
|  CATT |  We also agree with the observations.  |
|  NTT DOCOMO | Agree on observations/proposals.  |
| Ericsson | Agree on observations/proposals |
|  |  |
|  Intel | Agree. |

## 2.2 R2-2000859, SSB-ToMeasure related clarification (38.331)

|  |
| --- |
| R2-2000859 |
| COMPANY | COMMENT |
|  ZTE | We understand this was discussed/clarified last meeting, in our opinion, as long as all companies have the same understanding, it would be ok with current specification. But we are also ok if companies want to make is more clear in spec, and we suggest the following rewording:The IE SSB-ToMeasure is used to configure a pattern of SSBs. SSB-ToMeasure is based on the absolute SSB-Indexes, not the position ~~with~~within SMTC window. |
|  CATT |  We are ok to make this clear in the spec, and we slightly prefer ZTE’s suggested wording. |
|  NTT DOCOMO |  O.K with the change proposed by ZTE. |
| Ericsson | In the last meeting we had the following agreement:* RAN2 confirms that the SSB-ToMeasure is based on the absolute SSBIndexes.

According to this, we brough a CR that was not agreed. Therefore, we believe current specification seems ok (i.e., no changed needed). |
| Intel | We are OK to clarify as proposed. |

## 2.3 R2-2000353, Clarification on the PLMN-IdentityInfoList

|  |
| --- |
| R2-2000353 |
| COMPANY | COMMENT |
|  Samsung |  Agree with the intention of the CR that there should not be duplicated PLMN entry. The ASN.1 for PLMN is as follows:plmn-IdentityList                   PLMN-IdentityInfoList,PLMN-IdentityInfoList ::=               SEQUENCE (SIZE (1..maxPLMN)) OF PLMN-IdentityInfoPLMN-IdentityInfo ::=                   SEQUENCE {    plmn-IdentityList                       SEQUENCE (SIZE (1..maxPLMN)) OF PLMN-Identity,The ASN.1 provides the flexibility to include PLMN identities in the lower plmn-IdentityList:1. Only one entry in the  PLMN-IdentityInfo. ZTE CR clarifies that such entry should not be duplicated.
2. More than one PLMN identities in the  PLMN-IdentityInfo, when the TAC, CI and cellreservedforoperatoruse fields are coordinated to be the same for the PLMNs.

In our understanding regardless of how the PLMN is signalled, it should be only one entry.  On the wording in the CR we prefer “A given PLMN identity is listed only once in PLMN-IdentityInfo” |
|  Ericsson | We agree with the intention of the CR, and comments provided by Samsung above. We would like to propose a following wording: “A PLMN-identity can be included only once, and in only one entry of the *PLMN-IdentityInfoList*”  to more indicated more clearly that a PLMN identity can only be included once (in this list of lists). |
|  CATT |  We agree with the intention of the CR. And for the wording, we think Ericsson’s suggestion is clearer. |
| NTT DOCOMO | Agree on the intention and text proposed by Ericsson. |
| Intel | While we agree with the intention of the CR, we didn’t think there was a risk of wrong configuration in real networks (suspect this topics came about in the context of NPN). We are OK to clarify as suggested by Ericsson if other companies feel it is essential. |

## 2.4 R2-2000879, Correction on p-maxNR-FR1 for NE-DC

|  |
| --- |
| R2-2000879 |
| COMPANY | COMMENT |
|  ZTE |  We are in general OK with this CR. Similar to the field description of p-maxEUTRA, we perfer to add the same sentence, so it is clear the field can be reused in NE-DC.

|  |
| --- |
| ***p-maxEUTRA***Indicates the maximum total transmit power to be used by the UE in the E-UTRA cell group (see TS 36.104 [33]). This field is used in (NG)EN-DC and NE-DC. |
| ***p-maxNR-FR1***Indicates the maximum total transmit power to be used by the UE in the NR cell group across all serving cells in frequency range 1 (FR1) (see TS 38.104 [12]). The field is used in (NG)EN-DC and NE-DC. |

 |
|  CATT |  We agree with the intention of the CR. And we think ZTE’s suggested wording is clearer. |
|  NTT DOCOMO |  Agree on the intention and text proposed by ZTE. |
|  Intel | We agree with the correction. |

## 2.5 R2-2000880, Correction on SFTD frequency list in INM

|  |
| --- |
| R2-2000880 |
| COMPANY | COMMENT |
|  ZTE |  We are OK with this CR. |
|  CATT |  We are OK with this CR. |
|  NTT DOCOMO |  Agree on the CR to be in-line with measResultCellSFTD(-EUTRA). |
|  Intel |  Agree with the intention. But it may not be backward compatibility and should be checked. |

## 2.6 R2-2001612, Correction on handover preparation message

|  |
| --- |
| R2-2001612 |
| COMPANY | COMMENT |
|  ZTE | We agree with the intention of the CR. But in our opinion, LTE RETRIEVE UE CONTEXT is supported in RAN3 since Rel-13. So it is not a release 15 issue.We perfer to capture it in the Rapporteur’s CR. |
|  CATT |  For re-establishment case, context retrieval is already supported from Rel-13. So we don’t think this CR is essential for Rel-15.  |
|  NTT DOCOMO |  Same view as mentioned above. |
| Ericsson | Agree with ZTE proposal. |
| Intel | Agree with the intent and ZTE suggestion to include in rapporteur CR. |

# 3 Conclusion