3GPP TSG-RAN WG2 Meeting #109-e R2-200xxxx

Electronic Meeting, 24th February – 6th March 2020

Agenda: 5.4.3

Source: Intel Corporation

Title: [AT109e][009][NR15] Miscellaneous Corr UE cap (Intel)

Document for: Discussion, Decision

# 1 Introduction

This document is a placeholder for collecting comments from the Misc Corrections to the UE capabilities to 38.306. The Spec rapporteur plans to update/edit/remove based on the comments and also as noted below, potential additions/changes can be made to the CR based on the eMeeting discussion.

* [AT109e][009][NR15] Miscellaneous Corr UE cap (Intel)

Scope: Treat the CR above, items may be added to this CR during the meeting

Intended outcome: Agreed CR

Deadline: Mar 5 1200 CET

# 2 List of TDocs

Companies are invited to give their views on the below CR:

R2-2002073 Miscellaneous Corrections to UE capability parameters Intel Corporation, Lenovo, Motorola Mobility, NTT DOCOMO, INC., Samsung, Qualcomm Incorporated, Ericsson  CR Rel-15 38.306 15.8.0 0255 1 F NR\_newRAT-Core

## R2-2002073

|  |  |
| --- | --- |
| **Company** | **Views** |
| Huawei | For srs-SwitchingTimeNR and srs-SwitchingTimeEUTRA, we think “FD“ in Per column is correct, this capability is “per band pair“ but we don’t have this kind of level, so we used “FD“, per band is not accurate. Besides, in 38.306 spec, we provide the description for fields begin with lowercase letter, so I am not sure if it’s ok to add description for “SRS-SwitchingTimeNR“ and “SRS-SwitchingTimeEUTRA“.  For srs-TxSwitch, in our view, previous “per BC“ is correct. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 3 Conclusion

To be added