**3GPP TSG-RAN2 Meeting #109-e *R2-2002158***

**Online, 2020-02-24 - 2020-03-06**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **36.306** | **CR** | **1732** | **rev** | **1** | **Current version:** | **15.7.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Introduction of DL RRC segmentation |
|  |  |
| ***Source to WG:*** | Ericsson, Deutsche Telekom, Vodafone, AT&T, Apple, Qualcomm Incorporated, OPPO, KT, Turkcell, Verizon |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | TEI16 |  | ***Date:*** | 2020-02-27 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | This CR introduce RRC segmentation possibilities in downlink, for *RRCConnectionReconfiguration* and *RRCConnectionResume* downlink messages. |
|  |  |
| ***Summary of change:*** | Adding UE capability indication for RRC Segmentation of downlink messages. |
|  |  |
| ***Consequences if not approved:*** | RRC Segmentation for *RRCConnectionResume and RRCConnectionReconfiguration* is not supported. |
|  |  |
| ***Clauses affected:*** | 4.3.8.x (New) |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 36.300 CR 1258TS 36.331 CR 4200TS 38.300 CR 0187TS 38.306 CR 0243TS 38.331 CR 1465 |
| ***affected:*** |  | **X** |  Test specifications |  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

### 4.3.8 General parameters

#### 4.3.8.1 *accessStratumRelease*

This field defines the release of the E-UTRA layer 1, 2, and 3 specifications supported by the UE e.g. Rel-8, Rel-9, etc.

#### 4.3.8.1A *accessStratumRelease-r13*

This field defines the release of the E-UTRA layer 1, 2, and 3 specifications supported by the UE e.g. Rel-13, Rel-14, etc. This field is only applicable for UEs of any *ue-Category-NB*.

#### 4.3.8.2 *deviceType*

This field defines whether the device does not benefit from NW-based battery consumption optimisation.

#### 4.3.8.3 Void

#### 4.3.8.4 Void

#### 4.3.8.5 *multipleDRB-r13*

This field defines whether the UE supports multiple DRBs. This field is only applicable if the UE supports S1-U data transfer or User plane CIoT EPS Optimisation, as defined in TS 24.301 [28] and any *ue-Category-NB*. If a UE of this release supports multiple DRBs, the UE shall support two simultaneous DRBs.

#### 4.3.8.6 Void

#### 4.3.8.7 *earlyData-UP-r15*

This field defines whether the UE supports EDT for User Plane CIoT EPS optimizations for FDD, as defined in TS 24.301 [28]. This feature is only applicable if the UE supports *ce-ModeA-r13* or if the UE supports any *ue-Category-NB*.

#### 4.3.8.8 void

#### 4.3.8.9 *extendedNumberOfDRBs-r15*

This field defines whether the UE supports up to 15 DRBs. The UE shall support any combination of RLC AM and RLC UM entities for the configured DRBs. A UE that supports *extendedNumberOfDRBs-r15* shall also support the extended LCID as specified in TS 36.321 [4].

#### 4.3.8.10 *reducedCP-Latency-r15*

This field defines whether the UE supports reduced control plane latency as defined in TS 36.213 [22] and TS 36.331 [5].

#### 4.3.8.x *dl-DedicatedMessageSegmentation-r16*

Indicates whether the UE supports reception of segmented DL RRC messages.