**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** | **1** | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | RAN1 recently observed the following limitations on CSI-RS capabilities:Problem 1: Limitation of active CSI-RS ports/resources in a slot;TS 38.214, sub-clause 5.2.1.6 defines the active CSI-RS ports/resources as shown below.- *In any slot, the UE is not expected to have more active CSI-RS ports or active CSI-RS resources than reported as capability.*The “capability” in this sentence corresponds to the following triplet defined in *SupportedCSI-RS-Resource*:- *maxNumberTxPortsPerResource* (i.e. Max. number of Tx ports in a resource);- *maxNumberResourcesPerBand* (i.e. Max. number of resources across all CCs within a band simultaneously);- *totalNumberTxPortsPerBand* (i.e. Total number of Tx ports across all CCs within a band simultaneously).In case of CA, the definition turns out that the UE needs to support these max/total values for each band in the band combination, in any slots. Given that the triplet is defined per band outside the band combination signalling, the UE may not be able to support the triplet as it is for each band, due to the limitation of total processing capabilities. In this case, the UE may have to report the conservative values for the triplet, which is applicable to all supported band combinations. If the active CSI-RS ports/resources were configured via a TDM manner, i.e. across different slots, the UE would be able to report the higher values than the legacy triplet.Problem 2: Lack of overall capabilities per codebook type.For the feature group 2-33 (CSI-RS and CSI-IM reception for CSI feedback), the following component #4 and #5 were introduced to limit the total capability across all CCs per band combination:- *maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC* (i.e. Max. number of simultaneous CSI-RS resources in active BWPs across all CCs);- *totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC* (i.e. Total number of CSI-RS ports in simultaneous CSI-RS resources in active BWPs across all CCs).These two capabilities are defined as common to all codebook types. In other words, the UE may have to report the conservative values supported for all codebook types. if these capabilities were defined per codebook type, the UE would be able to report the optimised value for each codebook type.RAN2 is asked to extend the capability signalling to resolve the aforementioned problems as in [R2-1916482](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_108/Docs/R2-1916482.zip). |
|  |  |
| ***Summary of change:*** | For Problem 1:- A UE can report another triplet to indicate the values supported for the TDM case.- Another triplet is reported for each codebook type per band (i.e. *MIMO- ParametersPerBand*).For Problem 2:- For the TDM case, the UE can report another values of: 1) Max. number of simultaneous CSI-RS resources in active BWPs across all CCs; 2) Total number of CSI-RS ports in simultaneous CSI-RS resources in active BWPs across all CCs.- A UE can report a pairs of 1) and 2) for each codebook type per UE.- Per supported band combination, the UE can indicate supported the set of resources amongst the per-UE signalling. |
|  |  |
| ***Consequences if not approved:*** | The UE may have to report the conservative CSI-RS capabilities, according to the limitation explained in the reason for change. |
|  |  |
| ***Clauses affected:*** | 6.3.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **X** |  |  Other core specifications  | TS 38.306 CR 0237 |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

### 6.3.3 UE capability information elements

#### – *AccessStratumRelease*

The IE *AccessStratumRelease* indicates the release supported by the UE.

*AccessStratumRelease* information element

-- ASN1START

-- TAG-ACCESSSTRATUMRELEASE-START

AccessStratumRelease ::= ENUMERATED {

 rel15, spare7, spare6, spare5, spare4, spare3, spare2, spare1, ... }

-- TAG-ACCESSSTRATUMRELEASE-STOP

-- ASN1STOP

#### – *BandCombinationList*

The IE *BandCombinationList* contains a list of NR CA and/or MR-DC band combinations (also including DL only or UL only band).

*BandCombinationList* information element

-- ASN1START

-- TAG-BANDCOMBINATIONLIST-START

BandCombinationList ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination

BandCombinationList-v1540 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1540

BandCombinationList-v1550 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1550

BandCombinationList-v1560 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1560

BandCombinationList-v1570 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1570

BandCombinationList-v1580 ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v1580

BandCombinationList-v16xy ::= SEQUENCE (SIZE (1..maxBandComb)) OF BandCombination-v16xy

BandCombination ::= SEQUENCE {

 bandList SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters,

 featureSetCombination FeatureSetCombinationId,

 ca-ParametersEUTRA CA-ParametersEUTRA OPTIONAL,

 ca-ParametersNR CA-ParametersNR OPTIONAL,

 mrdc-Parameters MRDC-Parameters OPTIONAL,

 supportedBandwidthCombinationSet BIT STRING (SIZE (1..32)) OPTIONAL,

 powerClass-v1530 ENUMERATED {pc2} OPTIONAL

}

BandCombination-v1540::= SEQUENCE {

 bandList-v1540 SEQUENCE (SIZE (1..maxSimultaneousBands)) OF BandParameters-v1540,

 ca-ParametersNR-v1540 CA-ParametersNR-v1540 OPTIONAL

}

BandCombination-v1550 ::= SEQUENCE {

 ca-ParametersNR-v1550 CA-ParametersNR-v1550

}

BandCombination-v1560::= SEQUENCE {

 ne-DC-BC ENUMERATED {supported} OPTIONAL,

 ca-ParametersNRDC CA-ParametersNRDC OPTIONAL,

 ca-ParametersEUTRA-v1560 CA-ParametersEUTRA-v1560 OPTIONAL,

 ca-ParametersNR-v1560 CA-ParametersNR-v1560 OPTIONAL

}

BandCombination-v1570 ::= SEQUENCE {

 ca-ParametersEUTRA-v1570 CA-ParametersEUTRA-v1570

}

BandCombination-v1580 ::= SEQUENCE {

 mrdc-Parameters-v1580 MRDC-Parameters-v1580

}

BandCombination-v16xy ::= SEQUENCE {

 ca-ParametersNR-v16xy CA-ParametersNR-v16xy

}

BandParameters ::= CHOICE {

 eutra SEQUENCE {

 bandEUTRA FreqBandIndicatorEUTRA,

 ca-BandwidthClassDL-EUTRA CA-BandwidthClassEUTRA OPTIONAL,

 ca-BandwidthClassUL-EUTRA CA-BandwidthClassEUTRA OPTIONAL

 },

 nr SEQUENCE {

 bandNR FreqBandIndicatorNR,

 ca-BandwidthClassDL-NR CA-BandwidthClassNR OPTIONAL,

 ca-BandwidthClassUL-NR CA-BandwidthClassNR OPTIONAL

 }

}

BandParameters-v1540 ::= SEQUENCE {

 srs-CarrierSwitch CHOICE {

 nr SEQUENCE {

 srs-SwitchingTimesListNR SEQUENCE (SIZE (1..maxSimultaneousBands)) OF SRS-SwitchingTimeNR

 },

 eutra SEQUENCE {

 srs-SwitchingTimesListEUTRA SEQUENCE (SIZE (1..maxSimultaneousBands)) OF SRS-SwitchingTimeEUTRA

 }

 } OPTIONAL,

 srs-TxSwitch SEQUENCE {

 supportedSRS-TxPortSwitch ENUMERATED {t1r2, t1r4, t2r4, t1r4-t2r4, t1r1, t2r2, t4r4, notSupported},

 txSwitchImpactToRx INTEGER (1..32) OPTIONAL,

 txSwitchWithAnotherBand INTEGER (1..32) OPTIONAL

 } OPTIONAL

}

-- TAG-BANDCOMBINATIONLIST-STOP

-- ASN1STOP

|  |
| --- |
| *BandCombination* field descriptions |
| ***BandCombinationList-v1540, BandCombinationList-v1550, BandCombinationList-v1560, BandCombinationList-v1570, BandCombinationList-v1580, BandCombinationList-v16xy***The UE shall include the same number of entries, and listed in the same order, as in *BandCombinationList* (without suffix). |
| ***ca-ParametersNRDC***If the field is included for a band combination in the NR capability container, the field indicates support of NR-DC. Otherwise, the field is absent. |
| ***ne-DC-BC***If the field is included for a band combination in the MR-DC capability container, the field indicates support of NE-DC. Otherwise, the field is absent. |
| ***srs-SwitchingTimesListNR***Indicates, for a particular pair of NR bands, the RF retuning time when switching between a NR carrier corresponding to this band entry and another (PUSCH-less) NR carrier corresponding to the band entry in the order indicated below:- For the first NR band, the UE shall include the same number of entries for NR bands as in *bandList*, i.e. first entry corresponds to first NR band in *bandList* and so on,- For the second NR band, the UE shall include one entry less, i.e. first entry corresponds to the second NR band in *bandList* and so on- And so on |
| ***srs-SwitchingTimesListEUTRA***Indicates, for a particular pair of E-UTRA bands, the RF retuning time when switching between an E-UTRA carrier corresponding to this band entry and another (PUSCH-less) E-UTRA carrier corresponding to the band entry in the order indicated below:- For the first E-UTRA band, the UE shall include the same number of entries for E-UTRA bands as in *bandList,* i.e. first entry corresponds to first E-UTRA band in *bandList* and so on,- For the second E-UTRA band, the UE shall include one entry less, i.e. first entry corresponds to the second E-UTRA band in *bandList* and so on - And so on |

#### – *CA-BandwidthClassEUTRA*

The IE *CA-BandwidthClassEUTRA* indicates the E-UTRA CA bandwidth class as defined in TS 36.101 [22], table 5.6A-1.

*CA-BandwidthClassEUTRA* information element

-- ASN1START

-- TAG-CA-BANDWIDTHCLASSEUTRA-START

CA-BandwidthClassEUTRA ::= ENUMERATED {a, b, c, d, e, f, ...}

-- TAG-CA-BANDWIDTHCLASSEUTRA-STOP

-- ASN1STOP

#### – *CA-BandwidthClassNR*

The IE *CA-BandwidthClassNR* indicates the NR CA bandwidth class as defined in TS 38.101-1 [15], table 5.3A.5-1 and TS 38.101-2 [39], table 5.3A.4-1.

*CA-BandwidthClassNR* information element

-- ASN1START

-- TAG-CA-BANDWIDTHCLASSNR-START

CA-BandwidthClassNR ::= ENUMERATED {a, b, c, d, e, f, g, h, i, j, k, l, m, n, o, p, q, ...}

-- TAG-CA-BANDWIDTHCLASSNR-STOP

-- ASN1STOP

#### – *CA-ParametersEUTRA*

The IE *CA-ParametersEUTRA* contains the E-UTRA part of band combination parameters for a given MR-DC band combination.

NOTE: If additional E-UTRA band combination parameters are defined in TS 36.331 [10], which are supported for MR-DC, they will be defined here as well.

*CA-ParametersEUTRA* information element

-- ASN1START

-- TAG-CA-PARAMETERSEUTRA-START

CA-ParametersEUTRA ::= SEQUENCE {

 multipleTimingAdvance ENUMERATED {supported} OPTIONAL,

 simultaneousRx-Tx ENUMERATED {supported} OPTIONAL,

 supportedNAICS-2CRS-AP BIT STRING (SIZE (1..8)) OPTIONAL,

 additionalRx-Tx-PerformanceReq ENUMERATED {supported} OPTIONAL,

 ue-CA-PowerClass-N ENUMERATED {class2} OPTIONAL,

 supportedBandwidthCombinationSetEUTRA-v1530 BIT STRING (SIZE (1..32)) OPTIONAL,

 ...

}

CA-ParametersEUTRA-v1560 ::= SEQUENCE {

 fd-MIMO-TotalWeightedLayers INTEGER (2..128) OPTIONAL

}

CA-ParametersEUTRA-v1570 ::= SEQUENCE {

 dl-1024QAM-TotalWeightedLayers INTEGER (0..10) OPTIONAL

}

-- TAG-CA-PARAMETERSEUTRA-STOP

-- ASN1STOP

#### – *CA-ParametersNR*

The IE *CA-ParametersNR* contains carrier aggregation related capabilities that are defined per band combination.

*CA-ParametersNR* information element

-- ASN1START

-- TAG-CA-PARAMETERSNR-START

CA-ParametersNR ::= SEQUENCE {

 dummy ENUMERATED {supported} OPTIONAL,

 parallelTxSRS-PUCCH-PUSCH ENUMERATED {supported} OPTIONAL,

 parallelTxPRACH-SRS-PUCCH-PUSCH ENUMERATED {supported} OPTIONAL,

 simultaneousRxTxInterBandCA ENUMERATED {supported} OPTIONAL,

 simultaneousRxTxSUL ENUMERATED {supported} OPTIONAL,

 diffNumerologyAcrossPUCCH-Group ENUMERATED {supported} OPTIONAL,

 diffNumerologyWithinPUCCH-GroupSmallerSCS ENUMERATED {supported} OPTIONAL,

 supportedNumberTAG ENUMERATED {n2, n3, n4} OPTIONAL,

 ...

}

CA-ParametersNR-v1540 ::= SEQUENCE {

 simultaneousSRS-AssocCSI-RS-AllCC INTEGER (5..32) OPTIONAL,

 csi-RS-IM-ReceptionForFeedbackPerBandComb SEQUENCE {

 maxNumberSimultaneousNZP-CSI-RS-ActBWP-AllCC INTEGER (1..64) OPTIONAL,

 totalNumberPortsSimultaneousNZP-CSI-RS-ActBWP-AllCC INTEGER (2..256) OPTIONAL

 } OPTIONAL,

 simultaneousCSI-ReportsAllCC INTEGER (5..32) OPTIONAL,

 dualPA-Architecture ENUMERATED {supported} OPTIONAL

}

CA-ParametersNR-v1550 ::= SEQUENCE {

 dummy ENUMERATED {supported} OPTIONAL

}

CA-ParametersNR-v1560 ::= SEQUENCE {

 diffNumerologyWithinPUCCH-GroupLargerSCS ENUMERATED {supported} OPTIONAL

}

CA-ParametersNR-v16xy ::= SEQUENCE {

 codebookVariantsAllCC-Simultaneous-r16 SEQUENCE {

 fr1 INTEGER(0..19) OPTIONAL,

 fr2 INTEGER(0..19) OPTIONAL

 } OPTIONAL

}

-- TAG-CA-PARAMETERSNR-STOP

-- ASN1STOP

#### – CA-ParametersNRDC

The IE *CA-ParametersNRDC* contains dual connectivity related capabilities that are defined per band combination.

*CA-ParametersNRDC* information element

-- ASN1START

-- TAG-CA-PARAMETERS-NRDC-START

CA-ParametersNRDC ::= SEQUENCE {

 ca-ParametersNR-ForDC CA-ParametersNR OPTIONAL,

 ca-ParametersNR-ForDC-v1540 CA-ParametersNR-v1540 OPTIONAL,

 ca-ParametersNR-ForDC-v1550 CA-ParametersNR-v1550 OPTIONAL,

 ca-ParametersNR-ForDC-v1560 CA-ParametersNR-v1560 OPTIONAL,

 featureSetCombinationDC FeatureSetCombinationId OPTIONAL

}

-- TAG-CA-PARAMETERS-NRDC-STOP

-- ASN1STOP

|  |
| --- |
| *CA-ParametersNRDC* field descriptions |
| ***ca-ParametersNR-forDC (with and without suffix)***If this field is present for a band combination, it reports the UE capabilities when NR-DC is configured with the band combination. If no version of this field (i.e., with and without suffix) is present for a band combination, the *ca-ParametersNR* field versions (with and without suffix) in *BandCombination* are applicable to the UE configured with NR-DC for the band combination. |
| ***featureSetCombinationDC***If this field is present for a band combination, it reports the feature set combination supported for the band combination when NR-DC is configured. If this field is absent for a band combination, the *featureSetCombination* in *BandCombination* (without suffix) is applicable to the UE configured with NR-DC for the band combination. |

#### – *CodebookParameters*

The IE *CodebookParameters* is used to convey codebook related parameters.

*CodebookParameters* information element

-- ASN1START

-- TAG-CODEBOOKPARAMETERS-START

CodebookParameters ::= SEQUENCE {

 type1 SEQUENCE {

 singlePanel SEQUENCE {

 supportedCSI-RS-ResourceList SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources)) OF SupportedCSI-RS-Resource,

 modes ENUMERATED {mode1, mode1andMode2},

 maxNumberCSI-RS-PerResourceSet INTEGER (1..8)

 },

 multiPanel SEQUENCE {

 supportedCSI-RS-ResourceList SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources)) OF SupportedCSI-RS-Resource,

 modes ENUMERATED {mode1, mode2, both},

 nrofPanels ENUMERATED {n2, n4},

 maxNumberCSI-RS-PerResourceSet INTEGER (1..8)

 } OPTIONAL

 },

 type2 SEQUENCE {

 supportedCSI-RS-ResourceList SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources)) OF SupportedCSI-RS-Resource,

 parameterLx INTEGER (2..4),

 amplitudeScalingType ENUMERATED {wideband, widebandAndSubband},

 amplitudeSubsetRestriction ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 type2-PortSelection SEQUENCE {

 supportedCSI-RS-ResourceList SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources)) OF SupportedCSI-RS-Resource,

 parameterLx INTEGER (2..4),

 amplitudeScalingType ENUMERATED {wideband, widebandAndSubband}

 } OPTIONAL

}

SupportedCSI-RS-Resource ::= SEQUENCE {

 maxNumberTxPortsPerResource ENUMERATED {p2, p4, p8, p12, p16, p24, p32},

 maxNumberResourcesPerBand INTEGER (1..64),

 totalNumberTxPortsPerBand INTEGER (2..256)

}

CodebookParametersPerUE-r16 ::= SEQUENCE {

 configuredCSI-RS-ResourceListPerUE-r16 SEQUENCE {

 type1-SinglePanel-r16 SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources)) OF SupportedCSI-RS-Resource OPTIONAL,

 type1-MultiPanel-r16 SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources)) OF SupportedCSI-RS-Resource OPTIONAL,

 type2-r16 SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources)) OF SupportedCSI-RS-Resource OPTIONAL,

 type2-PortSelection-r16 SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources)) OF SupportedCSI-RS-Resource OPTIONAL

 } OPTIONAL

}

CodebookParametersPerBand-r16 ::= SEQUENCE {

 configuredCSI-RS-ResourceListPerBand-r16 SEQUENCE {

 type1-SinglePanel-r16 SEQUENCE (SIZE (1..3)) OF INTEGER (0..6) OPTIONAL,

 type1-MultiPanel-r16 SEQUENCE (SIZE (1..3)) OF INTEGER (0..6) OPTIONAL,

 type2-r16 SEQUENCE (SIZE (1..3)) OF INTEGER (0..6) OPTIONAL,

 type2-PortSelection-r16 SEQUENCE (SIZE (1..3)) OF INTEGER (0..6) OPTIONAL

 } OPTIONAL

}

CodebookVariantsList-r16 ::= SEQUENCE (SIZE (1..20)) OF CodebookVariants-r16

CodebookVariants-r16 ::= SEQUENCE {

type1-SinglePanel-r16 ResourcesAndPorts-r16 OPTIONAL,

type1-MultiPanel-r16 ResourcesAndPorts-r16 OPTIONAL,

type2-r16 ResourcesAndPorts-r16 OPTIONAL,

type2-PortSelection-r16 ResourcesAndPorts-r16 OPTIONAL

}

ResourcesAndPorts-r16 ::= SEQUENCE {

maxNumberResources-r16 INTEGER (1..64),

totalNumberTxPorts-r16 INTEGER (2..256)

}

-- TAG-CODEBOOKPARAMETERS-STOP

-- ASN1STOP

#### – *FeatureSetCombination*

The IE *FeatureSetCombination* is a two-dimensional matrix of *FeatureSet* entries.

Each *FeatureSetsPerBand* contains a list of feature sets applicable to the carrier(s) of one band entry of the associated band combination. Across the associated bands, the UE shall support the combination of *FeatureSets* at the same position in the *FeatureSetsPerBand*. All *FeatureSetsPerBand* in one *FeatureSetCombination* must have the same number of entries.

The number of *FeatureSetsPerBand* in the *FeatureSetCombination* must be equal to the number of band entries in an associated band combination. The first *FeatureSetPerBand* applies to the first band entry of the band combination, and so on.

Each *FeatureSet* contains either a pair of NR or E-UTRA feature set IDs for UL and DL.

In case of NR, the actual feature sets for UL and DL are defined in the *FeatureSets* IE and referred to from here by their ID, i.e., their position in the *featureSetsUplink* / *featureSetsDownlink* list in the FeatureSet IE.

In case of E-UTRA, the feature sets referred to from this list are defined in TS 36.331 [10] and conveyed as part of the *UE-EUTRA-Capability* container.

The *FeatureSetUplink* and *FeatureSetDownlink* referred to from the *FeatureSet* comprise, among other information, a set of *FeatureSetUplinkPerCC-Id:s* and *FeatureSetDownlinkPerCC-Id:s*. The number of these per-CC IDs determines the number of carriers that the UE is able to aggregate contiguously in frequency domain in the corresponding band. The number of carriers supported by the UE is also restricted by the bandwidth class indicated in the associated *BandCombination*, if present.

In feature set combinations the UE shall exclude entries for fallback combinations with same capabilities, since the network may anyway assume that the UE supports those.

NOTE 1: The UE may advertise fallback band-combinations in which it supports additional functionality explicitly in two ways: Either by setting FeatureSet IDs to zero (inter-band and intra-band non-contiguous fallback) and by reducing the number of FeatureSet-PerCC Ids in a Feature Set (intra-band contiguous fallback). Or by separate *BandCombination* entries with associated *FeatureSetCombinations*.

NOTE 2: The UE may advertise a *FeatureSetCombination* containing only fallback band combinations. That means, in a *FeatureSetCombination,* each group of *FeatureSets* across the bands may contain at least one pair of *FeatureSetUplinkId* and *FeatureSetDownlinkId* which is set to 0/0.

NOTE 3: The Network configures serving cell(s) and BWP(s) configuration to comply with capabilities derived from the combination of FeatureSets at the same position in the FeatureSetsPerBand, regardless of activated/deactivated serving cell(s) and BWP(s).

*FeatureSetCombination* information element

-- ASN1START

-- TAG-FEATURESETCOMBINATION-START

FeatureSetCombination ::= SEQUENCE (SIZE (1..maxSimultaneousBands)) OF FeatureSetsPerBand

FeatureSetsPerBand ::= SEQUENCE (SIZE (1..maxFeatureSetsPerBand)) OF FeatureSet

FeatureSet ::= CHOICE {

 eutra SEQUENCE {

 downlinkSetEUTRA FeatureSetEUTRA-DownlinkId,

 uplinkSetEUTRA FeatureSetEUTRA-UplinkId

 },

 nr SEQUENCE {

 downlinkSetNR FeatureSetDownlinkId,

 uplinkSetNR FeatureSetUplinkId

 }

}

-- TAG-FEATURESETCOMBINATION-STOP

-- ASN1STOP

#### – *FeatureSetCombinationId*

The IE *FeatureSetCombinationId* identifies a *FeatureSetCombination*. The *FeatureSetCombinationId* of a *FeatureSetCombination* is the position of the *FeatureSetCombination* in the featureSetCombinations list (in *UE-NR-Capability* or *UE-MRDC-Capability*). The *FeatureSetCombinationId* = 0 refers to the first entry in the *featureSetCombinations* list (in *UE-NR-Capability* or *UE-MRDC-Capability*).

NOTE: The *FeatureSetCombinationId* = 1024 is not used due to the maximum entry number of *featureSetCombinations*.

*FeatureSetCombinationId* information element

-- ASN1START

-- TAG-FEATURESETCOMBINATIONID-START

FeatureSetCombinationId ::= INTEGER (0.. maxFeatureSetCombinations)

-- TAG-FEATURESETCOMBINATIONID-STOP

-- ASN1STOP

#### – *FeatureSetDownlink*

The IE *FeatureSetDownlink* indicates a set of features that the UE supports on the carriers corresponding to one band entry in a band combination.

*FeatureSetDownlink* information element

-- ASN1START

-- TAG-FEATURESETDOWNLINK-START

FeatureSetDownlink ::= SEQUENCE {

 featureSetListPerDownlinkCC SEQUENCE (SIZE (1..maxNrofServingCells)) OF FeatureSetDownlinkPerCC-Id,

 intraBandFreqSeparationDL FreqSeparationClass OPTIONAL,

 scalingFactor ENUMERATED {f0p4, f0p75, f0p8} OPTIONAL,

 crossCarrierScheduling-OtherSCS ENUMERATED {supported} OPTIONAL,

 scellWithoutSSB ENUMERATED {supported} OPTIONAL,

 csi-RS-MeasSCellWithoutSSB ENUMERATED {supported} OPTIONAL,

 dummy1 ENUMERATED {supported} OPTIONAL,

 type1-3-CSS ENUMERATED {supported} OPTIONAL,

 pdcch-MonitoringAnyOccasions ENUMERATED {withoutDCI-Gap, withDCI-Gap} OPTIONAL,

 dummy2 ENUMERATED {supported} OPTIONAL,

 ue-SpecificUL-DL-Assignment ENUMERATED {supported} OPTIONAL,

 searchSpaceSharingCA-DL ENUMERATED {supported} OPTIONAL,

 timeDurationForQCL SEQUENCE {

 scs-60kHz ENUMERATED {s7, s14, s28} OPTIONAL,

 scs-120kHz ENUMERATED {s14, s28} OPTIONAL

 } OPTIONAL,

 pdsch-ProcessingType1-DifferentTB-PerSlot SEQUENCE {

 scs-15kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL,

 scs-30kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL,

 scs-60kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL,

 scs-120kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL

 } OPTIONAL,

 dummy3 DummyA OPTIONAL,

 dummy4 SEQUENCE (SIZE (1.. maxNrofCodebooks)) OF DummyB OPTIONAL,

 dummy5 SEQUENCE (SIZE (1.. maxNrofCodebooks)) OF DummyC OPTIONAL,

 dummy6 SEQUENCE (SIZE (1.. maxNrofCodebooks)) OF DummyD OPTIONAL,

 dummy7 SEQUENCE (SIZE (1.. maxNrofCodebooks)) OF DummyE OPTIONAL

}

FeatureSetDownlink-v1540 ::= SEQUENCE {

 oneFL-DMRS-TwoAdditionalDMRS-DL ENUMERATED {supported} OPTIONAL,

 additionalDMRS-DL-Alt ENUMERATED {supported} OPTIONAL,

 twoFL-DMRS-TwoAdditionalDMRS-DL ENUMERATED {supported} OPTIONAL,

 oneFL-DMRS-ThreeAdditionalDMRS-DL ENUMERATED {supported} OPTIONAL,

 pdcch-MonitoringAnyOccasionsWithSpanGap SEQUENCE {

 scs-15kHz ENUMERATED {set1, set2, set3} OPTIONAL,

 scs-30kHz ENUMERATED {set1, set2, set3} OPTIONAL,

 scs-60kHz ENUMERATED {set1, set2, set3} OPTIONAL,

 scs-120kHz ENUMERATED {set1, set2, set3} OPTIONAL

 } OPTIONAL,

 pdsch-SeparationWithGap ENUMERATED {supported} OPTIONAL,

 pdsch-ProcessingType2 SEQUENCE {

 scs-15kHz ProcessingParameters OPTIONAL,

 scs-30kHz ProcessingParameters OPTIONAL,

 scs-60kHz ProcessingParameters OPTIONAL

 } OPTIONAL,

 pdsch-ProcessingType2-Limited SEQUENCE {

 differentTB-PerSlot-SCS-30kHz ENUMERATED {upto1, upto2, upto4, upto7}

 } OPTIONAL,

 dl-MCS-TableAlt-DynamicIndication ENUMERATED {supported} OPTIONAL

}

DummyA ::= SEQUENCE {

 maxNumberNZP-CSI-RS-PerCC INTEGER (1..32),

 maxNumberPortsAcrossNZP-CSI-RS-PerCC ENUMERATED {p2, p4, p8, p12, p16, p24, p32, p40, p48, p56, p64, p72, p80,

 p88, p96, p104, p112, p120, p128, p136, p144, p152, p160, p168,

 p176, p184, p192, p200, p208, p216, p224, p232, p240, p248, p256},

 maxNumberCS-IM-PerCC ENUMERATED {n1, n2, n4, n8, n16, n32},

 maxNumberSimultaneousCSI-RS-ActBWP-AllCC ENUMERATED {n5, n6, n7, n8, n9, n10, n12, n14, n16, n18, n20, n22, n24, n26,

 n28, n30, n32, n34, n36, n38, n40, n42, n44, n46, n48, n50, n52,

 n54, n56, n58, n60, n62, n64},

 totalNumberPortsSimultaneousCSI-RS-ActBWP-AllCC ENUMERATED {p8, p12, p16, p24, p32, p40, p48, p56, p64, p72, p80,

 p88, p96, p104, p112, p120, p128, p136, p144, p152, p160, p168,

 p176, p184, p192, p200, p208, p216, p224, p232, p240, p248, p256}

}

DummyB ::= SEQUENCE {

 maxNumberTxPortsPerResource ENUMERATED {p2, p4, p8, p12, p16, p24, p32},

 maxNumberResources INTEGER (1..64),

 totalNumberTxPorts INTEGER (2..256),

 supportedCodebookMode ENUMERATED {mode1, mode1AndMode2},

 maxNumberCSI-RS-PerResourceSet INTEGER (1..8)

}

DummyC ::= SEQUENCE {

 maxNumberTxPortsPerResource ENUMERATED {p8, p16, p32},

 maxNumberResources INTEGER (1..64),

 totalNumberTxPorts INTEGER (2..256),

 supportedCodebookMode ENUMERATED {mode1, mode2, both},

 supportedNumberPanels ENUMERATED {n2, n4},

 maxNumberCSI-RS-PerResourceSet INTEGER (1..8)

}

DummyD ::= SEQUENCE {

 maxNumberTxPortsPerResource ENUMERATED {p4, p8, p12, p16, p24, p32},

 maxNumberResources INTEGER (1..64),

 totalNumberTxPorts INTEGER (2..256),

 parameterLx INTEGER (2..4),

 amplitudeScalingType ENUMERATED {wideband, widebandAndSubband},

 amplitudeSubsetRestriction ENUMERATED {supported} OPTIONAL,

 maxNumberCSI-RS-PerResourceSet INTEGER (1..8)

}

DummyE ::= SEQUENCE {

 maxNumberTxPortsPerResource ENUMERATED {p4, p8, p12, p16, p24, p32},

 maxNumberResources INTEGER (1..64),

 totalNumberTxPorts INTEGER (2..256),

 parameterLx INTEGER (2..4),

 amplitudeScalingType ENUMERATED {wideband, widebandAndSubband},

 maxNumberCSI-RS-PerResourceSet INTEGER (1..8)

}

-- TAG-FEATURESETDOWNLINK-STOP

-- ASN1STOP

|  |
| --- |
| *FeatureSetDownlink* field descriptions |
| ***crossCarrierScheduling-OtherSCS***The UE shall set this field to the same value as *crossCarrierScheduling-OtherSCS* in the associated *FeatureSetUplink* (if present). |
| ***featureSetListPerDownlinkCC***Indicates which features the UE supports on the individual DL carriers of the feature set (and hence of a band entry that refer to the feature set). The UE shall hence include at least as many *FeatureSetDownlinkPerCC-Id* in this list as the number of carriers it supports according to the *ca-BandwidthClassDL*, except if indicating additional functionality by reducing the number of *FeatureSetDownlinkPerCC-Id* in the feature set (see NOTE 1 in *FeatureSetCombination* IE description). The order of the elements in this list is not relevant, i.e., the network may configure any of the carriers in accordance with any of the *FeatureSetDownlinkPerCC-Id* in this list. |

#### – *FeatureSetDownlinkId*

The IE *FeatureSetDownlinkId* identifies a downlink feature set. The *FeatureSetDownlinkId* of a *FeatureSetDownlink* is the index position of the *FeatureSetDownlink* in the *featureSetsDownlink* list in the *FeatureSets* IE. The first element in that list is referred to by *FeatureSetDownlinkId* = 1. The *FeatureSetDownlinkId=0* is not used by an actual *FeatureSetDownlink* but means that the UE does not support a carrier in this band of a band combination.

*FeatureSetDownlinkId* information element

-- ASN1START

-- TAG-FEATURESETDOWNLINKID-START

FeatureSetDownlinkId ::= INTEGER (0..maxDownlinkFeatureSets)

-- TAG-FEATURESETDOWNLINKID-STOP

-- ASN1STOP

#### – *FeatureSetDownlinkPerCC*

The IE *FeatureSetDownlinkPerCC* indicates a set of features that the UE supports on the corresponding carrier of one band entry of a band combination.

*FeatureSetDownlinkPerCC* information element

-- ASN1START

-- TAG-FEATURESETDOWNLINKPERCC-START

FeatureSetDownlinkPerCC ::= SEQUENCE {

 supportedSubcarrierSpacingDL SubcarrierSpacing,

 supportedBandwidthDL SupportedBandwidth,

 channelBW-90mhz ENUMERATED {supported} OPTIONAL,

 maxNumberMIMO-LayersPDSCH MIMO-LayersDL OPTIONAL,

 supportedModulationOrderDL ModulationOrder OPTIONAL

}

-- TAG-FEATURESETDOWNLINKPERCC-STOP

-- ASN1STOP

#### – *FeatureSetDownlinkPerCC-Id*

The IE *FeatureSetDownlinkPerCC-Id* identifies a set of features applicable to one carrier of a feature set. The *FeatureSetDownlinkPerCC-Id* of a *FeatureSetDownlinkPerCC* is the index position of the *FeatureSetDownlinkPerCC* in the *featureSetsDownlinkPerCC*. The first element in the list is referred to by *FeatureSetDownlinkPerCC-Id* = 1, and so on.

*FeatureSetDownlinkPerCC-Id* information element

-- ASN1START

-- TAG-FEATURESETDOWNLINKPERCC-ID-START

FeatureSetDownlinkPerCC-Id ::= INTEGER (1..maxPerCC-FeatureSets)

-- TAG-FEATURESETDOWNLINKPERCC-ID-STOP

-- ASN1STOP

#### – *FeatureSetEUTRA-DownlinkId*

The IE *FeatureSetEUTRA-DownlinkId* identifies a downlink feature set in E-UTRA list (see TS 36.331 [10]. The first element in that list is referred to by *FeatureSetEUTRA-DownlinkId* = 1. The *FeatureSetEUTRA-DownlinkId=0* is used when the UE does not support a carrier in this band of a band combination.

*FeatureSetEUTRA-DownlinkId* information element

-- ASN1START

-- TAG-FEATURESETEUTRADOWNLINKID-START

FeatureSetEUTRA-DownlinkId ::= INTEGER (0..maxEUTRA-DL-FeatureSets)

-- TAG-FEATURESETEUTRADOWNLINKID-STOP

-- ASN1STOP

#### – *FeatureSetEUTRA-UplinkId*

The IE *FeatureSetEUTRA-UplinkId* identifies an uplink feature set in E-UTRA list (see TS 36.331 [10]. The first element in that list is referred to by *FeatureSetEUTRA-UplinkId* = 1. The *FeatureSetEUTRA-UplinkId* *=0* is used when the UE does not support a carrier in this band of a band combination.

*FeatureSetEUTRA-UplinkId* information element

-- ASN1START

-- TAG-FEATURESETEUTRAUPLINKID-START

FeatureSetEUTRA-UplinkId ::= INTEGER (0..maxEUTRA-UL-FeatureSets)

-- TAG-FEATURESETEUTRAUPLINKID-STOP

-- ASN1STOP

#### – *FeatureSets*

The IE *FeatureSets* is used to provide pools of downlink and uplink features sets. A *FeatureSetCombination* refers to the IDs of the feature set(s) that the UE supports in that *FeatureSetCombination*. The *BandCombination* entries in the *BandCombinationList* then indicate the ID of the *FeatureSetCombination* that the UE supports for that band combination.

The entries in the lists in this IE are identified by their index position. For example, the *FeatureSetUplinkPerCC-Id* = 4 identifies the 4th element in the *featureSetsUplinkPerCC* list.

NOTE: When feature sets (per CC) IEs require extension in future versions of the specification, new versions of the *FeatureSetDownlink*, *FeatureSetUplink*, *FeatureSets*, *FeatureSetDownlinkPerCC* and/or *FeatureSetUplinkPerCC* will be created and instantiated in corresponding new lists in the *FeatureSets* IE. For example, if new capability bits are to be added to the *FeatureSetDownlink*, they will instead be defined in a new *FeatureSetDownlink-rxy* which will be instantiated in a new *featureSetDownlinkList-rxy* list. If a UE indicates in a *FeatureSetCombination* that it supports the *FeatureSetDownlink* with ID #5, it implies that it supports both the features in *FeatureSetDownlink* #5 and *FeatureSetDownlink-rxy* #5 (if present). The number of entries in the new list(s) shall be the same as in the original list(s).

*FeatureSets* information element

-- ASN1START

-- TAG-FEATURESETS-START

FeatureSets ::= SEQUENCE {

 featureSetsDownlink SEQUENCE (SIZE (1..maxDownlinkFeatureSets)) OF FeatureSetDownlink OPTIONAL,

 featureSetsDownlinkPerCC SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetDownlinkPerCC OPTIONAL,

 featureSetsUplink SEQUENCE (SIZE (1..maxUplinkFeatureSets)) OF FeatureSetUplink OPTIONAL,

 featureSetsUplinkPerCC SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetUplinkPerCC OPTIONAL,

 ...,

 [[

 featureSetsDownlink-v1540 SEQUENCE (SIZE (1..maxDownlinkFeatureSets)) OF FeatureSetDownlink-v1540 OPTIONAL,

 featureSetsUplink-v1540 SEQUENCE (SIZE (1..maxUplinkFeatureSets)) OF FeatureSetUplink-v1540 OPTIONAL,

 featureSetsUplinkPerCC-v1540 SEQUENCE (SIZE (1..maxPerCC-FeatureSets)) OF FeatureSetUplinkPerCC-v1540 OPTIONAL

 ]]

}

-- TAG-FEATURESETS-STOP

-- ASN1STOP

#### – *FeatureSetUplink*

The IE *FeatureSetUplink* is used to indicate the features that the UE supports on the carriers corresponding to one band entry in a band combination.

*FeatureSetUplink* information element

-- ASN1START

-- TAG-FEATURESETUPLINK-START

FeatureSetUplink ::= SEQUENCE {

 featureSetListPerUplinkCC SEQUENCE (SIZE (1.. maxNrofServingCells)) OF FeatureSetUplinkPerCC-Id,

 scalingFactor ENUMERATED {f0p4, f0p75, f0p8} OPTIONAL,

 crossCarrierScheduling-OtherSCS ENUMERATED {supported} OPTIONAL,

 intraBandFreqSeparationUL FreqSeparationClass OPTIONAL,

 searchSpaceSharingCA-UL ENUMERATED {supported} OPTIONAL,

 dummy1 DummyI  OPTIONAL,

 supportedSRS-Resources SRS-Resources OPTIONAL,

 twoPUCCH-Group ENUMERATED {supported} OPTIONAL,

 dynamicSwitchSUL ENUMERATED {supported} OPTIONAL,

 simultaneousTxSUL-NonSUL ENUMERATED {supported} OPTIONAL,

 pusch-ProcessingType1-DifferentTB-PerSlot SEQUENCE {

 scs-15kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL,

 scs-30kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL,

 scs-60kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL,

 scs-120kHz ENUMERATED {upto2, upto4, upto7} OPTIONAL

 } OPTIONAL,

 dummy2 DummyF OPTIONAL

}

FeatureSetUplink-v1540 ::= SEQUENCE {

 zeroSlotOffsetAperiodicSRS ENUMERATED {supported} OPTIONAL,

 pa-PhaseDiscontinuityImpacts ENUMERATED {supported} OPTIONAL,

 pusch-SeparationWithGap ENUMERATED {supported} OPTIONAL,

 pusch-ProcessingType2 SEQUENCE {

 scs-15kHz ProcessingParameters OPTIONAL,

 scs-30kHz ProcessingParameters OPTIONAL,

 scs-60kHz ProcessingParameters OPTIONAL

 } OPTIONAL,

 ul-MCS-TableAlt-DynamicIndication ENUMERATED {supported} OPTIONAL

}

SRS-Resources ::= SEQUENCE {

 maxNumberAperiodicSRS-PerBWP ENUMERATED {n1, n2, n4, n8, n16},

 maxNumberAperiodicSRS-PerBWP-PerSlot INTEGER (1..6),

 maxNumberPeriodicSRS-PerBWP ENUMERATED {n1, n2, n4, n8, n16},

 maxNumberPeriodicSRS-PerBWP-PerSlot INTEGER (1..6),

 maxNumberSemiPersistentSRS-PerBWP ENUMERATED {n1, n2, n4, n8, n16},

 maxNumberSemiPersistentSRS-PerBWP-PerSlot INTEGER (1..6),

 maxNumberSRS-Ports-PerResource ENUMERATED {n1, n2, n4}

}

DummyF ::= SEQUENCE {

 maxNumberPeriodicCSI-ReportPerBWP INTEGER (1..4),

 maxNumberAperiodicCSI-ReportPerBWP INTEGER (1..4),

 maxNumberSemiPersistentCSI-ReportPerBWP INTEGER (0..4),

 simultaneousCSI-ReportsAllCC INTEGER (5..32)

}

-- TAG-FEATURESETUPLINK-STOP

-- ASN1STOP

|  |
| --- |
| *FeatureSetUplink* field descriptions |
| ***crossCarrierScheduling-OtherSCS***The UE shall set this field to the same value as *crossCarrierScheduling-OtherSCS* in the associated *FeatureSetDownlink* (if present). |
| ***featureSetListPerUplinkCC***Indicates which features the UE supports on the individual UL carriers of the feature set (and hence of a band entry that refers to the feature set). The UE shall hence include at least as many *FeatureSetUplinkPerCC-Id* in this list as the number of carriers it supports according to the *ca-BandwidthClassUL*, except if indicating additional functionality by reducing the number of *FeatureSetUplinkPerCC-Id* in the feature set (see NOTE 1 in *FeatureSetCombination* IE description). The order of the elements in this list is not relevant, i.e., the network may configure any of the carriers in accordance with any of the *FeatureSetUplinkPerCC-Id* in this list. |

#### – *FeatureSetUplinkId*

The IE *FeatureSetUplinkId* identifies an uplink feature set. The *FeatureSetUplinkId* of a *FeatureSetUplink* is the index position of the *FeatureSetUplink* in the *featureSetsUplink* list in the *FeatureSets* IE. The first element in the list is referred to by *FeatureSetUplinkId* = 1, and so on. The *FeatureSetUplinkId =0* is not used by an actual *FeatureSetUplink* but means that the UE does not support a carrier in this band of a band combination.

*FeatureSetUplinkId* information element

-- ASN1START

-- TAG-FEATURESETUPLINKID-START

FeatureSetUplinkId ::= INTEGER (0..maxUplinkFeatureSets)

-- TAG-FEATURESETUPLINKID-STOP

-- ASN1STOP

#### – *FeatureSetUplinkPerCC*

The IE *FeatureSetUplinkPerCC* indicates a set of features that the UE supports on the corresponding carrier of one band entry of a band combination.

*FeatureSetUplinkPerCC* information element

-- ASN1START

-- TAG-FEATURESETUPLINKPERCC-START

FeatureSetUplinkPerCC ::= SEQUENCE {

 supportedSubcarrierSpacingUL SubcarrierSpacing,

 supportedBandwidthUL SupportedBandwidth,

 channelBW-90mhz ENUMERATED {supported} OPTIONAL,

 mimo-CB-PUSCH SEQUENCE {

 maxNumberMIMO-LayersCB-PUSCH MIMO-LayersUL OPTIONAL,

 maxNumberSRS-ResourcePerSet INTEGER (1..2)

 } OPTIONAL,

 maxNumberMIMO-LayersNonCB-PUSCH MIMO-LayersUL OPTIONAL,

 supportedModulationOrderUL ModulationOrder OPTIONAL

}

FeatureSetUplinkPerCC-v1540 ::= SEQUENCE {

 mimo-NonCB-PUSCH SEQUENCE {

 maxNumberSRS-ResourcePerSet INTEGER (1..4),

 maxNumberSimultaneousSRS-ResourceTx INTEGER (1..4)

 } OPTIONAL

}

-- TAG-FEATURESETUPLINKPERCC-STOP

-- ASN1STOP

#### – *FeatureSetUplinkPerCC-Id*

The IE *FeatureSetUplinkPerCC-Id* identifies a set of features applicable to one carrier of a feature set. The *FeatureSetUplinkPerCC-Id* of a *FeatureSetUplinkPerCC* is the index position of the *FeatureSetUplinkPerCC* in the *featureSetsUplinkPerCC*. The first element in the list is referred to by *FeatureSetUplinkPerCC-Id* = 1, and so on.

*FeatureSetUplinkPerCC-Id* information element

-- ASN1START

-- TAG-FEATURESETUPLINKPERCC-ID-START

FeatureSetUplinkPerCC-Id ::= INTEGER (1..maxPerCC-FeatureSets)

-- TAG-FEATURESETUPLINKPERCC-ID-STOP

-- ASN1STOP

#### – *FreqBandIndicatorEUTRA*

-- ASN1START

-- TAG-FREQBANDINDICATOREUTRA-START

FreqBandIndicatorEUTRA ::= INTEGER (1..maxBandsEUTRA)

-- TAG-FREQBANDINDICATOREUTRA-STOP

-- ASN1STOP

#### – *FreqBandList*

The IE *FreqBandList* is used by the network to request NR CA and/or MR-DC band combinations for specific NR and/or E-UTRA frequency bands and/or up to a specific number of carriers and/or up to specific aggregated bandwidth. This is also used to request feature sets (for NR) and feature set combinations (for NR and MR-DC).

*FreqBandList* information element

-- ASN1START

-- TAG-FREQBANDLIST-START

FreqBandList ::= SEQUENCE (SIZE (1..maxBandsMRDC)) OF FreqBandInformation

FreqBandInformation ::= CHOICE {

 bandInformationEUTRA FreqBandInformationEUTRA,

 bandInformationNR FreqBandInformationNR

}

FreqBandInformationEUTRA ::= SEQUENCE {

 bandEUTRA FreqBandIndicatorEUTRA,

 ca-BandwidthClassDL-EUTRA CA-BandwidthClassEUTRA OPTIONAL, -- Need N

 ca-BandwidthClassUL-EUTRA CA-BandwidthClassEUTRA OPTIONAL -- Need N

}

FreqBandInformationNR ::= SEQUENCE {

 bandNR FreqBandIndicatorNR,

 maxBandwidthRequestedDL AggregatedBandwidth OPTIONAL, -- Need N

 maxBandwidthRequestedUL AggregatedBandwidth OPTIONAL, -- Need N

 maxCarriersRequestedDL INTEGER (1..maxNrofServingCells) OPTIONAL, -- Need N

 maxCarriersRequestedUL INTEGER (1..maxNrofServingCells) OPTIONAL -- Need N

}

AggregatedBandwidth ::= ENUMERATED {mhz50, mhz100, mhz150, mhz200, mhz250, mhz300, mhz350,

 mhz400, mhz450, mhz500, mhz550, mhz600, mhz650, mhz700, mhz750, mhz800}

-- TAG-FREQBANDLIST-STOP

-- ASN1STOP

#### – *FreqSeparationClass*

The IE *FreqSeparationClas*s is used for an intra-band non-contiguous CA band combination to indicate frequency separation between lower edge of lowest CC and upper edge of highest CC in a frequency band.

*FreqSeparationClass* information element

-- ASN1START

-- TAG-FREQSEPARATIONCLASS-START

FreqSeparationClass ::= ENUMERATED {c1, c2, c3, ...}

-- TAG-FREQSEPARATIONCLASS-STOP

-- ASN1STOP

#### – *IMS-Parameters*

The IE *IMS-Parameters* is used to convery capabilities related to IMS.

*IMS-Parameters* information element

-- ASN1START

-- TAG-IMS-PARAMETERS-START

IMS-Parameters ::= SEQUENCE {

 ims-ParametersCommon IMS-ParametersCommon OPTIONAL,

 ims-ParametersFRX-Diff IMS-ParametersFRX-Diff OPTIONAL,

 ...

}

IMS-ParametersCommon ::= SEQUENCE {

 voiceOverEUTRA-5GC ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 voiceOverSCG-BearerEUTRA-5GC ENUMERATED {supported} OPTIONAL

 ]]

}

IMS-ParametersFRX-Diff ::= SEQUENCE {

 voiceOverNR ENUMERATED {supported} OPTIONAL,

 ...

}

-- TAG-IMS-PARAMETERS-STOP

-- ASN1STOP

#### – *InterRAT-Parameters*

The IE *InterRAT-Parameters* is used convey UE capabilities related to the other RATs.

*InterRAT-Parameters* information element

-- ASN1START

-- TAG-INTERRAT-PARAMETERS-START

InterRAT-Parameters ::= SEQUENCE {

 eutra EUTRA-Parameters OPTIONAL,

 ...

}

EUTRA-Parameters ::= SEQUENCE {

 supportedBandListEUTRA SEQUENCE (SIZE (1..maxBandsEUTRA)) OF FreqBandIndicatorEUTRA,

 eutra-ParametersCommon EUTRA-ParametersCommon OPTIONAL,

 eutra-ParametersXDD-Diff EUTRA-ParametersXDD-Diff OPTIONAL,

 ...

}

EUTRA-ParametersCommon ::= SEQUENCE {

 mfbi-EUTRA ENUMERATED {supported} OPTIONAL,

 modifiedMPR-BehaviorEUTRA BIT STRING (SIZE (32)) OPTIONAL,

 multiNS-Pmax-EUTRA ENUMERATED {supported} OPTIONAL,

 rs-SINR-MeasEUTRA ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 ne-DC ENUMERATED {supported} OPTIONAL

 ]]

}

EUTRA-ParametersXDD-Diff ::= SEQUENCE {

 rsrqMeasWidebandEUTRA ENUMERATED {supported} OPTIONAL,

 ...

}

-- TAG-INTERRAT-PARAMETERS-STOP

-- ASN1STOP

#### – *MAC-Parameters*

The IE *MAC-Parameters* is used to convey capabilities related to MAC.

*MAC-Parameters* information element

-- ASN1START

-- TAG-MAC-PARAMETERS-START

MAC-Parameters ::= SEQUENCE {

 mac-ParametersCommon MAC-ParametersCommon OPTIONAL,

 mac-ParametersXDD-Diff MAC-ParametersXDD-Diff OPTIONAL

}

MAC-ParametersCommon ::= SEQUENCE {

 lcp-Restriction ENUMERATED {supported} OPTIONAL,

 dummy ENUMERATED {supported} OPTIONAL,

 lch-ToSCellRestriction ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 recommendedBitRate ENUMERATED {supported} OPTIONAL,

 recommendedBitRateQuery ENUMERATED {supported} OPTIONAL

 ]]

}

MAC-ParametersXDD-Diff ::= SEQUENCE {

 skipUplinkTxDynamic ENUMERATED {supported} OPTIONAL,

 logicalChannelSR-DelayTimer ENUMERATED {supported} OPTIONAL,

 longDRX-Cycle ENUMERATED {supported} OPTIONAL,

 shortDRX-Cycle ENUMERATED {supported} OPTIONAL,

 multipleSR-Configurations ENUMERATED {supported} OPTIONAL,

 multipleConfiguredGrants ENUMERATED {supported} OPTIONAL,

 ...

}

-- TAG-MAC-PARAMETERS-STOP

-- ASN1STOP

#### – *MeasAndMobParameters*

The IE *MeasAndMobParameters* is used to convey UE capabilities related to measurements for radio resource management (RRM), radio link monitoring (RLM) and mobility (e.g. handover).

*MeasAndMobParameters* information element

-- ASN1START

-- TAG-MEASANDMOBPARAMETERS-START

MeasAndMobParameters ::= SEQUENCE {

 measAndMobParametersCommon MeasAndMobParametersCommon OPTIONAL,

 measAndMobParametersXDD-Diff MeasAndMobParametersXDD-Diff OPTIONAL,

 measAndMobParametersFRX-Diff MeasAndMobParametersFRX-Diff OPTIONAL

}

MeasAndMobParametersCommon ::= SEQUENCE {

 supportedGapPattern BIT STRING (SIZE (22)) OPTIONAL,

 ssb-RLM ENUMERATED {supported} OPTIONAL,

 ssb-AndCSI-RS-RLM ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 eventB-MeasAndReport ENUMERATED {supported} OPTIONAL,

 handoverFDD-TDD ENUMERATED {supported} OPTIONAL,

 eutra-CGI-Reporting ENUMERATED {supported} OPTIONAL,

 nr-CGI-Reporting ENUMERATED {supported} OPTIONAL

 ]],

 [[

 independentGapConfig ENUMERATED {supported} OPTIONAL,

 periodicEUTRA-MeasAndReport ENUMERATED {supported} OPTIONAL,

 handoverFR1-FR2 ENUMERATED {supported} OPTIONAL,

 maxNumberCSI-RS-RRM-RS-SINR ENUMERATED {n4, n8, n16, n32, n64, n96} OPTIONAL

 ]],

 [[

 nr-CGI-Reporting-ENDC ENUMERATED {supported} OPTIONAL

 ]]

}

MeasAndMobParametersXDD-Diff ::= SEQUENCE {

 intraAndInterF-MeasAndReport ENUMERATED {supported} OPTIONAL,

 eventA-MeasAndReport ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 handoverInterF ENUMERATED {supported} OPTIONAL,

 handoverLTE-EPC ENUMERATED {supported} OPTIONAL,

 handoverLTE-5GC ENUMERATED {supported} OPTIONAL

 ]],

 [[

 sftd-MeasNR-Neigh ENUMERATED {supported} OPTIONAL,

 sftd-MeasNR-Neigh-DRX ENUMERATED {supported} OPTIONAL

 ]]

}

MeasAndMobParametersFRX-Diff ::= SEQUENCE {

 ss-SINR-Meas ENUMERATED {supported} OPTIONAL,

 csi-RSRP-AndRSRQ-MeasWithSSB ENUMERATED {supported} OPTIONAL,

 csi-RSRP-AndRSRQ-MeasWithoutSSB ENUMERATED {supported} OPTIONAL,

 csi-SINR-Meas ENUMERATED {supported} OPTIONAL,

 csi-RS-RLM ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 handoverInterF ENUMERATED {supported} OPTIONAL,

 handoverLTE-EPC ENUMERATED {supported} OPTIONAL,

 handoverLTE-5GC ENUMERATED {supported} OPTIONAL

 ]],

 [[

 maxNumberResource-CSI-RS-RLM ENUMERATED {n2, n4, n6, n8} OPTIONAL

 ]],

 [[

 simultaneousRxDataSSB-DiffNumerology ENUMERATED {supported} OPTIONAL

 ]]

}

-- TAG-MEASANDMOBPARAMETERS-STOP

-- ASN1STOP

#### – *MeasAndMobParametersMRDC*

The IE *MeasAndMobParametersMRDC* is used to convey capability parameters related to RRM measurements and RRC mobility.

*MeasAndMobParametersMRDC* information element

-- ASN1START

-- TAG-MEASANDMOBPARAMETERSMRDC-START

MeasAndMobParametersMRDC ::= SEQUENCE {

 measAndMobParametersMRDC-Common MeasAndMobParametersMRDC-Common OPTIONAL,

 measAndMobParametersMRDC-XDD-Diff MeasAndMobParametersMRDC-XDD-Diff OPTIONAL,

 measAndMobParametersMRDC-FRX-Diff MeasAndMobParametersMRDC-FRX-Diff OPTIONAL

}

MeasAndMobParametersMRDC-v1560 ::= SEQUENCE {

 measAndMobParametersMRDC-XDD-Diff-v1560 MeasAndMobParametersMRDC-XDD-Diff-v1560 OPTIONAL

}

MeasAndMobParametersMRDC-Common ::= SEQUENCE {

 independentGapConfig ENUMERATED {supported} OPTIONAL

}

MeasAndMobParametersMRDC-XDD-Diff ::= SEQUENCE {

 sftd-MeasPSCell ENUMERATED {supported} OPTIONAL,

 sftd-MeasNR-Cell ENUMERATED {supported} OPTIONAL

}

MeasAndMobParametersMRDC-XDD-Diff-v1560 ::= SEQUENCE {

 sftd-MeasPSCell-NEDC ENUMERATED {supported} OPTIONAL

}

MeasAndMobParametersMRDC-FRX-Diff ::= SEQUENCE {

 simultaneousRxDataSSB-DiffNumerology ENUMERATED {supported} OPTIONAL

}

-- TAG-MEASANDMOBPARAMETERSMRDC-STOP

-- ASN1STOP

#### – *MIMO-Layers*

The IE *MIMO-Layers* is used to convey the number of supported MIMO layers.

*MIMO-Layers* information element

-- ASN1START

-- TAG-MIMO-LAYERS-START

MIMO-LayersDL ::= ENUMERATED {twoLayers, fourLayers, eightLayers}

MIMO-LayersUL ::= ENUMERATED {oneLayer, twoLayers, fourLayers}

-- TAG-MIMO-LAYERS-STOP

-- ASN1STOP

#### – *MIMO-ParametersPerBand*

The IE *MIMO-ParametersPerBand* is used to convey MIMO related parameters specific for a certain band (not per feature set or band combination).

*MIMO-ParametersPerBand* information element

-- ASN1START

-- TAG-MIMO-PARAMETERSPERBAND-START

MIMO-ParametersPerBand ::= SEQUENCE {

 tci-StatePDSCH SEQUENCE {

 maxNumberConfiguredTCIstatesPerCC ENUMERATED {n4, n8, n16, n32, n64, n128} OPTIONAL,

 maxNumberActiveTCI-PerBWP ENUMERATED {n1, n2, n4, n8} OPTIONAL

 } OPTIONAL,

 additionalActiveTCI-StatePDCCH ENUMERATED {supported} OPTIONAL,

 pusch-TransCoherence ENUMERATED {nonCoherent, partialCoherent, fullCoherent} OPTIONAL,

 beamCorrespondenceWithoutUL-BeamSweeping ENUMERATED {supported} OPTIONAL,

 periodicBeamReport ENUMERATED {supported} OPTIONAL,

 aperiodicBeamReport ENUMERATED {supported} OPTIONAL,

 sp-BeamReportPUCCH ENUMERATED {supported} OPTIONAL,

 sp-BeamReportPUSCH ENUMERATED {supported} OPTIONAL,

 dummy1 DummyG OPTIONAL,

 maxNumberRxBeam INTEGER (2..8) OPTIONAL,

 maxNumberRxTxBeamSwitchDL SEQUENCE {

 scs-15kHz ENUMERATED {n4, n7, n14} OPTIONAL,

 scs-30kHz ENUMERATED {n4, n7, n14} OPTIONAL,

 scs-60kHz ENUMERATED {n4, n7, n14} OPTIONAL,

 scs-120kHz ENUMERATED {n4, n7, n14} OPTIONAL,

 scs-240kHz ENUMERATED {n4, n7, n14} OPTIONAL

 } OPTIONAL,

 maxNumberNonGroupBeamReporting ENUMERATED {n1, n2, n4} OPTIONAL,

 groupBeamReporting ENUMERATED {supported} OPTIONAL,

 uplinkBeamManagement SEQUENCE {

 maxNumberSRS-ResourcePerSet-BM ENUMERATED {n2, n4, n8, n16},

 maxNumberSRS-ResourceSet INTEGER (1..8)

 } OPTIONAL,

 maxNumberCSI-RS-BFD INTEGER (1..64) OPTIONAL,

 maxNumberSSB-BFD INTEGER (1..64) OPTIONAL,

 maxNumberCSI-RS-SSB-CBD INTEGER (1..256) OPTIONAL,

 dummy2 ENUMERATED {supported} OPTIONAL,

 twoPortsPTRS-UL ENUMERATED {supported} OPTIONAL,

 dummy5 SRS-Resources OPTIONAL,

 dummy3 INTEGER (1..4) OPTIONAL,

 beamReportTiming SEQUENCE {

 scs-15kHz ENUMERATED {sym2, sym4, sym8} OPTIONAL,

 scs-30kHz ENUMERATED {sym4, sym8, sym14, sym28} OPTIONAL,

 scs-60kHz ENUMERATED {sym8, sym14, sym28} OPTIONAL,

 scs-120kHz ENUMERATED {sym14, sym28, sym56} OPTIONAL

 } OPTIONAL,

 ptrs-DensityRecommendationSetDL SEQUENCE {

 scs-15kHz PTRS-DensityRecommendationDL OPTIONAL,

 scs-30kHz PTRS-DensityRecommendationDL OPTIONAL,

 scs-60kHz PTRS-DensityRecommendationDL OPTIONAL,

 scs-120kHz PTRS-DensityRecommendationDL OPTIONAL

 } OPTIONAL,

 ptrs-DensityRecommendationSetUL SEQUENCE {

 scs-15kHz PTRS-DensityRecommendationUL OPTIONAL,

 scs-30kHz PTRS-DensityRecommendationUL OPTIONAL,

 scs-60kHz PTRS-DensityRecommendationUL OPTIONAL,

 scs-120kHz PTRS-DensityRecommendationUL OPTIONAL

 } OPTIONAL,

 dummy4 DummyH OPTIONAL,

 aperiodicTRS ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 dummy6 ENUMERATED {true} OPTIONAL,

 beamManagementSSB-CSI-RS BeamManagementSSB-CSI-RS OPTIONAL,

 beamSwitchTiming SEQUENCE {

 scs-60kHz ENUMERATED {sym14, sym28, sym48, sym224, sym336} OPTIONAL,

 scs-120kHz ENUMERATED {sym14, sym28, sym48, sym224, sym336} OPTIONAL

 } OPTIONAL,

 codebookParameters CodebookParameters OPTIONAL,

 csi-RS-IM-ReceptionForFeedback CSI-RS-IM-ReceptionForFeedback OPTIONAL,

 csi-RS-ProcFrameworkForSRS CSI-RS-ProcFrameworkForSRS OPTIONAL,

 csi-ReportFramework CSI-ReportFramework OPTIONAL,

 csi-RS-ForTracking CSI-RS-ForTracking OPTIONAL,

 srs-AssocCSI-RS SEQUENCE (SIZE (1.. maxNrofCSI-RS-Resources)) OF SupportedCSI-RS-Resource OPTIONAL,

 spatialRelations SpatialRelations OPTIONAL

 ]],

 [[

 codebookParametersPerBand-r16 CodebookParametersPerBand-r16 OPTIONAL

 ]]}

DummyG ::= SEQUENCE {

 maxNumberSSB-CSI-RS-ResourceOneTx ENUMERATED {n8, n16, n32, n64},

 maxNumberSSB-CSI-RS-ResourceTwoTx ENUMERATED {n0, n4, n8, n16, n32, n64},

 supportedCSI-RS-Density ENUMERATED {one, three, oneAndThree}

}

BeamManagementSSB-CSI-RS ::= SEQUENCE {

 maxNumberSSB-CSI-RS-ResourceOneTx ENUMERATED {n0, n8, n16, n32, n64},

 maxNumberCSI-RS-Resource ENUMERATED {n0, n4, n8, n16, n32, n64},

 maxNumberCSI-RS-ResourceTwoTx ENUMERATED {n0, n4, n8, n16, n32, n64},

 supportedCSI-RS-Density ENUMERATED {one, three, oneAndThree} OPTIONAL,

 maxNumberAperiodicCSI-RS-Resource ENUMERATED {n0, n1, n4, n8, n16, n32, n64}

}

DummyH ::= SEQUENCE {

 burstLength INTEGER (1..2),

 maxSimultaneousResourceSetsPerCC INTEGER (1..8),

 maxConfiguredResourceSetsPerCC INTEGER (1..64),

 maxConfiguredResourceSetsAllCC INTEGER (1..128)

}

CSI-RS-ForTracking ::= SEQUENCE {

 maxBurstLength INTEGER (1..2),

 maxSimultaneousResourceSetsPerCC INTEGER (1..8),

 maxConfiguredResourceSetsPerCC INTEGER (1..64),

 maxConfiguredResourceSetsAllCC INTEGER (1..256)

}

CSI-RS-IM-ReceptionForFeedback ::= SEQUENCE {

 maxConfigNumberNZP-CSI-RS-PerCC INTEGER (1..64),

 maxConfigNumberPortsAcrossNZP-CSI-RS-PerCC INTEGER (2..256),

 maxConfigNumberCSI-IM-PerCC ENUMERATED {n1, n2, n4, n8, n16, n32},

 maxNumberSimultaneousNZP-CSI-RS-PerCC INTEGER (1..64),

 totalNumberPortsSimultaneousNZP-CSI-RS-PerCC INTEGER (2..256)

}

CSI-RS-ProcFrameworkForSRS ::= SEQUENCE {

 maxNumberPeriodicSRS-AssocCSI-RS-PerBWP INTEGER (1..4),

 maxNumberAperiodicSRS-AssocCSI-RS-PerBWP INTEGER (1..4),

 maxNumberSP-SRS-AssocCSI-RS-PerBWP INTEGER (0..4),

 simultaneousSRS-AssocCSI-RS-PerCC INTEGER (1..8)

}

CSI-ReportFramework ::= SEQUENCE {

 maxNumberPeriodicCSI-PerBWP-ForCSI-Report INTEGER (1..4),

 maxNumberAperiodicCSI-PerBWP-ForCSI-Report INTEGER (1..4),

 maxNumberSemiPersistentCSI-PerBWP-ForCSI-Report INTEGER (0..4),

 maxNumberPeriodicCSI-PerBWP-ForBeamReport INTEGER (1..4),

 maxNumberAperiodicCSI-PerBWP-ForBeamReport INTEGER (1..4),

 maxNumberAperiodicCSI-triggeringStatePerCC ENUMERATED {n3, n7, n15, n31, n63, n128},

 maxNumberSemiPersistentCSI-PerBWP-ForBeamReport INTEGER (0..4),

 simultaneousCSI-ReportsPerCC INTEGER (1..8)

}

PTRS-DensityRecommendationDL ::= SEQUENCE {

 frequencyDensity1 INTEGER (1..276),

 frequencyDensity2 INTEGER (1..276),

 timeDensity1 INTEGER (0..29),

 timeDensity2 INTEGER (0..29),

 timeDensity3 INTEGER (0..29)

}

PTRS-DensityRecommendationUL ::= SEQUENCE {

 frequencyDensity1 INTEGER (1..276),

 frequencyDensity2 INTEGER (1..276),

 timeDensity1 INTEGER (0..29),

 timeDensity2 INTEGER (0..29),

 timeDensity3 INTEGER (0..29),

 sampleDensity1 INTEGER (1..276),

 sampleDensity2 INTEGER (1..276),

 sampleDensity3 INTEGER (1..276),

 sampleDensity4 INTEGER (1..276),

 sampleDensity5 INTEGER (1..276)

}

SpatialRelations ::= SEQUENCE {

 maxNumberConfiguredSpatialRelations ENUMERATED {n4, n8, n16, n32, n64, n96},

 maxNumberActiveSpatialRelations ENUMERATED {n1, n2, n4, n8, n14},

 additionalActiveSpatialRelationPUCCH ENUMERATED {supported} OPTIONAL,

 maxNumberDL-RS-QCL-TypeD ENUMERATED {n1, n2, n4, n8, n14}

}

DummyI ::= SEQUENCE {

 supportedSRS-TxPortSwitch ENUMERATED {t1r2, t1r4, t2r4, t1r4-t2r4, tr-equal},

 txSwitchImpactToRx ENUMERATED {true} OPTIONAL

}

-- TAG-MIMO-PARAMETERSPERBAND-STOP

-- ASN1STOP

|  |
| --- |
| *MIMO-ParametersPerBand field description* |
| ***csi-RS-IM-ReceptionForFeedback/ csi-RS-ProcFrameworkForSRS/ csi-ReportFramework***CSI related capabilities which the UE supports on each of the carriers operated on this band. For mixed FR1-FR2 band combinations these values may be further limited by the corresponding fields in *Phy-ParametersFRX-Diff*. |

#### – *ModulationOrder*

The IE *ModulationOrder* is used to convey the maximum supported modulation order.

*ModulationOrder* information element

-- ASN1START

-- TAG-MODULATIONORDER-START

ModulationOrder ::= ENUMERATED {bpsk-halfpi, bpsk, qpsk, qam16, qam64, qam256}

-- TAG-MODULATIONORDER-STOP

-- ASN1STOP

#### – *MRDC-Parameters*

The IE *MRDC-Parameters* contains the band combination parameters specific to MR-DC for a given MR-DC band combination.

*MRDC-Parameters* information element

-- ASN1START

-- TAG-MRDC-PARAMETERS-START

MRDC-Parameters ::= SEQUENCE {

 singleUL-Transmission ENUMERATED {supported} OPTIONAL,

 dynamicPowerSharingENDC ENUMERATED {supported} OPTIONAL,

 tdm-Pattern ENUMERATED {supported} OPTIONAL,

 ul-SharingEUTRA-NR ENUMERATED {tdm, fdm, both} OPTIONAL,

 ul-SwitchingTimeEUTRA-NR ENUMERATED {type1, type2} OPTIONAL,

 simultaneousRxTxInterBandENDC ENUMERATED {supported} OPTIONAL,

 asyncIntraBandENDC ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 dualPA-Architecture ENUMERATED {supported} OPTIONAL,

 intraBandENDC-Support ENUMERATED {non-contiguous, both} OPTIONAL,

 ul-TimingAlignmentEUTRA-NR ENUMERATED {required} OPTIONAL

 ]]

}

MRDC-Parameters-v1580 ::= SEQUENCE {

 dynamicPowerSharingNEDC ENUMERATED {supported} OPTIONAL

}

-- TAG-MRDC-PARAMETERS-STOP

-- ASN1STOP

#### – *NRDC-Parameters*

The IE *NRDC-Parameters* contains parameters specific to NR-DC, i.e., which are not applicable to NR SA.

*NRDC-Parameters* information element

-- ASN1START

-- TAG-NRDC-PARAMETERS-START

NRDC-Parameters ::= SEQUENCE {

 measAndMobParametersNRDC MeasAndMobParametersMRDC OPTIONAL,

 generalParametersNRDC GeneralParametersMRDC-XDD-Diff OPTIONAL,

 fdd-Add-UE-NRDC-Capabilities UE-MRDC-CapabilityAddXDD-Mode OPTIONAL,

 tdd-Add-UE-NRDC-Capabilities UE-MRDC-CapabilityAddXDD-Mode OPTIONAL,

 fr1-Add-UE-NRDC-Capabilities UE-MRDC-CapabilityAddFRX-Mode OPTIONAL,

 fr2-Add-UE-NRDC-Capabilities UE-MRDC-CapabilityAddFRX-Mode OPTIONAL,

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 dummy SEQUENCE {} OPTIONAL

}

NRDC-Parameters-v1570 ::= SEQUENCE {

 sfn-SyncNRDC ENUMERATED {supported} OPTIONAL

}

-- TAG-NRDC-PARAMETERS-STOP

-- ASN1STOP

#### – *PDCP-Parameters*

The IE *PDCP-Parameters* is used to convey capabilities related to PDCP.

*PDCP-Parameters* information element

-- ASN1START

-- TAG-PDCP-PARAMETERS-START

PDCP-Parameters ::= SEQUENCE {

 supportedROHC-Profiles SEQUENCE {

 profile0x0000 BOOLEAN,

 profile0x0001 BOOLEAN,

 profile0x0002 BOOLEAN,

 profile0x0003 BOOLEAN,

 profile0x0004 BOOLEAN,

 profile0x0006 BOOLEAN,

 profile0x0101 BOOLEAN,

 profile0x0102 BOOLEAN,

 profile0x0103 BOOLEAN,

 profile0x0104 BOOLEAN

 },

 maxNumberROHC-ContextSessions ENUMERATED {cs2, cs4, cs8, cs12, cs16, cs24, cs32, cs48, cs64,

 cs128, cs256, cs512, cs1024, cs16384, spare2, spare1},

 uplinkOnlyROHC-Profiles ENUMERATED {supported} OPTIONAL,

 continueROHC-Context ENUMERATED {supported} OPTIONAL,

 outOfOrderDelivery ENUMERATED {supported} OPTIONAL,

 shortSN ENUMERATED {supported} OPTIONAL,

 pdcp-DuplicationSRB ENUMERATED {supported} OPTIONAL,

 pdcp-DuplicationMCG-OrSCG-DRB ENUMERATED {supported} OPTIONAL,

 ...

}

-- TAG-PDCP-PARAMETERS-STOP

-- ASN1STOP

#### – *PDCP-ParametersMRDC*

The IE *PDCP-ParametersMRDC* is used to convey PDCP related capabilities for MR-DC.

*PDCP-ParametersMRDC* information element

-- ASN1START

-- TAG-PDCP-PARAMETERSMRDC-START

PDCP-ParametersMRDC ::= SEQUENCE {

 pdcp-DuplicationSplitSRB ENUMERATED {supported} OPTIONAL,

 pdcp-DuplicationSplitDRB ENUMERATED {supported} OPTIONAL

}

-- TAG-PDCP-PARAMETERSMRDC-STOP

-- ASN1STOP

#### – *Phy-Parameters*

The IE *Phy-Parameters* is used to convey the physical layer capabilities.

*Phy-Parameters* information element

-- ASN1START

-- TAG-PHY-PARAMETERS-START

Phy-Parameters ::= SEQUENCE {

 phy-ParametersCommon Phy-ParametersCommon OPTIONAL,

 phy-ParametersXDD-Diff Phy-ParametersXDD-Diff OPTIONAL,

 phy-ParametersFRX-Diff Phy-ParametersFRX-Diff OPTIONAL,

 phy-ParametersFR1 Phy-ParametersFR1 OPTIONAL,

 phy-ParametersFR2 Phy-ParametersFR2 OPTIONAL

}

Phy-ParametersCommon ::= SEQUENCE {

 csi-RS-CFRA-ForHO ENUMERATED {supported} OPTIONAL,

 dynamicPRB-BundlingDL ENUMERATED {supported} OPTIONAL,

 sp-CSI-ReportPUCCH ENUMERATED {supported} OPTIONAL,

 sp-CSI-ReportPUSCH ENUMERATED {supported} OPTIONAL,

 nzp-CSI-RS-IntefMgmt ENUMERATED {supported} OPTIONAL,

 type2-SP-CSI-Feedback-LongPUCCH ENUMERATED {supported} OPTIONAL,

 precoderGranularityCORESET ENUMERATED {supported} OPTIONAL,

 dynamicHARQ-ACK-Codebook ENUMERATED {supported} OPTIONAL,

 semiStaticHARQ-ACK-Codebook ENUMERATED {supported} OPTIONAL,

 spatialBundlingHARQ-ACK ENUMERATED {supported} OPTIONAL,

 dynamicBetaOffsetInd-HARQ-ACK-CSI ENUMERATED {supported} OPTIONAL,

 pucch-Repetition-F1-3-4 ENUMERATED {supported} OPTIONAL,

 ra-Type0-PUSCH ENUMERATED {supported} OPTIONAL,

 dynamicSwitchRA-Type0-1-PDSCH ENUMERATED {supported} OPTIONAL,

 dynamicSwitchRA-Type0-1-PUSCH ENUMERATED {supported} OPTIONAL,

 pdsch-MappingTypeA ENUMERATED {supported} OPTIONAL,

 pdsch-MappingTypeB ENUMERATED {supported} OPTIONAL,

 interleavingVRB-ToPRB-PDSCH ENUMERATED {supported} OPTIONAL,

 interSlotFreqHopping-PUSCH ENUMERATED {supported} OPTIONAL,

 type1-PUSCH-RepetitionMultiSlots ENUMERATED {supported} OPTIONAL,

 type2-PUSCH-RepetitionMultiSlots ENUMERATED {supported} OPTIONAL,

 pusch-RepetitionMultiSlots ENUMERATED {supported} OPTIONAL,

 pdsch-RepetitionMultiSlots ENUMERATED {supported} OPTIONAL,

 downlinkSPS ENUMERATED {supported} OPTIONAL,

 configuredUL-GrantType1 ENUMERATED {supported} OPTIONAL,

 configuredUL-GrantType2 ENUMERATED {supported} OPTIONAL,

 pre-EmptIndication-DL ENUMERATED {supported} OPTIONAL,

 cbg-TransIndication-DL ENUMERATED {supported} OPTIONAL,

 cbg-TransIndication-UL ENUMERATED {supported} OPTIONAL,

 cbg-FlushIndication-DL ENUMERATED {supported} OPTIONAL,

 dynamicHARQ-ACK-CodeB-CBG-Retx-DL ENUMERATED {supported} OPTIONAL,

 rateMatchingResrcSetSemi-Static ENUMERATED {supported} OPTIONAL,

 rateMatchingResrcSetDynamic ENUMERATED {supported} OPTIONAL,

 bwp-SwitchingDelay ENUMERATED {type1, type2} OPTIONAL,

 ...,

 [[

 dummy ENUMERATED {supported} OPTIONAL

 ]],

 [[

 maxNumberSearchSpaces ENUMERATED {n10} OPTIONAL,

 rateMatchingCtrlResrcSetDynamic ENUMERATED {supported} OPTIONAL,

 maxLayersMIMO-Indication ENUMERATED {supported} OPTIONAL

 ]]}

Phy-ParametersXDD-Diff ::= SEQUENCE {

 dynamicSFI ENUMERATED {supported} OPTIONAL,

 twoPUCCH-F0-2-ConsecSymbols ENUMERATED {supported} OPTIONAL,

 twoDifferentTPC-Loop-PUSCH ENUMERATED {supported} OPTIONAL,

 twoDifferentTPC-Loop-PUCCH ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 dl-SchedulingOffset-PDSCH-TypeA ENUMERATED {supported} OPTIONAL,

 dl-SchedulingOffset-PDSCH-TypeB ENUMERATED {supported} OPTIONAL,

 ul-SchedulingOffset ENUMERATED {supported} OPTIONAL

 ]]

}

Phy-ParametersFRX-Diff ::= SEQUENCE {

 dynamicSFI ENUMERATED {supported} OPTIONAL,

 dummy1 BIT STRING (SIZE (2)) OPTIONAL,

 twoFL-DMRS BIT STRING (SIZE (2)) OPTIONAL,

 dummy2 BIT STRING (SIZE (2)) OPTIONAL,

 dummy3 BIT STRING (SIZE (2)) OPTIONAL,

 supportedDMRS-TypeDL ENUMERATED {type1, type1And2} OPTIONAL,

 supportedDMRS-TypeUL ENUMERATED {type1, type1And2} OPTIONAL,

 semiOpenLoopCSI ENUMERATED {supported} OPTIONAL,

 csi-ReportWithoutPMI ENUMERATED {supported} OPTIONAL,

 csi-ReportWithoutCQI ENUMERATED {supported} OPTIONAL,

 onePortsPTRS BIT STRING (SIZE (2)) OPTIONAL,

 twoPUCCH-F0-2-ConsecSymbols ENUMERATED {supported} OPTIONAL,

 pucch-F2-WithFH ENUMERATED {supported} OPTIONAL,

 pucch-F3-WithFH ENUMERATED {supported} OPTIONAL,

 pucch-F4-WithFH ENUMERATED {supported} OPTIONAL,

 pucch-F0-2WithoutFH ENUMERATED {notSupported} OPTIONAL,

 pucch-F1-3-4WithoutFH ENUMERATED {notSupported} OPTIONAL,

 mux-SR-HARQ-ACK-CSI-PUCCH-MultiPerSlot ENUMERATED {supported} OPTIONAL,

 uci-CodeBlockSegmentation ENUMERATED {supported} OPTIONAL,

 onePUCCH-LongAndShortFormat ENUMERATED {supported} OPTIONAL,

 twoPUCCH-AnyOthersInSlot ENUMERATED {supported} OPTIONAL,

 intraSlotFreqHopping-PUSCH ENUMERATED {supported} OPTIONAL,

 pusch-LBRM ENUMERATED {supported} OPTIONAL,

 pdcch-BlindDetectionCA INTEGER (4..16) OPTIONAL,

 tpc-PUSCH-RNTI ENUMERATED {supported} OPTIONAL,

 tpc-PUCCH-RNTI ENUMERATED {supported} OPTIONAL,

 tpc-SRS-RNTI ENUMERATED {supported} OPTIONAL,

 absoluteTPC-Command ENUMERATED {supported} OPTIONAL,

 twoDifferentTPC-Loop-PUSCH ENUMERATED {supported} OPTIONAL,

 twoDifferentTPC-Loop-PUCCH ENUMERATED {supported} OPTIONAL,

 pusch-HalfPi-BPSK ENUMERATED {supported} OPTIONAL,

 pucch-F3-4-HalfPi-BPSK ENUMERATED {supported} OPTIONAL,

 almostContiguousCP-OFDM-UL ENUMERATED {supported} OPTIONAL,

 sp-CSI-RS ENUMERATED {supported} OPTIONAL,

 sp-CSI-IM ENUMERATED {supported} OPTIONAL,

 tdd-MultiDL-UL-SwitchPerSlot ENUMERATED {supported} OPTIONAL,

 multipleCORESET ENUMERATED {supported} OPTIONAL,

 ...,

 [[

 csi-RS-IM-ReceptionForFeedback CSI-RS-IM-ReceptionForFeedback OPTIONAL,

 csi-RS-ProcFrameworkForSRS CSI-RS-ProcFrameworkForSRS OPTIONAL,

 csi-ReportFramework CSI-ReportFramework OPTIONAL,

 mux-SR-HARQ-ACK-CSI-PUCCH-OncePerSlot SEQUENCE {

 sameSymbol ENUMERATED {supported} OPTIONAL,

 diffSymbol ENUMERATED {supported} OPTIONAL

 } OPTIONAL,

 mux-SR-HARQ-ACK-PUCCH ENUMERATED {supported} OPTIONAL,

 mux-MultipleGroupCtrlCH-Overlap ENUMERATED {supported} OPTIONAL,

 dl-SchedulingOffset-PDSCH-TypeA ENUMERATED {supported} OPTIONAL,

 dl-SchedulingOffset-PDSCH-TypeB ENUMERATED {supported} OPTIONAL,

 ul-SchedulingOffset ENUMERATED {supported} OPTIONAL,

 dl-64QAM-MCS-TableAlt ENUMERATED {supported} OPTIONAL,

 ul-64QAM-MCS-TableAlt ENUMERATED {supported} OPTIONAL,

 cqi-TableAlt ENUMERATED {supported} OPTIONAL,

 oneFL-DMRS-TwoAdditionalDMRS-UL ENUMERATED {supported} OPTIONAL,

 twoFL-DMRS-TwoAdditionalDMRS-UL ENUMERATED {supported} OPTIONAL,

 oneFL-DMRS-ThreeAdditionalDMRS-UL ENUMERATED {supported} OPTIONAL

 ]],

 [[

 pdcch-BlindDetectionNRDC SEQUENCE {

 pdcch-BlindDetectionMCG-UE INTEGER (1..15),

 pdcch-BlindDetectionSCG-UE INTEGER (1..15)

 } OPTIONAL,

 mux-HARQ-ACK-PUSCH-DiffSymbol ENUMERATED {supported} OPTIONAL

 ]],

 [[

 codebookParametersPerUE-r16 CodebookParametersListPerUE-r16 OPTIONAL,

 codebookVariantsAllCC-SimultaneousList-r16 CodebookVariantsList-r16 OPTIONAL

 ]]

}

Phy-ParametersFR1 ::= SEQUENCE {

 pdcch-MonitoringSingleOccasion ENUMERATED {supported} OPTIONAL,

 scs-60kHz ENUMERATED {supported} OPTIONAL,

 pdsch-256QAM-FR1 ENUMERATED {supported} OPTIONAL,

 pdsch-RE-MappingFR1-PerSymbol ENUMERATED {n10, n20} OPTIONAL,

 ...,

 [[

 pdsch-RE-MappingFR1-PerSlot ENUMERATED {n16, n32, n48, n64, n80, n96, n112, n128,

 n144, n160, n176, n192, n208, n224, n240, n256} OPTIONAL

 ]]

}

Phy-ParametersFR2 ::= SEQUENCE {

 dummy ENUMERATED {supported} OPTIONAL,

 pdsch-RE-MappingFR2-PerSymbol ENUMERATED {n6, n20} OPTIONAL,

 ...,

 [[

 pCell-FR2 ENUMERATED {supported} OPTIONAL,

 pdsch-RE-MappingFR2-PerSlot ENUMERATED {n16, n32, n48, n64, n80, n96, n112, n128,

 n144, n160, n176, n192, n208, n224, n240, n256} OPTIONAL

 ]]

}

-- TAG-PHY-PARAMETERS-STOP

-- ASN1STOP

|  |
| --- |
| *Phy-ParametersFRX-Diff field description* |
| ***csi-RS-IM-ReceptionForFeedback/ csi-RS-ProcFrameworkForSRS/ csi-ReportFramework***These fields are optionally present in *fr1-fr2-Add-UE-NR-Capabilities* in *UE-NR-Capability*. For a band combination comprised of FR1 and FR2 bands, these parameters, if present, limit the corresponding parameters in *MIMO-ParametersPerBand*. |

#### – *Phy-ParametersMRDC*

The IE *Phy-ParametersMRDC* is used to convey physical layer capabilities for MR-DC.

*Phy-ParametersMRDC* information element

-- ASN1START

-- TAG-PHY-PARAMETERSMRDC-START

Phy-ParametersMRDC ::= SEQUENCE {

 naics-Capability-List SEQUENCE (SIZE (1..maxNrofNAICS-Entries)) OF NAICS-Capability-Entry OPTIONAL,

 ...

}

NAICS-Capability-Entry ::= SEQUENCE {

 numberOfNAICS-CapableCC INTEGER(1..5),

 numberOfAggregatedPRB ENUMERATED {n50, n75, n100, n125, n150, n175, n200, n225,

 n250, n275, n300, n350, n400, n450, n500, spare},

 ...

}

-- TAG-PHY-PARAMETERSMRDC-STOP

-- ASN1STOP

|  |
| --- |
| *PHY-ParametersMRDC* field descriptions |
| ***naics-Capability-List***Indicates that UE in MR-DC supports NAICS as defined in TS 36.331 [10]. |

#### – *ProcessingParameters*

The IE *ProcessingParameters* is used to indicate PDSCH/PUSCH processing capabilities supported by the UE.

*ProcessingParameters* information element

-- ASN1START

-- TAG-PROCESSINGPARAMETERS-START

ProcessingParameters ::= SEQUENCE {

 fallback ENUMERATED {sc, cap1-only},

 differentTB-PerSlot SEQUENCE {

 upto1 NumberOfCarriers OPTIONAL,

 upto2 NumberOfCarriers OPTIONAL,

 upto4 NumberOfCarriers OPTIONAL,

 upto7 NumberOfCarriers OPTIONAL

 } OPTIONAL

}

NumberOfCarriers ::= INTEGER (1..16)

-- TAG-PROCESSINGPARAMETERS-STOP

-- ASN1STOP

#### – *RAT-Type*

The IE *RAT-Type* is used to indicate the radio access technology (RAT), including NR, of the requested/transferred UE capabilities.

*RAT-Type* information element

-- ASN1START

-- TAG-RAT-TYPE-START

RAT-Type ::= ENUMERATED {nr, eutra-nr, eutra, spare1, ...}

-- TAG-RAT-TYPE-STOP

-- ASN1STOP

#### – *RF-Parameters*

The IE *RF-Parameters* is used to convey RF-related capabilities for NR operation.

*RF-Parameters* information element

-- ASN1START

-- TAG-RF-PARAMETERS-START

RF-Parameters ::= SEQUENCE {

 supportedBandListNR SEQUENCE (SIZE (1..maxBands)) OF BandNR,

 supportedBandCombinationList BandCombinationList OPTIONAL,

 appliedFreqBandListFilter FreqBandList OPTIONAL,

 ...,

 [[

 supportedBandCombinationList-v1540 BandCombinationList-v1540 OPTIONAL,

 srs-SwitchingTimeRequested ENUMERATED {true} OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1550 BandCombinationList-v1550 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1560 BandCombinationList-v1560 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v16xy BandCombinationList-v16xy OPTIONAL

 ]]

}

BandNR ::= SEQUENCE {

 bandNR FreqBandIndicatorNR,

 modifiedMPR-Behaviour BIT STRING (SIZE (8)) OPTIONAL,

 mimo-ParametersPerBand MIMO-ParametersPerBand OPTIONAL,

 extendedCP ENUMERATED {supported} OPTIONAL,

 multipleTCI ENUMERATED {supported} OPTIONAL,

 bwp-WithoutRestriction ENUMERATED {supported} OPTIONAL,

 bwp-SameNumerology ENUMERATED {upto2, upto4} OPTIONAL,

 bwp-DiffNumerology ENUMERATED {upto4} OPTIONAL,

 crossCarrierScheduling-SameSCS ENUMERATED {supported} OPTIONAL,

 pdsch-256QAM-FR2 ENUMERATED {supported} OPTIONAL,

 pusch-256QAM ENUMERATED {supported} OPTIONAL,

 ue-PowerClass ENUMERATED {pc1, pc2, pc3, pc4} OPTIONAL,

 rateMatchingLTE-CRS ENUMERATED {supported} OPTIONAL,

 channelBWs-DL CHOICE {

 fr1 SEQUENCE {

 scs-15kHz BIT STRING (SIZE (10)) OPTIONAL,

 scs-30kHz BIT STRING (SIZE (10)) OPTIONAL,

 scs-60kHz BIT STRING (SIZE (10)) OPTIONAL

 },

 fr2 SEQUENCE {

 scs-60kHz BIT STRING (SIZE (3)) OPTIONAL,

 scs-120kHz BIT STRING (SIZE (3)) OPTIONAL

 }

 } OPTIONAL,

 channelBWs-UL CHOICE {

 fr1 SEQUENCE {

 scs-15kHz BIT STRING (SIZE (10)) OPTIONAL,

 scs-30kHz BIT STRING (SIZE (10)) OPTIONAL,

 scs-60kHz BIT STRING (SIZE (10)) OPTIONAL

 },

 fr2 SEQUENCE {

 scs-60kHz BIT STRING (SIZE (3)) OPTIONAL,

 scs-120kHz BIT STRING (SIZE (3)) OPTIONAL

 }

 } OPTIONAL,

 ...,

 [[

 maxUplinkDutyCycle-PC2-FR1 ENUMERATED {n60, n70, n80, n90, n100} OPTIONAL

 ]],

 [[

 pucch-SpatialRelInfoMAC-CE ENUMERATED {supported} OPTIONAL,

 powerBoosting-pi2BPSK ENUMERATED {supported} OPTIONAL

 ]],

 [[

 maxUplinkDutyCycle-FR2 ENUMERATED {n15, n20, n25, n30, n40, n50, n60, n70, n80, n90, n100} OPTIONAL

 ]]

}

-- TAG-RF-PARAMETERS-STOP

-- ASN1STOP

|  |
| --- |
| *RF-Parameters* field descriptions |
| ***appliedFreqBandListFilter***In this field the UE mirrors the *FreqBandList* that the NW provided in the capability enquiry, if any. The UE filtered the band combinations in the *supportedBandCombinationList* in accordance with this *appliedFreqBandListFilter*. The UE does not include this field if the UE capability is requested by E-UTRAN and the network request includes the field *eutra-nr-only* [10]. |
| ***supportedBandCombinationList***A list of band combinations that the UE supports for NR (and NR-DC, if requested). The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-NR-Capability* IE. The UE does not include this field if the UE capability is requested by E-UTRAN and the network request includes the field *eutra-nr-only* [10]. |

#### – *RF-ParametersMRDC*

The IE *RF-ParametersMRDC* is used to convey RF related capabilities for MR-DC.

*RF-ParametersMRDC* information element

-- ASN1START

-- TAG-RF-PARAMETERSMRDC-START

RF-ParametersMRDC ::= SEQUENCE {

 supportedBandCombinationList BandCombinationList OPTIONAL,

 appliedFreqBandListFilter FreqBandList OPTIONAL,

 ...,

 [[

 srs-SwitchingTimeRequested ENUMERATED {true} OPTIONAL,

 supportedBandCombinationList-v1540 BandCombinationList-v1540 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1550 BandCombinationList-v1550 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1560 BandCombinationList-v1560 OPTIONAL,

 supportedBandCombinationListNEDC-Only BandCombinationList OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1570 BandCombinationList-v1570 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v1580 BandCombinationList-v1580 OPTIONAL

 ]],

 [[

 supportedBandCombinationList-v16xy BandCombinationList-v16xy OPTIONAL

 ]]

}

-- TAG-RF-PARAMETERSMRDC-STOP

-- ASN1STOP

|  |
| --- |
| *RF-ParametersMRDC* field descriptions |
| ***appliedFreqBandListFilter***In this field the UE mirrors the *FreqBandList* that the NW provided in the capability enquiry, if any. The UE filtered the band combinations in the *supportedBandCombinationList* in accordance with this *appliedFreqBandListFilter*. |
| ***supportedBandCombinationList***A list of band combinations that the UE supports for (NG)EN-DC and/or NE-DC. The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-MRDC-Capability* IE. |
| ***supportedBandCombinationListNEDC-Only***A list of band combinations that the UE supports only for NE-DC. The *FeatureSetCombinationId*:s in this list refer to the *FeatureSetCombination* entries in the *featureSetCombinations* list in the *UE-MRDC-Capability* IE. |

#### – *RLC-Parameters*

The IE *RLC-Parameters* is used to convey capabilities related to RLC.

*RLC-Parameters* information element

-- ASN1START

-- TAG-RLC-PARAMETERS-START

RLC-Parameters ::= SEQUENCE {

 am-WithShortSN ENUMERATED {supported} OPTIONAL,

 um-WithShortSN ENUMERATED {supported} OPTIONAL,

 um-WithLongSN ENUMERATED {supported} OPTIONAL,

 ...

}

-- TAG-RLC-PARAMETERS-STOP

-- ASN1STOP

#### – *SDAP-Parameters*

The IE *SDAP-Parameters* is used to convey capabilities related to SDAP.

*SDAP-Parameters* information element

-- ASN1START

-- TAG-SDAP-PARAMETERS-START

SDAP-Parameters ::= SEQUENCE {

 as-ReflectiveQoS ENUMERATED {true} OPTIONAL,

 ...

}

-- TAG-SDAP-PARAMETERS-STOP

-- ASN1STOP

#### – *SRS-SwitchingTimeNR*

The IE *SRS-SwitchingTimeNR* is used to indicate the SRS carrier switching time supported by the UE for one NR band pair.

*SRS-SwitchingTimeNR information element*

-- ASN1START

-- TAG-SRS-SWITCHINGTIMENR-START

SRS-SwitchingTimeNR ::= SEQUENCE {

 switchingTimeDL ENUMERATED {n0us, n30us, n100us, n140us, n200us, n300us, n500us, n900us} OPTIONAL,

 switchingTimeUL ENUMERATED {n0us, n30us, n100us, n140us, n200us, n300us, n500us, n900us} OPTIONAL

}

-- TAG-SRS-SWITCHINGTIMENR-STOP

-- ASN1STOP

#### – *SRS-SwitchingTimeEUTRA*

The IE *SRS-SwitchingTimeEUTRA* is used to indicate the SRS carrier switching time supported by the UE for one E-UTRA band pair.

*SRS-SwitchingTimeEUTRA information element*

-- ASN1START

-- TAG-SRS-SWITCHINGTIMEEUTRA-START

SRS-SwitchingTimeEUTRA ::= SEQUENCE {

 switchingTimeDL ENUMERATED {n0, n0dot5, n1, n1dot5, n2, n2dot5, n3, n3dot5, n4, n4dot5, n5, n5dot5, n6, n6dot5, n7}

 OPTIONAL,

 switchingTimeUL ENUMERATED {n0, n0dot5, n1, n1dot5, n2, n2dot5, n3, n3dot5, n4, n4dot5, n5, n5dot5, n6, n6dot5, n7}

 OPTIONAL

}

-- TAG-SRS-SWITCHINGTIMEEUTRA-STOP

-- ASN1STOP

#### – *SupportedBandwidth*

The IE *SupportedBandwidth* is used to indicate the maximum channel bandwidth supported by the UE on one carrier of a band of a band combination.

*SupportedBandwidth* information element

-- ASN1START

-- TAG-SUPPORTEDBANDWIDTH-START

SupportedBandwidth ::= CHOICE {

 fr1 ENUMERATED {mhz5, mhz10, mhz15, mhz20, mhz25, mhz30, mhz40, mhz50, mhz60, mhz80, mhz100},

 fr2 ENUMERATED {mhz50, mhz100, mhz200, mhz400}

}

-- TAG-SUPPORTEDBANDWIDTH-STOP

-- ASN1STOP

#### – *UE-CapabilityRAT-ContainerList*

The IE *UE-CapabilityRAT-ContainerList* contains a list of radio access technology specific capability containers.

*UE-CapabilityRAT-ContainerList* information element

-- ASN1START

-- TAG-UE-CAPABILITYRAT-CONTAINERLIST-START

UE-CapabilityRAT-ContainerList ::= SEQUENCE (SIZE (0..maxRAT-CapabilityContainers)) OF UE-CapabilityRAT-Container

UE-CapabilityRAT-Container ::= SEQUENCE {

 rat-Type RAT-Type,

 ue-CapabilityRAT-Container OCTET STRING

}

-- TAG-UE-CAPABILITYRAT-CONTAINERLIST-STOP

-- ASN1STOP

|  |
| --- |
| *UE-CapabilityRAT-ContainerList* field descriptions |
| ***ue-CapabilityRAT-Container***Container for the UE capabilities of the indicated RAT. The encoding is defined in the specification of each RAT:For *rat-Type* set to *nr*: the encoding of UE capabilities is defined in *UE-NR-Capability*.For *rat-Type* set to *eutra-nr*: the encoding of UE capabilities is defined in *UE-MRDC-Capability*.For *rat-Type* set to *eutra*: the encoding of UE capabilities is defined in *UE-EUTRA-Capability* specified in TS 36.331 [10]. |

#### – *UE-CapabilityRAT-RequestList*

The IE *UE-CapabilityRAT-RequestList* is used to request UE capabilities for one or more RATs from the UE.

*UE-CapabilityRAT-RequestList* information element

-- ASN1START

-- TAG-UE-CAPABILITYRAT-REQUESTLIST-START

UE-CapabilityRAT-RequestList ::= SEQUENCE (SIZE (1..maxRAT-CapabilityContainers)) OF UE-CapabilityRAT-Request

UE-CapabilityRAT-Request ::= SEQUENCE {

 rat-Type RAT-Type,

 capabilityRequestFilter OCTET STRING OPTIONAL, -- Need N

 ...

}

-- TAG-UE-CAPABILITYRAT-REQUESTLIST-STOP

-- ASN1STOP

|  |
| --- |
| *UE-CapabilityRAT-Request* field descriptions |
| ***capabilityRequestFilter***Information by which the network requests the UE to filter the UE capabilities.For *rat-Type* set to *nr* or *eutra-nr*: the encoding of the *capabilityRequestFilter* is defined in *UE-CapabilityRequestFilterNR*.For *rat-Type* set to *eutra*: the encoding of the *capabilityRequestFilter* is defined by *UECapabilityEnquiry* message defined in TS36.331 [10], in which *RAT-Type* in *UE-CapabilityRequest* includes only '*eutra'*. |
| ***rat-Type***The RAT type for which the NW requests UE capabilities. |

#### – *UE-CapabilityRequestFilterCommon*

The IE *UE-CapabilityRequestFilterCommon* is used to request filtered UE capabilities. The filter is common for all capability containers that are requested.

*UE-CapabilityRequestFilterCommon* information element

-- ASN1START

-- TAG-UE-CAPABILITYREQUESTFILTERCOMMON-START

UE-CapabilityRequestFilterCommon ::= SEQUENCE {

 mrdc-Request SEQUENCE {

 omitEN-DC ENUMERATED {true} OPTIONAL, -- Need N

 includeNR-DC ENUMERATED {true} OPTIONAL, -- Need N

 includeNE-DC ENUMERATED {true} OPTIONAL -- Need N

 } OPTIONAL, -- Need N

 ...

}

-- TAG-UE-CAPABILITYREQUESTFILTERCOMMON-STOP

-- ASN1STOP

|  |
| --- |
| *UE-CapabilityRequestFilterCommon field descriptions* |
| ***includeNE-DC***Only if this field is present, the UE supporting NE-DC shall indicate support for NE-DC in band combinations and include feature set combinations which are applicable to NE-DC. Band combinations supporting both NE-DC and (NG)EN-DC shall be included in *supportedBandCombinationList*, band combinations supporting only NE-DC shall be included in *supportedBandCombinationListNEDC-Only*. |
| ***includeNR-DC***Only if this field is present, the UE supporting NR-DC shall indicate support for NR-DC in band combinations and include feature set combinations which are applicable to NR-DC. |
| ***omitEN-DC***Only if this field is present, the UE shall omit band combinations and feature set combinations which are only applicable to (NG)EN-DC. |

#### – *UE-CapabilityRequestFilterNR*

The IE *UE-CapabilityRequestFilterNR* is used to request filtered UE capabilities.

*UE-CapabilityRequestFilterNR* information element

-- ASN1START

-- TAG-UE-CAPABILITYREQUESTFILTERNR-START

UE-CapabilityRequestFilterNR ::= SEQUENCE {

 frequencyBandListFilter FreqBandList OPTIONAL, -- Need N

 nonCriticalExtension UE-CapabilityRequestFilterNR-v1540 OPTIONAL

}

UE-CapabilityRequestFilterNR-v1540 ::= SEQUENCE {

 srs-SwitchingTimeRequest ENUMERATED {true} OPTIONAL, -- Need N

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

-- TAG-UE-CAPABILITYREQUESTFILTERNR-STOP

-- ASN1STOP

#### – *UE-MRDC-Capability*

The IE *UE-MRDC-Capability* is used to convey the UE Radio Access Capability Parameters for MR-DC, see TS 38.306 [26].

*UE-MRDC-Capability* information element

-- ASN1START

-- TAG-UE-MRDC-CAPABILITY-START

UE-MRDC-Capability ::= SEQUENCE {

 measAndMobParametersMRDC MeasAndMobParametersMRDC OPTIONAL,

 phy-ParametersMRDC-v1530 Phy-ParametersMRDC OPTIONAL,

 rf-ParametersMRDC RF-ParametersMRDC,

 generalParametersMRDC GeneralParametersMRDC-XDD-Diff OPTIONAL,

 fdd-Add-UE-MRDC-Capabilities UE-MRDC-CapabilityAddXDD-Mode OPTIONAL,

 tdd-Add-UE-MRDC-Capabilities UE-MRDC-CapabilityAddXDD-Mode OPTIONAL,

 fr1-Add-UE-MRDC-Capabilities UE-MRDC-CapabilityAddFRX-Mode OPTIONAL,

 fr2-Add-UE-MRDC-Capabilities UE-MRDC-CapabilityAddFRX-Mode OPTIONAL,

 featureSetCombinations SEQUENCE (SIZE (1..maxFeatureSetCombinations)) OF FeatureSetCombination OPTIONAL,

 pdcp-ParametersMRDC-v1530 PDCP-ParametersMRDC OPTIONAL,

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension UE-MRDC-Capability-v1560 OPTIONAL

}

UE-MRDC-Capability-v1560 ::= SEQUENCE {

 receivedFilters OCTET STRING (CONTAINING UECapabilityEnquiry-v1560-IEs) OPTIONAL,

 measAndMobParametersMRDC-v1560 MeasAndMobParametersMRDC-v1560 OPTIONAL,

 fdd-Add-UE-MRDC-Capabilities-v1560 UE-MRDC-CapabilityAddXDD-Mode-v1560 OPTIONAL,

 tdd-Add-UE-MRDC-Capabilities-v1560 UE-MRDC-CapabilityAddXDD-Mode-v1560 OPTIONAL,

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

UE-MRDC-CapabilityAddXDD-Mode ::= SEQUENCE {

 measAndMobParametersMRDC-XDD-Diff MeasAndMobParametersMRDC-XDD-Diff OPTIONAL,

 generalParametersMRDC-XDD-Diff GeneralParametersMRDC-XDD-Diff OPTIONAL

}

UE-MRDC-CapabilityAddXDD-Mode-v1560 ::= SEQUENCE {

 measAndMobParametersMRDC-XDD-Diff-v1560 MeasAndMobParametersMRDC-XDD-Diff-v1560 OPTIONAL

}

UE-MRDC-CapabilityAddFRX-Mode ::= SEQUENCE {

 measAndMobParametersMRDC-FRX-Diff MeasAndMobParametersMRDC-FRX-Diff

}

GeneralParametersMRDC-XDD-Diff ::= SEQUENCE {

 splitSRB-WithOneUL-Path ENUMERATED {supported}  OPTIONAL,

 splitDRB-withUL-Both-MCG-SCG ENUMERATED {supported} OPTIONAL,

 srb3 ENUMERATED {supported} OPTIONAL,

 v2x-EUTRA ENUMERATED {supported} OPTIONAL,

 ...

}

-- TAG-UE-MRDC-CAPABILITY-STOP

-- ASN1STOP

|  |
| --- |
| *UE-MRDC-Capability* field descriptions |
| ***featureSetCombinations***A list of *FeatureSetCombination*:s for *supportedBandCombinationList* and *supportedBandCombinationListNEDC-Only* in *UE-MRDC-Capability*. The *FeatureSetDownlink*:s and *FeatureSetUplink*:s referred to from these *FeatureSetCombination*:s are defined in the *featureSets* list in *UE-NR-Capability*. |

#### – *UE-NR-Capability*

The IE *UE-NR-Capability* is used to convey the NR UE Radio Access Capability Parameters, see TS 38.306 [26].

*UE-NR-Capability* information element

-- ASN1START

-- TAG-UE-NR-CAPABILITY-START

UE-NR-Capability ::= SEQUENCE {

 accessStratumRelease AccessStratumRelease,

 pdcp-Parameters PDCP-Parameters,

 rlc-Parameters RLC-Parameters OPTIONAL,

 mac-Parameters MAC-Parameters OPTIONAL,

 phy-Parameters Phy-Parameters,

 rf-Parameters RF-Parameters,

 measAndMobParameters MeasAndMobParameters OPTIONAL,

 fdd-Add-UE-NR-Capabilities UE-NR-CapabilityAddXDD-Mode OPTIONAL,

 tdd-Add-UE-NR-Capabilities UE-NR-CapabilityAddXDD-Mode OPTIONAL,

 fr1-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

 fr2-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

 featureSets FeatureSets OPTIONAL,

 featureSetCombinations SEQUENCE (SIZE (1..maxFeatureSetCombinations)) OF FeatureSetCombination OPTIONAL,

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1530 OPTIONAL

}

UE-NR-Capability-v1530 ::= SEQUENCE {

 fdd-Add-UE-NR-Capabilities-v1530 UE-NR-CapabilityAddXDD-Mode-v1530 OPTIONAL,

 tdd-Add-UE-NR-Capabilities-v1530 UE-NR-CapabilityAddXDD-Mode-v1530 OPTIONAL,

 dummy ENUMERATED {supported} OPTIONAL,

 interRAT-Parameters InterRAT-Parameters OPTIONAL,

 inactiveState ENUMERATED {supported} OPTIONAL,

 delayBudgetReporting ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1540 OPTIONAL

}

UE-NR-Capability-v1540 ::= SEQUENCE {

 sdap-Parameters SDAP-Parameters OPTIONAL,

 overheatingInd ENUMERATED {supported} OPTIONAL,

 ims-Parameters IMS-Parameters OPTIONAL,

 fr1-Add-UE-NR-Capabilities-v1540 UE-NR-CapabilityAddFRX-Mode-v1540 OPTIONAL,

 fr2-Add-UE-NR-Capabilities-v1540 UE-NR-CapabilityAddFRX-Mode-v1540 OPTIONAL,

 fr1-fr2-Add-UE-NR-Capabilities UE-NR-CapabilityAddFRX-Mode OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1550 OPTIONAL

}

UE-NR-Capability-v1550 ::= SEQUENCE {

 reducedCP-Latency ENUMERATED {supported} OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1560 OPTIONAL

}

UE-NR-Capability-v1560 ::= SEQUENCE {

 nrdc-Parameters NRDC-Parameters OPTIONAL,

 receivedFilters OCTET STRING (CONTAINING UECapabilityEnquiry-v1560-IEs) OPTIONAL,

 nonCriticalExtension UE-NR-Capability-v1570 OPTIONAL

}

UE-NR-Capability-v1570 ::= SEQUENCE {

 nrdc-Parameters-v1570 NRDC-Parameters-v1570 OPTIONAL,

 nonCriticalExtension SEQUENCE {} OPTIONAL

}

UE-NR-CapabilityAddXDD-Mode ::= SEQUENCE {

 phy-ParametersXDD-Diff Phy-ParametersXDD-Diff OPTIONAL,

 mac-ParametersXDD-Diff MAC-ParametersXDD-Diff OPTIONAL,

 measAndMobParametersXDD-Diff MeasAndMobParametersXDD-Diff OPTIONAL

}

UE-NR-CapabilityAddXDD-Mode-v1530 ::= SEQUENCE {

 eutra-ParametersXDD-Diff EUTRA-ParametersXDD-Diff

}

UE-NR-CapabilityAddFRX-Mode ::= SEQUENCE {

 phy-ParametersFRX-Diff Phy-ParametersFRX-Diff OPTIONAL,

 measAndMobParametersFRX-Diff MeasAndMobParametersFRX-Diff OPTIONAL

}

UE-NR-CapabilityAddFRX-Mode-v1540 ::= SEQUENCE {

 ims-ParametersFRX-Diff IMS-ParametersFRX-Diff OPTIONAL

}

-- TAG-UE-NR-CAPABILITY-STOP

-- ASN1STOP

|  |
| --- |
| *UE-NR-Capability* field descriptions |
| ***featureSetCombinations***A list of *FeatureSetCombination:s* for *supportedBandCombinationList* in *UE-NR-Capability*. The *FeatureSetDownlink:s* and *FeatureSetUplink:s* referred to from these *FeatureSetCombination:s* are defined in the *featureSets* list in *UE-NR-Capability*. |