3GPP TSG-RAN WG2 Meeting #109e [R2-200xxx](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-200xxxx.zip)x

Elbonia, Online, 24 February – 6 March 2020

**Agenda item: 4.5**

**Source: Nokia (offline email discussion rapporteur)**

**Title: Report of [AT109e][203][LTE15] LTE pre-Rel-15 CRs on CA (Nokia)**

**Document for: Report**

# 1 Scope of the offline email discussion

This document contains the summary of the offline email discussion “**[AT109e][203][LTE15] LTE pre-Rel-15 CRs on CA (Nokia)**”, as indicated below:

* [AT109e][203][LTE15] LTE pre-Rel-15 CRs on CA (Nokia)

Scope:

* + - Discuss the topics identified in [R2-2001134](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001134.zip)
    - Discuss which (if any) of the CRs [R2-2001135](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001135.zip), [R2-2001136](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001136.zip), [R2-2001137](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001137.zip), [R2-2001138](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001138.zip) are needed.
    - Discuss the CRs [R2-2001140](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001140.zip), [R2-2001141](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001141.zip), [R2-2001142](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001142.zip) to determine whether the proposed interpretation is correct and how should a correction (if needed) be captured

Intended outcome:

* + - Set of proposals with consensus (aim to agree to those over email), including the correct interpretation to both sets of CRs (by email rappporteur)

Deadline for providing comments and for rapporteur inputs:

* + - Companies input: Wednesday, Feb. 26th 17:00 CET
    - Rapporteur proposals: Thursday, Feb. 27th 17:00 CET (one day for rapporteur to make conclusions)
    - Updated CRs from each CR proponent: Friday Feb 28th 17:00 CET
    - Comments on the CR wording: Monday, March 2nd by 17:00 CET (i.e. one day to provide comments to the updated CR)

# 2 Interpretation of UE capabilities for non-contiguous intra-band CA

This section addresses topics identified in the input document to RAN2#109e in [R2-2001134](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001134.zip) [1] on UE capabilities for non-contiguous intra-band CA interpretation.

The following list of discussion points aim at clarifying the interpretation of associated UE capabilities.

## 2.1 Observations on differences of UE capabilities for intra-band contiguous and non-contiguous CA

While inter-band CA always consists of two or more disparate frequency blocks, Intra-band CA comes in two flavors: Intra-band contiguous CA (with at least two carriers aggregated together without frequency gaps) and intra-band non-contiguous CA (with at least two carriers aggregated together so that there is a frequency gap between the aggregated carriers). In [R2-2001134](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001134.zip) [1] we identified several issues that led to the following observations:

**Observation 1:** Intra-band contiguous CA capabilities are all contained within a single band entry of a band combination, while intra-band non-contiguous CA capabilities require at least two band entries.

**Observation 2:** For intra-band contiguous carriers, UE band combination capabilities specify that UE supports any ordering of the capabilities.

**Observation 3:** UE band combination capabilities do not clearly specify whether capabilities applicable for different carriers in case of intra-band non-contiguous behave similarly as with intra-band contiguous CA.

**Observation 4** (Based on TS36.306): If the MIMO capabilities are not agnostic to the order in which they are indicated for intra-band non-contigous band combinations, network may under-utilize the UE capabilities or require additional reconfigurations to utilize them fully

**Observation 5** (Based on TS36.101): The ordering of intra-band non-contiguous entries is relevant for the support of BCS.

**Observation 6** (Based on TS36.101): The ordering of BCS is not directly related to the MIMO capabilities.

**Question 1:** Do companies agree with the Observation 1-6?

|  |  |  |
| --- | --- | --- |
| **Company** | **Do you agree with the Observation 1 to 6?** | **Detailed comments** |
|  |  |  |
|  |  |  |

Conclusion: TBA

Proposal: TBA

## 2.2 Conclusion on interpretation of UE capabilities intra-band non-contiguous BCs

How should the UE indicate its capabilities if it supports order-agnostic MIMO with CA\_xA\_xA? Should it indicate:

1. Duplicate band combination entries, each with different MIMO layer ordering (i.e. one BC with (2,4) MIMO layers and one with (4,2) MIMO layers?  
   OR
2. Single band combination with e.g. (4,2) MIMO layers (assuming network comprehends this applies for either ordering)?

From network viewpoint, both capabilities are valid but either has its issues: For 1), it is clear that UE supports both orderings, but does it also mean that such a UE may NOT support all orderings in case it uses 2) for some intra-band non-contiguous BC? And similarly, for 2), is it clear that this UE only supports (4,2) and not (2,4), or does it always support both orderings if it never duplicates the BCs for any intra-band non-contiguous cases?

**Observation 7:** The example of UE capabilities for the intra-band non-contiguous BCs leads to two different interpretations.

**Question 2:** Do companies agree both interpretations are valid?

|  |  |  |
| --- | --- | --- |
| **Company** | **Do you agree with the Observation 7?** | **Detailed comments** |
|  |  |  |
|  |  |  |

Conclusion: TBA

Proposal: TBA

## 2.3 Need for clarification on UE capabilities intra-band non-contiguous BCs

We have observed both types of UEs can be seen in the field. At least in some cases, both types of UEs still do support both orderings, but since this is not clear in specifications it should be clarified whether this applies also to all UEs. Therefore, we would like to clarify what the common understanding in RAN2 is with regard to this to minimize any IODT issues.

RAN2 need to establish common understanding on MIMO layer and CSI processing capabilities with intra-band non-contiguous CA: E.g. If UE supports (2, 4) MIMO layers with CA\_xA\_xA, will it also support (4, 2) MIMO layers with CA\_xA\_xA?

**Question 3:** Do companies agree RAN2 specification(s) need to reflect common understanding on MIMO layer and CSI processing capabilities with intra-band non-contiguous CA

|  |  |  |
| --- | --- | --- |
| **Company** | **Do you agree with the Observation 8?** | **Detailed comments** |
|  |  |  |
|  |  |  |

Conclusion: TBA

Proposal: TBA

## 2.4 [R2-2001135](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001135.zip), “Clarification to UE capabilities for non-contiguous intra-band CA “

The CR in [R2-2001135](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001135.zip) [2] on UE capabilities for non-contiguous intra-band CA interpretation is addressing the issue and intends to clarify whether UE indicating support for a BC involving intra-band non-contiguous CA with certain capabilities (e.g. CA\_xA\_xA with MIMO layers set as 4 layers + 2 layers) also supports any ordering of the capabilities between the non-contiguous entries (e.g. also 2 layers + 4 layers in the example case).

**Question 4:** Do companies agree with the intent of the CR [R2-2001135](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001135.zip)?

|  |  |  |
| --- | --- | --- |
| **Company** | **Do you agree with the intent of the CR?** | **Detailed comments** |
|  |  |  |
|  |  |  |

Conclusion: TBA

Proposal: TBA

## 2.5 Which release to start with to incorporate the clarification?

The CR in [R2-2001135](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001135.zip) [2] introduce the clarification for Rel-12 version of the TS36.331. The clarification ensures all UE and network implementations comprehend it in the same way. Mirror corrections towards Rel-13, Rel-14 and Rel-15 are proposed in [3],[4],[5].

**Question 5:** Do companies agree the clarification should be introduced from Rel-12?

|  |  |  |
| --- | --- | --- |
| **Company** | **Do you agree with the first release of the clarification to be Rel-12?** | **Detailed comments** |
|  |  |  |
|  |  |  |

Conclusion: TBA

Proposal: TBA

# 3 Mandatory aspect of the HARQ ACK codebook capabilities

This section addresses an issue identified in the input document to RAN2#109e in [R2-2001140](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001140.zip) [6]. The CR intends to clarify UE’s *codebook-HARQ-ACK-r13* capability meaning.

The field is used to indicate a method which UE supports to determine HARQ-ACK codebook size. According to TS36.331, the UE signals the capability: codebook-HARQ-ACK-r13 as follows:

PhyLayerParameters-v1310 ::= SEQUENCE {

codebook-HARQ-ACK-r13 BIT STRING (SIZE (2)) OPTIONAL,

where:

* first bit of the capability set to "1" implies the UE supports the DAI-based codebook size determination
* second bit is set to "1" if the UE supports the codebook determination based on the number of configured CCs.

The requirement added on codebook-HARQ-ACK-r13 in Rel-13 (in the capability description in TS36.306), that was supposed to support Rel-13 CA aggregation enhancements was as follows:

“For both solutions, it is mandatory for UEs of this release of the specification if carrier aggregation with more than 5 DL component carriers is supported. “

This statement intended to follow the recommendation agreed by RAN1 on Rel-13 CA aggregation enhancements support:

|  |
| --- |
| RAN1#82bis agreed (see: [report](https://www.3gpp.org/ftp/TSG_RAN/WG1_RL1/TSGR1_82b/Report/)):   * eNodeB can configure by RRC signaling an eCA UE to determine HARQ-ACK codebook size according to either (a) or (b) as follows:   a) DAI based solution (…)  b) Number of configured CCs based solution (…)   * Both solution (a) and solution (b) are mandatory feature as UE capability from RAN1 recommendation point of views for UEs supporting more than 5 CCs |

**Observation 8:** Both solution (a)DAI based) and solution (b)CC based) are mandatory feature as UE capability from RAN1 point of views for UEs supporting more than 5 CCs

**Question 6:** Do companies agree with the Observation 8?

|  |  |  |
| --- | --- | --- |
| **Company** | **Do companies agree with the Observation 8?** | **Detailed comments** |
|  |  |  |
|  |  |  |

Conclusion: TBA

Proposal: TBA

## 3.2 [R2-2001140](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001140.zip), “Clarification on codebook-HARQ-ACK-r13 capability for CA with more than 5CCs

The CR in [R2-2001140](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001140.zip) [6] on UE capabilities for non-contiguous intra-band CA interpretation is addressing the issue that added statement to the concerned UE capability (i.e. “For both solutions, it is mandatory for UEs of this release of the specification if carrier aggregation with more than 5 DL component carriers is supported. “ ) does not explicitly reflect the RAN1 agreement.

The CR intent is to clarify the requirement added on codebook-HARQ-ACK-r13 in the TS36.306 should reflect the RAN1 agreement:

* Both solution (a) and solution (b) are mandatory feature as UE capability from RAN1 recommendation point of views for UEs supporting more than 5 CCs

**Question 7:** Do companies agree with the intent of the CR [R2-2001140](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001140.zip)?

|  |  |  |
| --- | --- | --- |
| **Company** | **Do you agree with the intent of the CR?** | **Detailed comments** |
| Ericsson | **No** | We think the change is not needed since it is clear from the spec that it is mandatory to support both solutions if the UE supports carrier aggregation with more than 5 DL. |
|  |  |  |

Conclusion: TBA

Proposal: TBA

## 3.3 Which release to start with to incorporate the clarification?

The CR in [R2-2001140](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001140.zip) [6] introduce the clarification starting from TS36.306 v13.12.0. The clarification ensures all UE and network implementations comprehend it in the same way. Mirror corrections towards Rel-14, and Rel-15 are proposed in [7],[8], respectively.

**Question 8:** Do companies agree the clarification should be introduced from Rel-13?

|  |  |  |
| --- | --- | --- |
| **Company** | **Do you agree with the first release of the clarification to be Rel-13?** | **Detailed comments** |
| Ericsson | **No** | Please see the comments above. |
|  |  |  |

Conclusion: TBA

Proposal: TBA

# 4 Conclusions

**Conclusions:**

TBA – list of conclusions for each CR.

**Agreed CRs:**

TBA – list of agreed CRs (with Tdoc numbers).

# 5 List of referenced documents

[1] [R2-2001134](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001134.zip) Interpretation of UE capabilities for non-contiguous intra-band CA Nokia, Nokia Shanghai Bell discussion Rel-12 LTE\_CA-Core, TEI12

[2] [R2-2001135](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001135.zip) Clarification to UE capabilities for non-contiguous intra-band CA Nokia, Nokia Shanghai Bell CR Rel-12 36.331 12.18.0 4206 - F LTE\_CA-Core, TEI12

[3] [R2-2001136](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001136.zip) Clarification to UE capabilities for non-contiguous intra-band CA Nokia, Nokia Shanghai Bell CR Rel-13 36.331 13.15.0 4207 - A LTE\_CA-Core, TEI12

[4] [R2-2001137](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001137.zip) Clarification to UE capabilities for non-contiguous intra-band CA Nokia, Nokia Shanghai Bell CR Rel-14 36.331 14.13.0 4208 - A LTE\_CA-Core, TEI12

[5] [R2-2001138](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001138.zip) Clarification to UE capabilities for non-contiguous intra-band CA Nokia, Nokia Shanghai Bell CR Rel-15 36.331 15.8.0 4209 - A LTE\_CA-Core, TEI12

[6] [R2-2001140](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001140.zip) Clarification on codebook-HARQ-ACK-r13 capability for CA with more than 5CCs Nokia, Nokia Shanghai Bell CR Rel-13 36.306 13.12.0 1737 - F LTE\_CA\_enh\_b5C-Core

[7] [R2-2001141](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001141.zip) Clarification on codebook-HARQ-ACK-r13 capability for CA with more than 5CCs Nokia, Nokia Shanghai Bell CR Rel-14 36.306 14.11.0 1738 - A LTE\_CA\_enh\_b5C-Core

[8] [R2-2001142](https://www.3gpp.org/ftp/TSG_RAN/WG2_RL2/TSGR2_109_e/Docs/R2-2001142.zip) Clarification on codebook-HARQ-ACK-r13 capability for CA with more than 5CCs Nokia, Nokia Shanghai Bell CR Rel-15 36.306 15.7.0 1739 - A LTE\_CA\_enh\_b5C-Core