3GPP TSG-RAN WG2 Meeting #109-e R2-200xxxx

Elbonia, Online, 24 February – 6 March 2020

**Agenda item: 7.3.2.3**

**Source: LG Electronics Inc. (summary rapporteur)**

**Title: Closing UP issues (PDCP/RLC/MAC) and discussing remaining open items for DAPS**

**WID/SID: NR\_Mob\_enh-Core/** **LTE\_feMob-Core - Release 16**

**Document for: Discussion and Decision**

# 1 Brief scope

The scope of this document is as follows.

* Agreeing on the proposals as per R2-2001532 and R2-2002099.
* Discuss open items as per R2-2001532 and R2-2002099 to seek companies feedback on open issues of UP for DAPS.

# 2 Summary

## 2.1 Is PDCP status report for UM DRB needed?

As stated in [1], it was indicated whether the PDCP status report for UM DRB should be introduced to minimize the number of the duplicated PDCP PDU. For this issue, we would like to ask the RAN2 companies to answer the following question:

Q1. Do you think the PDCP status report for UM DRBs is needed for DAPS HO?

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| LG | Yes | Considering that the purpose of the PDCP status report is to minimize the number of duplicated PDCP PDUs, PDCP status report UM DRBs should be considered for DAPS HO. |
|  |  |  |
|  |  |  |

The text proposal will be provided based on the submitted CR/contribution if needed.

Conclusion: To be updated

Text proposal: To be updated

## 2.2 Is the PDCP status report triggered when releasing the source link?

As stated in [1], it was addressed whether the PDCP status report is triggered when releasing the source link (let’s call it the second PDCP status report). For this issue, we would like to ask the RAN2 companies to answer the following question:

Q2. Do you think the second PDCP status report is needed?

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| LG | No | Since the time between the first PDCP status report (i.e. at the UL data switching) and the second PDCP status report (i.e. at the source cell release) may be very short, there will only be a few DL packets sent from the source cell to the UE and therefore there is no strong need for the second PDCP status report. |
|  |  |  |
|  |  |  |

Conclusion: To be updated

If the answer for Q2 is yes, we would like to ask company view on that the second PDCP status report is applied to only AM DRBs or AM and UM DRBs.

Q3. Do you think the second PDCP status report is triggered only for AM DRB or AM and UM DRBs?

|  |  |  |
| --- | --- | --- |
| Company | AM DRBs/ AM and UM DRBs | Comments |
| LG |  | The second PDCP status report should not be introduced. |
|  |  |  |
|  |  |  |

The text proposal will be provided based on the submitted CR/contribution if needed.

Conclusion: To be updated

Text proposal: To be updated

## 2.3 How to handle the stored PDCP PDUs received from the source cell when releasing the source cell

As stated in [1], it is addressed how to handle the stored PDCP PDUs received from the source cell when releasing the source cell. However, in the 108#66 email discussion, many companies thought that this issue can be resolved by UE implementation. For this issue, we would like to ask the RAN2 companies to answer the following question:

Q4: Do you think the stored PDCP PDUs received from the source cell can be handled by the UE implementation?

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| LG | No | According to the current specification, the PDCP entity decompresses the stored PDCP PDU at PDCP re-establishment. In other words, how to handle the stored PDCP PDU is already defined in the specification. Considering this, we think that how to handle the stored PDCP PDUs received from the source cell when releasing the source cell should be specified in the spec. |
|  |  |  |
|  |  |  |

The text proposal will be provided based on the submitted CR/contribution if needed.

Conclusion: To be updated

Text proposal: To be updated

## 2.4 Should the consecutive ROHC decompression failure be resolved?

As stated in [1], it is addressed how to prevent the consecutive ROHC decompression failure. However, in the 108#66 email discussion, companies thought that this issue can be resolved by UE/NW implementation. For this issue, we would like to ask the RAN2 companies to answer the following question:

Q5. Which option do you prefer to solve this issue?

* Option 1. The target cell always transmits the PDCP PDUs containing IR packet until releasing the source cell.
* Option 2. The PDCP entity in UE decompresses the PDCP PDUs received from the target cell even if the PDCP PDUs are discarded due to duplication detection and out-of-window.
* Option 3. It is leave up to UE implementation.

|  |  |  |
| --- | --- | --- |
| Company | Option | Comments |
| LG | Option 2 | In LTE, in order to prevent the consecutive ROHC decompression, the PDCP entity for none split bearer decompresses a PDCP PDU even if the PDCP PDU will be discarded due to out-of-window and duplication reception. We think that the same principle can be applied to the NR and LTE. |
|  |  |  |
|  |  |  |

If either option 1 or option 2 is agreed, the text proposal will be provided based on the submitted CR/contribution.

Conclusion: To be updated.

Text proposal: To be updated.

## 2.5 Are two PDCP reordering functions needed?

As stated in [1], it was addressed whether the two reordering functions should be specified or not, i.e., one is for decompression and another is for in-order delivery. For this issue, we would like to ask the RAN2 companies to answer the following question:

Q6: Do you think two PDCP reordering functions are needed, i.e., one is for decompression and another is for in-order delivery?

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| LG | No | In the current specification, when the PDCP entity receives the PDCP PDUs from the lower layers, the PDCP entity performs the security, i.e., deciphering and integrity verification to the received PDCP PDUs. After that, the PDCP entity decompresses the received PDCP PDUs when the received PDCP PDUs are delivered to the upper layer. Considering this, even if the one ordering function is used, i.e., current specification for LTE and NR, there is no problem to support in-order delivery and decompression. Thus, we do not think two reordering functions are needed. |
|  |  |  |
|  |  |  |

The text proposal will be provided based on the submitted CR/contribution if needed.

Conclusion: To be updated.

Text proposal: To be updated.

## 2.6 How to support the UDC for DAPS HO (only for LTE)?

As stated in [1], it was addressed whether and what will specify UDC for DAPS HO. However, RAN2 did not spend much time to discuss how to specify the UDC for DAPS HO. For this issue, we would like to ask the RAN2 companies to answer the following question:

Q7: What should be considered to support the UDC for DAPS?

|  |  |
| --- | --- |
| Company | Comments |
| LG | In our view, RAN2 should discuss many things to support the UDC for DAPS HO, e.g., are two UDC function needed, when the UDC function should be reset and so on. However, we think that RAN2 may not have enough time to discuss them. Thus, even if there is an agreement “support UDC”, we suggest that the UDC should not be considered for DAPS HO in Rel-16. |
|  |  |
|  |  |

The text proposal will be provided based on the submitted CR/contribution if needed.

Conclusion: To be updated.

Text proposal: To be updated.

## 2.7 How to prevent the transmission of the packet generated by the non-DAPS DRBs?

As stated in [3], it was addressed that the LCHs corresponding to non-DAPS DRBs should not be considered for LCP procedure of the source MAC entity during DAPS handover, not to allow the uplink resource to LCHs corresponding to non-DAPS DRBs, which should not perform data transmission. Thus, it is proposed that during DAPS handover, the source MAC entity selects only the logical channels corresponding to DAPS DRBs when the LCP procedure is applied.

For this issue, the summary rapporteur supposes that current running RRC CR [4] implies that the previous *LogicalChannelConfig* of non-DAPS DRBs from the source MAC entity has been already replaced. With this understanding, the summary rapporteur suggests that RAN2 confirm the understanding that whether the *LogicalChannelConfig* of non-DAPS DRBs from the source MAC entity should be released during DAPS HO. For this issue, we would like to ask the RAN2 companies to answer the following question:

Q8. Do you think the *LogicalChannelConfig* of non-DAPS DRBs from the source MAC entity should be released during DAPS HO?

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| LG | No | If the UE performs the DAPS HO, the RLC entity associated with non-DAPS HO performs the re-establishment procedure. In other words, there is no stored RLC PDUs in the transmission buffer. Thus, even if the previous LCH config is applied, the RLC PDUs associated with non-DAPS HO are not transmitted to the source cell. Thus, we do not need to specify anything to prevent the transmission of the packet generated by non-DAPS DRBs. |
|  |  |  |
|  |  |  |

Conclusion: To be updated.

Q9. If the answer for Q8 is yes, do you think that the further clarification in RRC is needed?

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| LG |  | We do not need to specify anything for this issue. |
|  |  |  |
|  |  |  |

Conclusion: To be updated.

Q10. If the answer for Q8 is no, do you agree that “the source MAC entity selects only the logical channels corresponding to DAPS DRBs when the LCP procedure is applied, and the LCHs corresponding to non-DAPS DRBs should not be considered for LCP procedure of the source MAC entity during DAPS HO”

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| LG |  | We do not need to specify anything for this issue. |
|  |  |  |
|  |  |  |

The text proposal will be provided based on the submitted CR/contribution if needed.

Conclusion: To be updated.

Text proposal: To be updated.

# 3 Conclusions

Based on the above discussion, we propose the followings.

**To be updated.**

# 4 List of referenced documents

[1] R2-2001532 “Summary on PDCP/RLC aspects of DAPS HO in AI 7.3.2.1.1” LG Electronics Inc.

[2] R2-2000461 “Report of [108#66][LTE NR Mob] Open issues for LTE and NR mobility” Intel.

[3] R2-2002099 “Summary of DAPS MAC” vivo.

[4] R2-2000462 “RRC running CR for introduction of NR mobility enhancement [108#34]” Intel.