3GPP TSG-RAN WG2 Meeting #109e R2-20xxxxx

Elbonia, Online, 24 February – 6 March 2020

**Agenda item: 6.9.4.2**

**Source: CATT (offline rapporteur)**

**Title: Terminology and other open issues for stage 3 capturing of CPC**

**WID/SID: NR\_Mob\_enh-Core - Release 16**

**Document for: Discussion and Decision**

# 1 Brief scope of the Conditional PSCell Change

This document is to discuss the open issues for TS 38.331 CR capturing agreements for CPC. The issue of terminology was raised during the email discussion 108#67. Any other stage 3 issues requiring discussion/ wider company opinion can be included in other section of this document.

# 2 Terminology for capturing CPC

During email discussion 108#67, all companies agree to reuse the IE defined for CHO even for CPC. The field name of the IE could be changed to reflect that the IE is used for both CHO and CPC.

The draft CR for TS 38.331 uses the terminology option 1 while [R2-2001163] proposes a terminology option 2. “csc” in option 2 stands for “Conditional SPCell Change”.

|  |  |
| --- | --- |
| Option 1(used in draft CR) | Option 2 [R2-2001163] |
| * conditionalReconfiguration
* condConfigToRemoveList
* condConfigToAddModList
* CondConfigId
* condTriggerConfig
* eventAN
 | * csc-Config
* csc-CandidateToReleaseList
* csc-CandidateToAddModList
* csc-CandidateId
* eventTriggerConfigCSC
* eventAN-CSC
 |

**Question 1: Could company provide their preference for the terminology for capturing of CPC in TS38.331?**

|  |  |  |
| --- | --- | --- |
| **company** | **Preferred terminology option** | **comment** |
| Ericsson | Option 1 | Option 2 is unclear regarding what the abbreviation means and it relies on specific name while reconfiguration is more generic and in line with current naming rules for mobility |

# 3 Any other issue for discussion

# 3 Conclusions