**3GPP TSG-RAN WG2 Meeting #109e R2-2002022**

**24 February – 6 March 2020**

**Agenda item: 6.2.3**

**Source: Qualcomm Incorporated**

**Title: Summary of NR-U Control Plane (AI 6.2.3.1 and 6.2.3.2)**

**Document for: Discussion and decision**

# Introduction

This document will capture the summary of contributions submitted to Agenda Items 6.2.3.1 and 6.2.3.2 and capture a baseline for further discussion via:

* [AT109e][503][NR-U] CP open issues (Qualcomm)

Scope:

* + - Identify/Summarize all remaining open issues related to Mobility and Others from AI 6.2.3.1 and 6.2.3.2 and seek companies feedback on the need to solve the critical issue and preferred solutions.

 Intended outcome:

* + - Set of proposals with full consensus (aim to agree to those over email)
		- Set of proposals with almost full consensus and easy to agree
		- Set of open issues and proposals to postpone to next meeting.
		- Open issues that should no longer be pursued

 Deadline for providing comments:

* + - Companies input: Thursday, Feb. 27th 18:00 CET
		- Rapporteur proposals: Friday, Feb. 28th 4:00 CET (one day for rapporteur to make conclusions)
		- Comments on proposals’ wording, Monday March 2nd by 17:00 CET

The new essential issues are prefixed by “E” and optimizations are prefixed by “O”.

The proposals here, after email discussion conclusion, will be color-coded per Session Chair instructions as follows:

* Green for easy agreements (obvious or there is consensus)
* Yellow if further online discussion is needed
* Blue if they should be discussed offline.

# Contributions on existing open issues

Many papers were submitted on issues which were already covered by the email discussion report in R2-2001437 where the companies provided input. These are listed as follows for completeness:

**Stopping of paging monitoring:**

R2-2000151 (Vivo): stop paging monitoring upon SI change or ETWS/CMAS indication

R2-2000336 (Ericsson): do not introduce a new bit for stopping the paging (i.e. revert the RAN2#108 agreement)

R2-2000418 (Oppo): stopPagingMonitoring bit in short message can be used to indicate that UEs either stop monitoring additional paging occasions or continue to monitor.

R2-2001548 (LG): UE stops monitoring further PDCCH monitoring occasion within the PO when any short message is received. Do not introduce the stopping indication in short message.

**Signaling of Q in MIB:**

R2-2000358 (Ericsson) proposes to define a new MIB instead of reusing the existing *ssbSubcarrierSpacingCommon* and possibly *ssb-SubcarrierOffset* with modified interpretations.

**Signaling of intra-cell guard bands:**

R2-2002673 (Nokia) proposes to “signal length of GB”.

**Signaling of interlaced waveform configuration:**

R2-2002672 (Nokia) proposes “single parameter, e.g. in BWP-UplinkCommon (suggested by Nokia) used by all useInterlacePUCH and useInterlacePUSCH parameters proposed by RAN1.

R2-2000964 (HW) proposes “Use one and only one parameter in BWP-UplinkConfigCommon to configure whether interlace is configured for the cell.”

# Contributions with easy agreements

R2-2000336 has proposed to confirm the relationship between SSBs and additional paging monitoring occasions. In particular, the following are proposed:

Proposal 1 Confirm in the chairman minutes that the SSB relation remains unchanged across the ‘X’ PMO subsets.

Proposal 2 Confirm that the legacy NR Rel-15 PO calculation is reused, i.e. the legacy set starts according to legacy, and the additional beam sweeping set(s) occupy the subsequent PDCCH monitoring occasions (PMOs).

The rapporteur thinks that these are obvious from the existing text in 38.304 and nothing new needs to be added to the specification. However, they can be agreed for even further clarification.

# Essential proposals which need further discussion

These are issues which need to be resolved for the completion of the Work Item.

### Issue E1: UE Capability

R2-2000150 (Vivo) has submitted a 38.306 CR, proposing to introduce two UE capabilities: one for 2-step RACH and one for RSSI/CO measurements. The second one has already been agreed by RAN2. R2-2000442 (MTK) also proposed to add capability for RSSI/CO measurements.

Even though RAN1 is still discussing UE features, it might be worthwhile to gather RAN2 feedback at least on the features introduced by RAN2, including:

1. Capability for 2-step RACH for NR-U. Note that 2-step RACH will have its own capabilities, so this should be for whether those are applicable to NR-U as well as other NR-U specific support such as no gap between preamble and PUSCH.
2. Capability for consistent UL LBT detection and recovery (can be separate for PCell, PSCell, and SCells)

**Please provide your opinion on whether UE capabilities should be introduced for above. Please list other UE capabilities if any.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Response** | **Comments** |
| **Samsung** | y | At least UE capabilities for above features should be introduced so that network may configure it to the UE (as for all other features). |
| **MediaTek** | Yes | UE capabilities of the features should be introduced. There should also be some basic capabilities, mentioning if UE can support (1) NR-U in downlink, (2) NR-U in uplink and (3) handle consistent LBT failure |
| Charter Communications | Yes | For 2-Step RACH, additional capabilities relevant to NR-U may be present for NR-U cells. For UL LBT failure detection, agree the need for capabilities per cell-type. |
| LG | Yes | UE capabilities should be introduced for above. |

**Summary:**

**Proposal.**

### Issue E2: Signaling of Q in SIBs

R2-2000338 proposes to introduce a new IE *SSB-QCL-RelationList* in SIB3 and SIB4 to carry the Q for each cell. In the current running CR, this IE is signaled per cell by using the existing *IntraFreqNeighCellList* in SIB2 and *InterFreqNeighCellList* in SIB4 are used.

**Do you support a new list for neighbour cells in SIB3 or SIB4 to include Q value or prefer to keep the current running CR option of re-using existing lists? Please list other options if any.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Response** | **Comments** |
| **Samsung** | n | prefer to keep the current running CR |
| **MediaTek** | No | Prefer to use re-use existing lists |
| Charter Communications | No |  |
| LG | No | keep the current running CR |

**Summary:**

**Proposal.**

### Issue E3: Bands which can be both licensed and unlicensed

The regulations for 6Ghz band are still under discussion by the relevant agencies. One of the proposals for Europe is to use certain sections of 6Ghz band for licensed and the rest for shared spectrum. If this proposal gets through, it is feasible that a band can be licensed in certain parts of the world (e.g. Europe) while unlicensed in other parts (e.g. North America).

This was discussed in two papers:

R2-2000358 (Ericsson) proposes to define a new MIB for shared spectrum where the UE should attempt to decode both legacy and new MIB and use the one for which SIB decoding is successful. The rapporteur thinks that the same can be achieved with the legacy MIB with different interpretations of the fields as being discussed (so-called Alt 1-2 and Alt 1-4) so it is not clear if defining a new MIB helps in any way to solve this problem.

R2-2001469 (Oppo) proposes that *“RAN2 discusses whether it’s an issue that UE may not differentiate NR and NR-U for a given spectrum due to different spectrum allocation policy.”* and *“If the issue is confirmed, RAN2 discusses how to enhance MIB to solve it.”.*

There are several options as a way-forward for RAN2 on this, not mutually exclusive:

* Option 1: Wait for conclusion of regulations on 6Ghz band before making any decision
* Option 2: Wait for RAN1/RAN4 discussion on this, which can happen after conclusion of regulations. For example, RAN4 can introduce different channel rasters for licensed and shared spectrum which can solve this problem without any RAN2 procedural and ASN.1 impact. RAN1 can also potentially come up with a PHY based solution.
* Option 3: UE decoding both MIB options (either legacy MIB or new MIB) and uses SIB1 to determine the band status
* Option 4: Use the spare bit in MIB to differentiate shared and licensed spectrum

**Which Option do you prefer regarding the possible issue of 6Ghz being used for both licensed and shared spectrum?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Response** | **Comments** |
| **Samsung** | Option 2 |  |
| **MediaTek** | Option 2 | Agree with Samsung. We should wait for decision of RAN1/RAN4. |
| **Charter Communications** | Option 2 |  |
| **LG** | Option 2 |  |

**Summary:**

**Proposal.**

### Issue E4: SIB1 decoding error

R2-2000443 (Nokia) discusses the FFS issue for UE behavior when SIB1 decoding fails and proposes the following:

*If a cell is barred in NR-U,* *the IntraFreqReselection is set “not allowed” and the UE is not able to decode SIB1 then the UE shall exclude the barred cell and the cells on the same frequency as a candidate for cell selection/reselection for up to 300 seconds.*

The paper argues that SIB1 decoding error is likely due to interference on this frequency and thus the UE should not try to reselect other cells. In the current running CR, the behavior is opposite where the UE still checks other cells on this frequency. The underlying assumption was that the UE should only follow “not allowed” in MIB if the cells belongs to the UE’s own PLMN and the UE does not know this is the case if it can’t decode the SIB1.

**Do you support barring all cells on a frequency if *IntraFreqReselection* in MIB is set “not allowed” and the UE is not able to decode SIB1?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Response** | **Comments** |
| **Samsung** | No | There is no FFS for this issue. We have discussed this issue in RAN2#107bis and running CR correctly captures the RAN2 agreement made in RAN2#107bis. RAN2#107bis Agreement:If a cell is barred in NR-U, due to the registered PLMN or selected PLMN does not match one of the PLMN IDs in SIB1, “IntraFreqReselection” shall be always interpreted as “allowed”. The same applies if SIB1 is not decoded.Since the UE does not know whether the cell belongs to its PLMN or not, UE should be allowed to search other cells on same frequency. Even if the SIB1 decoding error is due to interference on a cell of a PLMN on frequency F1 does not mean that cells of other PLMN on same frequency F1 will encounter interference as time/frequency location of SIB1 is not same for cells of different PLMNs. |
| **MediaTek** | No | We agree with Samsung and do not prefer barring all cells in the frequency.  |
| **Charter Communications** | No | There maybe various reasons for failed SIB1 decoding, and unless it’s accompanied with other measurements, it’s difficult to conclude that failure is due to co-channel interference etc. Hence, prefer not to bar all cells. |

**Summary:**

**Proposal.**

### Issue E5: Abandoning measurement reporting

R2-2000669 (Nokia) discusses an open issue in RAN4 on whether the “the UE shall abandon the measurement report in case the delay caused by successive UL LBT failures exceeds a maximum value”. The paper concludes that “There is no functionality in the U-plane to do withdraw procedure of SRB messages being discussed in RAN4” based on the following observations (copied from the paper):

1. *The uplink transmissions are scheduled by the gNB.*
2. *The measurement report data is mapped in a transport block (TB)*
3. *If a TB is not received at the gNB due to either LBT failure, or poor channel conditions, the gNB will schedule other opportunities for the UE transmissions.*
4. *After a measurement report is mapped in a TB, it is not possible for the UE to drop selectively the data that carries the measurement report, without affecting the TB.*
5. *Other specifications have procedures to control the TB retransmissions.*

*Additionally For the SRB messages there is no possibility to set PDCP discard timer thus having some kind of expiry function would be change to existing U-plane design. Only way to currently to get rid off SRB messages is to do MAC reset e.g. by handover.*

It is proposed that “*we should inform RAN4 that from RAN2 point of view we should not introduce any kind of “withdraw” procedure as it will be either close to impossible or requires huge redesign of U-plane protocols.”*

**Do you support informing RAN4 that there is no “withdraw” procedure for abandoning reporting of measurement results and introduction of such a mechanism will have significant impacts on RAN2 specifications?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Response** | **Comments** |
| **Samsung** | y | We agree with Nokia. |
| **MediaTek** | Yes | Agree. |
| **Charter Communications** | Yes |  |
| **LG** | Yes | Agree |

**Summary:**

**Proposal.**

### Issue E6: Usage of NR-U term

The running 38.300 used the term NR-U in initial versions to represent NR operation in unlicensed spectrum. In later version and other RAN2 running CRs, the phrase “NR operation with shared spectrum channel access” was used in consistent with RAN1 CRs. It was suggested to remove the term “NR-U” completely from RAN2 CRs.

**Do you support removing the term “NR-U” from RAN2 running CRs and use “NR operation with shared spectrum channel access” instead?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Response** | **Comments** |
| **Samsung** | No strong view |  |
| **MediaTek** | No strong opinion |  |
| **Charter Communications** | Need clarification | It is not clear what type of spectrum the phrase “shared spectrum” refers to? Is it 5/6/60GHz spectrum? Or does it also include CBRS spectrum. If the latter, then LBT is not applicable in CBRS, hence the unlicensed spectrum is more accurate. Note that in wider wireless community, “shared spectrum” primary refers to multi-tier spectrum like CBRS.  |

**Summary:**

**Proposal.**

### Issue E7: Inter-RAT mobility to NR-U

R2-2000337 (Ericsson) discusses mobility from E-UTRAN to NR-U (stand-alone) and proposes the following:

*Proposal 1 In order to support handover from LTE to NR-U, include ssb-QCL-RelationCommon in RS-ConfigSSB-NR.*

*Proposal 2 In order to include cell-specific Q values for handover from LTE to NR-U, include ssb-QCL-Relation in a new IE SSB-QCL-RelationList within RS-ConfigSSB-NR.*

*Proposal 3 In order to support idle/inactive mode mobility from LTE to NR-U, include ssb-QCL-RelationCommon in CarrierFreqNR within SIB24.*

*Proposal 4 In order to include cell-specific Q values for idle/inactive mode mobility from LTE to NR-U, include ssb-QCL-Relation in a new IE SSB-QCL-RelationList in CarrierFreqNR within SIB24.*

Since NR is the baseline for NR-U and there was no agreement to restrict inter-RAT mobility to NR-U, these proposals seem reasonable. RAN2 can make the high-level agreement and the exact placement of the Q value in LTE RRC can be discussed further.

**Do you see any problems in signalling of Q value in E-UTRAN to enable Connected and Idle mode mobility from E-UTRAN to NR-U?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Response** | **Comments** |
| **MediaTek** | No |  |
| **Charter Communications** | No |  |
| **LG** | No |  |

**Summary:**

**Proposal.**

### Issue E8: New MIB

Related to the Issue 2 whether to define a new MIB instead of changing the interpretation of the above IEs in the field description and/or possibly adding a new IE for the last spare bit.

**Do you prefer to define a new MIB to incorporate the new meaning of *ssbSubcarrierSpacingCommon* and possibly *ssb-SubcarrierOffset*****(or alternatively a new IE)** **for NR-U? The other option is to state the new interpretations in the field descriptions.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Response** | **Comments** |
| **Nokia** | **No (we prefer new interpretation)** | **In theory both options would work but we think it would be easy to just redefine meaning of existing two parameters. This way Ues do not need to change how to decode SIB1 based on what kind of carrier UE is camping on.** |
| **Intel** | **No** | **See our response to Issue 2** |
| **Ericsson** | **Yes** | If one adopts RAN1’s Alt 1-2, the ASN.1 encoder of the network expects to get the “*ssb-SubcarrierOffset*” as an Integer in the range {0..15}. However, when operating in unlicensed spectrum, the actual SSB subcarrier offset could only be in the range {0..7}. A wrapper around the ASN.1 would have to shift this value by one bit to the left and then fill the right most bit (LSB) with one of the two bits from the node-internal ENUM holding one of the Q bits. If the integer values {0..7} are not appropriate for the new subcarrier offset, one would have to implement also a new mapping from the 8 integer values to the corresponding actual subcarrier offsets. For the *subCarrierSpacingCommon* the ASN.1 encoder expects the ENUMERATED values scs15or60 or scs30or120 (1 bit). As a consequence, the other Q bit would have to be converted to scs15or60 or scs30or120 and then be fed into the ASN.1 encoder’s field for subCarrierSpacingCommon. **Certainly, all of this is doable, but it reduces readability based on the ASN.1 parameter names and defeats the purpose of ASN.1 to take care of complex and error-prone conversion of variables into serial bit strings.**  |
| **Huawei** | **Yes** | E// has explained a good reason why a new MIB is desirable from the implementation point of view. Our understanding is mainly that, based on the agreement in NRU, a lot of fields in the legacy R15 MIB will not be useful, which are- PDCCH-configSIB1 does not need 8 bits- intraCellFrequencyReselection is not needed from RAN2 point of view- ssb-SubcarrierOffset does not need 4 bits, like E// explained- subCarrierSpacingCommon not needed, eitherSo, we prefer to create a new MIB, just like what we did for NB-IoT |
| **vivo** | **No** | **There is no big difference between defining a new MIB and redefining the meaning of the two existing Ies. We think the latter may cause less impact to specification.** |
| **MediaTek** | **-** | **No strong opinion** |
| **Charter Communications** | **No** | **Prefer the new interpretation** |
| **Samsung** | **No** | **We prefer the minimum impact: new interpretation. Note that RAN1 did not list the option for the new MIB from their agreements (see below).**For signaling of Q for a serving cell with possible values {1,2,4,8}, the following is supported:• If RAN2 agrees to use the spare bit and still allow release independent introduction of the 6 GHz band, then Alt 1-4 is supported, otherwise Alt 1-2 is supported:o Alt 1-2: For operation with shared spectrum channel access, the UE interprets the following 2 bits of the Rel-15 MIB for providing the value of Q§ ssbSubcarrierSpacingCommon (1 bit)§ LSB of ssb-SubcarrierOffset (1 bit)o Alt 1-4: For operation with shared spectrum channel access, the UE interprets the 2 bits in the following two fields of the Rel-15 MIB for providing the value of Q§ ssbSubcarrierSpacingCommon (1 bit)§ spare (1 bit)  |
| **LG** | **No** | **Prefer the new interpretation** |

**Summary:**

**Proposal.**

### Issue E9: Short Message for Paging Stop

At the first online session in RAN2#109e, it was agreed that “The UE can stop paging monitoring if it receives a short message for SI update and PWS”. It wasn’t concluded if the short message can be used to request the UE to continue paging monitoring when there is an SI update or ETWS/CMAS notification as “FFS on whether we can set the new bit to zero with SI bit set to 1”.

The considered scenario is when the gNB has an SI update or ETWS/CMAS message and also a paging message for the UE but wants to defer the scheduling of the paging message to a later time.

**Do you support gNB asking the UE to extend paging monitoring when there is also an SI update or ETWS/CMAS in this PO? This will be done by setting the corresponding SI or ETWS/CMAS bit to 1 and paging bit to 0 in the short message.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Response** | **Comments** |
| **MediaTek** | **No** | **We prefer using short message only to indicate “Stop Monitoring” PDCCH, as receiving any short message means DL LBT in gNB is successful and UE can stop monitoring to save power.** |
| **Charter Communications** | **Yes** | **It is helpful to extend paging monitoring in above circumstances.** |
| **Samsung** | **No** | **This is reopening the discussion which we had in last meeting as well as in RAN2 107.** **To minimise UE power consumption, once channel is available, the behaviour should be same as in legacy i.e. gNB indicates SI/PWS notification and Paging together.** |
| **LG** | **No** | **We prefer using short message only to indicate “Stop Monitoring”. This is a RAN2 agreement in the previous meeting. We cannot see any clear reason to revisit this.** |

**Summary:**

**Proposal.**

### Issue E10: Signaling of intra-cell guard bands

RAN2#109e has discussed the signaling of guard bands and agreed on the following:

1. The guard bands for a cell are signalled by using a starting index and length for each guard band, only when the network wants to configure it.

*(FFS – move to offline) RAN2 should further discuss the signalling for the cases when there is no guard band, when RAN4 specs should be used, and when/if the UE does not support guard bands.*

Several options have come up during the email discussion on how to signal the default case (when RAN4 specs are used) and when there is no guard band (e.g. 20Mhz). Ericsson has also suggested that the UE may not support guard bands; however, RAN1 has not yet made any agreements on this.

**Please provide your suggestions on ASN.1 signaling for the cases there is no guard band, when RAN4 specs should be used, and when/if the UE does not support guard bands. The feedback could be without an ASN.1 snippet, e.g. by saying that explicit IEs are used for default and no guard band or by omitting the configuration for the default case etc.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Response** | **Comments** |
|  |  |  |

**Summary:**

**Proposal.**

### Issue E11: Configuration of RSSI measurement

In the current running CR, RSSI measurement configuration was added to *ReportConfigNR* IE as follows:

ReportConfigNR ::= SEQUENCE {

 reportType CHOICE {

 periodical PeriodicalReportConfig,

 eventTriggered EventTriggerConfig,

 ...,

 reportCGI ReportCGI,

 reportSFTD ReportSFTD-NR,

 measRSSI-ReportConfig-r16 MeasRSSI-ReportConfig-r16

 }

}

**The choice of this place by the rapporteur was for to have a similar structure as to LTE LAA where the same IE is in *ReportConfigEUTRA* and also given that both RAN1 and RAN2 agreements on RSSI reporting were to use the LTE LAA baseline.**

**Do you agree on the above signalling? If not, please list other option(s).**

|  |  |  |
| --- | --- | --- |
| **Company** | **Response** | **Comments** |
| **LG** | **No** | RAN2 agreed that the RSSI and CO results can be included in periodic reporting or event based reporting triggered by RSRP/RSRQ, as in LTE. However, according to the current CR, only periodic reporting is possible. measRSSI-ReportConfig-r16 should be placed in PeriodicalReportConfig and EventTriggerConfig. |
| **Huawei** | **No** | Same view as NOK |
| **Ericsson** | **Yes** | reportConfigEUTRA has a different structure than the ReportConfigNR.measRSSI-ReportConfig was added on top of the triggerType (event or periodical), however, with the following restrictions:***measRSSI-ReportConfig***If this field is present, the UE shall perform measurement reporting for RSSI and channel occupancy and ignore the *triggerQuantity*, *reportQuantity* and *maxReportCells* fields. E-UTRAN only sets this field to *true* when setting*triggerType* to *periodical* and *purpose* to *reportStrongestCells*.RSSI/CO measurements report are thus configured separately from other cell measurements. We think that we can use a similar as for **CLI-RSSI**, i.e. *RSSI-PeriodicalReportConfig* can be added. RSSI-PeriodicalReportConfig-r16 ::= SEQUENCE { reportInterval-r16 ReportInterval, reportAmount-r16 ENUMERATED {r1, r2, r4, r8, r16, r32, r64, infinity}, maxReportRSSI-r16 INTEGER (1..maxRSSI-Report-r16), ...}*maxReportRSSI* (to be confirmed) allows to define a number of RSSI measurement resources to be included in the measurement report.This is similar to *maxReportCells* in legacy *PeriodicalReportConfig* or *maxReportCLI* in the CLI reporting config. |
| **MediaTek** | **No** | Agree with LG and Huawei that measRSSI-ReportConfig-r16 should be placed in PeriodicalReportConfig and EventTriggerConfig  |

**Summary:**

**Proposal.**

### Issue 12: Handling of Forbidden TAs

In the 38.304 running CR, the legacy behaviour for the handling of “forbidden TAs for roaming” was not changed for shared spectrum. In particular, the CR has the following:

If the highest ranked cell or best cell according to absolute priority reselection rules is an intra-frequency or inter-frequency cell which is not suitable due to being part of the "list of 5GS forbidden TAs for roaming", the UE shall not consider this cell and other cells on the same frequency, as candidates for reselection for a maximum of 300 seconds

Ericsson commented that this may not be suitable for shared spectrum when multiple PLMNs are present. It is not clear to the rapporteur why that would make any difference for the UE behaviour since the UE is only registered on one PLMN.

**Do you see any new issues regarding handling of “forbidden TAs for roaming” for NR shared spectrum? If yes, please suggest solutions.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Response** | **Comments** |
| **Nokia** | **No** | We think it is a corner case when 2 ePLMNs use the same NR-U band and one of them has a cell that belongs to a forbidden TA for roaming while the other PLMN’s cell is not.  |
| **Huawei** | **No** |  |
| **Ericsson** | **Yes** | It may be a corner case that there are two E-PLMNs on the same frequency where cell 1 belongs to E-PLMN 1; forbidden TA: yescell 2 belongs to E-PLMN 2; forbidden TA: noThe solution is simple: the UE is only required to exclude the cell belonging to the forbidden TA from the candidate list, while it is not required to exclude all cells on a frequency as candidates for cell reselection for a maximum of 300 seconds. It can be left to UE implementation whether it evaluates SIB1 of other candidate cells on the same frequency or not. It is only necessary to clarify that the UE needs to check the TA and PLMN IDs to evaluate whether it can consider the cell as candidate for reselection or not. |
| **Charter Communications** | **No** |  |
| **LG** | **No** |  |

**Summary:**

**Proposal.**

# Open issues from RAN2#108 email discussion

PLACEHOLDER

There was no consensus on some of the open issues reported in R2-2001437. If they are not resolved during the first online session, they will be added here for further discussion.

# Optimizations

These are issues which do not need to be resolved for the completion of the Work Item.

### Issue O1: SUL for NR-U

R2-2001422 discusses SUL operation for NR-U and propose the following:

*Proposal 1: RAN2 to confirm that SUL is applicable for NR-U.*

*Proposal 2: RAN2 to consider a NR-U specific uplink selection rule. FFS on details.*

Since NR licensed is the baseline for NR-U, Proposal 1 seems obvious but can be confirmed. The open issue is whether SUL selection should be modified for NR-U specific reasons, e.g. channel occupancy.

**Do you support modifying or enhancing SUL selection rules for NR-U? If “Yes”, elaborate on the mechanism.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Response** | **Comments** |
| **Samsung** | Yes | When RSRP of the downlink pathloss reference is >= rsrp-ThresholdSSB-SUL, NUL is selected. However SUL can also be used in this case.When RSRP of the downlink pathloss reference is >= rsrp-ThresholdSSB-SUL, UE can select SUL if there are consistent LBT failures on NUL. |
| **MediaTek** | - | No strong opinion |
| **Charter Communications** |  | No strong opinion. Nut there maybe use cases where SUL in sub-7GHz are used.  |

**Summary:**

**Proposal.**

### Issue O2: RLF due to DL LBT failures

This was discussed several times in RAN2 before and it was not adopted. There were two contributions on this.

R2-2001549 (LG) proposes *“Regardless of whether new RLF mechanism is defined purely based on the “missing RS” indication, the “missing RS” indication should be considered in the existing T310 based mechanism.”*

R2-2000405 (MTK) counter proposes *“Given the fact that it is not possible to clearly distinguish between missing RS samples due to failure and poor DL RS quality in NR-U, UE can still continue with the same RLM process with an increased RLF triggering timer, configured by NR-U gNB.”*

The rapporteur notes that neither RAN1 or RAN4 have not introduced any differentiation between missing RS or poor DL RS.

**Should RAN2 still consider RLF based on missing DL RS samples?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Response** | **Comments** |
| **Samsung** | No |  |
| **MediaTek** | No | Based on current agreements in RAN1 and RAN4, it seems it is not possible to distinguish between missing RS and poor DL RS Quality (R2-2000405). |
| **Charter Communications** | No |  |

**Summary:**

**Proposal.**

### Issue O3: CHO for NR-U

R2-2001547 (LG) has the following regarding CHO for NR-U:

*Observation 1: It is beneficial to support the conditional handover that RAN2 is discussing under mobility enhancement WI for UE mobility in unlicensed carriers.*

*Observation 2: Even if a serving cell is still good, UE may need to perform inter-frequency mobility (e.g. within same gNB) due to high channel occupancy on the serving frequency.*

*Proposal: NR-U specific execution condition for conditional handover based on channel occupancy and RSSI measurement should be supported.*

Since legacy HO in NR-U will not use event triggers for channel occupancy and RSSI, the rapporteur thinks that the same should apply to CHO. It would be good to confirm this in order to prevent further discussion.

**Should Channel Occupancy and RSSI based execution conditions be introduced for CHO in shared spectrum?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Response** | **Comments** |
| **Samsung** | Yes |  |
| **MediaTek** | Yes | Channel Occupancy and RSSI based execution conditions can be introduced for CHO in NR-U |
| **Charter Communications** | Yes |  |
| **LG** | Yes | CHO is the most suitable mechanism to reduce the handover failure caused by LBT failure on unlicensed frequency, but it cannot guarantee the quality of the target cell on unlicensed frequency in terms of channel occupancy.Therefore, we need to define a new event based on the channel occupancy and RSSI, and the new event can be set as execution condition of CHO in combination with event A3 or A5. |

**Summary:**

**Proposal.**

### Issue O4: Cell selection after LBT failures

R2-2001546 (LG) proposes the following:

*Proposal If the RLF is declared due to the consecutive LBT failures, UE treats all cells on the last PCell frequency as if cell status is “Barred” for a given period of time.*

The rapporteur thinks that the cell selection is up to UE implementation and it can consider LBT failures in this decision.

**Do you support the above proposal for barring a frequency after consistent LBT failures on a Pcell on this frequency?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Response** | **Comments** |
| **Samsung** | Yes |  |
| **MediaTek** | No | We prefer to leave cell selection on UE implementation |
| **Charter Communications** |  | While agree with the logic presented above, UE implementation should be able to take care of this.  |
| **LG** | Yes (for cell re-selection in IDLE/INACTIVE also) | We need to consider the cell re-selection in IDLE/INACIVE also. When the consecutive LBT failures happen in IDLE/INACTIVE, e.g. when UE performs the UL LBT for RACH, the UE should be able to perform the cell re-selection on another frequency. To achieve this, UE needs to deprioritize the congested frequency or consider all cells on that frequency as barred. Considering that the consecutive UL LBT failures can happen in IDLE/INACTIVE as well as CONNECTED, it would be desirable to introduce a unified solution that works in both cell selection and cell re-selection. |
|  |  |  |

**Summary:**

**Proposal.**

# Open issues waiting for RAN1/RAN4

Some papers had proposals on issues which are being discussed in RAN1 and RAN4. Therefore, it is better to postpone these discussions.

R2-200964 (HW) discusses multi-TTI grant and proposes to changes to TDRA table.

# Conclusion

Based on the contributions submitted to RAN2#109e Agenda Items 6.2.3, the following are proposed: