**3GPP TSG-RAN WG2 Meeting #109 electronic *R2-20xxxxx***

**Online, 24 Feb – 6 Mar 2020**

|  |
| --- |
| *CR-Form-v12.0* |
| **CHANGE REQUEST** |
|  |
|  | **37.355** | **CR** | **0249** | **rev** | **1** | **Current version:** | **15.0.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network |  | Core Network | **x** |

|  |
| --- |
|  |
| ***Title:***  | Addition of broadcast TBS assistance data |
|  |  |
| ***Source to WG:*** | NextNav, AT&T, FirstNet, Polaris Wireless |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | TEI16, LCS\_LTE\_acc\_enh-Core |  | ***Date:*** | 2020-02-26 |
|  |  |  |  |  |
| ***Category:*** | **C** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)Rel-12 (Release 12)**Rel-13 (Release 13)Rel-14 (Release 14)Rel-15 (Release 15)Rel-16 (Release 16)* |
|  |  |
| ***Reason for change:*** | Broadcast of network assistance data for various wide area positioning methods have been supported for some time to reduce network load, latency and energy consumption. This will add support for the broadcast of TBS (Terrestrial Beacon System) assistance data leveraging the existing framework. |
|  |  |
| ***Summary of change:*** |  Support for broadcast of TBS assistance data is added with the addition of a new positioning SIB type enumeration value. Based on the online and offline discussion [RAN2#107bis Offline-404], added an additional change is necessary to support assistance data for more than one beacon. Supporting text also added in section 7.2 and clarification that it is TBS (based on MBS signals). Also, since the CR in R2-1914076 was endorsed as a baseline CR, RAN#86 has approved the LPP specification (TS 36.355) is upgraded to 37.355, which is the new specification under change control.R1: Updates the cover sheet and directly references *TBS-AssistanceDataList*  |
|  |  |
| ***Consequences if not approved:*** | No support for broadcast of Terrestrial Beacon System (TBS) assistance data, which is inconsistent with other wide area positioning methods. |
|  |  |
| ***Clauses affected:*** | 7.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** | **x** |  |  Other core specifications  | TS 36.331 CR 4134, TS 36.455 CR0105  |
| ***affected:*** |  | **x** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **x** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

<Unchanged Text omitted>

<Start of first changed section>

## 7.2 Mapping of *posSibType* to assistance data element

The supported *posSibType*'s are specified in Table 7.2-1. The GNSS Common and Generic Assistance Data IEs are defined in sub-clause 6.5.2.2. The OTDOA Assistance Data IEs are defined in sub-clause 7.4.2. The TBS (based on MBS signals) Assistance Data IEs are defined in sub-clause 6.5.4.8.

Table 7.2-1: Mapping of posSibType to assistanceDataElement

|  |  |  |
| --- | --- | --- |
|  | *posSibType* [12] | *assistanceDataElement* |
| GNSS Common Assistance Data (clause 6.5.2.2) | *posSibType1-1* | *GNSS-ReferenceTime* |
| *posSibType1-2* | *GNSS-ReferenceLocation* |
| *posSibType1-3* | *GNSS-IonosphericModel* |
| *posSibType1-4* | *GNSS-EarthOrientationParameters* |
| *posSibType1-5* | *GNSS-RTK-ReferenceStationInfo* |
| *posSibType1-6* | *GNSS-RTK-CommonObservationInfo* |
| *posSibType1-7* | *GNSS-RTK-AuxiliaryStationData* |
| GNSS Generic Assistance Data (clause 6.5.2.2) | *posSibType2-1* | *GNSS-TimeModelList* |
| *posSibType2-2* | *GNSS-DifferentialCorrections* |
| *posSibType2-3* | *GNSS-NavigationModel* |
| *posSibType2-4* | *GNSS-RealTimeIntegrity* |
| *posSibType2-5* | *GNSS-DataBitAssistance* |
| *posSibType2-6* | *GNSS-AcquisitionAssistance* |
| *posSibType2-7* | *GNSS-Almanac* |
| *posSibType2-8* | *GNSS-UTC-Model* |
| *posSibType2-9* | *GNSS-AuxiliaryInformation* |
| *posSibType2-10* | *BDS-DifferentialCorrections* |
| *posSibType2-11* | *BDS-GridModelParameter* |
| *posSibType2-12* | *GNSS-RTK-Observations* |
| *posSibType2-13* | *GLO-RTK-BiasInformation* |
| *posSibType2-14* | *GNSS-RTK-MAC-CorrectionDifferences* |
| *posSibType2-15* | *GNSS-RTK-Residuals* |
| *posSibType2-16* | *GNSS-RTK-FKP-Gradients* |
| *posSibType2-17* | *GNSS-SSR-OrbitCorrections* |
| *posSibType2-18* | *GNSS-SSR-ClockCorrections* |
| *posSibType2-19* | *GNSS-SSR-CodeBias* |
| OTDOA Assistance Data (clause 7.4.2) | *posSibType3-1* | *OTDOA-UE-Assisted* |
| TBS Assistance Data(clause 6.5.4.8) | *posSibTypeX-Y* | *TBS-AssistanceDataList* |

<End of changed section>

<End of changes>