**3GPP TSG-RAN WG2 Meeting #109 electronic Draft R2-2001960**

**Elbonia, 24 Feb – 6 Mar 2020**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR--Form--v12.0* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.300** | **CR** | **0209** | **rev** | **-** | **Current version:** | **16.0.0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network | **X** | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | RAN1 stage 2 agreements related to positioning | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Intel Corporation | | | | | | | | | |
| ***Source to TSG:*** | R2 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_pos-Core | | | | |  | ***Date:*** | | | 2020-02-13 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | B |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) Rel-12 (Release 12) Rel-13 (Release 13) Rel-14 (Release 14) Rel-15 (Release 15) Rel-16 (Release 16)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | To capture RAN1 stage 2 agreements (in R1-2001356) for positioning. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | To capture RAN1 stage 2 agreements for positioning. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | RAN1 stage 2 agreements for positioning.is missing. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 2, 3.1, 5.2.x, 5.3.x | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR... CR TBD ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* TP start \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 36.300: "Evolved Universal Terrestrial Radio Access (E-UTRA) and Evolved Universal Terrestrial Radio Access Network (E-UTRAN); Overall description; Stage 2".

[3] 3GPP TS 23.501: "System Architecture for the 5G System; Stage 2".

[4] 3GPP TS 38.401: "NG-RAN; Architecture description".

[5] 3GPP TS 33.501: "Security Architecture and Procedures for 5G System".

[6] 3GPP TS 38.321: "NR; Medium Access Control (MAC) protocol specification".

[7] 3GPP TS 38.322: "NR; Radio Link Control (RLC) protocol specification".

[8] 3GPP TS 38.323: "NR; Packet Data Convergence Protocol (PDCP) specification".

[9] 3GPP TS 37.324: " E-UTRA and NR; Service Data Protocol (SDAP) specification".

[10] 3GPP TS 38.304: "NR; User Equipment (UE) procedures in Idle mode and RRC Inactive state".

[11] 3GPP TS 38.306: "NR; User Equipment (UE) radio access capabilities".

[12] 3GPP TS 38.331: "NR; Radio Resource Control (RRC); Protocol specification".

[13] 3GPP TS 38.133: "NR; Requirements for support of radio resource management".

[14] 3GPP TS 22.168: "Earthquake and Tsunami Warning System (ETWS) requirements; Stage 1".

[15] 3GPP TS 22.268: "Public Warning System (PWS) Requirements".

[16] 3GPP TS 38.410: "NG-RAN; NG general aspects and principles".

[17] 3GPP TS 38.420: "NG-RAN; Xn general aspects and principles".

[18] 3GPP TS 38.101-1: "NR; User Equipment (UE) radio transmission and reception; Part 1: Range 1 Standalone".

[19] 3GPP TS 22.261: "Service requirements for next generation new services and markets".

[20] 3GPP TS 38.202: "NR; Physical layer services provided by the physical layer"

[21] 3GPP TS 37.340: "NR; Multi-connectivity; Overall description; Stage-2".

[22] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[23] IETF RFC 4960 (2007-09): "Stream Control Transmission Protocol".

[24] 3GPP TS 26.114: "Technical Specification Group Services and System Aspects; IP Multimedia Subsystem (IMS); Multimedia Telephony; Media handling and interaction".

[25] Void.

[26] 3GPP TS 38.413: "NG-RAN; NG Application Protocol (NGAP)".

[27] IETF RFC 3168 (09/2001): "The Addition of Explicit Congestion Notification (ECN) to IP".

[28] 3GPP TS 24.501: "NR; Non-Access-Stratum (NAS) protocol for 5G System (5GS)".

[29] 3GPP TS 36.331: "Evolved Universal Terrestrial Radio Access (E-UTRA); Radio Resource Control (RRC); Protocol specification".

[30] 3GPP TS 38.415: "NG-RAN; PDU Session User Plane Protocol".

[x1] 3GPP TS 38.305: "NG Radio Access Network (NG-RAN); Stage 2 functional specification of User Equipment (UE) positioning in NG-RAN".

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Unchanged part omitted \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

# 3 Abbreviations and Definitions

## 3.1 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1], in TS 36.300 [2] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1] and TS 36.300 [2].

5GC 5G Core Network

5QI 5G QoS Identifier

A-CSI Aperiodic CSI

AKA Authentication and Key Agreement

AMBR Aggregate Maximum Bit Rate

AMC Adaptive Modulation and Coding

AMF Access and Mobility Management Function

ARP Allocation and Retention Priority

BA Bandwidth Adaptation

BCH Broadcast Channel

BPSK Binary Phase Shift Keying

C-RNTI Cell RNTI

CBRA Contention Based Random Access

CCE Control Channel Element

CD-SSB Cell Defining SSB

CFRA Contention Free Random Access

CMAS Commercial Mobile Alert Service

CORESET Control Resource Set

DFT Discrete Fourier Transform

DCI Downlink Control Information

DL-AoD Downlink Angle-of-DepartureDL-SCH Downlink Shared Channel

DL-TDOA Downlink Time Difference Of Arrival

DMRS Demodulation Reference Signal

DRX Discontinuous Reception

E-CID Enhanced Cell-ID (positioning method)

ETWS Earthquake and Tsunami Warning System

GFBR Guaranteed Flow Bit Rate

I-RNTI Inactive RNTI

INT-RNTI Interruption RNTI

LDPC Low Density Parity Check

MDBV Maximum Data Burst Volume

MIB Master Information Block

MICO Mobile Initiated Connection Only

MFBR Maximum Flow Bit Rate

MMTEL Multimedia telephony

MNO Mobile Network Operator

MU-MIMO Multi User MIMO

Multi-RTT Multi-Round Trip Time

NCGI NR Cell Global Identifier

NCR Neighbour Cell Relation

NCRT Neighbour Cell Relation Table

NGAP NG Application Protocol

NR NR Radio Access

P-RNTI Paging RNTI

PCH Paging Channel

PCI Physical Cell Identifier

PDCCH Physical Downlink Control Channel

PDSCH Physical Downlink Shared Channel

PO Paging Occasion

PRACH Physical Random Access Channel

PRB Physical Resource Block

PRG Precoding Resource block Group

PSS Primary Synchronisation Signal

PUCCH Physical Uplink Control Channel

PUSCH Physical Uplink Shared Channel

PWS Public Warning System

QAM Quadrature Amplitude Modulation

QFI QoS Flow ID

QPSK Quadrature Phase Shift Keying

RA-RNTI Random Access RNTI

RACH Random Access Channel

RANAC RAN-based Notification Area Code

REG Resource Element Group

RIM Remote Interference Management

RMSI Remaining Minimum SI

RNA RAN-based Notification Area

RNAU RAN-based Notification Area Update

RNTI Radio Network Temporary Identifier

RQA Reflective QoS Attribute

RQoS Reflective Quality of Service

RS Reference Signal

RSRP Reference Signal Received Power

RSRQ Reference Signal Received Quality

RSTD Reference Signal Time Difference

SD Slice Differentiator

SDAP Service Data Adaptation Protocol

SFI-RNTI Slot Format Indication RNTI

SIB System Information Block

SI-RNTI System Information RNTI

SLA Service Level Agreement

SMC Security Mode Command

SMF Session Management Function

S-NSSAI Single Network Slice Selection Assistance Information

SPS Semi-Persistent Scheduling

SR Scheduling Request

SRS Sounding Reference Signal

SS Synchronization Signal

SSB SS/PBCH block

SSS Secondary Synchronisation Signal

SST Slice/Service Type

SU-MIMO Single User MIMO

SUL Supplementary Uplink

TA Timing Advance

TPC Transmit Power Control

UCI Uplink Control Information

UL-AoA Uplink Angles of Arrival

UL-RTOA Uplink Relative Time of ArrivalUL-SCH Uplink Shared Channel

UPF User Plane Function

URLLC Ultra-Reliable and Low Latency Communications

Xn-C Xn-Control plane

Xn-U Xn-User plane

XnAP Xn Application Protocol

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Unchanged part omitted \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### 5.2.X Downlink Reference Signals and Measurements for Positioning

The DL Positioning Reference Signals (DL PRS) are defined to facilitate support of different positioning methods such as DL-TDOA, DL-AoD, multi-RTT through the following set of UE measurements DL RSTD, DL PRS-RSRP, and UE Rx-Tx time difference respectively as described in TS 38.305 [x1].

Besides DL PRS signals, UE can use SSB and CSI-RS RRM (RSRP and RSRQ) measurements for E-CID type of positioning.

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* Unchanged part omitted \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

### 5.3.X Uplink Reference Signals and Measurements for Positioning

Both Release 15 SRS as well as the Release 16-introduced sounding reference signals (SRS) for positioning can be used for positioning.

The periodic, semipersistent and aperiodic transmission of Release 15 SRS is defined for gNB UL RTOA, UL SRS-RSRP, UL-AoA measurements to facilitate support of UL TDOA and UL AoA positioning methods as described in TS 38.305 [x1].

The periodic, semipersistent and aperiodic transmission of SRS for positioning is defined for gNB UL RTOA, UL SRS-RSRP, UL-AoA, gNB Rx-Tx time difference measurements to facilitate support of UL TDOA, UL AoA and multi-RTT positioning methods as described in TS 38.305 [x1].

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\* TP end \*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*