**3GPP TSG-RAN WG2 Meeting #112e DRAFT R2-2010839**

**eMeeting, 02 – 13 November 2020**

**Title: [DRAFT]** LS to RAN3 on small data transmission

**Response to:** -

**Release:** Release 17

**Work Item:** NR\_SmallData\_INACTIVE-Core

**Source:** Ericsson [TSG RAN WG2]

**To:** TSG RAN WG1

**Contact Person:**

#### Name: Henrik Enbuske

E-mail Address: henrik dot enbuske at ericsson dot com

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**1. Overall Description:**

RAN2 has started work on the NR Small Data Enhancements WI (RP-201305). The objectives of this WI include solutions for UE AS Context fetch and data forwarding with and without anchor re-location.

In RAN2 the assumption is that the details of the procedures and possible adaptations related to UE AS context handling for SDT is handled and decided in RAN3. To benefit in those discussion for this Work Item, RAN2 would like to highlight the following related agreements reached so far in RAN2.

**Agreements:**

* RAN2 confirm that RACH based SDT is supported with and without UE context relocation(RAN2 #112e)
* From RAN2 perspective, stored “configuration” in the UE Context is used for the RLC bearer configuration for any SDT mechanism (RACH and CG). (RAN2 #111e)
* Inform RAN3 on UE SDT data handling impact including using a stored RLC configuration. (RAN2 #112e)

SDT can be initiated by the UE in RRC INACTIVE state either in the same cell/gNB where the UE received RRC Release with suspend configuration, or in another cell/gNB. In addition, RAN2 also agreed that the first UL message (i.e. MSG3 for 4-step RACH and MSGA payload for 2-step RACH and the CG transmission for CG) may contain DRB data from one or more DRBs which are configured by the network for SDT. The RLC configuration used for the DRB data in this first UL message will be based on the stored configuration. UE can also send or receive subsequent packets to/from the network, using the stored RLC configuration, without transitioning to RRC CONNECTED state. The discussion leading to the above agreements included aspects of handling of SDT data as a result of using a stored UE AS context and that depending on when or if a UE AS context exchange is made irrespective of performing an anchor relocation, the SDT data may incur additional latency as the deciphering cannot be made in the receiving target node.

RAN2 would like RAN3 to take the above aspects into consideration in their work and specify the context fetch and data forwarding related procedures to support SDT data transmission with and without anchor relocation.

**2. Actions:**

**To RAN3 group.**

**ACTION:** RAN2 respectfully requests RAN3 to take the above into account and specify the context fetch and data forwarding related procedures to support SDT data transmission with and without anchor relocation.

**3. Date of Next TSG-RAN WG2 Meetings:**

3GPP RAN2#113-e 25 Jan – 05 Feb 2021 Electronic Meeting