3GPP TSG-RAN WG1 Meeting #116bis-e Tdoc R2-22xxxxx

January 17th - 25th 2022

Agenda: 8.14.3

Source: Ericsson

Title: Feature summary for 8.14.3

Document for: Discussion, Decision

# 1 Introduction

In this document the following offline is discussed:

* [AT116bis-e][030][QoE] Other open issues (Ericsson)

 Scope: List the remaining other open issues not related to Mobility, Pause Resume, RV QoE or UE cap. Determine agreements (agreed offline), and points for online CB, if any.

 Intended outcome: Report

 Deadline: Friday W1 (can CB Mon W2 if needed).

Contact information:

|  |  |
| --- | --- |
| **Company** | **Contact Name, Email** |
| Huawei, HiSilicon | dawid.koziol@huawei.com |
| Apple | Pavan Nuggehalli, pnuggehalli@apple.com |
| Qualcomm | Jianhua Liu, jianhua@qti.qualcomm.com |
| CMCC | liukangyi@chinamobile.com |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 2 Discussion

## 2.1 Multiple QoE reports in one message

The following proposals are related to the possibility to include multiple QoE reports in one *MeasurementReportAppLayer* message.

* It is not allowed to add multiple QoE reports in one RRC message.
* Select one option among:
- Option 1. MeasurementReportAppLayer message includes a single QoE report with a MeasConfigAppLayerID.
- Option 2. MeasurementReportAppLayer message includes multiple QoE reports with the same MeasConfigAppLayerID.
- Option 3. MeasurementReportAppLayer message includes multiple QoE reports with different MeasConfigAppLayerID.
* RAN2 to agree that it is up to UE implementation whether or not transmit multiple QoE reports in one RRC msg, and ASN.1 should support including more than one QoE report and measConfigAppLayerId in the one RRC msg.
* Multiple QoE report containers can be included in one *MeasReportAppLayer* message, and it is up to UE implementation on whether to include multiple QoE report container in one message.
* Multiple QoE reports can be included in a single QoE report message.
* allow multiple QoE reports in the same RRC message, and discuss in what scenrios QoE report aggeration should be performed.
* Allow multiple QoE reports in the same MeasurementReportAppLayer message.
* Add the report of QoE measurements by means of list to enable report of multiple simultaneous measurements.

Based on the proposals above, the following questions are asked:

Question 1: Do you think ASN.1 should support including multiple QoE reports in one *MeasurementReportAppLayer* message? If so, do you think there should be multiple QoE reports with different *measConfigAppLayerId* or multiple QoE reports with the same *measConfigAppLayerId* or both?

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments** |
| Huawei, HiSilicon | Yes | For the 1st question, we are okFor the 2nd question, we think both situations may happen in theory and the UE can simply include the reports it currently has in its buffer, regardless of their corresponding ID.For “QoE reports”, we think the meaning can be container based QoE for now. Whether the discussion can be applied to RAN visible QoE can be checked later. |
| Apple | Yes | Depends on RRC segmentation |
| Qualcomm | Yes | From specification point of view, it should support both; how to generate the message is up to UE implementation. |
| CMCC | Yes | Both.We think such flexibility should be provided to UE. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.2 Container size limitations

The following proposals are related to container size limitations and how to capture them in the specification.

* Maximum size of the QoE configuration container should be specified as 8000 bytes in RRC, to account for an overhead of other fields that may need to be included in the RRC Reconfiguration message.
* To avoid oversized QoE reports from being provided from application layer to the AS layer, AS layer should inform application layer whether the reports larger than 8000 bytes can be transmitted by the UE (i.e. depending on whether the UE is capable of and configured with RRC segmentation or not).
* Add a Note in field description of measConfigAppLayerContainer saying that the message containing the QoE configuration container(s) cannot exceed 9000 bytes.
* Add a Note in the field description of MeasurementReportAppLayerContainer saying that the message containing the QoE report container(s) cannot exceed 144 000 bytes.
* Send the reply LS to SA4 with the new size limitations for QoE configuration and report.

It is assumed that RAN2 sends a reply LS with the relevant RAN2 agreements related to size limitations as the size limitations are currently captured also in SA4 specifications and a reply LS has not been sent so far. Regarding the other proposals, the following questions are asked :

Question 2: Do you think the container size limitations should be captured as a maximum size of the BITSTRING in ASN.1 or in the field description with a maximum size of the RRC messages containing the containers?

|  |  |
| --- | --- |
| **Company** | **Comments** |
| Huawei, HiSilicon | This should be captured as the maximum size of the container. Field descriptions are not a good place to capture such limitations in our opinion. Furthermore, we need to decide about the maximum size of the QoE configuration which in our opinion should be 8 kBytes. |
| Apple | Ok to limit the maximum size to 8K. Neutral on how it is specified. |
| Qualcomm | Seems it is more straight-forward to capture the maximum size of the container. |
| CMCC | For QoE configuration container, we agree with Huawei.For QoE report, we think it depends on Q3, i.e. whether UE capability of RRC segmentation is conditionally mandatory or not. If so, the message containing QoE reports cannot exceed 144KB. If not, i.e. RRC segmentation is optionally supported, then there are two sub-cases: 1. if RRC segmentation is supported by UE, then the message containing QoE reports cannot exceed 144KB; while 2. If RRC segmentation is not supported by UE, then the message containing QoE reports cannot exceed 9KB. |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

Question 3: In case the UE capability of RRC segmentation is not conditionally mandatory, do you think application layer needs to be informed of the UE capability to support RRC segmentation?

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Additional comments** |
| Huawei, HiSilicon | Yes | Informing APP layer about the segmentation capability allows avoiding oversized QoE reports from being provided from application layer to the AS layer. To be specific – what APP layer needs to understand is the maximum size of the report that it can provide (i.e. either 8kBytes which is a legacy maximum size or more than that, e.g. calculated based on the maximum number of RRC message segments). |
| Apple | Maybe | Need to solicit SA4 input on whether such a limitation is even possible. |
| Qualcomm |  | Actually, we want to discuss whether all capabilities related parameters need to be interacted between AS layer and application layer, that means we will specify in AT command for all capabilities? For example, AS layer needs to know whether application layer supports QoE, RAN visible QoE, per-slice QoE, do we need to specify this? |
| CMCC | Yes | If not, QoE measurement configuration has to guarantee that APP layer must not generate oversized QoE report. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.3 AT-commands

The following proposals are related to AT commands and what to request CT1 to add in TS 27.007.

* Discuss whether the service type needs to be included in the AT command at release.
* Ask CT1 to define the QoE configuration in terms of a list.
* Ask CT1 to define the possibility to release all QoE configurations in an AT command.

The service type is used in the UE for routing the QoE configuration to the right application. The question is whether it is also needed at release to route the release command to the right application. In such case, the AS layer in the UE needs to store the service type together with the *measConfigAppLayerId*. Alternatively, the *measConfigAppLayerId* may be sufficient to route the release command to the right application.

RAN2 has agreed to support multiple QoE configurations, but the AT-command currently only supports one QoE configuration.

The AT command for release all QoE configurations seems to be needed e.g. in the case where an *RRCSetup* is triggered in a gNB not supporting QoE measurements and where the RRC layer has been cleared and does not know which QoE configurations that are configured in the application layer. In LTE, only one QoE configuration can be configured and then the release command also has the meaning release all.

Based on the proposals above, the following questions are asked:

Question 4: Do you think the service type needs to be forwarded to the application layer at release?

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Additional comments** |
| Huawei, HiSilicon | Probably yes | It depends on how AS and APP co-ordinate during the QoE measurement setup phase, but as mentioned above, in order to route the release to a proper application, this may be needed. We can check with CT1. |
| Apple | No | measConfigAppLayerId should be sufficient. |
| Qualcomm | No | There should be two questions here.When UE AS layer receives one QoE configuration with service type and measConfigAppLayerId, UE should determine the concerned applications based on service type and only forward measConfigAppLayerId to concerned application layer.When RAN release one QoE configuration, RAN only indicates *measConfigAppLayerId* for the to be release QoE configuration. So, anyway, UE AS layer needs to store the association of service type and *measConfigAppLayerId,* and then UE will forward release command to the concerned applications based on service type. |
| CMCC | No | Agree with Apple. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Question 5: Do you agree that the AT-command needs to include QoE configurations in terms of a list, i.e. corresponding to the list in the RRC message? If you don’t agree, please explain why it is not needed.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Additional comments** |
| Huawei, HiSilicon | Up to CT1 | AT command design is up to CT1 in general, so there is no need for RAN2 to discuss this. It can be left up to CT1 discussions whether they would like to have a single AT command with a list of configurations or they prefer to indicate each configuration separately. E.g. if AT command is anyway sent to a specific application, then it is not clear how the list would work for different services. |
| Apple | Yes | But can leave CT1 to take final decision |
| Qualcomm |  | Can leave to CT1 decision |
| CMCC |  | Agree with Huawei. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

Question 6: Do you agree that the AT-command needs to include the option to release all QoE configurations? If you don’t agree, please explain why it is not needed.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Additional comments** |
| Huawei, HiSilicon | Up to CT1 | Similarly as above, if AT command is sent to a specific application, then a single AT command may not be feasible. From RAN2 perspective we need to indicate to higher layers that the QoE configurations are released (either all or one). How this is communicated to application layer depends on CT1.  |
| Apple | Maybe | But can leave CT1 to take final decision.  |
| Qualcomm | Yes | For easy implementation in case of all QoE release. |
| CMCC |  | Agree with Huawei. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 2.4 Other proposals

These are the remaining proposals:

* RAN2 to agree that source gNB should send the information of the air-interface resource consumption for transmission of the measurement report for each QoE configuration towards the target gNB to assist the target gNB to choose which QoE measurement configuration should be released.
* RAN2 to agree that the granularity of the indication of the release is of per QoE configuration, and the source gNB should send the historical information of the air-interface resource consumption for transmission of the measurement report for each QoE configuration towards the target gNB when UE context is retrieved.
* Categorize all QoE measurement in different sets/containers by service type and assgin the set/container with unique identify.
* Prioritize the use of identify of set/container to indicate gNB which QoE configurations should be kept.
* For QoE reporting control, RAN node is made aware of the reporting interval applied for QoE data collection as an assistance information to help RAN decide whether to pause or release the QoE.
* To support QoE measurement reporting control, RAN supports optionally configuration of QoE data collection cycle in AS layer.

The proposals seem not to be strictly needed in rel-17 in order to complete the WI with the defined scope and they are also not proposed by more than one company.

Question 7: Would you like to proceed with any of the proposals above? Which ones? Please motivate.

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Additional comments** |
| Huawei, HiSilicon | No | These proposals do not seem essential to complete the work and many of them have also impact on RAN3. We prefer not to discuss them in this release.  |
| Apple | No | Agree with Huawei. |
| Qualcomm | No | Agree with Huawei. |
| CMCC | No | Some proposals can be postponed. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# 3 Conclusion

# 4 References

1. [R2-2200267](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116bis-e/Docs/R2-2200267.zip)**,** Discussion on QoE configuration, ZTE Corporation, Sanechips
2. [R2-2200548](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116bis-e/Docs/R2-2200548.zip)**,** Remaining QoE issues, Samsung
3. [R2-2200557](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116bis-e/Docs/R2-2200557.zip)**,** Discussion on QoE measurement collection configuration in NR, OPPO
4. [R2-2200684](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116bis-e/Docs/R2-2200684.zip)**,** Leftover issues of QoE configuration, reporting, pause, resume and mobility, Qualcomm Incorporated
5. [R2-2200820](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116bis-e/Docs/R2-2200820.zip)**,** Discussion on QoE open issues, Huawei, HiSilicon
6. [R2-2200851](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116bis-e/Docs/R2-2200851.zip)**,** Remaining open issues on QoE measurement and mobility, CMCC
7. [R2-2200997](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116bis-e/Docs/R2-2200997.zip)**,** Configuration and reporting of QoE measurements, Ericsson
8. [R2-2201046](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116bis-e/Docs/R2-2201046.zip)**,** Discussion on open issues for QoE, Nokia, Nokia Shanghai Bell
9. [R2-2201421](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_116bis-e/Docs/R2-2201421.zip)**,** Discussion on the remaining open issues, CATT