3GPP TSG-RAN WG2 #117-e Tdoc R2-21xxxxx

Electronic meeting, 2022-02-21 - 2022-03-03

Agenda Item: 8.11.1

Source: Ericsson

Title: [Pre117-e][613][POS] RAN1 parameter list impact to RRC

Document for: Discussion, Decision

# 1 Introduction

# 1 Introduction

This document is to collect comments for the CR:

* [Pre117-e][613][POS] RAN1 parameter list impact to RRC running CR (Ericsson)

Please provide your comments related to the CR

# 2 Contact Information

|  |  |
| --- | --- |
| Company | Contact: Name (E-mail) |
| Intel | Yi Guo (yi.guo@intel.com) |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# 3 Comments

**Please provide the comments on the CR here:**

|  |  |
| --- | --- |
| Company | Comments |
| Intel | 1 Following RAN1 parameter is missing, should be added in reconfiguration message?UETxTEG\_Request\_UL-TDOA, The parameter is used for the serving gNB to request a UE to provide UE Tx TEG association for UL-TDOA .2 comma is missing for uePositioningAssistanceInfo-r17 UEPositioningAssistanceInfo-IES-r173 For new message, why SRB3 is needed? We should not consider SCG case; |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Conclusion

In the previous sections we made the following observations: