**3GPP TSG-RAN WG2 Meeting #121bis-e draft R2-2304247**

**Online, Apr 17th-26th, 2023**

**Source: Samsung**

**Title: Report of [AT121bis-e][107][NR NTN Enh] NW type information (Samsung)**

**Agenda item:** **7.7.4.1.1**

**Document for:** **Discussion and Decision**

# Introduction

This document records the discussion and outcome for the following offline discussion.

* [AT121bis-e][107][NR NTN Enh] NW type information (Samsung)

Initial scope: discussion p4 and p5 from [R2-2303766](file:///C%3A%5C%5CData%5C%5C3GPP%5C%5CExtracts%5C%5CR2-2303766.docx%22%20%5Co%20%22C%3AData3GPPExtractsR2-2303766.docx) and p1 from [R2-2303736](file:///C%3A%5C%5CData%5C%5C3GPP%5C%5CExtracts%5C%5CR2-2303736%20-%20TN%20NTN%20mobility%20enhancements.docx%22%20%5Co%20%22C%3AData3GPPExtractsR2-2303736%20-%20TN%20NTN%20mobility%20enhancements.docx)

Initial intended outcome: Summary of the offline discussion with e.g.:

* List of proposals for agreement (if any)
* List of proposals that require online discussions
* List of proposals that should not be pursued (if any)

Deadline for companies' feedback: Monday 2023-04-24 12:00 UTC

Deadline for rapporteur's summary (in R2-2304247): Monday 2023-04-24 18:00 UTC

Proposals marked "for agreement" in R2-2304247 not challenged until Tuesday 2023-04-25 08:00 UTC will be declared as agreed via email by the session chair (for the rest the discussion might continue online in the Tuesday CB session).

Rapporteur encourages the participating delegates to provide their contact information in this table.

|  |  |  |
| --- | --- | --- |
| Company | Name | Email Address |
| Samsung | Shiyang Leng | shiyang.leng@samsung.com |
| Ericsson | Ignacio Pascual | Ignacio.pascual.pelayo@ericsson.com |
| Transsion Holding | Junwei Huang | Junwei.huang@transsion.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Discussion

As specified in TS 38.101-5 [1], NTN satellite operating band is assigned with different frequency band numbers than TN frequency band numbers: n255 and n256. Even though the frequency bands used for TN and NTN are overlapped, i.e. n255 overlaps with n24, n256 overlaps with n65, UE can know a neighbour cell is NTN by the indicated frequency band in SIB3/4*.*

For HAPS, frequency band n1 can be applied as specified in TS 38.104 [2]. Both TN and HAPS can operate on frequency band n1. In this case, UE cannot distinguish TN and NTN (HAPS) neighbour cells by the frequency band number, which may have impacts on neighbour cell measurement for cell reselection.

|  |  |  |
| --- | --- | --- |
| NR *operating band* | Uplink MHz / NR-ARFCN(First – <Step size> – Last) | Downlink MHz / NR-ARFCN (First – <Step size> – Last) |
| n1 | 1920 MHz – 1980 MHz384000 – <20> – 396000 | 2110 MHz – 2170 MHz422000 – <20> – 434000 |
| n24 | 1626.5 MHz – 1660.5 MHz325300 –< 20 >– 332100 | 1525 MHz – 1559 MHz305000 –< 20 >– 311800 |
| n255 | 1626.5 MHz – 1660.5 MHz325300 – <20> – 332100 | 1525 MHz – 1559 MHz305000 – <20> – 311800 |
| n65 | 1920 MHz – 2010 MHz384000 –< 20 >– 402000 | 2110 MHz – 2200 MHz422000 –< 20 >– 440000 |
| n256 | 1980MHz – 2010 MHz396000 – <20> – 402000 | 2170 MHz – 2200 MHz434000 – <20> – 440000 |

R2-2303736 and R2-2303766 discussed this issue.

**Case 1: when camping on a TN cell**

When camping on an TN cell, idle/inative UE obtains its neighbour cell information only from SIB3/4. TN cell does not broadcast SIB19. Without NTN-specific assistance information, a UE may not be able to measure an NTN neighbour cell leading to restricted TN to NTN mobility in RRC\_IDLE/INACTIVE. Therefore, a TN cell needs to provide satellite assistance information in System Information. The proposed solution is that TN cell broadcasts *NTN-config-r17* in SIB3/SIB4 for NTN neighbour cells.

**Q1) Do you agree in TN cell SIB3/SIB4 NTN-config-r17 is provided for NTN neighbour cells?**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments**  |
| Samsung | Yes | NTN-config-r17 has to be provided by a TN serving cell for NTN neighbour cell measurement, otherwise UE cannot measure NTN neighbour cells. TN cell does not need to broadcast SIB19, NTN-config-r17 in SIB3/4 works. |
| MediaTek | Yes | This is needed if TN-NTN mobility needs to be supported in overlapping bands. |
| Ericsson | Yes | This information is needed for a UE to measure NTN cells. |
| Transsion | Yes | From TN-NTN mobility perspective, it need another means to identify whether a neighor cell is HAPS or TN. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

If Q1 is agreed, for a neighbour cell is indicated in SIB3/4, NTN-config-r17 allows UE to know this is an NTN cell, so that UE can measure it if needed or does not measure it if not supporting NTN. However, on frequency band n1, if neither NTN-config-r17 nor TN coverage information is provided for a neigbor cell, UE cannot know whether the neighbour cell is TN or NTN (HAPS).

If Q1 is not agreed, on frequency band n1, if TN coverage information is NOT provided for a neighbour cell, UE cannot known whether the neighbour cell is TN or NTN (HAPS).

**Case 2: when camping on an NTN cell**

When camping on an NTN cell, UE obtains its neighbour cell information from SIB3/4/19: SIB3 contains intra-frequency information, SIB4 contains inter-frequency information, and SIB19 provides NTN-config-r17. Frequency and PCI are used to associate neighbour cell information in SIB3/4 with NTN-config-r17 in SIB19.

For a neighbour cell indicated in SIB3/4, if the associated NTN-config-r17 is provided in SIB19, UE knows this is an NTN cell and can measure it if needed. However, on frequency band n1, if neither NTN-config-r17 nor TN coverage information is provided for a neigbor cell, UE cannot know whether the neighbour cell is TN or NTN (HAPS).

In summary, on frequency band n1, if neither NTN-config-r17 nor TN coverage information is provided for a neigbor cell, UE cannot know whether the neighbour cell is TN or NTN (HAPS). In this case, UE has to determine whether the neighbour cell is TN or NTN: if the neighbour cell is TN UE should perform TN cell measurement, if the neighbour cell is NTN UE can skip measure it without NTN assistance information. Futhermore, an NTN UE can prioritize TN cell measurement (e.g., by UE implementation) if it can distinguish TN and NTN neighbour cells; an non-NTN UE can skip measuring NTN neighbour cells for power saving if it can distinguish TN and NTN neighbour cells.

**Q2) Do you agree on frequency band n1, if neither NTN-config-r17 nor TN coverage information is provided for a neigbor cell, UE needs to determine whether the neighbour cell is TN or NTN (HAPS)? If not, please explain the reason in comment.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments**  |
| Samsung | Yes |  |
| MediaTek | Yes, but | We think this is a corner case (neither NTN-config-r17 nor TN coverage information is provided for a neigbor cell). In such corner cases the UE implementation can take care of it. |
| Ericsson | No | If neither *NTN-config-r17* nor TN coverage information is provided for a neighbour cell, UE can safely determine the neighbour cell is TN.There is no ambiguity.From 38.300: “For a UE in Idle/Inactive mode it's up to UE implementation whether to perform NTN neighbour cell measurements on a cell indicated in SIB4 but not included in SIB19”Network is aware of this limitation. Thus, it will not include an NTN frequency in SIB3/4, unless *NTN-config-r17* is provided in SIB19. |
| Transsion | No | We should identify if there exist such scenario firstly，i.e. neither NTN-config-r17 nor TN coverage information is provided for a neigbor cell. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Q3) If yes to Q2, do you agree to introduce an explicit cell type indiation for UE to determine whether a neighbour cell is TN or NTN (HAPS)? If not, please provide other solutions in comment.**

|  |  |  |
| --- | --- | --- |
| **Company** | **Yes/No** | **Comments**  |
| Samsung | Yes |  |
| MediaTek | No strong opinion | We think this is possibly not needed. As mentioned in our response to Q2), this is a corner case and not likely to happen. However, we are open to go with the majority. |
| Transsion | No | As commnet as above. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Conclusions

**For agreement:**

**For discussion:**

# References

1. 3GPP TS 38.101-5, User Equipment (UE) radio transmission and reception, Part 5: Satellite access Radio Frequency (RF) and performance, Release 17, V17.2.0.
2. 3GPP TS 38.104, Base Station (BS) radio transmission and reception, Release 17, V17.8.0.