3GPP TSG-RAN WG2 Meeting #121bis-e***R2-230xxxx***

Online, April 17 – 26, 2023

**Agenda item:** 7.2.1

**Source:** Qualcomm Incorporated

**Title:** Summary of [AT121bis-e][421][POS] Reply LS to SA2 on PRU procedures

**Document for:**  Discussion and Decision

# 1. Introduction

This document summarizes the following email discussion:

* [AT121bis-e][421][POS] Reply LS to SA2 on PRU procedures (Qualcomm)

 Scope: Draft a reply to R2-2302449, taking related contributions into account.

 Intended outcome: Approved LS (without CB if possible)

 Deadline: Monday 2023-04-24 2359 UTC

# 2. Background

The following LS on PRU procedures from SA2 was received in [R2-2302449](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_121bis-e/Docs/R2-2302449.zip) [1]:

|  |
| --- |
| **1. Overall Description:**SA2 would like to inform RAN1 and RAN2 that the SA2 has agreed the attached CR to TS 23.273 on procedure enhancements for PRU support.Regarding the procedure for location of a target UE using PRUs (clause 6.x.4 of the attached CR), SA2 noticed that RAN had agreements to support some positioning methods that require simultaneous measurements of the target UE and PRU. In the SA2 agreed procedures, it is assumed that the LMF can make the decision and realize such simultaneous measurements by using a common scheduled location time.SA2 would like to seek RAN1 and RAN2’s feedback on such assumption and whether additional enhancement would be needed to support the simultaneous measurements for the target UE and PRU. SA2 would update the specification according to the RAN1 and RAN2 feedbacks if necessary.Additionally, SA2 also would like to know what location information can be provided by PRU, and whether RAN1 and RAN2 see benefit to allow PRU to provide its location information together with the location measurements reports.**2. Actions:****To RAN1 and RAN2 group****ACTION:** SA2 would like to ask RAN1 and RAN2 to provide feedback on whether any enhancement to the PRU procedures is required. |

Essentially, SA2 asks for feedback on the following 3 issues:

(1) Support for simultaneous location measurements of a target UE and a PRU (e.g., using a common scheduled location time).

(2) Location information provided by a PRU.

(3) Whether any enhancement to the PRU procedures is required (S2-2303860, attached to the LS [1]).

RAN1 answered the SA2 question already at RAN1#112 ([R2-2302409](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_121bis-e/Docs/R2-2302409.zip) [2]) as follows:

|  |  |  |
| --- | --- | --- |
| **1. Overall Description**RAN1 thanks SA2 for their LS on PRU procedures and would like to provide the replies below.**SA2 request:**

|  |
| --- |
| Regarding the procedure for location of a target UE using PRUs (clause 6.x.4 of the attached CR), SA2 noticed that RAN had agreements to support some positioning methods that require simultaneous measurements of the target UE and PRU. In the SA2 agreed procedures, it is assumed that the LMF can make the decision and realize such simultaneous measurements by using a common scheduled location time.SA2 would like to seek RAN1 and RAN2’s feedback on such assumption and whether additional enhancement would be needed to support the simultaneous measurements for the target UE and PRU. SA2 would update the specification according to the RAN1 and RAN2 feedbacks if necessary. |

**RAN1 reply:**Current RAN1 specifications do not support a mechanism to ensure simultaneous measurements/transmissions (e.g. in the same slot(s)) for multiple UEs, including a target UE and a PRU.RAN1 will continue discussions on what enhancements to LPP, NRPPa, and/or RAN signaling are necessary to support simultaneous measurements of the same DL-PRS for multiple UEs, including a target UE and a PRU; and to support simultaneous transmission of SRS for multiple UEs, including a target UE and a PRU.Note: The enhancements might or might not have RAN1 specification impact.**SA2 request:**

|  |
| --- |
| Additionally, SA2 also would like to know what location information can be provided by PRU, and whether RAN1 and RAN2 see benefit to allow PRU to provide its location information together with the location measurements reports. |

**RAN1 reply:**A PRU can report its location and associated uncertainty as is the case for other UEs. It is not necessary to always include the PRU location information with the PRU measurements in the same report. The PRU location information and measurements should be decoupled, where decoupled means that the PRU location information is determined independently of the reported measurements, even if the PRU location information and the PRU measurements would be included in the same report. |

In a previous LS, SA2 have asked RAN1 whether a PRU can "support the positioning signal transmission capability and signal measurement capability on PC5" ([R2-2211130](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_120/LSin/R2-2211130.zip) [3]), where RAN1 replied in [R2-2300009](https://www.3gpp.org/ftp/tsg_ran/WG2_RL2/TSGR2_121/LSin/R2-2300009.zip) [4] as follows (which was noted at RAN2#121 [2]):

 "From RAN1's perspective, a UE (which could be a PRU) that supports SL positioning can be allowed to support the positioning reference signal transmission capability and signal measurement capability on PC5, if the capability is introduced in R18."

Draft RAN2 Reply LSs (at least on some parts of the SA2 questions) have been submitted to this meeting in:

R2-2302875 [5]: "PRU Procedures (draft response LS to R2-2301939 (S2-2303861)) ", Qualcomm Incorporated.

R2-2302957 [6]: "Discussion and draft LS reply on PRU procedures, vivo.

R2-2303707 [7]: "On the Positioning Reference Units aspects", Ericsson.

NOTE: General PRU functionality is specified in TS 38.305, clause 5.4.5 [8].

# 3. Discussion

## 3.1 Support for simultaneous location measurements of a target UE and a PRU

SA2 request:

|  |
| --- |
| Regarding the procedure for location of a target UE using PRUs (clause 6.x.4 of the attached CR), SA2 noticed that RAN had agreements to support some positioning methods that require simultaneous measurements of the target UE and PRU. In the SA2 agreed procedures, it is assumed that the LMF can make the decision and realize such simultaneous measurements by using a common scheduled location time.SA2 would like to seek RAN1 and RAN2’s feedback on such assumption and whether additional enhancement would be needed to support the simultaneous measurements for the target UE and PRU. SA2 would update the specification according to the RAN1 and RAN2 feedbacks if necessary. |

R2-2302875 [5] proposed the following answer:

**Proposal 1 [5]:** Regarding the 1st SA2 question on "Support for simultaneous location measurements of a target UE and a PRU", RAN2 to reply the following:

"Dependent on the RAN1 requirements for simultaneous location measurements of the target UE and PRU, RAN2 will add signalling support for such a feature in LPP (and potentially in SLPP, if needed). Whether the LPP "scheduled location time" can be reused and/or enhanced for this purpose will be decided once the RAN1 requirements for this feature are agreed/available. Since this feature is positioning method specific and affects LPP (and potentially NRPPa and SLPP, if needed), RAN2 believes that the solution will have no impacts on the PRU procedures agreed by SA2 in S2-2303860."

R2-2302957 [6] proposes the following answer:

**Proposal 1 [6]:** Reply to SA2 that RAN2 will leave it to RAN1’s decision on the enhancement to support the simultaneous measurements for the target UE and PRU.

 Specifically:

|  |
| --- |
| Question 1: SA2 would like to seek RAN1 and RAN2’s feedback on such assumption and whether additional enhancement would be needed to support the simultaneous measurements for the target UE and PRU?Answer: RAN2 observed that RAN1 will further discuss it and would leave it to RAN1. |

R2-2303707 [7] does not propose an answer to this question.

Rapporteur comments:

- Both, R2-2302875 [5] and R2-2302957 [6] essentially conclude that this depends on further RAN1 requirements/agreements/input.

- However, R2-2302875 [5] is more specific on the SA2 request regarding:

(a) the assumption made by SA2 to "realize such simultaneous measurements by using a common scheduled location time" (i.e., NOTE 2 in Clause 6.X.4 in the agreed SA2 CR attached to the LS in R2-2302449 [1]).

(b) the specific action requested by SA2 "to provide feedback on whether any enhancement to the PRU procedures is required" [1].

- Therefore, it is proposed to use the draft response in R2-2302875 as baseline (see also discussion in R2-2302875 [5]).

**Question1:**

Regarding the 1st SA2 question on "Support for simultaneous location measurements of a target UE and a PRU", do you agree with the following RAN2 response:

"Dependent on the RAN1 requirements for simultaneous location measurements of the target UE and PRU, RAN2 will add signalling support for such a feature in LPP (and potentially in SLPP, if needed). Whether the LPP "scheduled location time" can be reused and/or enhanced for this purpose will be decided once the RAN1 requirements for this feature are agreed/available. Since this feature is positioning method specific and affects LPP (and potentially NRPPa and SLPP, if needed), RAN2 believes that the solution will have no impacts on the PRU procedures agreed by SA2 in S2-2303860."

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| OPPO |  | RAN1 still work on the detail of the configuration of the indicated time window, as well as the relationship with the schedule location time. We may postpone to discuss our reply after we get a confirmation of their discussion result latter. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

## 3.2 Location information provided by a PRU

SA2 Request:

|  |
| --- |
| Additionally, SA2 also would like to know what location information can be provided by PRU, and whether RAN1 and RAN2 see benefit to allow PRU to provide its location information together with the location measurements reports. |

R2-2302875 [5] proposed the following answer:

**Proposal 2 [5]:** Regarding the 2nd SA2 question on "Location information provided by a PRU", RAN2 to reply the following:

"A PRU should be able to report

(a) the location coordinates of the PRU only,

(b) the location measurements performed by the PRU only, or

(c) the location coordinates of the PRU together with any performed location measurements,

where location measurements above include the currently defined location measurements in LPP and potential new location measurements defined in Rel-18 and location coordinates provide the known location of the PRU, obtained independently from the location measurements.
Since the above reporting affects LPP (and potentially SLPP, if needed), RAN2 believes that the above reporting has no impacts on the PRU procedures agreed by SA2 in S2-2303860."

R2-2302957 [6] proposes the following answer:

**Proposal 2 [6]:** Reply to SA2 that RAN2 sees the benefit to allow PRU to provide its location information together with the measurement report.

 Specifically:

|  |
| --- |
| Question 2: SA2 also would like to know what location information can be provided by PRU, and whether RAN1 and RAN2 see benefit to allow PRU to provide its location information together with the location measurements reports.Answer: RAN2 sees the benefit to allow PRU to provide its location information together with the measurement reports, and will discuss what enhancements of LPP are needed. |

R2-2303707 [7] proposes the following answer:

**Proposal 1 [7]:** PRU UE provides location measurement and current location estimate using the same transaction upon NW request.

 Specifically:

|  |
| --- |
| RAN2 reply:PRU UE is a cooperative UE and hence such UEs are expected of assisting NW by providing both measurement and location.As PRU UE could have moved from previous location or because of change in radio condition there can be errors in the new computed location (delta as compared to previous stationary well known location); hence a PRU UE should provide both measurements and location to allow all the possible calibration parameters to the LMF.PRU UE should provide both location measurement and current location estimate using the same transaction upon NW request. |

Rapporteur comments:

- All 3 proposed RAN2 responses agree that a PRU should be able to report both, location measurements and known PRU location coordinates.

- This is also in agreement with the RAN1 response to the same SA2 question [2].

- However, both R2-2302957 [6] and R2-2303707 [7] do not to address the first part of SA2's question ("what location information can be provided by PRU") and the specific action requested by SA2 ("to provide feedback on whether any enhancement to the PRU procedures is required").

- Therefore, it is proposed to use the draft response in R2-2302875 [5] as baseline (see also discussion in R2-2302875 [5]).

NOTE: All 3 contributions (R2-2302875 [5], R2-2302957 [6], and R2-2303707[7]) propose also specific Stage 3 LPP design aspects, which however, requires further discussion in appropriate agenda items (possibly together with RAN1 input) and seems not affecting the answer to the specific SA2 question.

**Question 2:**

Regarding the 2nd SA2 question on "Location information provided by a PRU", do you agree with the following RAN2 reply:

"A PRU should be able to report:

(a) the location coordinates of the PRU only,

(b) the location measurements performed by the PRU only, or

(c) the location coordinates of the PRU together with any performed location measurements,

where location measurements above include the currently defined location measurements in LPP and potential new location measurements defined in Rel-18 and location coordinates provide the known location of the PRU, obtained independently from the location measurements.
Since the above reporting affects LPP (and potentially SLPP, if needed), RAN2 believes that the above reporting has no impacts on the PRU procedures agreed by SA2 in S2-2303860."

|  |  |  |
| --- | --- | --- |
| Company | Yes/No | Comments |
| OPPP | Yes for c, a and b needs further clarification of the purpose | Cannot see a straightforward reason why a PRU reports solely the location coordinates of the PUR or the location measurement performed by the PRU. The location coordinates and the measurement results should work together for network positioning result calibration.If reporting the location coordinates of the PRU in one-shot way is for the network to start to recognize the location information of the PRU and use such information together with following obtained solely location measurement results, that is OK. But we need to clarify the purpose firstly. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# References

[1] R2-2302449, "LS on PRU procedures (S2-2303861; contact: Qualcomm)", SA2 LS in Rel-18 5G\_eLCS\_Ph3 To:RAN2, RAN1.

[2] R2-2302409 (R1-2302146), "LS Reply on PRU Procedures (R1-2302146; contact Qualcomm)", RAN1 LS in REl-18 NR\_pos\_enh2-Core, 5G\_eLCS\_Ph3 To: SA2 Cc: RAN2, RAN3.

[3] R2-2211130, "LS Out on Positioning Reference Units (S2-2209590; contact: CATT)", SA2 LS in Rel-18 FS\_eLCS\_Ph3 To:RAN1 Cc:RAN2, RAN3.

[4] R2-2300009, "Reply LS on Positioning Reference Units (R1-2212715; contact: CATT)", RAN1 LS in Rel-18 FS\_eLCS\_Ph3 To:SA2 Cc:RAN2, RAN3.

[5] R2-2302875, "PRU Procedures (draft response LS to R2-2301939 (S2-2303861)) ", Qualcomm Incorporated.

[6] R2-2302957, "Discussion and draft LS reply on PRU procedures", vivo.

[7] R2-2303707, "On the Positioning Reference Units aspects", Ericsson.

[8] 3GPP TS 38.305: "Stage 2 functional specification of User Equipment (UE) positioning in NG-RAN".