3GPP TSG-RAN WG2 Meeting #121bis-e R2-230xxxx

Elbonia, 17 – 26 April 2023

**Agenda item: 7.2.2**

**Source: Nokia**

**Title: [AT121bis-e][423][POS] Sidelink positioning parameters in discovery signalling (Nokia)**

**WID/SID: NR\_pos\_enh - Release 18**

**Document for: Discussion and Decision**

# Introduction

This document is to start the following Email discussion:

* [AT121bis-e][423][POS] Sidelink positioning parameters in discovery signalling (Nokia)

Scope: Discuss the necessary parameters in discovery signalling for identifying the involved UEs in a sidelink positioning operation and establishing a session.

Intended outcome: Report to Monday week 2 session

Deadline: Friday 2023-04-21 1000 UTC

# Contact Points

Respondents to the email discussion are kindly asked to fill in the following table:

|  |  |  |
| --- | --- | --- |
| Company | Name | Email Address |
| Nokia (Rapporteur) | Stepan Kucera | stepan.kucera@nokia.com |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Discussion

In the context of UE discovery for sidelink positioning purposes, SA2 already made several agreements.

In the conclusion of KI#3 in 23.700-86, it is specified that

For Ranging/Sidelink Positioning device discovery, Model A and Model B Direct Discovery as defined in TS 23.304 [4] are reused for the 5G ProSe capable UE (including commercial and public safety use cases); and procedures for V2X communication over PC5 reference point as defined in TS 23.287 [3] are reused for the V2X capable UEs, with the following enhancements:

-     When 5G ProSe Direct Discovery procedures as defined in 6.3.1 of TS 23.304 [4] are used, the ProSe identifier indicates "Ranging/Sidelink Positioning";

-     When Group Member Discovery procedures as defined in 6.3.2.2 of TS 23.304 [4] are used, the Application Layer Group ID indicates a Ranging/Sidelink Positioning group that the UE belongs to;

-     When unicast mode V2X communication procedure is used, the Service Type in Layer-2 link establishment procedure indicates "Ranging/Sidelink Positioning";

-     When broadcast mode or groupcast mode V2X communication procedure is used, it is used with Service Type as "Ranging/Sidelink Positioning";

-     The expected roles of the UEs (e.g. Target UE, SL Reference UE) can be reflected in discovery procedure.

Furthermore, the clause 5.2.2 in TS 23.586 specifies that

The discovery of Located UEs follows the same principles as specified in clause 5.2.1. **The UE can indicate its role “Located UE” in its list of supported roles during discovery.**

As for the actual discovery procedures, SA2 states in 28.700-86 for example the following in clauses 6.4.2.2 (Model A) and 6.4.2.3 (Model B), respectively:

**[Model A]**

In this procedure, Reference UE and Target UE can take the design of UE Assisted and UE Based Positioning Procedure as specified in clause 6.11.1 of TS 23.273 [11] to enable the Ranging/Sidelink Positioning.

1. The Target UE sends an Announcement message. The Announcement message may include the Type of Discovery Message, Target UE info, Ranging/Sidelink Positioning service Code, Role indication (target UE) and Target UE capability (e.g. ranging support).

2. Reference UEs monitor the Announcement message. If the Target info is the Reference UE to be discovered, the Reference UEs have the interests on the Ranging service and support the Ranging/Sidelink Positioning capability of the Target UE if any, the Reference UE performs the direct PC5 link establishment procedure with target UE as described in clause 6.4.3.1 of TS 23.304 [4].

3. The Target UE and the Reference UE perform the Ranging/Sidelink Positioning control interaction procedure to exchange the coordination & configuration information, e.g. the Ranging capability and Ranging Assistance Data, as described in clause 6.4.2.4.

**[Model B]**

In this procedure, Reference UE and Target UE can take the design of UE Assisted and UE Based Positioning Procedure as specified in clause 6.11.1 of TS 23.273 [11] to enable the Ranging/Sidelink Positioning.

1. The Reference UE sends a Solicitation message. The Solicitation message may include Type of Discovery Message, Ranging/Sidelink Positioning service Code, Reference UE info, Target UE info, Role indication (Reference UE) and Reference UE capability.

2. Target UE monitors the Solicitation message. If the Target UE decides to be discovered and ranged based on the included Target info and the Reference UE capability in the Solicitation message, the Target UE responds to the Reference UE with a Discovery response message. The Discovery response message may include the Target UE capability.

3. After the target UE discovery, the Reference UE performs the PC5 Unicast communication establishment with target UE.

From RAN2 perspective, the exchange of both discovery and SLPP messages can be used to determine peer UEs that satisfy minimal service and performance requirements for a new or existing SL positioning process. These requirements include for example

* support of a specific SL positioning role (*eg as anchor / target / server UE*) on both capability and procedural level
* support of specific SL positioning capabilities / tasks (*eg, wide-band SL PRS transmission by an RSU, or specific positioning method by a server UE*)
* contribution to SL positioning QoS and performance (eg, *avoidance of NLOS conditions / co-located anchor UEs*)
* resource and latency efficiency (*eg, reusability of already active anchor / server UE).*

An open question is then how to balance the complexity-performance trade-off between using

* ProSe for initial signalling of UE attributes for their efficient pre-filtration and/or pre-configuration, and
* SLPP for subsequent detailed (delta)-signalling and setup of well-performing positioning sessions.

In this context, the rapporteur would like to ask the following questions:

1. **Do you generally agree that discovery messages shall be used to provide information relevant to UE selection? By said information are understood specific UE capabilities, service status attributes and/or AS conditions.**

|  |  |  |
| --- | --- | --- |
| Company | YES / NO | Technical Arguments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 1**: TBD.

**Proposal 1**: TBD.

1. **Assuming discovery messages carry auxiliary information as per Q1, which information from the following list shall be included?**

***Capability***

* + - 1. **capability to serve as anchor UE**
      2. **capability to serve as server UE for self and/or other nodes**
      3. **support of specific positioning method(s)**

***Status***

1. **active anchor UE status (eg, for fast reuse purposes)**
2. **active server UE status (eg, for fast reuse purposes)**
3. **“located UE” status (ie position is known by self or other node like LMF)**

***Condition***

1. **LOS/NLOS condition wrt discovering UE**
2. **synchronization information (eg, source)**
3. **measurement report (eg, to indicate co-location with / distance from other candidate anchors)**
4. **mobility-related information (eg, mobile/stationary, speed)**

***Network***

1. **PLMN ID**
2. **cell ID**
3. **network coverage status (IC, OOC)**
4. **area / zone information**

***Other***

1. **other**

|  |  |  |
| --- | --- | --- |
| Company | YES / NO | Technical Arguments |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

**Summary 2**: TBD.

**Proposal 2**: TBD.

# Conclusion

TBD.