3GPP TSG-RAN WG2 #121bis R2-23XXXXX

Online, 17th April– 26th April 2023

**Agenda item: 7.2.2**

**Source: Xiaomi**

**Title:** **[AT121bis-e][424][POS] Group positioning and multiple targets (Xiaomi/Qualcomm)**

**Document for: Discussion and Agreement**

# 1 Introduction

This document is to kick off the following Email discussion:

* [AT121bis-e][424][POS] Group positioning and multiple targets (Xiaomi/Qualcomm)

 Scope: Discuss P17-P19 of R2-2302740, attempt to conclude, and evaluate whether we can reply to the SA2 LS on multiple target UEs.

 Intended outcome: Report (Xiaomi) and agreeable reply LS (Qualcomm)

 Deadline: Friday 2023-04-21 1000 UTC

# 2 Contact Information

|  |  |
| --- | --- |
| Company | Contact: Name (E-mail) |
| Ericsson | Ritesh Shreevastav |
| Qualcomm | Dan Vassilovski (dvassilo@qti.qualcomm.com) |
| OPPO | Yang Liu |
| CATT | Jianxiang Li (lijianxiang@catt.cn) |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |
|  |  |

# Discussions

In LS from SA2 [8], SA2 indicates that the group management aspect can be handled by the application layer and is out of scope of SA2:

|  |
| --- |
| - A Ranging/SL Positioning layer is introduced on the Target UE/Reference UE/SL Positioning Server UE under Application layer and above AS layer to handle service request received from application layer and to control the Sidelink Positioning and Ranging operation:- Functionalities supported by the Ranging/SL Positioning layer include discovery of the UE(s) in proximity that can participate in Sidelink Positioning and Ranging service sessions and control signalling between UEs or among a group of UEs or between UE and LMF to manage and coordinate the Sidelink Positioning and Ranging operations.- The group management can be performed at application layer, and the application layer may provide group identifier information to the Ranging/SL Positioning layer. NOTE 1: Potential group management within RSPP layer is out-of-scope of SA2. |

As analyzed in [3], it is similar to how group operation was designed for NR Sidelink in Rel-16, whereby any group management operations (e.g. discovery for group formation, group members entering or leaving the group, etc.) were transparent to the AS layer. The application layer group ID in this case is managed by the application layer in the UE and/or the application server, which then interacts with the ProSe Layer to determine the Destination L2 ID for use over sidelink interface. From AS layer perspective, the mapping of L2 IDs to specific UEs within the group is handled by the upper layers and no impact is foreseen in RAN2 specifications.

So rapporteur would like to ask:

1. **Whether do you agree that the group management for group positioning is handled by the upper/application layer and no impact is foreseen in RAN2?**

|  |  |  |
| --- | --- | --- |
| Company | Agree or not | Comments |
| Ericsson | Agree | Yes no impact in RAN2 |
| Qualcomm | Partially Agree | Per TS 23.586, communication procedures as defined in 23.287 and 23.304 are used for SLPP (RSPP) when SLPP is carried over V2X or ProSe, respectively. As such, the upper/application layer performs group management through the procedures defined in 23.287 and 23.304. As RAN2 has agreed to support SLPP session-based operation, there can be instances of sessions requiring removal and/or addition of UEs to a session. Some examples could include SLPP Capability Exchange may determine not all UEs in an application-layer provided group have necessary capabilities for a session, or due to UE mobility, some UEs are no longer in range. As such, the SLPP layer may determine the UEs constituting a session group may need to be changed and disseminate this to the application layer. Thus, the SLPP layer may also be a participant in group management, including by informing the application layer of circumstances require change in group composition.  |
| OPPO | Agree | If AS layer find that radio condition of some UEs becomes worse and are not qualified for the SLPP, the AS layer should inform the application layer of the related UE AS level ID, for example, the L2 ID, and let the app layer perform the group management. |
| CATT | Not sure | We should clarify what the group positioning is and define the group positioning at first before we jump into the discussion of group positioning. I did not find any definition of group positioning in TS 23.586. Is group positioning a type of service or the positioning operations in a group which is defined in ProSe?Can rapporteur clarify where the group positioning is defined? |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

1. **If the answer to the above question is yes, do you agree that the group ID and/or L2 Destination IDs is provided by upper layers of SLPP?**

|  |  |  |
| --- | --- | --- |
| Company | Agree or not | Comments |
| Ericsson  | Agree | However, there should be provision in the Core Network to map the L2ID with the SUPI |
| Qualcomm | Agree | We agree that the application/upper layer can provide the SLPP layer with individual UE L2 IDs, individual UE Application-layer IDs, Application-layer Group ID and L2 Group ID. More generally, as noted in our answer to Q1, the procedures defined in 23.287 and 23.304 are used for SLPP (RSPP) when SLPP is carried over V2X or ProSe, respectively. This incudes the dissemination of relevant Application-layer IDs and Destination Layer 2 IDs.  |
| OPPO | Agree |  |
| CATT |  | We should clarify what the group positioning is and the definition of group positioning before we jump into the discussion of group positioning. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

In the LS from SA2 [1], SA2 askes whether the SLPP would support multiple Target UEs in the same signalling session. As analyzed in [3], if group management is performed by upper layer, multiple target UEs can be set in one group. Given that RAN2 has already confirmed that the SL positioning capability and assistance data can be sent in a groupcast/broadcast way, the groupcast of capability/assistant data to the group of multiple target UEs can trigger the session establishment at target UEs. Thus, it is technically feasible to support multiple target UEs in the same signalling session. So, rapporteur would like to ask:

1. **Whether the SLPP would support multiple Target UEs in the same signalling session?**

|  |  |  |
| --- | --- | --- |
| Company | Yes or not | Comments |
| Ericsson | No | We would like to first have solutions with single target only and if there is time left; we can discuss this case.We should first complete the work for single target UE case. It is already difficult with all different permutation and combination; i.e several UE roles; anchor, SL server, target and the interactions and may be for now for simplicity we should have only one target. |
| Qualcomm | Yes | We agree with the rapporteur that based on the agreements RAN2 has reached it is technically feasible to support multiple target UEs within the same signaling session.  |
| OPPO | For now no. | For multiple target UEs cases, the SLPP session management involves the addition/remove of anchor UEs for multiple target UEs. If these target UEs require for different anchor UEs due to their different location distribution/accuracy demand, SLPP session management overload may become overwhelmingly large. Also, considering the time limit, we should settle down the signaling procedure for the one target UE case firstly. |
| CATT |  | Multiple Target UEs are mentioned in TS 23.859: “The service exposure in clause 5.5 of TS 23.273 [8] is reused with enhancements. The request may indicate with corresponding events if the server requires relative distance/direction of target UEs, absolute positioning of target UEs, or both. The request shall include one or multiple target UEs and optionally it may include additional information such as the SL reference UE for relative distance/direction, the required positioning QoS, etc.”We would like to first discuss solutions with two target UEs in SLPP for the case in TS 23.859. Under this assumption, SLPP may support multiple Target UEs in the same signalling session. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

1. **If the answer to the above question is yes, do you agree the following procedure and signaling flow for sidelink based group positioning from [3] as baseline?**



|  |  |  |
| --- | --- | --- |
| Company | Yes or not | Comments |
| Qualcomm | Yes | We agree the above call flow should be supported by SLPP as a baseline call flow. Additionally, since RAN2 has agreed to support centralized positioning, where one UE performs range and/or position calculations based on measurement/location information related to itself and/or other UEs, a companion flow to the above illustrating the centralized operation should be included.  |
| OPPO |  | More details should be clarified for the signaling flow such as the UE roles. Is the UE1~4 in the given signaling flow are all target UEs? or anchor UEs are missing in the signaling flow?If UE 1~4 are all target UEs, it seems that absolute positioning for them is not workable. Then we assume that only ranging/relative positioning is the main purpose of the group positioning?  |
| CATT | postpone | RAN2 can discuss this issue based on the conclusion of Q1 and the progress of SA2. |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

In addition, SA2 asked RAN2 about whether there is possibility of signalling the positioning results of multiple Target UEs in the same message. From rapporteur point of view, the case mentioned by SA2 is majorly about distributing location estimate of one target UE to other UEs in the group. Technically, it is feasible for SLPP to do so. But there might be security/privacy concern of exposing location estimates to other UEs, which should be addressed by SA3.

1. **Do you agree that it is technically feasible from RAN2 point of view to signal the positioning results of multiple Target UEs in the same SLPP message, and the security/privacy issue, if any, should be addressed by SA3？**

|  |  |  |
| --- | --- | --- |
| Company | Yes or not | Comments |
| Ericsson | Down prioritize this scenario for now | We should first complete the work for single target UE case. It is already difficult with all different permutation and combination; i.e several UE roles; anchor, SL server, target and the interactions and may be for now for simplicity we should have only one target. |
| Qualcomm | Yes | We agree that it is technically feasible for SLPP to distribute positioning results of multiple Target UEs in the same SLPP message. From a security point of view, we see no impediment to doing so, since for unicast there is a well-established security mechanism, and for Groupcast/Broadcast SA3 has indicated security is feasible and is currently designing a security solution. From a privacy point of view, 3GPP RAN2 current V2X design already supports distribution of UE position and UE position accuracy to multiple UEs through application-layer signaling carried as V2X payload (e.g., CAM, BSM, etc.). Since SLPP signaling can be carried as V2X payload, SLPP signaling should not pose a privacy concern.  |
| OPPO |  | The security concern should be address by SA3. It is feasible from RAN2 perspective |
| CATT | Yes | It is technically feasible for SLPP to distribute positioning results of multiple Target UEs in the same SLPP message, at least for unicast message.  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |
|  |  |  |

# Reference

##  R2-2302448 LS on support of multiple Target UEs (S2-2303837; contact: Qualcomm) SA2 LS in Rel-18 Ranging\_SL To:RAN2 Cc:RAN1

1. R2-2302503 Discussion on sidelink positioning CATT discussion Rel-18 NR\_pos\_enh2
2. R2-2302740 Further considerations on sidelink positioning Intel Corporation discussion Rel-18 NR\_pos\_enh2
3. R2-2302958 Discussion on sidelink positioning vivo discussion Rel-18 FS\_NR\_pos\_enh2
4. R2-2303497 Discussion on sidelink positioning ZTE Corporation discussion Rel-18 NR\_pos\_enh2
5. R2-2303591 Sidelink Positioning Protocol (SLPP) Signaling and Procedures Qualcomm Incorporated discussion
6. R2-2304033 Discussion on SL positioning Xiaomi discussion Rel-18
7. S2-2301786, Reply LS on SL positioning groupcast and broadcast.