**3GPP T****SG-RAN WG2 Meeting #121bis-e R2-230xxxx**

**Electronic, 18th – 26th April, 2023**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **38.331** | **CR** | **draft** | **rev** | **-** | **Current version:** | **17.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **x** | Radio Access Network | **x** | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Running 38.331 CR for R18 Network-controlled repeaters |
|  |  |
| ***Source to WG:*** | ZTE Corporation (Rapporteur) |
| ***Source to TSG:*** | R2 |
|  |  |
| ***Work item code:*** | NR\_netcon\_repeater |  | ***Date:*** | 2023-04-07 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Introduction of Rel-18 Network-controlled repeaters (NCR).  |
|  |  |
| ***Summary of change:*** | Introduction of Rel-18 Network-controlled repeaters (NCR). |
|  |  |
| ***Consequences if not approved:*** | Network-controlled repeaters are not supported |
|  |  |
| ***Clauses affected:*** | 3.2, 4.4, 5.2.2.4.2, 5.3.1.1, 5.3.3.4, 5.3.5.2, 5.3.5.8.2, 5.3.7.1, 5.3.7.2, 5.3.8.1, 5.3.8.2, 5.3.8.3, 5.3.10.3, 5.3.13.2, 5.3.14.16.2.2, 6.3.2, 6.4 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

START OF CHANGES

# 3 Definitions, symbols and abbreviations

## 3.2 Abbreviations

For the purposes of the present document, the abbreviations given in TR 21.905 [1] and the following apply. An abbreviation defined in the present document takes precedence over the definition of the same abbreviation, if any, in TR 21.905 [1].

5GC 5G Core Network

ACK Acknowledgement

AM Acknowledged Mode

ARQ Automatic Repeat Request

AS Access Stratum

ASN.1 Abstract Syntax Notation One

BAP Backhaul Adaptation Protocol

BCD Binary Coded Decimal

BFD Beam Failure Detection

BH Backhaul

BLER Block Error Rate

BWP Bandwidth Part

CA Carrier Aggregation

CAG Closed Access Group

CAG-ID Closed Access Group Identifier

CAPC Channel Access Priority Class

CBR Channel Busy Ratio

CCCH Common Control Channel

CFR Common Frequency Resources

CG Cell Group

CHO Conditional Handover

CLI Cross Link Interference

CMAS Commercial Mobile Alert Service

CP Control Plane

CPA Conditional PSCell Addition

CPC Conditional PSCell Change

C-RNTI Cell RNTI

CSI Channel State Information

DAPS Dual Active Protocol Stack

DC Dual Connectivity

DCCH Dedicated Control Channel

DCI Downlink Control Information

DCP DCI with CRC scrambled by PS-RNTI

DFN Direct Frame Number

DL Downlink

DL-PRS Downlink Positioning Reference Signal

DL-SCH Downlink Shared Channel

DM-RS Demodulation Reference Signal

DRB (user) Data Radio Bearer

DRX Discontinuous Reception

DTCH Dedicated Traffic Channel

ECEF Earth-Centered, Earth-Fixed

ECI Earth-Centered Inertial

EN-DC E-UTRA NR Dual Connectivity with E-UTRA connected to EPC

EPC Evolved Packet Core

EPS Evolved Packet System

ETWS Earthquake and Tsunami Warning System

E-UTRA Evolved Universal Terrestrial Radio Access

E-UTRA/5GC E-UTRA connected to 5GC

E-UTRA/EPC E-UTRA connected to EPC

E-UTRAN Evolved Universal Terrestrial Radio Access Network

FDD Frequency Division Duplex

FFS For Further Study

G-CS-RNTI Group Configured Scheduling RNTI

GERAN GSM/EDGE Radio Access Network

GIN Group ID for Network selection

GNSS Global Navigation Satellite System

G-RNTI Group RNTI

GSM Global System for Mobile Communications

HARQ Hybrid Automatic Repeat Request

HRNN Human Readable Network Name

HSDN High Speed Dedicated Network

H-SFN Hyper SFN

IAB Integrated Access and Backhaul

IAB-DU IAB-node DU

IAB-MT IAB Mobile Termination

IDC In-Device Coexistence

IE Information element

IMSI International Mobile Subscriber Identity

kB Kilobyte (1000 bytes)

L1 Layer 1

L2 Layer 2

L3 Layer 3

LBT Listen Before Talk

LEO Low Earth Orbit

MAC Medium Access Control

MBS Multicast/Broadcast Service

MBS FSAI MBS Frequency Selection Area Identity

MCCH MBS Control Channel

MCG Master Cell Group

MDT Minimization of Drive Tests

MIB Master Information Block

MPE Maximum Permissible Exposure

MRB MBS Radio Bearer

MR-DC Multi-Radio Dual Connectivity

MTCH MBS Traffic Channel

MTSI Multimedia Telephony Service for IMS

MUSIM Multi-Universal Subscriber Identity Module

N/A Not Applicable

NCR Network-Controlled Repeater

NCR-Fwd NCR Forwarding

NCR-MT NCR Mobile Termination

NE-DC NR E-UTRA Dual Connectivity

(NG)EN-DC E-UTRA NR Dual Connectivity (covering E-UTRA connected to EPC or 5GC)

NGEN-DC E-UTRA NR Dual Connectivity with E-UTRA connected to 5GC

NID Network Identifier

NPN Non-Public Network

NR-DC NR-NR Dual Connectivity

NR/5GC NR connected to 5GC

NSAG Network Slice AS Group

NTN Non-Terrestrial Network

PCell Primary Cell

PDCP Packet Data Convergence Protocol

PDU Protocol Data Unit

PEI Paging Early Indication

PEI-O Paging Early Indication-Occasion

PLMN Public Land Mobile Network

PNI-NPN Public Network Integrated Non-Public Network

posSIB Positioning SIB

PPW PRS Processing Window

PRS Positioning Reference Signal

PSCell Primary SCG Cell

PTM Point to Multipoint

PTP Point to Point

PWS Public Warning System

QoE Quality of Experience

QoS Quality of Service

RAN Radio Access Network

RAT Radio Access Technology

RLC Radio Link Control

RLM Radio Link Monitoring

RMTC RSSI Measurement Timing Configuration

RNA RAN-based Notification Area

RNTI Radio Network Temporary Identifier

ROHC Robust Header Compression

RPLMN Registered Public Land Mobile Network

RRC Radio Resource Control

RS Reference Signal

SBAS Satellite Based Augmentation System

SCell Secondary Cell

SCG Secondary Cell Group

SCS Subcarrier Spacing

SD-RSRP Sidelink Discovery RSRP

SDT Small Data Transmission

SFN System Frame Number

SFTD SFN and Frame Timing Difference

SI System Information

SIB System Information Block

SL Sidelink

SLSS Sidelink Synchronisation Signal

SNPN Stand-alone Non-Public Network

SpCell Special Cell

SRAP Sidelink Relay Adaptation Protocol

SRB Signalling Radio Bearer

SRS Sounding Reference Signal

SSB Synchronization Signal Block

TAG Timing Advance Group

TDD Time Division Duplex

TEG Timing Error Group

TM Transparent Mode

TMGI Temporary Mobile Group Identity

U2N UE-to-Network

UDC Uplink Data Compression

UE User Equipment

UL Uplink

UM Unacknowledged Mode

UP User Plane

VR Virtual Reality

In the ASN.1, lower case may be used for some (parts) of the above abbreviations e.g. c-RNTI.

NEXT CHANGE

# 4 General

## 4.4 Functions

The RRC protocol includes the following main functions:

- Broadcast of system information:

- Including NAS common information;

- Information applicable for UEs in RRC\_IDLE and RRC\_INACTIVE (e.g. cell (re-)selection parameters, neighbouring cell information) and information (also) applicable for UEs in RRC\_CONNECTED (e.g. common channel configuration information);

- Including ETWS notification, CMAS notification;

- Including positioning assistance data.

- RRC connection control:

- Paging;

- Establishment/modification/suspension/resumption/release of RRC connection, including e.g. assignment/modification of UE identity (C-RNTI, fullI-RNTI, etc.), establishment/modification/suspension/resumption/release of SRBs (except for SRB0);

- Access barring;

- Initial AS security activation, i.e. initial configuration of AS integrity protection (SRBs, DRBs) and AS ciphering (SRBs, DRBs);

- RRC connection mobility including e.g. intra-frequency and inter-frequency handover, path switch from a PCell to a target L2 U2N Relay UE or from a L2 U2N Relay UE to a target PCell, associated AS security handling, i.e. key/algorithm change, specification of RRC context information transferred between network nodes;

- Establishment/modification/suspension/resumption/release of RBs carrying user data (DRBs/MRBs);

- Radio configuration control including e.g. assignment/modification of ARQ configuration, HARQ configuration, DRX configuration;

- In case of DC, cell management including e.g. change of PSCell, addition/modification/release of SCG cell(s);

- In case of CA, cell management including e.g. addition/modification/release of SCell(s);

- QoS control including assignment/ modification of semi-persistent scheduling (SPS) configuration and configured grant configuration for DL and UL respectively, assignment/ modification of parameters for UL rate control in the UE, i.e. allocation of a priority and a prioritised bit rate (PBR) for each RB of UE and logical channel of IAB-MT.

- Recovery from radio link failure.

- Inter-RAT mobility including e.g. AS security activation, transfer of RRC context information;

- Measurement configuration and reporting:

- Establishment/modification/release of measurement configuration (e.g. intra-frequency, inter-frequency and inter- RAT measurements);

- Setup and release of measurement gaps;

- Measurement reporting.

- Configuration of BAP entity and BH RLC channels for the support of IAB-node.

- Configuration of SRAP entity and Uu/PC5 Relay RLC channels for the support of L2 U2N relay.

- Other functions including e.g. generic protocol error handling, transfer of dedicated NAS information, transfer of UE radio access capability information.

- Support of self-configuration and self-optimisation.

- Support of measurement logging and reporting for network performance optimisation, as specified in TS 37.320 [61];

- Support of transfer of application layer measurement configuration and reporting.

- Configuration of side control information for NCR-node.

NEXT CHANGE

# 5 Procedures

## 5.2 System information

### 5.2.2 System information acquisition

#### 5.2.2.4 Actions upon receipt of System Information

##### 5.2.2.4.2 Actions upon reception of the *SIB1*

Upon receiving the *SIB1* the UE shall:

1> store the acquired *SIB1*;

1> if the UE is a RedCap UE and it is in RRC\_IDLE or in RRC\_INACTIVE, or if the RedCap UE is in RRC\_CONNECTED while *T311* is running:

2> if *intraFreqReselectionRedCap* is not present in *SIB1*:

3> consider the cell as barred in accordance with TS 38.304 [20];

3> perform barring as if *intraFreqReselectionRedCap* is set to allowed;

2> else:

3> if the *cellBarredRedCap1Rx* is present in the acquired *SIB1* and is set to *barred* and the UE is equipped with 1 Rx branch; or

3> if the *cellBarredRedCap2Rx* is present in the acquired *SIB1* and is set to *barred* and the UE is equipped with 2 Rx branches; or

3> if the *halfDuplexRedCapAllowed* is not present in the acquired *SIB1* and the UE supports only half-duplex FDD operation:

4> consider the cell as barred in accordance with TS 38.304 [20];

4> perform barring based on *intraFreqReselectionRedCap* as specified in TS 38.304 [20];

1> if the *cellAccessRelatedInfo* contains an entry of a selected SNPN or PLMN and in case of PLMN the UE is either allowed or instructed to access the PLMN via a cell for which at least one CAG ID is broadcast:

2> in the remainder of the procedures use *npn-IdentityList, trackingAreaCode,* and *cellIdentity* for the cell as received in the corresponding entry of *npn-IdentityInfoList* containing the selected PLMN or SNPN;

1> else if the *cellAccessRelatedInfo* contains an entry with the *PLMN-Identity* of the selected PLMN:

2> in the remainder of the procedures use *plmn-IdentityList*, *trackingAreaCode*, *trackingAreaList,* and *cellIdentity* for the cell as received in the corresponding *PLMN-IdentityInfo* containing the selected PLMN;

1> if in RRC\_CONNECTED while T311 is not running:

2> disregard the *frequencyBandList*, if received, while in RRC\_CONNECTED;

2> forward the *cellIdentity* to upper layers;

2> forward the *trackingAreaCode* to upper layers, if included;

2> forward the *trackingAreaList* to upper layers, if included;

2> forward the received *posSIB-MappingInfo* to upper layers, if included;

2> apply the configuration included in the *servingCellConfigCommon*;

2> if the UE has a stored valid version of a SIB or posSIB, in accordance with clause 5.2.2.2.1, that the UE requires to operate within the cell in accordance with clause 5.2.2.1:

3> use the stored version of the required SIB or posSIB;

2> else:

3> acquire the required SIB or posSIB requested by upper layer as defined in clause 5.2.2.3.5;

NOTE: Void.

1> else:

2> if the UE supports one or more of the frequency bands indicated in the *frequencyBandList* for downlink for TDD, or one or more of the frequency bands indicated in the *frequencyBandList* for uplink for FDD, and they are not downlink only bands, and

2> if the UE is IAB-MT or supports at least one *additionalSpectrumEmission* in the *NR-NS-PmaxList* for a supported band in the downlink for TDD, or a supported band in uplink for FDD, and

2> if the UE supports an uplink channel bandwidth with a maximum transmission bandwidth configuration (see TS 38.101-1 [15] and TS 38.101-2 [39]) which

- is smaller than or equal to the *carrierBandwidth* (indicated in *uplinkConfigCommon* for the SCS of the initial uplink BWP or, for RedCap UE, of the RedCap-specific initial uplink BWP if configured), and which

- is wider than or equal to the bandwidth of the initial uplink BWP or, for RedCap UE, of the RedCap-specific initial uplink BWP if configured, and

2> if the UE supports a downlink channel bandwidth with a maximum transmission bandwidth configuration (see TS 38.101-1 [15] and TS 38.101-2 [39]) which

- is smaller than or equal to the *carrierBandwidth* (indicated in *downlinkConfigCommon* for the SCS of the initial downlink BWP or, for RedCap UE, of the RedCap-specific initial downlink BWP if configured), and which

- is wider than or equal to the bandwidth of the initial downlink BWP or, for RedCap UE, of the RedCap-specific initial downlink BWP if configured, and

2> if *frequencyShift7p5khz* is present and the UE supports corresponding 7.5kHz frequency shift on this band; or *frequencyShift7p5khz* is not present:

3> if neither *trackingAreaCode* nor *trackingAreaList* is provided for the selected PLMN nor the registered PLMN nor PLMN of the equivalent PLMN list:

4> consider the cell as barred in accordance with TS 38.304 [20];

4> perform cell re-selection to other cells on the same frequency as the barred cell as specified in TS 38.304 [20];

3> else if UE is IAB-MT and if *iab-Support* is not provided for the selected PLMN nor the registered PLMN nor PLMN of the equivalent PLMN list nor the selected SNPN nor the registered SNPN:

4> consider the cell as barred in accordance with TS 38.304 [20];

3> else if UE is NCR-MT and if *ncr-Support* is not provided:

4> consider the cell as barred in accordance with TS 38.304 [20];

3> else:

4> apply a supported uplink channel bandwidth with a maximum transmission bandwidth which

- is contained within the *carrierBandwidth* indicated in *uplinkConfigCommon* for the SCS of the initial uplink BWP or, for RedCap UEs, RedCap-specific initial uplink BWP, if configured, and which

- is wider than or equal to the bandwidth of the initial BWP for the uplink or, for a RedCap UE, of the RedCap-specific initial uplink BWP if configured;

4> apply a supported downlink channel bandwidth with a maximum transmission bandwidth which

- is contained within the *carrierBandwidth* indicated in *downlinkConfigCommon* for the SCS of the initial downlink BWP or, for RedCap UEs, RedCap-specific initial downlink BWP, if configured, and which

- is wider than or equal to the bandwidth of the initial BWP for the downlink or, for a RedCap UE, of the RedCap-specific initial downlink BWP if configured;

4> select the first frequency band in the *frequencyBandList*, for FDD from *frequencyBandList* for uplink, or for TDD from *frequencyBandList* for downlink,which the UE supports and for which the UE supports at least one of the *additionalSpectrumEmission* values in *nr-NS-PmaxList*, if present;

4> forward the *cellIdentity* to upper layers;

4> forward the *trackingAreaCode* to upper layers;

4> forward the *trackingAreaList* to upper layers, if included;

4> forward the received *posSIB-MappingInfo* to upper layers, if included;

4> forward the PLMN identity or SNPN identity or PNI-NPN identity to upper layers;

4> if in RRC\_INACTIVE and the forwarded information does not trigger message transmission by upper layers:

5> if the serving cell does not belong to the configured *ran-NotificationAreaInfo*:

6> initiate an RNA update as specified in 5.3.13.8;

4> forward the *ims-EmergencySupport* to upper layers, if present;

4> forward the *eCallOverIMS-Support* to upper layers, if present;

4> forward the *UAC-AccessCategory1-SelectionAssistanceInfo* or *UAC-AC1-SelectAssistInfo* for the selected PLMN/SNPNto upper layers, if present and set to *a*, *b* or *c*;

4> if the UE is in SNPN access mode:

5> forward the *imsEmergencySupportForSNPN* indicators with the corresponding SNPN identities to upper layers, if present;

4> apply the configuration included in the *servingCellConfigCommon*;

4> apply the specified PCCH configuration defined in 9.1.1.3;

4> if the UE has a stored valid version of a SIB, in accordance with clause 5.2.2.2.1, that the UE requires to operate within the cell in accordance with clause 5.2.2.1:

5> use the stored version of the required SIB;

4> if the UE has not stored a valid version of a SIB, in accordance with clause 5.2.2.2.1, of one or several required SIB(s), in accordance with clause 5.2.2.1:

5> for the SI message(s) that, according to the *si-SchedulingInfo*, contain at least one required SIB and for which *si-BroadcastStatus* is set to broadcasting:

6> acquire the SI message(s) as defined in clause 5.2.2.3.2;

5> for the SI message(s) that, according to the *si-SchedulingInfo*, contain at least one required SIB and for which *si-BroadcastStatus* is set to *notBroadcasting*:

6> trigger a request to acquire the SI message(s) as defined in clause 5.2.2.3.3;

4> if the UE has a stored valid version of a posSIB, in accordance with clause 5.2.2.2.1, of one or several required posSIB(s), in accordance with clause 5.2.2.1:

5> use the stored version of the required posSIB;

4> if the UE has not stored a valid version of a posSIB, in accordance with clause 5.2.2.2.1, of one or several posSIB(s) in accordance with clause 5.2.2.1:

5> for the SI message(s) that, according to the *posSI-SchedulingInfo*, contain at least one requested posSIB and for which *posSI-BroadcastStatus* is set to *broadcasting*:

6> acquire the SI message(s) as defined in clause 5.2.2.3.2;

5> for the SI message(s) that, according to the *posSI-SchedulingInfo*, contain at least one requested posSIB for which *posSI-BroadcastStatus* is set to *notBroadcasting*:

6> trigger a request to acquire the SI message(s) as defined in clause 5.2.2.3.3a;

4> apply the first listed *additionalSpectrumEmission* which it supports among the values included in *NR-NS-PmaxList* within *frequencyBandList* in *uplinkConfigCommon* for FDD or in *downlinkConfigCommon* for TDD;

4> if the *additionalPmax* is present in the same entry of the selected *additionalSpectrumEmission* within *NR-NS-PmaxList*:

5> apply the *additionalPmax* for UL;

4> else:

5> apply the *p-Max* in *uplinkConfigCommon* for UL;

4> if *supplementaryUplink* is present in *servingCellConfigCommon*; and

4> if the UE supports one or more of the frequency bands indicated in the *frequencyBandList* for the *supplementaryUplink*; and

4> if the UE supports at least one *additionalSpectrumEmission* in the *NR-NS-PmaxList* for a supported supplementary uplink band; and

4> if the UE supports an uplink channel bandwidth with a maximum transmission bandwidth configuration (see TS 38.101-1 [15] and TS 38.101-2 [39]) which

- is smaller than or equal to the *carrierBandwidth* (indicated in *supplementaryUplink* for the SCS of the initial uplink BWP), and which

- is wider than or equal to the bandwidth of the initial uplink BWP of the SUL:

5> consider supplementary uplink as configured in the serving cell;

5> select the first frequency band in the *frequencyBandList* for the *supplementaryUplink* which the UE supports and for which the UE supports at least one of the *additionalSpectrumEmission* values in *nr-NS-PmaxList*, if present;

5> apply a supported supplementary uplink channel bandwidth with a maximum transmission bandwidth which

- is contained within the *carrierBandwidth* (indicated in *supplementaryUplink* for the SCS of the initial uplink BWP), and which

- is wider than or equal to the bandwidth of the initial BWP of the SUL;

5> apply the first listed *additionalSpectrumEmission* which it supports among the values included in *NR-NS-PmaxList* within *frequencyBandList* for the *supplementaryUplink*;

5> if the *additionalPmax* is present in the same entry of the selected *additionalSpectrumEmission* within *NR-NS-PmaxList* for the *supplementaryUplink*:

6> apply the *additionalPmax* in *supplementaryUplink* for SUL;

5> else:

6> apply the *p-Max* in *supplementaryUplink* for SUL;

2> else:

3> consider the cell as barred in accordance with TS 38.304 [20]; and

3> perform barring as if *intraFreqReselection*, or *intraFreqReselectionRedCap* for RedCap UEs, is set to *notAllowed*;

NEXT CHANGE

## 5.3 Connection control

### 5.3.1 Introduction

#### 5.3.1.1 RRC connection control

RRC connection establishment involves the establishment of SRB1. The network completes RRC connection establishment prior to completing the establishment of the NG connection, i.e. prior to receiving the UE context information from the 5GC. Consequently, AS security is not activated during the initial phase of the RRC connection. During this initial phase of the RRC connection, the network may configure the UE to perform measurement reporting, but the UE only sends the corresponding measurement reports after successful AS security activation. However, the UE only accepts a re-configuration with sync message when AS security has been activated.

Upon receiving the UE context from the 5GC, the RAN activates AS security (both ciphering and integrity protection) using the initial AS security activation procedure. The RRC messages to activate AS security (command and successful response) are integrity protected, while ciphering is started only after completion of the procedure. That is, the response to the message used to activate AS security is not ciphered, while the subsequent messages (e.g. used to establish SRB2, DRBs and multicast MRBs) are both integrity protected and ciphered. After having initiated the initial AS security activation procedure, the network may initiate the establishment of SRB2 and DRBs and/or multicast MRBs, i.e. the network may do this prior to receiving the confirmation of the initial AS security activation from the UE. In any case, the network will apply both ciphering and integrity protection for the RRC reconfiguration messages used to establish SRB2, DRBs and/or multicast MRBs. The network should release the RRC connection if the initial AS security activation and/ or the radio bearer establishment fails. A configuration with SRB2 without DRB or multicast MRB, or with DRB or multicast MRB without SRB2 is not supported (i.e., SRB2 and at least one DRB or multicast MRB must be configured in the same RRC Reconfiguration message, and it is not allowed to release all the DRBs and multicast MRBs without releasing the RRC Connection). For IAB-MT and NCR-MT, a configuration with SRB2 without any DRB/MRB is supported.

The release of the RRC connection normally is initiated by the network. The procedure may be used to re-direct the UE to an NR frequency or an E-UTRA carrier frequency.

The suspension of the RRC connection is initiated by the network. When the RRC connection is suspended, the UE stores the UE Inactive AS context and any configuration received from the network, and transits to RRC\_INACTIVE state. The RRC message to suspend the RRC connection is integrity protected and ciphered.

The resumption of a suspended RRC connection is initiated by upper layers when the UE needs to transit from RRC\_INACTIVE state to RRC\_CONNECTED state or by RRC layer to perform a RNA update or by RAN paging from NG-RAN or for SDT. When the RRC connection is resumed, network configures the UE according to the RRC connection resume procedure based on the stored UE Inactive AS context and any RRC configuration received from the network. The RRC connection resume procedure re-activates AS security and re-establishes SRB(s) and DRB(s) and/or multicast MRB(s), if configured.

Upon initiating the resume procedure for SDT, AS security (both ciphering and integrity protection) is re-activated for SRB2 (if configured for SDT) and for SRB1. In addition, AS security is also re-activated (if security is configured) for all the DRBs configured for SDT. Further, the PDCP entities of SRB1 and PDCP entities of the radio bearers configured for SDT are re-established and resumed whilst the UE remains in RRC\_INACTIVE state. Transmission and reception of data and/or signalling messages over radio bearers configured for SDT can happen whilst the UE is in RRC\_INACTIVE state and SDT procedure is ongoing.

In response to a request to resume the RRC connection or in response to a resume procedure initiated for SDT, the network may resume the suspended RRC connection and send UE to RRC\_CONNECTED, or reject the request to resume and send UE to RRC\_INACTIVE (with a wait timer), or directly re-suspend the RRC connection and send UE to RRC\_INACTIVE, or directly release the RRC connection and send UE to RRC\_IDLE, or instruct the UE to initiate NAS level recovery (in this case the network sends an RRC setup message).

NOTE: In case the UE receives the configurations for NR sidelink communication via the E-UTRA, the configurations for NR sidelink communication in *SIB12* and *sl-ConfigDedicatedNR* within *RRCReconfiguration* used in clause 5.3 are provided by the configurations in *SystemInformationBlockType28* and *sl-ConfigDedicatedForNR* within *RRCConnectionReconfiguration* as specified in TS 36.331[10], respectively.

NEXT CHANGE

### 5.3.3 RRC connection establishment

#### 5.3.3.4 Reception of the *RRCSetup* by the UE

The UE shall perform the following actions upon reception of the *RRCSetup*:

1> if the *RRCSetup* is received in response to an *RRCReestablishmentRequest*; or

1> if the *RRCSetup* is received in response to an *RRCResumeRequest* or *RRCResumeRequest1*:

2> if *sdt-MAC-PHY-CG-Config* is configured:

3> instruct the MAC entity to stop the *cg-SDT-TimeAlignmentTimer*, if it is running;

3> instruct the MAC entity to start the *timeAlignmentTimer* associated with the PTAG*,* if it is not running;

2> if *srs-PosRRC-InactiveConfig* is configured:

3> instruct the MAC entity to stop the *inactivePosSRS-TimeAlignmentTimer*, if it is running;

2> discard any stored UE Inactive AS context and *suspendConfig*;

2> discard any current AS security context including the KRRCenc key, the KRRCint key, the KUPint key and the KUPenc key;

2> release radio resources for all established RBs except SRB0 and broadcast MRBs, including release of the RLC entities, of the associated PDCP entities and of SDAP;

2> release the RRC configuration except for the default L1 parameter values, default MAC Cell Group configuration, CCCH configuration and broadcast MRBs;

2> indicate to upper layers fallback of the RRC connection;

2> discard any application layer measurement reports which were not transmitted yet;

2> inform upper layers about the release of all application layer measurement configurations;

2> stop timer T380, if running;

1> perform the cell group configuration procedure in accordance with the received *masterCellGroup* and as specified in 5.3.5.5;

1> perform the radio bearer configuration procedure in accordance with the received *radioBearerConfig* and as specified in 5.3.5.6;

1> if stored, discard the cell reselection priority information provided by the *cellReselectionPriorities* or inherited from another RAT;

1> stop timer T300, T301, T319;

1> if T319a is running:

2> stop T319a;

2> consider SDT procedure is not ongoing;

1> if T390 is running:

2> stop timer T390 for all access categories;

2> perform the actions as specified in 5.3.14.4;

1> if T302 is running:

2> stop timer T302;

2> perform the actions as specified in 5.3.14.4;

1> stop timer T320, if running;

1> if the *RRCSetup* is received in response to an *RRCResumeRequest*, *RRCResumeRequest1* or *RRCSetupRequest*:

2> if T331 is running:

3> stop timer T331;

3> perform the actions as specified in 5.7.8.3;

2> enter RRC\_CONNECTED;

2> stop the cell re-selection procedure;

2> stop relay (re)selection procedure if any for L2 U2N Remote UE;

1> consider the current cell to be the PCell;

1> perform the L2 U2N Remote UE configuration procedure in accordance with the received *sl-L2RemoteUE-Config* as specified in 5.3.5.16;

1> perform the sidelink dedicated configuration procedure in accordance with the received *sl-ConfigDedicatedNR* as specified in 5.3.5.14;

1> if the UE has radio link failure or handover failure information available in *VarRLF-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report*:

2> if *reconnectCellId* in *VarRLF-Report* is not set after failing to perform reestablishment:

3> if the UE supports RLF-Report for conditional handover and if *choCellId* in *VarRLF-Report* is set:

4> set *timeUntilReconnection* in *VarRLF-Report* to the time that elapsed since the radio link failure or handover failure experienced in the *failedPCellId* stored in *VarRLF-Report*;

3> else:

4> set *timeUntilReconnection* in *VarRLF-Report* to the time that elapsed since the last radio link failure or handover failure;

3> set *nrReconnectCellId* in *reconnectCellId* in *VarRLF-Report* to the global cell identity and the tracking area code of the PCell;

1> if the UE supports RLF report for inter-RAT MRO NR as defined in TS 36.306 [62], and if the UE has radio link failure or handover failure information available in *VarRLF-Report* of TS 36.331 [10] and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report* of TS 36.331 [10]:

2> if *reconnectCellId* in *VarRLF-Report* of TS 36.331[10] is not set after failing to perform reestablishment:

3> set *timeUntilReconnection* in *VarRLF-Report* of TS 36.331[10] to the time that elapsed since the last radio link failure or handover failure in LTE;

3> set *nrReconnectCellId* in *reconnectCellId* in *VarRLF-Report* of TS 36.331[10] to the global cell identity and the tracking area code of the PCell;

1> set the content of *RRCSetupComplete* message as follows:

2> if upper layers provide a 5G-S-TMSI:

3> if the *RRCSetup* is received in response to an *RRCSetupRequest*:

4> set the *ng-5G-S-TMSI-Value* to *ng-5G-S-TMSI-Part2*;

3> else:

4> set the *ng-5G-S-TMSI-Value* to *ng-5G-S-TMSI*;

2> if upper layers selected an SNPN or a PLMN and in case of PLMN UE is either allowed or instructed to access the PLMN via a cell for which at least one CAG ID is broadcast:

3> set the *selectedPLMN-Identity* from the *npn-IdentityInfoList*;

2> else:

3> set the *selectedPLMN-Identity* to the PLMN selected by upper layers from the *plmn-IdentityInfoList*;

2> if upper layers provide the 'Registered AMF':

3> include and set the *registeredAMF* as follows:

4> if the PLMN identity of the 'Registered AMF' is different from the PLMN selected by the upper layers:

5> include the *plmnIdentity* in the *registeredAMF* and set it to the value of the PLMN identity in the 'Registered AMF' received from upper layers;

4> set the *amf-Identifier* to the value received from upper layers;

3> include and set the *guami-Type* to the value provided by the upper layers;

2> if upper layers provide one or more S-NSSAI (see TS 23.003 [21]):

3> include the *s-NSSAI-List* and set the content to the values provided by the upper layers;

2> if upper layers provide onboarding request indication:

3> include the *onboardingRequest*;

2> set the *dedicatedNAS-Message* to include the information received from upper layers;

2> if connecting as an IAB-node:

3> include the *iab-NodeIndication*;

2> if connecting as an NCR-node:

3> include the *ncr-NodeIndication*;

2> if the SIB1 contains *idleModeMeasurementsNR* and the UE has NR idle/inactive measurement information concerning cells other than the PCell available in *VarMeasIdleReport*; or

2> if the SIB1 contains *idleModeMeasurementsEUTRA* and the UE has E-UTRA idle/inactive measurement information available in *VarMeasIdleReport*:

3> include the *idleMeasAvailable*;

2> if the UE has logged measurements available for NR and if the RPLMN is included in *plmn-IdentityList* stored in *VarLogMeasReport*:

3> include the *logMeasAvailable* in the *RRCSetupComplete* message;

3> if Bluetooth measurement results are included in the logged measurements the UE has available for NR:

4> include the *logMeasAvailableBT* in the *RRCSetupComplete* message;

3> if WLAN measurement results are included in the logged measurements the UE has available for NR:

4> include the *logMeasAvailableWLAN* in the *RRCSetupComplete* message;

2> if the *sigLoggedMeasType* in *VarLogMeasReport* is included:

3> if T330 timer is running and the logged measurements configuration is for NR:

4> set *sigLogMeasConfigAvailable* to *true* in the *RRCSetupComplete* message;

3> else:

4> if the UE has logged measurements available for NR:

5> set *sigLogMeasConfigAvailable* to *false* in the *RRCSetupComplete* message;

2> if the UE has connection establishment failure or connection resume failure information available in *VarConnEstFailReport* or *VarConnEstFailReportList* and if the RPLMN is equal to *plmn-Identity* stored in *VarConnEstFailReport* or in at least one of the entries of *VarConnEstFailReportList*:

3> include *connEstFailInfoAvailable* in the *RRCSetupComplete* message;

2> if the UE has radio link failure or handover failure information available in *VarRLF-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report*, or

2> if the UE has radio link failure or handover failure information available in *VarRLF-Report* of TS 36.331 [10], and if the UE is capable of cross-RAT RLF reporting and if the RPLMN is included in *plmn-IdentityList* stored in *VarRLF-Report* of TS 36.331 [10]:

3> include *rlf-InfoAvailable* in the *RRCSetupComplete* message;

2> if the UE has successful handover information available in *VarSuccessHO-Report* and if the RPLMN is included in *plmn-IdentityList* stored in *VarSuccessHO-Report*:

3> include *successHO-InfoAvailable* in the *RRCSetupComplete* message;

2> if the UE supports storage of mobility history information and the UE has mobility history information available in *VarMobilityHistoryReport*:

3> include the *mobilityHistoryAvail* in the *RRCSetupComplete* message;

2> if the UE supports uplink RRC message segmentation of *UECapabilityInformation*:

3> may include the *ul-RRC-Segmentation* in the *RRCSetupComplete* message;

2> if the *RRCSetup* is received in response to an *RRCResumeRequest*, *RRCResumeRequest1* or *RRCSetupRequest*:

3> if *speedStateReselectionPars* is configured in the *SIB2*:

4> include the *mobilityState* in the *RRCSetupComplete* message and set it to the mobility state (as specified in TS 38.304 [20]) of the UE just prior to entering RRC\_CONNECTED state;

1> submit the *RRCSetupComplete* message to lower layers for transmission, upon which the procedure ends.

NEXT CHANGE

### 5.3.5 RRC reconfiguration

#### 5.3.5.2 Initiation

The Network may initiate the RRC reconfiguration procedure to a UE in RRC\_CONNECTED. The Network applies the procedure as follows:

- the establishment of RBs (other than SRB1, that is established during RRC connection establishment) is performed only when AS security has been activated;

- the establishment of BH RLC Channels for IAB is performed only when AS security has been activated;

- the establishment of Uu Relay RLC channels and PC5 Relay RLC channels (other than SL-RLC0 and SL-RLC1) for L2 U2N Relay UE is performed only when AS security has been activated, and the establishment of PC5 Relay RLC channels for L2 U2N Remote UE (other than SL-RLC0 and SL-RLC1) is performed only when AS security has been activated;

- the addition of Secondary Cell Group and SCells is performed only when AS security has been activated;

- the *reconfigurationWithSync* is included in *secondaryCellGroup* only when at least one RLC bearer or BH RLC channel is setup in SCG;

- the *reconfigurationWithSync* is included in *masterCellGroup* only when AS security has been activated, and SRB2 with at least one DRB or multicast MRB or, for IAB and NCR, SRB2, are setup and not suspended;

- the *conditionalReconfiguration* for CPC is included only when at least one RLC bearer is setup in SCG;

- the *conditionalReconfiguration* for CHO or CPA is included only when AS security has been activated, and SRB2 with at least one DRB or multicast MRB or, for IAB, SRB2, are setup and not suspended.

#### 5.3.5.8 Reconfiguration failure

##### 5.3.5.8.2 Inability to comply with *RRCReconfiguration*

NOTE 00: The UE behaviour specified in this clause does not apply to the following, and the UE ignores, i.e. does not take an action on and does not store, the fields that it does not support or does not comprehend:

- The fields in *ServingCellConfigCommon* that are defined in Rel-16 and later.

- The fields of *searchSpaceMCCH* and s*earchSpaceMTCH* in *PDCCH-ConfigCommon* that are defined in Rel-17 and later.

The UE shall:

1> if the UE is in (NG)EN-DC:

2> if the UE is unable to comply with (part of) the configuration included in the *RRCReconfiguration* message received over SRB3;

3> if the *RRCReconfiguration* message was received as part of *ConditionalReconfiguration*:

4> continue using the configuration used prior to when the inability to comply with the *RRCReconfiguration* message was detected;

3> else:

4> continue using the configuration used prior to the reception of *RRCReconfiguration* message;

3> if MCG transmission is not suspended:

4> initiate the SCG failure information procedure as specified in clause 5.7.3 to report SCG reconfiguration error, upon which the connection reconfiguration procedure ends;

3> else:

4> initiate the connection re-establishment procedure as specified in TS 36.331 [10], clause 5.3.7, upon which the connection reconfiguration procedure ends;

2> else, if the UE is unable to comply with (part of) the configuration included in the *RRCReconfiguration* message received over SRB1;

3> if the *RRCReconfiguration* message was received as part of *ConditionalReconfiguration*:

4> continue using the configuration used prior to when the inability to comply with the *RRCReconfiguration* message was detected;

3> else:

4> continue using the configuration used prior to the reception of *RRCReconfiguration* message;

3> initiate the connection re-establishment procedure as specified in TS 36.331 [10], clause 5.3.7, upon which the connection reconfiguration procedure ends.

1> else if *RRCReconfiguration* is received via NR (i.e., NR standalone, NE-DC, or NR-DC):

2> if the UE is unable to comply with (part of) the configuration included in the *RRCReconfiguration* message received over SRB3;

NOTE 0: This case does not apply in NE-DC.

3> if the *RRCReconfiguration* message was received as part of *ConditionalReconfiguration*:

4> continue using the configuration used prior to when the inability to comply with the *RRCReconfiguration* message was detected;

3> else:

4> continue using the configuration used prior to the reception of *RRCReconfiguration* message;

3> if MCG transmission is not suspended:

4> initiate the SCG failure information procedure as specified in clause 5.7.3 to report SCG reconfiguration error, upon which the connection reconfiguration procedure ends;

3> else:

4> initiate the connection re-establishment procedure as specified in clause 5.3.7, upon which the connection reconfiguration procedure ends;

2> else if the UE is unable to comply with (part of) the configuration included in the *RRCReconfiguration* message received over the SRB1 or if the upper layers indicate that the *nas-Container* is invalid:

NOTE 0a: The compliance also covers the SCG configuration carried within octet strings e.g. field *mrdc-SecondaryCellGroupConfig*. I.e. the failure behaviour defined also applies in case the UE cannot comply with the embedded SCG configuration or with the combination of (parts of) the MCG and SCG configurations.

NOTE 0b: The compliance also covers the V2X sidelink configuration carried within an octet string, e.g. field *sl-ConfigDedicatedEUTRA*. I.e. the failure behaviour defined also applies in case the UE cannot comply with the embedded V2X sidelink configuration.

3> if the *RRCReconfiguration* message was received as part of *ConditionalReconfiguration*:

4> continue using the configuration used prior to when the inability to comply with the *RRCReconfiguration* message was detected;

3> else:

4> continue using the configuration used prior to the reception of *RRCReconfiguration* message;

3> if AS security has not been activated:

4> perform the actions upon going to RRC\_IDLE as specified in 5.3.11, with release cause 'other'

3> else if AS security has been activated but SRB2 and at least one DRB or multicast MRB or, for IAB and NCR, SRB2, have not been setup:

4> perform the actions upon going to RRC\_IDLE as specified in 5.3.11, with release cause 'RRC connection failure';

3> else:

4> initiate the connection re-establishment procedure as specified in 5.3.7, upon which the reconfiguration procedure ends;

1> else if *RRCReconfiguration* is received via other RAT (Handover to NR failure):

2> if the UE is unable to comply with any part of the configuration included in the *RRCReconfiguration* message or if the upper layers indicate that the *nas-Container* is invalid:

3> perform the actions defined for this failure case as defined in the specifications applicable for the other RAT.

NOTE 1: The UE may apply above failure handling also in case the *RRCReconfiguration* message causes a protocol error for which the generic error handling as defined in clause 10 specifies that the UE shall ignore the message.

NOTE 2: If the UE is unable to comply with part of the configuration, it does not apply any part of the configuration, i.e. there is no partial success/failure.

NOTE 3: It is up to UE implementation whether the compliance check for an *RRCReconfiguration* received as part of *ConditionalReconfiguration* is performed upon the reception of the message or upon CHO, CPA and CPC execution (when the message is required to be applied).

NEXT CHANGE

### 5.3.7 RRC connection re-establishment

#### 5.3.7.1 General

 

Figure 5.3.7.1-1: RRC connection re-establishment, successful



Figure 5.3.7.1-2: RRC re-establishment, fallback to RRC establishment, successful

The purpose of this procedure is to re-establish the RRC connection. A UE in RRC\_CONNECTED, for which AS security has been activated with SRB2 and at least one DRB/multicast MRB setup or, for IAB and NCR, SRB2, may initiate the procedure in order to continue the RRC connection. The connection re-establishment succeeds if the network is able to find and verify a valid UE context or, if the UE context cannot be retrieved, and the network responds with an *RRCSetup* according to clause 5.3.3.4.

The network applies the procedure e.g as follows:

- When AS security has been activated and the network retrieves or verifies the UE context:

- to re-activate AS security without changing algorithms;

- to re-establish and resume the SRB1;

- When UE is re-establishing an RRC connection, and the network is not able to retrieve or verify the UE context:

- to discard the stored AS Context and release all RBs and BH RLC channels and Uu Relay RLC channels;

- to fallback to establish a new RRC connection.

If AS security has not been activated, the UE shall not initiate the procedure but instead moves to RRC\_IDLE directly, with release cause 'other'. If AS security has been activated, but SRB2 and at least one DRB or multicast MRB or, for IAB and NCR, SRB2, are not setup, the UE does not initiate the procedure but instead moves to RRC\_IDLE directly, with release cause 'RRC connection failure'.

#### 5.3.7.2 Initiation

The UE initiates the procedure when one of the following conditions is met:

1> upon detecting radio link failure of the MCG and *t316* is not configured, in accordance with 5.3.10; or

1> upon detecting radio link failure of the MCG while SCG transmission is suspended, in accordance with 5.3.10; or

1> upon detecting radio link failure of the MCG while PSCell change or PSCell addition is ongoing, in accordance with 5.3.10; or

1> upon detecting radio link failure of the MCG while the SCG is deactivated, in accordance with 5.3.10; or

1> upon re-configuration with sync failure of the MCG, in accordance with clause 5.3.5.8.3; or

1> upon mobility from NR failure, in accordance with clause 5.4.3.5; or

1> upon integrity check failure indication from lower layers concerning SRB1 or SRB2, except if the integrity check failure is detected on the *RRCReestablishment* message; or

1> upon an RRC connection reconfiguration failure, in accordance with clause 5.3.5.8.2; or

1> upon detecting radio link failure for the SCG while MCG transmission is suspended, in accordance with clause 5.3.10.3 in NR-DC or in accordance with TS 36.331 [10] clause 5.3.11.3 in NE-DC; or

1> upon reconfiguration with sync failure of the SCG while MCG transmission is suspended in accordance with clause 5.3.5.8.3; or

1> upon SCG change failure while MCG transmission is suspended in accordance with TS 36.331 [10] clause 5.3.5.7a; or

1> upon SCG configuration failure while MCG transmission is suspended in accordance with clause 5.3.5.8.2 in NR-DC or in accordance with TS 36.331 [10] clause 5.3.5.5 in NE-DC; or

1> upon integrity check failure indication from SCG lower layers concerning SRB3 while MCG is suspended; or

1> upon T316 expiry, in accordance with clause 5.7.3b.5; or

1> upon detecting sidelink radio link failure by L2 U2N Remote UE in RRC\_CONNECTED, in accordance with clause 5.8.9.3; or

1> upon reception of *NotificationMessageSidelink* including *indicationType* by L2 U2N Remote UE in RRC\_CONNECTED, in accordance with clause 5.8.9.10; or

1> upon PC5 unicast link release indicated by upper layer at L2 U2N Remote UE in RRC\_CONNECTED.

NOTE 0: It is up to UE implementation whether to initiate the procedure while T346g is running.

Upon initiation of the procedure, the UE shall:

1> stop timer T310, if running;

1> stop timer T312, if running;

1> stop timer T304, if running;

1> start timer T311;

1> stop timer T316, if running;

1> if UE is not configured with *attemptCondReconfig*:

2> reset MAC;

2> release *spCellConfig*, if configured;

2> suspend all RBs, and BH RLC channels for IAB-MT, and Uu Relay RLC channels for L2 U2N Relay UE, except SRB0 and broadcast MRBs;

2> release the MCG SCell(s), if configured;

2> if MR-DC is configured:

3> perform MR-DC release, as specified in clause 5.3.5.10;

2> release *delayBudgetReportingConfig*, if configured and stop timer T342, if running;

2> release *overheatingAssistanceConfig*, if configured and stop timer T345, if running;

2> release *idc-AssistanceConfig*, if configured;

2> release *btNameList*, if configured;

2> release *wlanNameList*, if configured;

2> release *sensorNameList*, if configured;

2> release *drx-PreferenceConfig* for the MCG, if configured and stop timer T346a associated with the MCG, if running;

2> release *maxBW-PreferenceConfig* for the MCG, if configured and stop timer T346b associated with the MCG, if running;

2> release *maxCC-PreferenceConfig* for the MCG, if configured and stop timer T346c associated with the MCG, if running;

2> release *maxMIMO-LayerPreferenceConfig* for the MCG, if configured and stop timer T346d associated with the MCG, if running;

2> release *minSchedulingOffsetPreferenceConfig* for the MCG, if configured stop timer T346e associated with the MCG, if running;

2> release *rlm-RelaxationReportingConfig* for the MCG, if configured and stop timer T346j associated with the MCG, if running;

2> release *bfd-RelaxationReportingConfig* for the MCG, if configured and stop timer T346k associated with the MCG, if running;

2> release *releasePreferenceConfig*, if configured stop timer T346f, if running;

2> release *onDemandSIB-Request* if configured, and stop timer T350, if running;

2> release *referenceTimePreferenceReporting*, if configured;

2> release *sl-AssistanceConfigNR*, if configured;

2> release *obtainCommonLocation*, if configured;

2> release *musim-GapAssistanceConfig*, if configured and stop timer T346h, if running;

2> release *musim-LeaveAssistanceConfig*, if configured;

2> release*ul-GapFR2-PreferenceConfig*, if configured;

2> release *scg-DeactivationPreferenceConfig*, if configured, and stop timer T346i, if running;

2> release *propDelayDiffReportConfig*, if configured;

2> release *rrm-MeasRelaxationReportingConfig*, if configured;

2> release *maxBW-PreferenceConfigFR2-2*, if configured;

2> release *maxMIMO-LayerPreferenceConfigFR2-2*, if configured;

2> release *minSchedulingOffsetPreferenceConfigExt*, if configured;

1> release *successHO-Config*, if configured;

1> if any DAPS bearer is configured:

2> reset the source MAC and release the source MAC configuration;

2> for each DAPS bearer:

3> release the RLC entity or entities as specified in TS 38.322 [4], clause 5.1.3, and the associated logical channel for the source SpCell;

3> reconfigure the PDCP entity to release DAPS as specified in TS 38.323 [5];

2> for each SRB:

3> release the PDCP entity for the source SpCell;

3> release the RLC entity as specified in TS 38.322 [4], clause 5.1.3, and the associated logical channel for the source SpCell;

2> release the physical channel configuration for the source SpCell;

2> discard the keys used in the source SpCell (the KgNB key, the KRRCenc key, the KRRCint key, the KUPint key and the KUPenc key), if any;

1> release *sl-L2RelayUE-Config*, if configured;

1> release *sl-L2RemoteUE-Config*, if configured;

1> release the SRAP entity, if configured;

1> release *NCR-FwdConfig*, if configured;

1> if the UE is NCR-MT:

2> indicate to NCR-Fwd to cease forwarding;

1> if the UE is acting as L2 U2N Remote UE:

2> if the PC5-RRC connection with the U2N Relay UE is determined to be released:

3> indicate upper layers to trigger PC5 unicast link release;

3> perform either cell selection in accordance with the cell selection process as specified in TS 38.304 [20], or relay selection as specified in clause 5.8.15.3, or both;

2> else (i.e., maintain the PC5 RRC connection):

3> consider the connected L2 U2N Relay UE as suitable and perform actions as specified in clause 5.3.7.3a;

NOTE 1: It is up to Remote UE implementation whether to release or keep the current PC5 unicast link.

1> else:

2> if the UE is capable of L2 U2N Remote UE:

3> perform either cell selection as specified in TS 38.304 [20], or relay selection as specified in clause 5.8.15.3, or both;

2> else:

3> perform cell selection in accordance with the cell selection process as specified in TS 38.304 [20].

NOTE 2: For L2 U2N Remote UE, if both a suitable cell and a suitable relay are available, the UE can select either one based on its implementation.

### 5.3.8 RRC connection release

#### 5.3.8.1 General



Figure 5.3.8.1-1: RRC connection release, successful

The purpose of this procedure is:

- to release the RRC connection, which includes the release of the established radio bearers (except for broadcast MRBs), BH RLC channels, Uu Relay RLC channels, PC5 Relay RLC channels as well as all radio resources; or

- to suspend the RRC connection only if SRB2 and at least one DRB or multicast MRB or, for IAB and NCR, SRB2, are setup, which includes the suspension of the established radio bearers (except for broadcast MRBs).

#### 5.3.8.2 Initiation

The network initiates the RRC connection release procedure to transit a UE in RRC\_CONNECTED to RRC\_IDLE; or to transit a UE in RRC\_CONNECTED to RRC\_INACTIVE only if SRB2 and at least one DRB or multicast MRB or, for IAB and NCR, SRB2, is setup in RRC\_CONNECTED; or to transit a UE in RRC\_INACTIVE back to RRC\_INACTIVE when the UE tries to resume (for resuming a suspended RRC connection or for initiating SDT); or to transit a UE in RRC\_INACTIVE to RRC\_IDLE when the UE tries to resume (for resuming of a suspended RRC connection or for initiating SDT). The procedure can also be used to release and redirect a UE to another frequency.

#### 5.3.8.3 Reception of the *RRCRelease* by the UE

The UE shall:

1> delay the following actions defined in this clause 60 ms from the moment the *RRCRelease* message was received or optionally when lower layers indicate that the receipt of the *RRCRelease* message has been successfully acknowledged, whichever is earlier;

1> stop timer T380, if running;

1> stop timer T320, if running;

1> if timer T316 is running;

2> stop timer T316;

2> clear the information included in *VarRLF-Report,* if any;

1> stop timer T350, if running;

1> stop timer T346g, if running;

1> if theAS security is not activated:

2> ignore any field included in *RRCRelease* message except *waitTime*;

2> perform the actions upon going to RRC\_IDLE as specified in 5.3.11 with the release cause 'other' upon which the procedure ends;

1> if the *RRCRelease* message includes *redirectedCarrierInfo* indicating redirection to *eutra*:

2> if *cnType* is included:

3> after the cell selection, indicate the available CN Type(s) and the received *cnType* to upper layers;

NOTE 1: Handling the case if the E-UTRA cell selected after the redirection does not support the core network type specified by the *cnType,* is up to UE implementation.

2> if *voiceFallbackIndication* is included:

3> consider the RRC connection release was for EPS fallback for IMS voice (see TS 23.502 [43]);

1> if the *RRCRelease* message includes the *cellReselectionPriorities*:

2> store the cell reselection priority information provided by the *cellReselectionPriorities*;

2> if the *t320* is included:

3> start timer T320, with the timer value set according to the value of *t320*;

1> else:

2> apply the cell reselection priority information broadcast in the system information;

1> if *deprioritisationReq* is included and the UE supports RRC connection release with deprioritisation:

2> start or restart timer T325 with the timer value set to the *deprioritisationTimer* signalled;

2> store the *deprioritisationReq* until T325 expiry;

NOTE 1a: The UE stores the deprioritisation request irrespective of any cell reselection absolute priority assignments (by dedicated or common signalling) and regardless of RRC connections in NR or other RATs unless specified otherwise.

1> if the *RRCRelease* includes the *measIdleConfig*:

2> if T331 is running:

3> stop timer T331;

3> perform the actions as specified in 5.7.8.3;

2> if the *measIdleConfig* is set to *setup*:

3> store the received *measIdleDuration* in *VarMeasIdleConfig*;

3> start timer T331 with the value set to *measIdleDuration*;

3> if the *measIdleConfig* contains *measIdleCarrierListNR*:

4> store the received *measIdleCarrierListNR* in *VarMeasIdleConfig*;

3> if the *measIdleConfig* contains *measIdleCarrierListEUTRA*:

4> store the received *measIdleCarrierListEUTRA* in *VarMeasIdleConfig*;

3> if the *measIdleConfig* contains *validityAreaList*:

4> store the received *validityAreaList* in *VarMeasIdleConfig*;

1> if the *RRCRelease* includes *suspendConfig*:

2> reset MAC and release the default MAC Cell Group configuration, if any;

2> apply the received *suspendConfig* except the received *nextHopChainingCount*;

2> if the *sdt-Config* is configured:

3> for each of the DRB in the *sdt-DRB-List*:

4> consider the DRB to be configured for SDT;

3> if *sdt-SRB2-Indication* is configured:

4> consider the SRB2 to be configured for SDT;

3> for each RLC bearer (except those associated with broadcast MRBs) that is not suspended:

4> re-establish the RLC entity as specified in TS 38.322 [4];

3> for SRB2 (if it is resumed) and for SRB1:

4> trigger the PDCP entity to perform SDU discard as specified in TS 38.323 [5];

3> if *sdt-MAC-PHY-CG-Config* is configured:

4> configure the PCell with the configured grant resources for SDT and instruct the MAC entity to start the *cg-SDT-TimeAlignmentTimer*;

2> if *srs-PosRRC-Inactive* is configured:

3> apply the configuration and instruct MAC to start the *inactivePosSRS-TimeAlignmentTimer*;

NOTE 1b: The Network should provide full configuration to UE for SRS for Positioning in RRC\_INACTIVE.

2> remove all the entries within the MCG and the SCG *VarConditionalReconfig*, if any;

2> for each *measId* of the MCG *measConfig* and for each *measId* of the SCG *measConfig*, if configured, if the associated *reportConfig* has a *reportType* set to *condTriggerConfig*:

3> for the associated *reportConfigId*:

4> remove the entry with the matching *reportConfigId* from the *reportConfigList* within the *VarMeasConfig*;

3> if the associated *measObjectId* is only associated to a *reportConfig* with *reportType* set to *condTriggerConfig*:

4> remove the entry with the matching *measObjectId* from the *measObjectList* within the *VarMeasConfig*;

3> remove the entry with the matching *measId* from the *measIdList* within the *VarMeasConfig*;

2> if the UE is NCR-MT and the *NCR-FwdConfig* was configured and not removed before *RRCRelease*:

3> if the *NCR-FwdConfig* includes the periodic forwarding resource configuration:

4> NCR-Fwd shall continue forwarding in accordance with the received periodic forwarding resource set(s);

3> if the *NCR-FwdConfig* includes the semi-persistent forwarding resource configuration that has been activated by the network:

4> NCR-Fwd shall continue forwarding in accordance with the activated semi-persistent forwarding resource set;

2> if the UE is acting as L2 U2N Remote UE:

3> if the PC5-RRC connection with the U2N Relay UE is determined to be released:

4> indicate upper layers to trigger PC5 unicast link release;

3> else (i.e., maintain the PC5 RRC connection):

4> establish or re-establish (e.g. via release and add) SL RLC entity for SRB1;

2> else:

3> re-establish RLC entities for SRB1;

2> if the *RRCRelease* message with *suspendConfig* was received in response to an *RRCResumeRequest* or an *RRCResumeRequest1*:

3> stop the timer T319 if running;

3> in the stored UE Inactive AS context:

4> replace the KgNB and KRRCint keys with the current KgNB and KRRCint keys;

4> replace the *nextHopChainingCount* with the value of *nextHopChainingCount* received in the *RRCRelease* message*;*

4> replace the *cellIdentity* with the *cellIdentity* of the cell the UE has received the *RRCRelease* message;

4> if the *suspendConfig* contains the *sl-UEIdentityRemote* (i.e. the UE is a L2 U2N Remote UE):

5> replace the C-RNTI with the value of the *sl-UEIdentityRemote*;

5> replace the physical cell identitywith the value of the *sl-PhysCellId* in *sl-ServingCellInfo* contained in the discovery message received from the connected L2 U2N Relay UE;

4> else:

5> replace the C-RNTI with the C-RNTI used in the cell (see TS 38.321 [3]) the UE has received the *RRCRelease* message;

5> replace the physical cell identitywith the physical cell identity of the cell the UE has received the *RRCRelease* message;

3> replace the *nextHopChainingCount* with the value associated with the current KgNB;

3> stop the timer T319a if running and consider SDT procedure is not ongoing;

2> else:

3> store in the UE Inactive AS Context the *nextHopChainingCount* received in the *RRCRelease* message*,* the current KgNB and KRRCint keys, the ROHC state, the EHC context(s), the UDC state, the stored QoS flow to DRB mapping rules, the application layer measurement configuration, the C-RNTI used in the source PCell, the *cellIdentity* and the physical cell identity of the source PCell, the *NCR-FwdConfig* (if configured), the *spCellConfigCommon* within *ReconfigurationWithSync* of the NR PSCell (if configured) and all other parameters configured except for:

- parameters within *ReconfigurationWithSync* of the PCell;

- parameters within *ReconfigurationWithSync* of the NR PSCell, if configured;

- parameters within *MobilityControlInfoSCG* of the E-UTRA PSCell, if configured;

- *servingCellConfigCommonSIB*;

- *sl-L2RelayUE-Config*, if configured;

- *sl-L2RemoteUE-Config*, if configured;

NOTE 1c: *suspendConfig* is not stored as part of UE Inactive AS Context, except for the fields explicitly specified.

3> store any previously or subsequently received application layer measurement reports for which no segment, or full message, has been submitted to lower layers for transmission;

NOTE 2: NR sidelink communication/discovery related configurations and logged measurement configuration are not stored as UE Inactive AS Context, when UE enters RRC\_INACTIVE.

2> suspend all SRB(s) and DRB(s) and multicast MRB(s), except SRB0 and broadcast MRBs;

2> indicate PDCP suspend to lower layers of all DRBs and multicast MRBs;

2> release the SRAP entity, if configured;

2> if the *t380* is included:

3> start timer T380, with the timer value set to *t380*;

2> if the *RRCRelease* message is including the *waitTime*:

3> start timer T302 with the value set to the *waitTime*;

3> inform upper layers that access barring is applicable for all access categories except categories '0' and '2';

2> if T390 is running:

3> stop timer T390 for all access categories;

3> perform the actions as specified in 5.3.14.4;

2> indicate the suspension of the RRC connection to upper layers;

2> if the UE is capable of L2 U2N Remote UE:

3> enter RRC\_INACTIVE, and perform either cell selection as specified in TS 38.304 [20], or relay selection as specified in clause 5.8.15.3, or both;

2> else:

3> enter RRC\_INACTIVE and perform cell selection as specified in TS 38.304 [20];

1> else:

2> perform the actions upon going to RRC\_IDLE as specified in 5.3.11, with the release cause 'other'.

NOTE 3: Whether to release the PC5 unicast link is left to L2 U2N Remote UE's implementation.

NOTE 4: It is left to UE implementation whether to stop T430, if running, when going to RRC\_INACTIVE.

### 5.3.10 Radio link failure related actions

#### 5.3.10.3 Detection of radio link failure

The UE shall:

1> if any DAPS bearer is configured and T304 is running:

2> upon T310 expiry in source SpCell; or

2> upon random access problem indication from source MCG MAC; or

2> upon indication from source MCG RLC that the maximum number of retransmissions has been reached; or

2> upon consistent uplink LBT failure indication from source MCG MAC:

3> consider radio link failure to be detected for the source MCG i.e. source RLF;

3> suspend the transmission and reception of all DRBs and multicast MRBs in the source MCG;

3> reset MAC for the source MCG;

3> release the source connection.

1> else:

2> during a DAPS handover: the following only applies for the target PCell;

2> upon T310 expiry in PCell; or

2> upon T312 expiry in PCell; or

2> upon random access problem indication from MCG MAC while neither T300, T301, T304, T311 nor T319 are running and SDT procedure is not ongoing; or

2> upon indication from MCG RLC that the maximum number of retransmissions has been reached while SDT procedure is not ongoing; or

2> if connected as an IAB-node, upon BH RLF indication received on BAP entity from the MCG; or

2> upon consistent uplink LBT failure indication from MCG MAC while T304 is not running:

3> if the indication is from MCG RLC and CA duplication is configured and activated for MCG, and for the corresponding logical channel *allowedServingCells* only includes SCell(s):

4> initiate the failure information procedure as specified in 5.7.5 to report RLC failure.

3> else:

4> consider radio link failure to be detected for the MCG, i.e. MCG RLF;

4> discard any segments of segmented RRC messages stored according to 5.7.6.3;

NOTE: Void.

4> if AS security has not been activated:

5> perform the actions upon going to RRC\_IDLE as specified in 5.3.11, with release cause 'other';-

4> else if AS security has been activated but SRB2 and at least one DRB or multicast MRB or, for IAB and NCR, SRB2, have not been setup:

5> store the radio link failure information in the *VarRLF-Report* as described in clause 5.3.10.5;

5> perform the actions upon going to RRC\_IDLE as specified in 5.3.11, with release cause 'RRC connection failure';

4> else:

5> store the radio link failure information in the *VarRLF-Report* as described in clause 5.3.10.5;

5> if T316 is configured; and

5> if SCG transmission is not suspended; and

5> if the SCG is not deactivated; and

5> if neither PSCell change nor PSCell addition is ongoing (i.e. timer T304 for the NR PSCell is not running in case of NR-DC or timer T307 of the E-UTRA PSCell is not running as specified in TS 36.331 [10], clause 5.3.10.10, in NE-DC):

6> initiate the MCG failure information procedure as specified in 5.7.3b to report MCG radio link failure.

5> else:

6> initiate the connection re-establishment procedure as specified in 5.3.7.

A L2/L3 U2N Relay UE shall:

1> upon detecting radio link failure:

2> it either indicates to upper layers (to trigger PC5 unicast link release) or sends Notification message to the connected L2/L3 U2N Remote UE(s) in accordance with 5.8.9.10.

The UE shall:

1> upon T310 expiry in PSCell; or

1> upon T312 expiry in PSCell; or

1> upon random access problem indication from SCG MAC; or

1> upon indication from SCG RLC that the maximum number of retransmissions has been reached; or

1> if connected as an IAB-node, upon BH RLF indication received on BAP entity from the SCG; or

1> upon consistent uplink LBT failure indication from SCG MAC:

2> if the indication is from SCG RLC and CA duplication is configured and activated for SCG, and for the corresponding logical channel *allowedServingCells* only includes SCell(s):

3> initiate the failure information procedure as specified in 5.7.5 to report RLC failure.

2> else:

3> consider radio link failure to be detected for the SCG, i.e. SCG RLF;

3> if the SCG is deactivated:

4> stop radio link monitoring on the SCG;

4> indicate to lower layers to stop beam failure detection on the PSCell;

3> if MCG transmission is not suspended:

4> initiate the SCG failure information procedure as specified in 5.7.3 to report SCG radio link failure.

3> else:

4> if the UE is in NR-DC:

5> initiate the connection re-establishment procedure as specified in 5.3.7;

4> else (the UE is in (NG)EN-DC):

5> initiate the connection re-establishment procedure as specified in TS 36.331 [10], clause 5.3.7;

NEXT CHANGE

### 5.3.11 UE actions upon going to RRC\_IDLE

The UE shall:

1> if the UE is NCR-MT:

2> indicate to NCR-Fwd to cease forwarding;

1> reset MAC;

1> set the variable *pendingRNA-Update* to *false*, if that is set to *true*;

1> if going to RRC\_IDLE was triggered by reception of the *RRCRelease* message including a *waitTime*:

2> if T302 is running:

3> stop timer T302;

2> start timer T302 with the value set to the *waitTime*;

2> inform upper layers that access barring is applicable for all access categories except categories '0' and '2'.

1> else:

2> if T302 is running:

3> stop timer T302;

3> perform the actions as specified in 5.3.14.4;

1> if T390 is running:

2> stop timer T390 for all access categories;

2> perform the actions as specified in 5.3.14.4;

1> if the UE is leaving RRC\_INACTIVE:

2> if going to RRC\_IDLE was not triggered by reception of the *RRCRelease message*:

3> if stored, discard the cell reselection priority information provided by the *cellReselectionPriorities*;

3> stop the timer T320, if running;

2> if T319a is running:

3> stop timer T319a;

3> consider SDT procedure is not ongoing;

1> stop all timers that are running except T302, T320, T325, T330, T331, T400 and T430;

1> discard the UE Inactive AS context, if any;

1> release the *suspendConfig*, if configured;

1> remove all the entries within the MCG and the SCG *VarConditionalReconfig*, if any;

1> for each *measId*, if the associated *reportConfig* has a *reportType* set to *condTriggerConfig*:

2> for the associated *reportConfigId*:

3> remove the entry with the matching *reportConfigId* from the *reportConfigList* within the *VarMeasConfig*;

2> if the associated *measObjectId* is only associated to a *reportConfig* with *reportType* set to *condTriggerConfig*:

3> remove the entry with the matching *measObjectId* from the *measObjectList* within the *VarMeasConfig*;

2> remove the entry with the matching *measId* from the *measIdList* within the *VarMeasConfig*;

1> discard the KgNB key, the S-KgNB key, the S-KeNB key, the KRRCenc key, the KRRCint key, the KUPint key and the KUPenc key, if any;

1> release all radio resources, including release of the RLC entity, the BAP entity, the MAC configuration and the associated PDCP entity and SDAP for all established RBs (except for broadcast MRBs), BH RLC channels, Uu Relay RLC channels, PC5 Relay RLC channels and SRAP entity;

1> indicate the release of the RRC connection to upper layers together with the release cause;

1> inform upper layers about the release of all application layer measurement configurations;

1> discard any application layer measurement reports which were not yet submitted to lower layers for transmission;

1> discard any segments of segmented RRC messages stored according to 5.7.6.3;

1> except if going to RRC\_IDLE was triggered by inter-RAT cell reselection while the UE is in RRC\_INACTIVE or RRC\_IDLE or when selecting an inter-RAT cell while T311 was running or when selecting an E-UTRA cell for EPS fallback for IMS voice as specified in 5.4.3.5:

2> if the UE is capable of L2 U2N Remote UE:

3> enter RRC\_IDLE, and perform either cell selection as specified in TS 38.304 [20], or relay selection as specified in clause 5.8.15.3, or both;

2> else:

3> enter RRC\_IDLE and perform cell selection as specified in TS 38.304 [20];

NOTE 1: Whether to release the PC5 unicast link is left to L2 U2N Remote UE's implementation.

NOTE 2: It is left to UE implementation whether to stop T430, if running, when going to RRC\_IDLE.

NEXT CHANGE

### 5.3.14 Unified Access Control

#### 5.3.14.1 General

The purpose of this procedure is to perform access barring check for an access attempt associated with a given Access Category and one or more Access Identities upon request from upper layers according to TS 24.501 [23] or the RRC layer. This procedure does not apply to IAB-MT and NCR-MT. This procedure does not apply to L2 U2N Relay UE initiating RRC connection establishment or RRC connection resume upon reception of any message from a L2 U2N remote UE via SL-RLC0 or SL-RLC1 in accordance to 5.3.3.1a or 5.3.13.1a.

After a PCell change in RRC\_CONNECTED the UE shall defer access barring checks until it has obtained *SIB1* (as specified in 5.2.2.2) from the target cell.

NEXT CHANGE

# 6 Protocol data units, formats and parameters (ASN.1)

## 6.2 RRC messages

### 6.2.2 Message definitions

#### – *MIB*

The *MIB* includes the system information transmitted on BCH.

Signalling radio bearer: N/A

RLC-SAP: TM

Logical channel: BCCH

Direction: Network to UE

*MIB*

-- ASN1START

-- TAG-MIB-START

MIB ::= SEQUENCE {

 systemFrameNumber BIT STRING (SIZE (6)),

 subCarrierSpacingCommon ENUMERATED {scs15or60, scs30or120},

 ssb-SubcarrierOffset INTEGER (0..15),

 dmrs-TypeA-Position ENUMERATED {pos2, pos3},

 pdcch-ConfigSIB1 PDCCH-ConfigSIB1,

 cellBarred ENUMERATED {barred, notBarred},

 intraFreqReselection ENUMERATED {allowed, notAllowed},

 spare BIT STRING (SIZE (1))

}

-- TAG-MIB-STOP

-- ASN1STOP

|  |
| --- |
| *MIB* field descriptions |
| ***cellBarred***Value *barred* means that the cell is barred, as defined in TS 38.304 [20]. This field is ignored by IAB-MT and NCR-MT. This field is ignored for connectivity to NTN. |
| ***dmrs-TypeA-Position***Position of (first) DM-RS for downlink (see TS 38.211 [16], clause 7.4.1.1.2) and uplink (see TS 38.211 [16], clause 6.4.1.1.3). |
| ***intraFreqReselection***Controls cell selection/reselection to intra-frequency cells when the highest ranked cell is barred, or treated as barred by the UE, as specified in TS 38.304 [20]. This field is ignored by IAB-MT and NCR-MT. |
| ***pdcch-ConfigSIB1***Determines a common *ControlResourceSet* (CORESET), a common search space and necessary PDCCH parameters. If the field *ssb-SubcarrierOffset* indicates that *SIB1* is absent, the field *pdcch-ConfigSIB1* indicates the frequency positions where the UE may find SS/PBCH block with *SIB1* or the frequency range where the network does not provide SS/PBCH block with *SIB1* (see TS 38.213 [13], clause 13). |
| ***ssb-SubcarrierOffset***Corresponds to kSSB (see TS 38.213 [13]), which is the frequency domain offset between SSB and the overall resource block grid in number of subcarriers. (See TS 38.211 [16], clause 7.4.3.1). For operation with shared spectrum channel access in FR1 (see 37.213 [48]), this field corresponds to $\overbar{k}\_{SSB}$, and kSSB is obtained from $\overbar{k}\_{SSB}$ (see TS 38.211 [16], clause 7.4.3.1); the LSB of this field is used also for deriving the QCL relation between SS/PBCH blocks as specified in TS 38.213 [13], clause 4.1.The value range of this field may be extended by an additional most significant bit encoded within PBCH as specified in TS 38.213 [13].This field may indicate that this cell does not provide *SIB1* and that there is hence no CORESET#0 configured in *MIB* (see TS 38.213 [13], clause 13). In this case, the field *pdcch-ConfigSIB1* may indicate the frequency positions where the UE may (not) find a SS/PBCH with a control resource set and search space for *SIB1* (see TS 38.213 [13], clause 13). |
| ***subCarrierSpacingCommon***Subcarrier spacing for *SIB1*, Msg.2/4 and MsgB for initial access, paging and broadcast SI-messages. If the UE acquires this *MIB* on an FR1 carrier frequency, the value *scs15or60* corresponds to 15 kHz and the value *scs30or120* corresponds to 30 kHz. If the UE acquires this *MIB* on an FR2 carrier frequency, the value *scs15or60* corresponds to 60 kHz and the value *scs30or120* corresponds to 120 kHz. For operation with shared spectrum channel access in FR1 (see 37.213 [48]) and for operation in FR2-2, the subcarrier spacing for *SIB1*, Msg.2/4 and MsgB for initial access, paging and broadcast SI-messages is same as that for the corresponding SSB. For operation with shared spectrum channel access, this field instead is used for deriving the QCL relation between SS/PBCH blocks as specified in TS 38.213 [13], clause 4.1. |
| ***systemFrameNumber***The 6 most significant bits (MSB) of the 10-bit System Frame Number (SFN). The 4 LSB of the SFN are conveyed in the PBCH transport block as part of channel coding (i.e. outside the *MIB* encoding), as defined in clause 7.1 in TS 38.212 [17]. |

NEXT CHANGE

#### – *RRCSetupComplete*

The *RRCSetupComplete* message is used to confirm the successful completion of an RRC connection establishment.

Signalling radio bearer: SRB1

RLC-SAP: AM

Logical channel: DCCH

Direction: UE to Network

*RRCSetupComplete* message

-- ASN1START

-- TAG-RRCSETUPCOMPLETE-START

RRCSetupComplete ::= SEQUENCE {

 rrc-TransactionIdentifier RRC-TransactionIdentifier,

 criticalExtensions CHOICE {

 rrcSetupComplete RRCSetupComplete-IEs,

 criticalExtensionsFuture SEQUENCE {}

 }

}

RRCSetupComplete-IEs ::= SEQUENCE {

 selectedPLMN-Identity INTEGER (1..maxPLMN),

 registeredAMF RegisteredAMF OPTIONAL,

 guami-Type ENUMERATED {native, mapped} OPTIONAL,

 s-NSSAI-List SEQUENCE (SIZE (1..maxNrofS-NSSAI)) OF S-NSSAI OPTIONAL,

 dedicatedNAS-Message DedicatedNAS-Message,

 ng-5G-S-TMSI-Value CHOICE {

 ng-5G-S-TMSI NG-5G-S-TMSI,

 ng-5G-S-TMSI-Part2 BIT STRING (SIZE (9))

 } OPTIONAL,

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension RRCSetupComplete-v1610-IEs OPTIONAL

}

RRCSetupComplete-v1610-IEs ::= SEQUENCE {

 iab-NodeIndication-r16 ENUMERATED {true} OPTIONAL,

 idleMeasAvailable-r16 ENUMERATED {true} OPTIONAL,

 ue-MeasurementsAvailable-r16 UE-MeasurementsAvailable-r16 OPTIONAL,

 mobilityHistoryAvail-r16 ENUMERATED {true} OPTIONAL,

 mobilityState-r16 ENUMERATED {normal, medium, high, spare} OPTIONAL,

 nonCriticalExtension RRCSetupComplete-v1690-IEs OPTIONAL

}

RRCSetupComplete-v1690-IEs ::= SEQUENCE {

 ul-RRC-Segmentation-r16 ENUMERATED {true} OPTIONAL,

 nonCriticalExtension RRCSetupComplete-v1700-IEs OPTIONAL

}

RRCSetupComplete-v1700-IEs ::= SEQUENCE {

 onboardingRequest-r17 ENUMERATED {true} OPTIONAL,

 nonCriticalExtension RRCSetupComplete-v18xy-IEs OPTIONAL

}

RRCSetupComplete-v18xy-IEs ::= SEQUENCE {

 ncr-NodeIndication-r18 ENUMERATED {true} OPTIONAL,

 nonCriticalExtension SEQUENCE{} OPTIONAL

}

RegisteredAMF ::= SEQUENCE {

 plmn-Identity PLMN-Identity OPTIONAL,

 amf-Identifier AMF-Identifier

}

-- TAG-RRCSETUPCOMPLETE-STOP

-- ASN1STOP

|  |
| --- |
| *RRCSetupComplete-IEs* field descriptions |
| ***guami-Type***This field is used to indicate whether the GUAMI included is native (derived from native 5G-GUTI) or mapped (from EPS, derived from EPS GUTI) as specified in TS 24.501 [23]. |
| ***iab-NodeIndication***This field is used to indicate that the connection is being established by an IAB-node as specified in TS 38.300 [2]. |
| ***ncr-NodeIndication***This field is used to indicate that the connection is being established by an NCR-node as specified in TS 38.300 [2]. |
| ***idleMeasAvailable***Indication that the UE has idle/inactive measurement report available. |
| ***mobilityState***This field indicates the UE mobility state (as defined in TS 38.304 [20], clause 5.2.4.3) just prior to UE going into RRC\_CONNECTED state. The UE indicates the value of *medium* and *high* when being in Medium-mobility and High-mobility states respectively. Otherwise the UE indicates the value *normal*. |
| ***ng-5G-S-TMSI-Part2***The leftmost 9 bits of 5G-S-TMSI. |
| ***onboardingRequest***This field indicates that the connection is being established for UE onboarding in the selected onboarding SNPN, see TS 23.501 [32]. |
| ***registeredAMF***This field is used to transfer the GUAMI of the AMF where the UE is registered, as provided by upper layers, see TS 23.003 [21]. |
| ***selectedPLMN-Identity***Index of the PLMN or SNPN selected by the UE from the *plmn-IdentityInfoList* or *npn-IdentityInfoList* fields included in SIB1. |
| ***ul-RRC-Segmentation***This field indicates the UE supports uplink RRC segmentation of *UECapabilityInformation.* |

NEXT CHANGE

#### – *SIB1*

*SIB1* contains information relevant when evaluating if a UE is allowed to access a cell and defines the scheduling of other system information.It also contains radio resource configuration information that is common for all UEs and barring information applied to the unified access control.

Signalling radio bearer: N/A

RLC-SAP: TM

Logical channels: BCCH

Direction: Network to UE

*SIB1* message

-- ASN1START

-- TAG-SIB1-START

SIB1 ::= SEQUENCE {

 cellSelectionInfo SEQUENCE {

 q-RxLevMin Q-RxLevMin,

 q-RxLevMinOffset INTEGER (1..8) OPTIONAL, -- Need S

 q-RxLevMinSUL Q-RxLevMin OPTIONAL, -- Need R

 q-QualMin Q-QualMin OPTIONAL, -- Need S

 q-QualMinOffset INTEGER (1..8) OPTIONAL -- Need S

 } OPTIONAL, -- Cond Standalone

 cellAccessRelatedInfo CellAccessRelatedInfo,

 connEstFailureControl ConnEstFailureControl OPTIONAL, -- Need R

 si-SchedulingInfo SI-SchedulingInfo OPTIONAL, -- Need R

 servingCellConfigCommon ServingCellConfigCommonSIB OPTIONAL, -- Need R

 ims-EmergencySupport ENUMERATED {true} OPTIONAL, -- Need R

 eCallOverIMS-Support ENUMERATED {true} OPTIONAL, -- Need R

 ue-TimersAndConstants UE-TimersAndConstants OPTIONAL, -- Need R

 uac-BarringInfo SEQUENCE {

 uac-BarringForCommon UAC-BarringPerCatList OPTIONAL, -- Need S

 uac-BarringPerPLMN-List UAC-BarringPerPLMN-List OPTIONAL, -- Need S

 uac-BarringInfoSetList UAC-BarringInfoSetList,

 uac-AccessCategory1-SelectionAssistanceInfo CHOICE {

 plmnCommon UAC-AccessCategory1-SelectionAssistanceInfo,

 individualPLMNList SEQUENCE (SIZE (2..maxPLMN)) OF UAC-AccessCategory1-SelectionAssistanceInfo

 } OPTIONAL -- Need S

 } OPTIONAL, -- Need R

 useFullResumeID ENUMERATED {true} OPTIONAL, -- Need R

 lateNonCriticalExtension OCTET STRING OPTIONAL,

 nonCriticalExtension SIB1-v1610-IEs OPTIONAL

}

SIB1-v1610-IEs ::= SEQUENCE {

 idleModeMeasurementsEUTRA-r16 ENUMERATED{true} OPTIONAL, -- Need R

 idleModeMeasurementsNR-r16 ENUMERATED{true} OPTIONAL, -- Need R

 posSI-SchedulingInfo-r16 PosSI-SchedulingInfo-r16 OPTIONAL, -- Need R

 nonCriticalExtension SIB1-v1630-IEs OPTIONAL

}

SIB1-v1630-IEs ::= SEQUENCE {

 uac-BarringInfo-v1630 SEQUENCE {

 uac-AC1-SelectAssistInfo-r16 SEQUENCE (SIZE (2..maxPLMN)) OF UAC-AC1-SelectAssistInfo-r16

 } OPTIONAL, -- Need R

 nonCriticalExtension SIB1-v1700-IEs OPTIONAL

}

SIB1-v1700-IEs ::= SEQUENCE {

 hsdn-Cell-r17 ENUMERATED {true} OPTIONAL, -- Need R

 uac-BarringInfo-v1700 SEQUENCE {

 uac-BarringInfoSetList-v1700 UAC-BarringInfoSetList-v1700

 } OPTIONAL, -- Cond MINT

 sdt-ConfigCommon-r17 SDT-ConfigCommonSIB-r17 OPTIONAL, -- Need R

 redCap-ConfigCommon-r17 RedCap-ConfigCommonSIB-r17 OPTIONAL, -- Need R

 featurePriorities-r17 SEQUENCE {

 redCapPriority-r17 FeaturePriority-r17 OPTIONAL, -- Need R

 slicingPriority-r17 FeaturePriority-r17 OPTIONAL, -- Need R

 msg3-Repetitions-Priority-r17 FeaturePriority-r17 OPTIONAL, -- Need R

 sdt-Priority-r17 FeaturePriority-r17 OPTIONAL -- Need R

 } OPTIONAL, -- Need R

 si-SchedulingInfo-v1700 SI-SchedulingInfo-v1700 OPTIONAL, -- Need R

 hyperSFN-r17 BIT STRING (SIZE (10)) OPTIONAL, -- Need R

 eDRX-AllowedIdle-r17 ENUMERATED {true} OPTIONAL, -- Need R

 eDRX-AllowedInactive-r17 ENUMERATED {true} OPTIONAL, -- Cond EDRX-RC

 intraFreqReselectionRedCap-r17 ENUMERATED {allowed, notAllowed} OPTIONAL, -- Need S

 cellBarredNTN-r17 ENUMERATED {barred, notBarred} OPTIONAL, -- Need S

 nonCriticalExtension SIB1-v1740-IEs OPTIONAL

}

SIB1-v1740-IEs ::= SEQUENCE {

 si-SchedulingInfo-v1740 SI-SchedulingInfo-v1740 OPTIONAL, -- Need R

 nonCriticalExtension SIB1-v1800-IEs OPTIONAL

}

SIB1-v1800-IEs ::= SEQUENCE {

 ncr-Support-r18 ENUMERATED {true} OPTIONAL, -- Need S

 nonCriticalExtension SEQUENCE {}

}

UAC-AccessCategory1-SelectionAssistanceInfo ::= ENUMERATED {a, b, c}

UAC-AC1-SelectAssistInfo-r16 ::= ENUMERATED {a, b, c, notConfigured}

SDT-ConfigCommonSIB-r17 ::= SEQUENCE {

 sdt-RSRP-Threshold-r17 RSRP-Range OPTIONAL, -- Need R

 sdt-LogicalChannelSR-DelayTimer-r17 ENUMERATED { sf20, sf40, sf64, sf128, sf512, sf1024, sf2560, spare1} OPTIONAL, -- Need R

 sdt-DataVolumeThreshold-r17 ENUMERATED {byte32, byte100, byte200, byte400, byte600, byte800, byte1000, byte2000, byte4000,

 byte8000, byte9000, byte10000, byte12000, byte24000, byte48000, byte96000},

 t319a-r17 ENUMERATED { ms100, ms200, ms300, ms400, ms600, ms1000, ms2000,

 ms3000, ms4000, spare7, spare6, spare5, spare4, spare3, spare2, spare1}

}

RedCap-ConfigCommonSIB-r17 ::= SEQUENCE {

 halfDuplexRedCapAllowed-r17 ENUMERATED {true} OPTIONAL, -- Need R

 cellBarredRedCap-r17 SEQUENCE {

 cellBarredRedCap1Rx-r17 ENUMERATED {barred, notBarred},

 cellBarredRedCap2Rx-r17 ENUMERATED {barred, notBarred}

 } OPTIONAL, -- Need R

 ...

}

FeaturePriority-r17 ::= INTEGER (0..7)

-- TAG-SIB1-STOP

-- ASN1STOP

|  |
| --- |
| *SIB1* field descriptions |
| ***cellBarredNTN***Value *barred* means that the cell is barred for connectivity to NTN, as defined in TS 38.304 [20]. Value *notBarred* means that the cell is allowed for connectivity to NTN. If not present, the UE considers the cell is not allowed for connectivity to NTN, as defined in TS 38.304 [20]. This field is only applicable to NTN-capable UEs. |
| ***cellBarredRedCap1Rx***Value *barred* means that the cell is barred for a RedCap UE with 1 Rx branch, as defined in TS 38.304 [20]. This field is ignored by non-RedCap UEs. |
| ***cellBarredRedCap2Rx***Value *barred* means that the cell is barred for a RedCap UE with 2 Rx branches, as defined in TS 38.304 [20]. This field is ignored by non-RedCap UEs. |
| ***cellSelectionInfo***Parameters for cell selection related to the serving cell. |
| ***eCallOverIMS-Support***Indicates whether the cell supports eCall over IMS services as defined in TS 23.501 [32]. If absent, eCall over IMS is not supported by the network in the cell. |
| ***eDRX-AllowedIdle***The presence of this field indicates that extended DRX for CN paging is allowed in the cell for UEs in RRC\_IDLE or RRC\_INACTIVE. The UE shall stop using extended DRX for CN paging in RRC\_IDLE or RRC\_INACTIVE if *eDRX-AllowedIdle* is not present. |
| ***eDRX-AllowedInactive***The presence of this field indicates that extended DRX for RAN paging is allowed in the cell for UEs in RRC\_INACTIVE. The UE shall stop using extended DRX for RAN paging in RRC\_INACTIVE if *eDRX-AllowedInactive* is not present. |
| ***featurePriorities***Indicates priorities for features, such as RedCap, Slicing, SDT and MSG3-Repetitions for Coverage Enhancements. These priorities are used to determine which *FeatureCombinationPreambles* the UE shall use when a feature maps to more than one *FeatureCombinationPreambles*, as specified in TS 38.321 [3]. A lower value means a higher priority. The network does not signal the same priority for more than one feature. The network signals a priority for all feature that map to at least one *FeatureCombinationPreambles*. |
| ***halfDuplexRedCap-Allowed***The presence of this field indicates that the cell supports half-duplex FDD RedCap UEs. |
| ***hsdn-Cell***This field indicates this is a HSDN cell as specified in TS 38.304 [20]. |
| ***hyperSFN***Indicates hyper SFN which increments by one when the SFN wraps around. This field is excluded when determining changes in system information, i.e. changes of hyper SFN should not result in system information change notifications. |
| ***idleModeMeasurementsEUTRA***This field indicates that a UE that is configured for EUTRA idle/inactive measurements shall perform the measurements while camping in this cell and report availability of these measurements when establishing or resuming a connection in this cell. If absent, a UE is not required to perform EUTRA idle/inactive measurements. |
| ***idleModeMeasurementsNR***This field indicates that a UE that is configured for NR idle/inactive measurements shall perform the measurements while camping in this cell and report availability of these measurements when establishing or resuming a connection in this cell. If absent, a UE is not required to perform NR idle/inactive measurements. |
| ***ims-EmergencySupport***Indicates whether the cell supports IMS emergency bearer services for UEs in limited service mode. If absent, IMS emergency call is not supported by the network in the cell for UEs in limited service mode. |
| ***intraFreqReselectionRedCap***Controls cell selection/reselection to intra-frequency cells for RedCap UEs when this cell is barred, or treated as barred by the RedCap UE, as specified in TS 38.304 [20]. If not present, a RedCap UE treats the cell as barred, i.e.,the UE considers that the cell does not support RedCap. |
| ***ncr-Support***This field combines both the support of NCR and the cell status for NCR. If the field is present, the cell supports NCR and the cell is also considered as a candidate for cell (re)selection for NCR-node; if the field is absent, the cell does not support NCR and/or the cell is barred for NCR-node. |
| ***q-QualMin***Parameter "Qqualmin" in TS 38.304 [20], applicable for serving cell. If the field is absent, the UE applies the (default) value of negative infinity for Qqualmin.  |
| ***q-QualMinOffset***Parameter "Qqualminoffset" in TS 38.304 [20]. Actual value Qqualminoffset = field value [dB]. If the field is absent, the UE applies the (default) value of 0 dB for Qqualminoffset.Affects the minimum required quality level in the cell. |
| ***q-RxLevMin***Parameter "Qrxlevmin" in TS 38.304 [20], applicable for serving cell. |
| ***q-RxLevMinOffset***Parameter "Qrxlevminoffset" in TS 38.304 [20]. Actual value Qrxlevminoffset = field value \* 2 [dB]. If absent, the UE applies the (default) value of 0 dB for Qrxlevminoffset*.* Affects the minimum required Rx level in the cell. |
| ***q-RxLevMinSUL***Parameter "Qrxlevmin" in TS 38.304 [20], applicable for serving cell. |
| ***sdt-RSRP-Threshold***RSRP threshold used to determine whether SDT procedure can be initiated, as specified in TS 38.321 [3]. |
| ***sdt-DataVolumeThreshold***Data volume threshold used to determine whether SDT can be initiated, as specified in TS 38.321 [3]. Value *byte32* corresponds to 32 bytes, value *byte100* corresponds to 100 bytes, and so on. |
| ***sdt-LogicalChannelSR-DelayTimer***The value of *logicalChannelSR-DelayTimer* applied during SDT for logical channels configured with SDT, as specified in TS 38.321 [3]. Value in number of subframes. Value *sf20* corresponds to 20 subframes, *sf40* corresponds to 40 subframes, and so on. If this field is not configured, then logicalChannelSR-DelayTimer is not applied for SDT logical channels. |
| ***servingCellConfigCommon***Configuration of the serving cell. |
| ***t319a***Initial value of the timer T319a used for detection of SDT failure. Value *ms100* corresponds to 100 milliseconds, value *ms200* corresponds to 200 milliseconds and so on. |
| ***uac-AccessCategory1-SelectionAssistanceInfo***Information used to determine whether Access Category 1 applies to the UE, as defined in TS 22.261 [25]. If *plmnCommon* is chosen, the *UAC-AccessCategory1-SelectionAssistanceInfo* is applicable to all the PLMNs and SNPNs in *plmn-IdentityInfoList* and *npn-IdentityInfoList*. If *individualPLMNList* is chosen, the 1st entry in the list corresponds to the first network within all of the PLMNs and SNPNs across the *plmn-IdentityList* and the *npn-IdentityInfoList*, the 2nd entry in the list corresponds to the second network within all of the PLMNs and SNPNs across the *plmn-IdentityList* and the *npn-IdentityInfoList* and so on. If *uac-AC1-SelectAssistInfo-r16* is present, the UE shall ignore the *uac-AccessCategory1-SelectionAssistanceInfo*. |
| ***uac-AC1-SelectAssistInfo***Information used to determine whether Access Category 1 applies to the UE, as defined in TS 22.261 [25]. The 1st entry in the list corresponds to the first network within all of the PLMNs and SNPNs across the *plmn-IdentityList* and *npn-IdentityInfoList*, the 2nd entry in the list corresponds to the second network within all of the PLMNs and SNPNs across the *plmn-IdentityList* and the *npn-IdentityInfoList* and so on. Value *notConfigured* indicates that Access Category1 is not configured for the corresponding PLMN/SNPN. |
| ***uac-BarringForCommon***Common access control parameters for each access category. Common values are used for all PLMNs/SNPNs, unless overwritten by the PLMN/SNPN specific configuration provided in *uac-BarringPerPLMN-List*. The parameters are specified by providing an index to the set of configurations (*uac-BarringInfoSetList*). UE behaviour upon absence of this field is specified in clause 5.3.14.2. |
| ***ue-TimersAndConstants***Timer and constant values to be used by the UE. The cell operating as PCell always provides this field. |
| ***useFullResumeID***Indicates which resume identifier and Resume request message should be used. UE uses *fullI-RNTI* and *RRCResumeRequest1* if the field is present, or *shortI-RNTI* and *RRCResumeRequest* if the field is absent. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *EDRX-RC* | The field is optionally present, Need R, in a cell that enables *eDRX-AllowedIdle*, otherwise it is absent. |
| *MINT* | The field is optionally present, Need R, in a cell that provides a configuration for disaster roaming, otherwise it is absent, Need R. |
| *Standalone* | The field is mandatory present in a cell that supports standalone operation, otherwise it is absent. |

NEXT CHANGE

## 6.3 RRC information elements

### 6.3.2 Radio resource control information elements

#### – *CellAccessRelatedInfo*

The IE *CellAccessRelatedInfo* indicates cell access related information for this cell.

*CellAccessRelatedInfo* information element

-- ASN1START

-- TAG-CELLACCESSRELATEDINFO-START

CellAccessRelatedInfo ::= SEQUENCE {

 plmn-IdentityInfoList PLMN-IdentityInfoList,

 cellReservedForOtherUse ENUMERATED {true} OPTIONAL, -- Need R

 ...,

 [[

 cellReservedForFutureUse-r16 ENUMERATED {true} OPTIONAL, -- Need R

 npn-IdentityInfoList-r16 NPN-IdentityInfoList-r16 OPTIONAL -- Need R

 ]],

 [[

 snpn-AccessInfoList-r17 SEQUENCE (SIZE (1..maxNPN-r16)) OF SNPN-AccessInfo-r17 OPTIONAL -- Need R

 ]]

}

SNPN-AccessInfo-r17 ::= SEQUENCE {

 extCH-Supported-r17 ENUMERATED {true} OPTIONAL, -- Need R

 extCH-WithoutConfigAllowed-r17 ENUMERATED {true} OPTIONAL, -- Need R

 onboardingEnabled-r17 ENUMERATED {true} OPTIONAL, -- Need R

 imsEmergencySupportForSNPN-r17 ENUMERATED {true} OPTIONAL -- Need R

}

-- TAG-CELLACCESSRELATEDINFO-STOP

-- ASN1STOP

|  |
| --- |
| *CellAccessRelatedInfo* field descriptions |
| ***cellReservedForFutureUse***Indicates whether the cell is reserved, as defined in 38.304 [20] for future use. The field is applicable to all PLMNs and NPNs. This field is ignored by IAB-MT and NCR-MT. |
| ***cellReservedForOtherUse***Indicates whether the cell is reserved, as defined in 38.304 [20]. The field is applicable to all PLMNs. This field is ignored by IAB-MT and NCR-MT for cell barring determination, but still considered by NPN capable IAB-MT and NPN capable NCR-MT for determination of an NPN-only cell. |
| ***npn-IdentityInfoList***The *npn-IdentityInfoList* is used to configure a set of *NPN-IdentityInfo* elements. Each of those elements contains a list of one or more NPN Identities and additional information associated with those NPNs. The total number of PLMNs (identified by a PLMN identity in *plmn -IdentityList*), PNI-NPNs (identified by a PLMN identity and a CAG-ID), and SNPNs (identified by a PLMN identity and a NID) together in the *PLMN-IdentityInfoList* and *NPN-IdentityInfoList* does not exceed 12, except for the NPN-only cells. A PNI-NPN and SNPN can be included only once, and in only one entry of the *NPN-IdentityInfoList*. In case of NPN-only cells the *PLMN-IdentityList* contains a single element that does not count to the limit of 12 and the *cellIdentity* of the first entry of the *PLMN-IdentityInfoList* is set to the same value as the *cellIdentity-r16* of the first entry of the *NPN-IdentityInfoList*. The NPN index is defined as *B+c1+c2+…+c(n-1)+d1+d2+…+d(m-1)+e(i)* for the NPN identity included in the *n*-th entry of *NPN-IdentityInfoList* and in the *m*-th entry of *npn-Identitylist* within that *NPN-IdentityInfoList* entry, and the *i*-th entry of its corresponding *NPN-Identity*, where- *B* is the index used for the last PLMN in the *PLMN-IdentittyInfoList*; in NPN-only cells *B* is considered 0;- *c(j)* is the number of NPN index values used in the *j*-th *NPN-IdentityInfoList* entry;- *d(k)* is the number of NPN index values used in the *k*-th *npn-IdentityList* entry within the *n*-th *NPN-IdentityInfoList* entry;- e(i) is - *i* if the *n*-th entry of *NPN-IdentityInfoList* entry is for SNPN(s); - 1 if the *n*-th entry of *NPN-IdentityInfoList* entry is for PNI-NPN(s). |
| ***plmn-IdentityInfoList***The *plmn-IdentityInfoList* is used to configure a set of *PLMN-IdentityInfo* elements. Each of those elements contains a list of one or more PLMN Identities and additional information associated with those PLMNs. A PLMN-identity can be included only once, and in only one entry of the *PLMN-IdentityInfoList*. The PLMN index is defined as *b1+b2+…+b(n-1)+i* for the PLMN included at the *n*-th entry of *PLMN-IdentityInfoList* and the *i*-th entry of its corresponding *PLMN-IdentityInfo*, where *b(j)* is the number of *PLMN-Identity* entries in each *PLMN-IdentityInfo*, respectively. |
| ***snpn-AccessInfoList***This list provides access related information for each SNPN in *npn-IdentityInfoList*, see TS 23.501 [32]. The n-th entry of the list contains the access related information of the n-th SNPN in *npn-IdentityInfoList*.  |

|  |
| --- |
| *SNPN-AccessInfo* field descriptions |
| ***extCH-Supported***Indicates whether the SNPN supports access using credentials from a Credentials Holder as specified in TS 23.501 [32]. |
| ***extCH-WithoutConfigAllowed***Indicates whether the SNPN allows registration attempts with credentials from a Credentials Holder from UEs that are not explicitly configured to select the SNPN as specified in TS 23.501 [32]. |
| ***imsEmergencySupportForSNPN***Indicates whether the SNPN supports IMS emergency bearer services for UEs in limited service mode in the cell. If absent, IMS emergency call is not supported by the SNPN in the cell for UEs in limited service mode. |
| ***onboardingEnabled***Indicates whether the onboarding SNPN allows registration for onboarding in the cell as specified in TS 23.501 [32]. |

NEXT CHANGE

#### – *CellGroupConfig*

The *CellGroupConfig* IE is used to configure a master cell group (MCG) or secondary cell group (SCG). A cell group comprises of one MAC entity, a set of logical channels with associated RLC entities and of a primary cell (SpCell) and one or more secondary cells (SCells). For an NCR-MT, the *CellGroupConfig* IE is also used to provide the configuration of side control information for the NCR-Fwd access link.

*CellGroupConfig* information element

-- ASN1START

-- TAG-CELLGROUPCONFIG-START

-- Configuration of one Cell-Group:

CellGroupConfig ::= SEQUENCE {

 cellGroupId CellGroupId,

 rlc-BearerToAddModList SEQUENCE (SIZE(1..maxLC-ID)) OF RLC-BearerConfig OPTIONAL, -- Need N

 rlc-BearerToReleaseList SEQUENCE (SIZE(1..maxLC-ID)) OF LogicalChannelIdentity OPTIONAL, -- Need N

 mac-CellGroupConfig MAC-CellGroupConfig OPTIONAL, -- Need M

 physicalCellGroupConfig PhysicalCellGroupConfig OPTIONAL, -- Need M

 spCellConfig SpCellConfig OPTIONAL, -- Need M

 sCellToAddModList SEQUENCE (SIZE (1..maxNrofSCells)) OF SCellConfig OPTIONAL, -- Need N

 sCellToReleaseList SEQUENCE (SIZE (1..maxNrofSCells)) OF SCellIndex OPTIONAL, -- Need N

 ...,

 [[

 reportUplinkTxDirectCurrent ENUMERATED {true} OPTIONAL -- Cond BWP-Reconfig

 ]],

 [[

 bap-Address-r16 BIT STRING (SIZE (10)) OPTIONAL, -- Need M

 bh-RLC-ChannelToAddModList-r16 SEQUENCE (SIZE(1..maxBH-RLC-ChannelID-r16)) OF BH-RLC-ChannelConfig-r16 OPTIONAL, -- Need N

 bh-RLC-ChannelToReleaseList-r16 SEQUENCE (SIZE(1..maxBH-RLC-ChannelID-r16)) OF BH-RLC-ChannelID-r16 OPTIONAL, -- Need N

 f1c-TransferPath-r16 ENUMERATED {lte, nr, both} OPTIONAL, -- Need M

 simultaneousTCI-UpdateList1-r16 SEQUENCE (SIZE (1..maxNrofServingCellsTCI-r16)) OF ServCellIndex OPTIONAL, -- Need R

 simultaneousTCI-UpdateList2-r16 SEQUENCE (SIZE (1..maxNrofServingCellsTCI-r16)) OF ServCellIndex OPTIONAL, -- Need R

 simultaneousSpatial-UpdatedList1-r16 SEQUENCE (SIZE (1..maxNrofServingCellsTCI-r16)) OF ServCellIndex OPTIONAL, -- Need R

 simultaneousSpatial-UpdatedList2-r16 SEQUENCE (SIZE (1..maxNrofServingCellsTCI-r16)) OF ServCellIndex OPTIONAL, -- Need R

 uplinkTxSwitchingOption-r16 ENUMERATED {switchedUL, dualUL} OPTIONAL, -- Need R

 uplinkTxSwitchingPowerBoosting-r16 ENUMERATED {enabled} OPTIONAL -- Need R

 ]],

 [[

 reportUplinkTxDirectCurrentTwoCarrier-r16 ENUMERATED {true} OPTIONAL -- Need N

 ]],

 [[

 f1c-TransferPathNRDC-r17 ENUMERATED {mcg, scg, both} OPTIONAL, -- Need M

 uplinkTxSwitching-2T-Mode-r17 ENUMERATED {enabled} OPTIONAL, -- Cond 2Tx

 uplinkTxSwitching-DualUL-TxState-r17 ENUMERATED {oneT, twoT} OPTIONAL, -- Cond 2Tx

 uu-RelayRLC-ChannelToAddModList-r17 SEQUENCE (SIZE(1..maxUu-RelayRLC-ChannelID-r17)) OF Uu-RelayRLC-ChannelConfig-r17

 OPTIONAL, -- Need N

 uu-RelayRLC-ChannelToReleaseList-r17 SEQUENCE (SIZE(1..maxUu-RelayRLC-ChannelID-r17)) OF Uu-RelayRLC-ChannelID-r17

 OPTIONAL, -- Need N

 simultaneousU-TCI-UpdateList1-r17 SEQUENCE (SIZE (1..maxNrofServingCellsTCI-r16)) OF ServCellIndex OPTIONAL, -- Need R

 simultaneousU-TCI-UpdateList2-r17 SEQUENCE (SIZE (1..maxNrofServingCellsTCI-r16)) OF ServCellIndex OPTIONAL, -- Need R

 simultaneousU-TCI-UpdateList3-r17 SEQUENCE (SIZE (1..maxNrofServingCellsTCI-r16)) OF ServCellIndex OPTIONAL, -- Need R

 simultaneousU-TCI-UpdateList4-r17 SEQUENCE (SIZE (1..maxNrofServingCellsTCI-r16)) OF ServCellIndex OPTIONAL, -- Need R

 rlc-BearerToReleaseListExt-r17 SEQUENCE (SIZE(1..maxLC-ID)) OF LogicalChannelIdentityExt-r17 OPTIONAL, -- Need N

 iab-ResourceConfigToAddModList-r17 SEQUENCE (SIZE(1..maxNrofIABResourceConfig-r17)) OF IAB-ResourceConfig-r17 OPTIONAL, -- Need N

 iab-ResourceConfigToReleaseList-r17 SEQUENCE (SIZE(1..maxNrofIABResourceConfig-r17)) OF IAB-ResourceConfigID-r17 OPTIONAL -- Need N

 ]],

 [[

 reportUplinkTxDirectCurrentMoreCarrier-r17 ReportUplinkTxDirectCurrentMoreCarrier-r17 OPTIONAL -- Need N

 ]],

 [[

 ncr-FwdConfig-r18 SetupRelease { NCR-FwdConfig-r18 } OPTIONAL -- Cond NCR

 ]]

}

-- Serving cell specific MAC and PHY parameters for a SpCell:

SpCellConfig ::= SEQUENCE {

 servCellIndex ServCellIndex OPTIONAL, -- Cond SCG

 reconfigurationWithSync ReconfigurationWithSync OPTIONAL, -- Cond ReconfWithSync

 rlf-TimersAndConstants SetupRelease { RLF-TimersAndConstants } OPTIONAL, -- Need M

 rlmInSyncOutOfSyncThreshold ENUMERATED {n1} OPTIONAL, -- Need S

 spCellConfigDedicated ServingCellConfig OPTIONAL, -- Need M

 ...,

 [[

 lowMobilityEvaluationConnected-r17 SEQUENCE {

 s-SearchDeltaP-Connected-r17 ENUMERATED {dB3, dB6, dB9, dB12, dB15, spare3, spare2, spare1},

 t-SearchDeltaP-Connected-r17 ENUMERATED {s5, s10, s20, s30, s60, s120, s180, s240, s300, spare7, spare6, spare5,

 spare4, spare3, spare2, spare1}

 } OPTIONAL, -- Need R

 goodServingCellEvaluationRLM-r17 GoodServingCellEvaluation-r17 OPTIONAL, -- Need R

 goodServingCellEvaluationBFD-r17 GoodServingCellEvaluation-r17 OPTIONAL, -- Need R

 deactivatedSCG-Config-r17 SetupRelease { DeactivatedSCG-Config-r17 } OPTIONAL -- Cond SCG-Opt

 ]]

}

ReconfigurationWithSync ::= SEQUENCE {

 spCellConfigCommon ServingCellConfigCommon OPTIONAL, -- Need M

 newUE-Identity RNTI-Value,

 t304 ENUMERATED {ms50, ms100, ms150, ms200, ms500, ms1000, ms2000, ms10000},

 rach-ConfigDedicated CHOICE {

 uplink RACH-ConfigDedicated,

 supplementaryUplink RACH-ConfigDedicated

 } OPTIONAL, -- Need N

 ...,

 [[

 smtc SSB-MTC OPTIONAL -- Need S

 ]],

 [[

 daps-UplinkPowerConfig-r16 DAPS-UplinkPowerConfig-r16 OPTIONAL -- Need N

 ]],

 [[

 sl-PathSwitchConfig-r17 SL-PathSwitchConfig-r17 OPTIONAL -- Cond DirectToIndirect-PathSwitch

 ]]

}

DAPS-UplinkPowerConfig-r16 ::= SEQUENCE {

 p-DAPS-Source-r16 P-Max,

 p-DAPS-Target-r16 P-Max,

 uplinkPowerSharingDAPS-Mode-r16 ENUMERATED {semi-static-mode1, semi-static-mode2, dynamic }

}

SCellConfig ::= SEQUENCE {

 sCellIndex SCellIndex,

 sCellConfigCommon ServingCellConfigCommon OPTIONAL, -- Cond SCellAdd

 sCellConfigDedicated ServingCellConfig OPTIONAL, -- Cond SCellAddMod

 ...,

 [[

 smtc SSB-MTC OPTIONAL -- Need S

 ]],

 [[

 sCellState-r16 ENUMERATED {activated} OPTIONAL, -- Cond SCellAddSync

 secondaryDRX-GroupConfig-r16 ENUMERATED {true} OPTIONAL -- Cond DRX-Config2

 ]],

 [[

 preConfGapStatus-r17 BIT STRING (SIZE (maxNrofGapId-r17)) OPTIONAL, -- Cond PreConfigMG

 goodServingCellEvaluationBFD-r17 GoodServingCellEvaluation-r17 OPTIONAL, -- Need R

 sCellSIB20-r17 SetupRelease { SCellSIB20-r17 } OPTIONAL -- Need M

 ]]

}

SCellSIB20-r17 ::= OCTET STRING (CONTAINING SystemInformation)

DeactivatedSCG-Config-r17 ::= SEQUENCE {

 bfd-and-RLM-r17 BOOLEAN,

 ...

}

GoodServingCellEvaluation-r17 ::= SEQUENCE {

 offset-r17 ENUMERATED {db2, db4, db6, db8} OPTIONAL -- Need S

}

SL-PathSwitchConfig-r17 ::= SEQUENCE {

 targetRelayUE-Identity-r17 SL-SourceIdentity-r17,

 t420-r17 ENUMERATED {ms50, ms100, ms150, ms200, ms500, ms1000, ms2000, ms10000},

 ...

}

IAB-ResourceConfig-r17 ::= SEQUENCE {

 iab-ResourceConfigID-r17 IAB-ResourceConfigID-r17,

 slotList-r17 SEQUENCE (SIZE (1..5120)) OF INTEGER (0..5119) OPTIONAL, -- Need M

 periodicitySlotList-r17 ENUMERATED {ms0p5, ms0p625, ms1, ms1p25, ms2, ms2p5, ms5, ms10, ms20, ms40, ms80, ms160} OPTIONAL, -- Need M

 slotListSubcarrierSpacing-r17 SubcarrierSpacing OPTIONAL, -- Need M

 ...

}

IAB-ResourceConfigID-r17 ::= INTEGER(0..maxNrofIABResourceConfig-1-r17)

ReportUplinkTxDirectCurrentMoreCarrier-r17 ::= SEQUENCE (SIZE(1.. maxSimultaneousBands)) OF IntraBandCC-CombinationReqList-r17

IntraBandCC-CombinationReqList-r17::= SEQUENCE {

 servCellIndexList-r17 SEQUENCE (SIZE(1.. maxNrofServingCells)) OF ServCellIndex,

 cc-CombinationList-r17 SEQUENCE (SIZE(1.. maxNrofReqComDC-Location-r17)) OF IntraBandCC-Combination-r17

}

IntraBandCC-Combination-r17::= SEQUENCE (SIZE(1.. maxNrofServingCells)) OF CC-State-r17

CC-State-r17::= SEQUENCE {

 dlCarrier-r17 CarrierState-r17 OPTIONAL, -- Need N

 ulCarrier-r17 CarrierState-r17 OPTIONAL -- Need N

}

CarrierState-r17::= CHOICE {

 deActivated-r17 NULL,

 activeBWP-r17 INTEGER (0..maxNrofBWPs)

}

-- TAG-CELLGROUPCONFIG-STOP

-- ASN1STOP

|  |
| --- |
| *CC-State* field descriptions |
| ***dlCarrier***Indicates DL carrier activation state for this carrier and the related active BWP Index, if activated. |
| ***ulCarrier***Indicates UL carrier activation state for this carrier and the related active BWP Index, if activated. |

|  |
| --- |
| *CellGroupConfig* field descriptions |
| ***bap-Address***BAP address of the parent node in cell group. |
| ***bh-RLC-ChannelToAddModList***Configuration of the backhaul RLC entities and the corresponding MAC Logical Channels to be added and modified. |
| ***bh-RLC-ChannelToReleaseList***List of the backhaul RLC entities and the corresponding MAC Logical Channels to be released. |
| ***f1c-TransferPath***The F1-C transfer path that an EN-DC IAB-MT should use for transferring F1-C packets to the IAB-donor-CU. If IAB-MT is configured with *lte*, IAB-MT can only use LTE leg for F1-C transfer. If IAB-MT is configured with *nr*, IAB-MT can only use NR leg for F1-C transfer. If IAB-MT is configured with *both*, it is up to IAB-MT to select an LTE leg or a NR leg for F1-C transfer. If the field is not configured, the IAB node uses the NR leg as the default one. |
| ***f1c-TransferPathNRDC***The F1-C transfer path that an NR-DC IAB-MT should use for transferring F1-C packets to the IAB-donor-CU. If IAB-MT is configured with *mcg*, IAB-MT can only use the MCG for F1-C transfer. If IAB-MT is configured with *scg*, IAB-MT can only use the SCG for F1-C transfer. If IAB-MT is configured with *both*, it is up to IAB-MT to select the MCG or the SCG for F1-C transfer. |
| ***mac-CellGroupConfig***MAC parameters applicable for the entire cell group. |
| ***ncr-FwdConfig***Configuration of side control information for the NCR-Fwd access link. The NCR-Fwd stops forwarding when this field is released. |
| ***rlc-BearerToAddModList***Configuration of the MAC Logical Channel, the corresponding RLC entities and association with radio bearers. |
| ***reportUplinkTxDirectCurrent***Enables reporting of uplink and supplementary uplink Direct Current location information upon BWP configuration and reconfiguration. This field is only present when the BWP configuration is modified or any serving cell is added or removed. This field is absent in the IE *CellGroupConfig* when provided as part of *RRCSetup* message. If UE is configured with SUL carrier, UE reports both UL and SUL Direct Current locations. |
| ***reportUplinkTxDirectCurrentMoreCarrier***Enables reporting of uplink Direct Current location information when the UE is configured with intra-band CA. This field is absent in the IE *CellGroupConfig* when provided as part of *RRCSetup* message. The UE only reports the uplink Direct Current location information that are related to the indicated *cc-CombinationList*. The network does not include carriers which locate in DL only spectrum described in TS 38.101-2 [39], clause 5.3A.4 and defined by Fsd according to Table 5.3A.4-3 in FR2 in the *IntraBandCC-CombinationReqList*. I.e. DL-only carrier in FR2 frequency spectrum is not used to calculate the default DC location. |
| ***reportUplinkTxDirectCurrentTwoCarrier***Enables reporting of uplink Direct Current location information when the UE is configured with uplink intra-band CA with two carriers. This field is absent in the IE *CellGroupConfig* when provided as part of *RRCSetup* message. |
| ***rlc-BearerToReleaseListExt***List of the RLC entities and the corresponding MAC Logical Channels to be released for multicast MRBs. |
| ***rlmInSyncOutOfSyncThreshold***BLER threshold pair index for IS/OOS indication generation, see TS 38.133 [14], table 8.1.1-1. *n1* corresponds to the value 1. When the field is absent, the UE applies the value 0. Whenever this is reconfigured, UE resets N310 and N311, and stops T310, if running. Network does not include this field. |
| ***sCellSIB20***This field is used to transfer *SIB20* of the SCell in order to allow the UE for MBS broadcast reception on SCell. The network configures this field only for a single SCell at a time. |
| ***sCellState***Indicates whether the SCell shall be considered to be in activated state upon SCell configuration. If the field is included for an SCell configured with TRS for fast activation of the SCell, such TRS is not used for the corresponding SCell. |
| ***sCellToAddModList***List of secondary serving cells (SCells) to be added or modified. |
| ***sCellToReleaseList***List of secondary serving cells (SCells) to be released. |
| ***secondaryDRX-GroupConfig***The field is used to indicate whether the SCell belongs to the secondary DRX group. All serving cells in the secondary DRX group shall belong to one Frequency Range and all serving cells in the legacy DRX group shall belong to another Frequency Range. |
| ***simultaneousSpatial-UpdatedList1, simultaneousSpatial-UpdatedList2***List of serving cells which can be updated simultaneously for spatial relation with a MAC CE. The *simultaneousSpatial-UpdatedList1* and *simultaneousSpatial-UpdatedList2* shall not contain same serving cells. Network should not configure serving cells that are configured with a BWP with two different values for the *coresetPoolIndex* in these lists. |
| ***simultaneousTCI-UpdateList1, simultaneousTCI-UpdateList2***List of serving cells which can be updated simultaneously for TCI relation with a MAC CE. The *simultaneousTCI-UpdateList1* and *simultaneousTCI-UpdateList2* shall not contain same serving cells. Network should not configure serving cells that are configured with a BWP with two different values for the *coresetPoolIndex* in these lists. |
| ***simultaneousU-TCI-UpdateList1, simultaneousU-TCI-UpdateList2, simultaneousU-TCI-UpdateList3, simultaneousU-TCI-UpdateList4***List of serving cells for which the Unified TCI States Activation/Deactivation MAC CE applies simultaneously, as specified in TS 38.321 [3] clause 6.1.3.47. The different lists shall not contain same serving cells. Network only configures in these lists serving cells that are configured with *unifiedTCI-StateType*. |
| ***spCellConfig***Parameters for the SpCell of this cell group (PCell of MCG or PSCell of SCG).  |
| ***uplinkTxSwitchingOption***Indicates which option is configured for dynamic UL Tx switching for inter-band UL CA or (NG)EN-DC. The field is set to *switchedUL* if network configures option 1 as specified in TS 38.214 [19], or *dualUL* if network configures option 2 as specified in TS 38.214 [19]. Network always configures UE with a value for this field in inter-band UL CA case and (NG)EN-DC case where UE supports dynamic UL Tx switching. |
| ***uplinkTxSwitchingPowerBoosting***Indicates whether the UE is allowed to enable 3dB boosting on the maximum output power for transmission on carrier2 under the operation state in which 2-port transmission can be supported on carrier2 for inter-band UL CA case with dynamic UL Tx switching as defined in TS 38.101-1 [15]. Network can only configure this field for dynamic UL Tx switching in inter-band UL CA case with power Class 3 as defined in TS 38.101-1 [15]. |
| ***uplinkTxSwitching-2T-Mode***Indicates 2Tx-2Tx switching mode is configured for inter-band UL CA or SUL, in which the switching gap duration for a triggered uplink switching (as specified in TS 38.214 [19]) is equal to the switching time capability value reported for the switching mode.If this field is absent and *uplinkTxSwitching* is configured, it is interpreted that 1Tx-2Tx UL Tx switching is configured as specified in TS 38.214 [19]. In this case, there is one uplink (or one uplink band in case of intra-band) configured with *uplinkTxSwitching*, on which the maximum number of antenna ports among all configured P-SRS/A-SRS and activated SP-SRS resources should be 1 and non-codebook based UL MIMO is not configured. |
| ***uplinkTxSwitching-DualUL-TxState***Indicates the state of Tx chains if the state of Tx chains after the UL Tx switching is not unique (as specified in TS 38.214 [19]) in case of 2Tx-2Tx switching is configured and *uplinkTxSwitchingOption* is set to *dualUL*. Value *oneT* indicates 1Tx is assumed to be supported on the carriers on each band, value *twoT* indicates 2Tx is assumed to be supported on that carrier. |
| ***uu-RelayRLC-ChannelToAddModList***List of the Uu RLC entities and the corresponding MAC Logical Channels to be added or modified. |
| ***uu-RelayRLC-ChannelToReleaseList***List of the Uu RLC entities and the corresponding MAC Logical Channels to be released. |

|  |
| --- |
| *DeactivatedSCG-Config* field descriptions |
| ***bfd-and-RLM***If the field is set to *true*, the UE shall perform RLM and BFD on the PSCell when the SCG is deactivated and the network ensures that *beamFailure-r17* is not configured in the *radioLinkMonitoringConfig* of the DL BWP of the PSCell in which the UE performs BFD. If set to *false*, the UE is not required to perform RLM and BFD on the PSCell when the SCG is deactivated. |

|  |
| --- |
| *DAPS-UplinkPowerConfig* field descriptions |
| ***p-DAPS-Source***The maximum total transmit power to be used by the UE in the source cell group during DAPS handover. |
| ***p-DAPS-Target***The maximum total transmit power to be used by the UE in the target cell group during DAPS handover. |
| ***uplinkPowerSharingDAPS-Mode***Indicates the uplink power sharing mode that the UE uses in DAPS handover (see TS 38.213 [13]). |

|  |
| --- |
| *GoodServingCellEvaluation* field descriptions |
| ***offset***The parameter "X" (dB) for the good serving cell quality criterion in RRC\_CONNECTED, for a cell operating in FR1 and FR2, respectively. If this field is absent, the UE applies the (default) value of 0 dB for "X". |

|  |
| --- |
| *IAB-ResourceConfig* field descriptions |
| ***iab-ResourceConfigID***This ID is used to indicate the specific resource configuration addressed by the MAC CEs specified in TS 38.321 [3]. |
| ***periodicitySlotList***Indicates the periodicity in ms of the list of slot indexes indicated in *slotList*. |
| ***slotList***Indicates the list of slot indexes to which the information indicated in the specific MAC CE applies to, as specified in TS 38.321 [3]. The values of the entries in the *slotList* are strictly less than the value of the *periodicitySlotList*. |
| ***slotListSubcarrierSpacing***Subcarrier spacing used as reference for the *slotList* configuration.Only the following values are applicable depending on the used frequency:FR1: 15 or 30 kHzFR2-1: 60 or 120 kHzFR2-2: 120 or 480 kHz |

|  |
| --- |
| *ReconfigurationWithSync* field descriptions |
| ***rach-ConfigDedicated***Random access configuration to be used for the reconfiguration with sync (e.g. handover). The UE performs the RA according to these parameters in the *firstActiveUplinkBWP* (see *UplinkConfig*). |
| ***smtc***The SSB periodicity/offset/duration configuration of target cell for NR PSCell change and NR PCell change. The network sets the *periodicityAndOffset* to indicate the same periodicity as *ssb-periodicityServingCell* in *spCellConfigCommon* or sets to the same periodicity as *ssb-Periodicity-r17* in *nonCellDefiningSSB-r17* if the first active DL BWP included in this RRC message is configured with *nonCellDefiningSSB-r17* for RedCap.For case of NR PCell change, the *smtc* is based on the timing reference of (source) PCell. For case of NR PSCell change, it is based on the timing reference of source PSCell.If both this field and *targetCellSMTC-SCG* are absent, the UE uses the SMTC in the *measObjectNR* having the same SSB frequency and subcarrier spacing, as configured before the reception of the RRC message. For a RedCap UE, if the first active DL BWP included in this RRC message is configured with *nonCellDefiningSSB-r17*, this field corresponds to the NCD-SSB indicated by *nonCellDefiningSSB-r17*, otherwise, this field corresponds to the CD-SSB indicated by *absoluteFrequencySSB* in *frequencyInfoDL*. |

|  |
| --- |
| *ReportUplinkTxDirectCurrentMoreCarrier* field descriptions |
| ***IntraBandCC-Combination***Indicates the state of the carriers and BWPs indexes of the carriers in a CC combination, each carrier in this combination corresponds to an entry in *servCellIndexList* with same order. This IE shall have the same size as *servCellIndexList*. |
| ***IntraBandCC-CombinationReqList***Indicates the list of the requested carriers/BWPs combinations for an intra-band CA component. |
| ***servCellIndexList***indicates the list of cell index for an intra-band CA component. |

|  |
| --- |
| *SCellConfig* field descriptions |
| ***goodServingCellEvaluationBFD***Indicates the criterion for a UE to detect the good serving cell quality for BFD relaxation in an SCell in RRC\_CONNECTED. This field is always configured when the network enables BFD relaxation for the UE in this SCell. This field is absent if *failureDetectionSetN* is present for the SCell. |
| ***preConfGapStatus***Indicates whether the pre-configured measurement gaps (i.e. the gaps configured with *preConfigInd*) are activated or deactivated while this SCell is deactivated. If this field is configured, the UE shall apply network-controlled mechanism for activation and deactivation of the pre-configured measurement gaps, otherwise the UE shall apply the autonomous activation/deactivation mechanism, as specified in TS 38.133 [14]. The first/leftmost bit corresponds to the measurement gap with gap ID 1, the second bit corresponds to measurement gap with gap ID 2, and so on. Value 0 indicates that the corresponding pre-configured measurement gap is deactivated while value 1 indicates that the corresponding pre-configured measurement gap is activated. The UE shall ignore the bit if the corresponding measurement gap is not a pre-configured measurement gap. |
| ***smtc***The SSB periodicity/offset/duration configuration of target cell for NR SCell addition. The network sets the *periodicityAndOffset* to indicate the same periodicity as *ssb-periodicityServingCell* in *sCellConfigCommon*. The *smtc* is based on the timing of the SpCell of associated cell group. In case of inter-RAT handover to NR, the timing reference is the NR PCell. In case of intra-NR PCell change (standalone NR) or NR PSCell change (EN-DC), the timing reference is the target SpCell. If the field is absent, the UE uses the SMTC in the *measObjectNR* having the same SSB frequency and subcarrier spacing, as configured before the reception of the RRC message. |

|  |
| --- |
| *SpCellConfig* field descriptions |
| ***deactivatedSCG-Config***Configuration applicable when the SCG is deactivated. The network always configures this field before or when indicating that the SCG is deactivated in an *RRCReconfiguration*, *RRCResume*, E-UTRA *RRCConnectionReconfiguration* or E-UTRA *RRCConnectionResume* message. |
| ***goodServingCellEvaluationBFD***Indicates the criterion for a UE to detect the good serving cell quality for BFD relaxation in the SpCell in RRC\_CONNECTED. The field is always configured when the network enables BFD relaxation for the UE in this SpCell. This field is absent if *failureDetectionSetN* is present for the SpCell. |
| ***goodServingCellEvaluationRLM***Indicates the criterion for a UE to detect the good serving cell quality for RLM relaxation in the SpCell in RRC\_CONNECTED. The field is always configured when the network enables RLM relaxation for the UE in this SpCell. |
| ***lowMobilityEvaluationConnected***Indicates the criterion for a UE to detect low mobility in RRC\_CONNECTED in an SpCell. The *s-SearchDeltaP-Connected* is the parameter "SSearchDeltaP-connected". Value *dB*3 corresponds to 3 dB, *dB*6 corresponds to 6 dB and so on. The *t-SearchDeltaP-Connected* is the parameter "TSearchDeltaP-Connected". Value *s5* means 5 seconds, value *s10* means 10 seconds and so on. Low mobility criterion is configured in NR PCell for the case of NR SA/ NR CA/ NE-DC/NR-DC, and in the NR PSCell for the case of EN-DC. |
| ***reconfigurationWithSync***Parameters for the synchronous reconfiguration to the target SpCell. |
| ***rlf-TimersAndConstants***Timers and constants for detecting and triggering cell-level radio link failure. For the SCG, *rlf-TimersAndConstants* can only be set to *setup* and is always included at SCG addition. |
| ***servCellIndex***Serving cell ID of a PSCell. The PCell of the Master Cell Group uses ID = 0. |

|  |
| --- |
| *SL-PathSwitchConfig* field descriptions |
| ***targetRelayUE-Identity***Indicates the L2 source ID of the target L2 U2N Relay UE during path switch. |
| ***T420***Indicates the timer value of T420 to be used during path switch. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *2Tx* | The field is optionally present, Need R, if *uplinkTxSwitching* is configured; otherwise it is absent, Need R. |
| *BWP-Reconfig* | The field is optionally present, Need N, if the BWPs are reconfigured or if serving cells are added or removed. Otherwise it is absent.  |
| *DirectToIndirect-PathSwitch* | The field is mandatory present for the L2 U2N remote UE at path switch to the target L2 U2N Relay UE. It is absent otherwise. |
| *DRX-Config2* | The field is optionally present, Need N, if *drx-ConfigSecondaryGroup* is configured. It is absent otherwise. |
| *NCR* | The field is optionally present, Need M, for NCR-MT. It is absent otherwise. |
| *PreConfigMG* | The field is optionally present, Need R, if there is at least one per UE gap configured with *preConfigInd* or there is at least one per FR gap of the same FR which the SCell belongs to and configured with *preConfigInd*. It is absent, Need R, otherwise. |
| *ReconfWithSync* | The field is mandatory present in the *RRCReconfiguration* message:- in each configured *CellGroupConfig* for which the SpCell changes,- in the *masterCellGroup:*- at change of AS security key derived from KgNB,- in an *RRCReconfiguration* message contained in a *DLInformationTransferMRDC* message,- path switch of L2 U2N remote UE to the target PCell,- path switch of L2 U2N remote UE to the target L2 U2N Relay UE,- in the *secondaryCellGroup* at:- PSCell addition,- SCG resume with NR-DC or (NG)EN-DC,- update of required SI for PSCell,- change of AS security key derived from S-KgNB in NR-DC while the UE is configured with at least one radio bearer with *keyToUse* set to *secondary* and that is not released by this *RRCReconfiguration* message,- MN handover in (NG)EN-DC.Otherwise, it is optionally present, need M. The field is absent in the *masterCellGroup* in *RRCResume* and *RRCSetup* messages and is absent in the *masterCellGroup* in *RRCReconfiguration* messages if source configuration is not released during DAPS handover. |
| *SCellAdd* | The field is mandatory present upon SCell addition; otherwise it is absent, Need M. |
| *SCellAddMod* | The field is mandatory present upon SCell addition; otherwise it is optionally present, need M. |
| *SCellAddSync* | The field is optionally present, Need N:- in the *masterCellGroup* at- SCell addition,- reconfiguration with sync,- resume of an RRC connection.- in the *secondaryCellGroup*, when the SCG is not indicated as deactivated at:- SCG activation while the SCG was previously deactivated,- SCell addition,- reconfiguration with sync.It is absent otherwise. |
| *SCG* | The field is mandatory present in an *SpCellConfig* for the PSCell. It is absent otherwise.  |
| *SCG-Opt* | The field is optionally present, Need M, in an SpCellConfig for the PSCell. It is absent otherwise. |

NOTE: In case of change of AS security key derived from S-KgNB/S-KeNB, if *reconfigurationWithSync* is not included in the *masterCellGroup*, the network releases all existing MCG RLC bearers associated with a radio bearer with *keyToUse* set to *secondary*. In case of change of AS security key derived from KgNB/KeNB, if *reconfigurationWithSync* is not included in the *secondaryCellGroup*, the network releases all existing SCG RLC bearers associated with a radio bearer with *keyToUse* set to *primary*.

NEXT CHANGE

*– NCR-FwdConfig*

The IE *NCR-FwdConfig* contains configuration related to periodic, aperiodic and semi-persistent beam indication for NCR-Fwd access link.

***NCR-FwdConfig* information element**

-- ASN1START

-- TAG-NCR-FWDCONFIG-START

NCR-FwdConfig-r18 ::= SEQUENCE {

 periodicFwdRsrcSetToAddModList-r18 SEQUENCE (SIZE (1..maxNrofPeriodicFwdResourceSet-r18)) OF NCR-PeriodicFwdResourceSet-r18 OPTIONAL, -- Need N

 periodicFwdRsrcSetToReleaseList-r18 SEQUENCE (SIZE (1..maxNrofPeriodicFwdResourceSet-r18)) OF NCR-PeriodicFwdResourceSetId-r18 OPTIONAL, -- Need N

 aperiodicFwdConfig-r18 NCR-AperiodicFwdConfig-r18 OPTIONAL, -- Need N

 semiPersistentFwdRsrcSetToAddModList-r18 SEQUENCE (SIZE (1..maxNrofSemiPersistentFwdResourceSet-r18)) OF NCR-SemiPersistentFwdResourceSet-r18 OPTIONAL, -- Need N

 semiPersistentFwdRsrcSetToReleaseList-r18 SEQUENCE (SIZE (1..maxNrofSemiPersistentFwdResourceSet-r18)) OF NCR-SemiPersistentFwdResourceSetId-r18 OPTIONAL, -- Need N

 ...

}

-- TAG-NCR-FWDCONFIG-STOP

-- ASN1STOP

|  |
| --- |
| ***NCR-FwdConfig field descriptions*** |
| ***aperiodicFwdConfig***Aperiodic time resource configuration for beam indication for NCR. The configuration includes a list of time domain resources that can be selected for aperiodic forwarding. |
| ***periodicFwdRsrcSetToAddModList***List of periodic forwarding resource configurations to be added or modified. |
| ***periodicFwdRsrcSetToReleaseList***List of periodic forwarding resource configurations to be released. |
| ***semiPersistentFwdRsrcSetToAddModList***List of semi-persistent forwarding resources configurations to be added or modified. |
| ***semiPersistentFwdRsrcSetToReleaseList***List of semi-persistent forwarding resource configurations to be released. |

– *NCR-AperiodicFwdConfig*

The IE *NCR-AperiodicFwdConfig* is used to configure a list of aperiodic forwarding time resources for NCR-Fwd access link.

***NCR-AperiodicFwdConfig* information element**

-- ASN1START

-- TAG-NCR-APERIODICFWDCONFIG-START

NCR-AperiodicFwdConfig-r18 ::= SEQUENCE {

 aperiodicFwdTimeRsrcToAddModList-r18 SEQUENCE (SIZE (1..maxNrofAperiodicFwdTimeResource-r18)) OF NCR-AperiodicFwdTimeResource-r18 OPTIONAL, -- Need N

 aperiodicFwdTimeRsrcToReleaseList-r18 SEQUENCE (SIZE (1..maxNrofAperiodicFwdTimeResource-r18)) OF NCR-AperiodicFwdTimeResourceId-r18 OPTIONAL, -- Need N

 referenceSCS-r18 SubcarrierSpacing OPTIONAL, -- Need M,

 aperiodicBeamFieldWidth-r18 INTEGER (1..6) OPTIONAL, -- Need M,

 ...

}

NCR-AperiodicFwdTimeResource-r18 ::= SEQUENCE {

 aperiodicFwdTimeRsrcId-r18 NCR-AperiodicFwdTimeResourceId-r18,

 slotOffsetAperiodic-r18 INTEGER (0..14),

 symbolOffset-r18 INTEGER (0..maxNrofSymbols-1),

 durationInSymbols-r18 INTEGER (1..ffs)

}

-- TAG-NCR-APERIODICFWDCONFIG-STOP

-- ASN1STOP

|  |
| --- |
| ***NCR-AperiodicFwdConfig field descriptions*** |
| ***aperiodicBeamFieldWidth***Indicates the bitwidth of each beam index field in DCI carrying aperiodic beam indication. |
| ***durationInSymbols***Indicates the time duration in number of symbols. |
| ***aperiodicFwdTimeRsrcToAddModList***List of aperiodic forwarding time resources to be added or modified. |
| ***aperiodicFwdTimeRsrcToReleaseList***List of aperiodic forwarding time resources to be released. |
| ***referenceSCS-r18***Indicates the reference subcarrier spacing for all the time resource in the list. Only Values *kHz15*, *kHz30*, *kHz60*, *kHz120* and *kHz240* are applicable. |
| ***slotOffsetAperiodic***Indicates slot offset used to define the start slot of aperiodic time resource. |
| ***symbolOffset***Indicates symbol offset in one slot. |

– *NCR-AperiodicFwdTimeResourceId*

The IE *NCR-AperiodicFwdTimeResourceId* is used to identify one *NCR-AperiodicFwdTimeResource*.

***NCR-AperiodicFwdTimeResourceId* information element**

-- ASN1START

-- TAG-NCR-APERIODICFWDTIMERESOURCEID-START

NCR-AperiodicFwdTimeResourceId-r18 ::= INTEGER (0..maxNrofAperiodicFwdTimeResource-1-r18)

-- TAG-NCR-APERIODICFWDTIMERESOURCEID-STOP

-- ASN1STOP

*– NCR-PeriodicFwdResourceId*

The IE *NCR-PeriodicFwdResourceId* is used to identify one *NCR-PeriodicFwdResource.*

***NCR-PeriodicFwdResourceId* information element**

-- ASN1START

-- TAG-NCR-PERIODICFWDRESOURCEID-START

NCR-PeriodicFwdResourceId-r18 ::= INTEGER (0..maxNrofPeriodicFwdResource-1-r18)

-- TAG-NCR-PERIODICFWDRESOURCEID-STOP

-- ASN1STOP

– *NCR-PeriodicFwdResourceSet*

The IE *NCR-PeriodicFwdResourceSet* is used to configure a list of periodic forwarding resources for NCR-Fwd access link. Each periodic forwarding configuration includes a list of periodic forwarding resources, a common periodicity and a common reference SCS.

***NCR-PeriodicFwdResourceSet* information element**

-- ASN1START

-- TAG-NCR-PERIODICFWDRESOURCESET-START

NCR-PeriodicFwdResourceSet-r18 ::= SEQUENCE {

 periodicFwdRsrcSetId-r18 NCR-PeriodicFwdResourceSetId-r18

 periodicFwdRsrcToAdddModList-r18 SEQUENCE (SIZE (1..maxNrofPeriodicFwdResource-r18)) OF NCR-PeriodicFwdResource-r18 OPTIONAL, -- Need N

 periodicFwdRsrcToReleaseList-r18 SEQUENCE (SIZE (1..maxNrofPeriodicFwdResource-r18)) OF NCR-PeriodicFwdResourceId-r18 OPTIONAL, -- Need N

 periodicity-r18 ENUMERATED {ffs} OPTIONAL, -- Need M

 referenceSCS-r18 SubcarrierSpacing OPTIONAL, -- Need M

 priorityFlag-r18 ENUMERATED {true} OPTIONAL, -- Need R

 ...

}

NCR-PeriodicFwdResource-r18 ::= SEQUENCE {

 periodicFwdRsrcId-r18 NCR-PeriodicFwdResourceId-r18,

 beamIndex-r18 INTEGER (0..63),

 periodicTimeRsrc-r18 ::= SEQUENCE {

 slotOffsetPeriodic-r18 INTEGER (0..999999),

 symbolOffset-r18 INTEGER (0..maxNrofSymbols-1),

 durationInSymbols-r18 INTEGER (1..112)

 }

}

-- TAG-NCR-PERIODICFWDRESOURCESET-STOP

-- ASN1STOP

|  |
| --- |
| ***NCR-PeriodicFwdResourceSet field descriptions*** |
| ***durationInSymbols***Indicates the time duration in number of symbols. |
| ***beamIndex***Indicates logical beam index for NCR-Fwd access link. NCR-Fwd is assumed to be ON over the indicated time domain resource if there is beam indication. |
| ***periodicFwdRsrcToAdddModList***List of periodic forwarding resources to be added or modified. |
| ***periodicFwdRsrcToReleaseList***List of periodic forwarding resources to be released. |
| ***periodicity***Indicates the periodicity for the list of forwarding resource in [slot]. |
| ***priorityFlag***Indicates the priority for the list of periodic forwarding resource, if present, the list of periodic forwarding resources will have higher priority over aperiodic beam indication. |
| ***referenceSCS***Indicates the reference subcarrier spacing for all the time resource in the list. Only Values *kHz15*, *kHz30*, *kHz60*, *kHz120* and *kHz240* are applicable. |
| ***slotOffsetPeriodic***Indicates slot offset in one period. |
| ***symbolOffset***Indicates symbol offset in one slot. |

– *NCR-PeriodicFwdResourceSetId*

The IE *NCR-PeriodicFwdResourceSetId* is used to identify one *NCR-PeriodicFwdResourceSet*.

***NCR-PeriodicFwdResourceSetId* information element**

-- ASN1START

-- TAG-NCR-PERIODICFWDRESOURCESETID-START

NCR-PeriodicFwdResourceSetId-r18 ::= INTEGER (0..maxNrofPeriodicFwdResourceSet-1-r18)

-- TAG-NCR-PERIODICFWDRESOURCESETID-STOP

-- ASN1STOP

*– NCR-**SemiPersistentFwdResourceId*

The IE *NCR-SemiPersistentFwdResourceId* is used to identify one *NCR-SemiPersistentFwdResource.*

***NCR-SemiPersistentFwdResourceId* information element**

-- ASN1START

-- TAG-NCR-SEMIPERSISTENTFWDRESOURCEID-START

NCR-SemiPersistentFwdResourceId-r18 ::= INTEGER (0..maxNrofSemiPersistentFwdResource-1-r18)

-- TAG-NCR-SEMIPERSISTENTFWDRESOURCEID-STOP

-- ASN1STOP

– *NCR-SemiPersistentFwdResourceSet*

The IE *NCR-SemiPersistentFwdResourceSet* is used to configure a list of semi-persistent forwarding resources for NCR-Fwd access link. Each semi-persistent forwarding resource configuration includes a list of semi-persistent forwarding resources, a common periodicity and a common reference SCS

***NCR-SemiPersistentFwdResourceSet* information element**

-- ASN1START

-- TAG-NCR-SEMIPERSISTENTFWDRESOURCESET-START

NCR-SemiPersistentFwdResourceSet-r18 ::= SEQUENCE {

 semiPersistentFwdRsrcSetId-r18 NCR-SemiPersistentFwdResourceSetId-r18

 semiPersistentFwdRsrcToAdddModList-r18 SEQUENCE (SIZE (1..maxNrofSemiPersistentFwdResource-r18)) OF NCR-SemiPersistentFwdResource-r18 OPTIONAL, -- Need N

 semiPersistentFwdRsrcToReleaseList-r18 SEQUENCE (SIZE (1..maxNrofSemiPersistentFwdResource-r18)) OF NCR-SemiPersistentFwdResourceId-r18 OPTIONAL, -- Need N

 periodicity-r18 ENUMERATED {ffs} OPTIONAL, -- Need M

 referenceSCS-r18 SubcarrierSpacing OPTIONAL, -- Need M

 priorityFlag-r18 ENUMERATED {true} OPTIONAL, -- Need R

 ...

}

NCR-SemiPersistentFwdResource-r18 ::= SEQUENCE {

 semiPersistentFwdRsrcId-r18 NCR-SemiPersistentFwdResourceId-r18

 beamIndex-r18 INTEGER (0..63)

 semiPersistentTimeRsrc-r18 ::= SEQUENCE {

 slotOffsetSemiPersistent-r18 INTEGER (0..999999),

 symbolOffset-r18 INTEGER (0..maxNrofSymbols-1),

 durationInSymbols-r18 INTEGER (1..112)

 }

}

-- TAG-NCR-SEMIPERSISTENTFWDRESOURCESET-STOP

-- ASN1STOP

|  |
| --- |
| ***NCR-SemiPersistentFwdResourceSet field descriptions*** |
| ***durationInSymbols***Indicates the time duration in number of symbols. |
| ***beamIndex***Indicates logical beam index for NCR-Fwd access link. NCR-Fwd is assumed to be ON over the indicated time domain resource if there is beam indication. |
| ***semiPersistentFwdRsrcToAdddModList***List of semi-persistent forwarding resources to be added or modified. |
| ***semiPersistentFwdRsrcToReleaseList***List of semi-persistent forwarding resources to be released. |
| ***periodicity***Indicates the periodicity for the list of forwarding resource in [slot]. |
| ***priorityFlag***Indicates the priority for the list of semi-persistent forwarding resource, if present, the list of semi-persistent forwarding resources will have higher priority over aperiodic beam indication. |
| ***referenceSCS***Indicates the reference subcarrier spacing for all the time resource in the list. Only Values *kHz15*, *kHz30*, *kHz60*, *kHz120* and *kHz240* are applicable. |
| ***slotOffsetSemiPersistent***Indicates slot offset in one period. |
| ***symbolOffset***Indicates symbol offset in one slot. |

– *NCR-SemiPersistentFwdResourceSetId*

The IE *NCR-SemiPersistentFwdResourceSetId* is used to identify one *NCR-SemiPersistentFwdResourceSet*.

***NCR-SemiPersistentFwdResourceSetId* information element**

-- ASN1START

-- TAG-NCR-SEMIPERSISTENTFWDRESOURCESETID-START

NCR-SemiPersistentFwdResourceSetId-r18 ::= INTEGER (0..maxNrofSemiPersistentFwdResourceSet-1-r18)

-- TAG-NCR-SEMIPERSISTENTFWDRESOURCESETID-STOP

-- ASN1STOP

NEXT CHANGE

#### – *NPN-IdentityInfoList*

The IE *NPN-IdentityInfoList* includes a list of NPN identity information.

*NPN-IdentityInfoList* information element

-- ASN1START

-- TAG-NPN-IDENTITYINFOLIST-START

NPN-IdentityInfoList-r16 ::= SEQUENCE (SIZE (1..maxNPN-r16)) OF NPN-IdentityInfo-r16

NPN-IdentityInfo-r16 ::= SEQUENCE {

 npn-IdentityList-r16 SEQUENCE (SIZE (1..maxNPN-r16)) OF NPN-Identity-r16,

 trackingAreaCode-r16 TrackingAreaCode,

 ranac-r16 RAN-AreaCode OPTIONAL, -- Need R

 cellIdentity-r16 CellIdentity,

 cellReservedForOperatorUse-r16 ENUMERATED {reserved, notReserved},

 iab-Support-r16 ENUMERATED {true} OPTIONAL, -- Need S

 ...,

 [[

 gNB-ID-Length-r17 INTEGER (22..32) OPTIONAL -- Need R

 ]]

}

-- TAG-NPN-IDENTITYINFOLIST-STOP

-- ASN1STOP

|  |
| --- |
| *NPN-IdentityInfoList* field descriptions |
| ***iab-Support***This field combines both the support of IAB and the cell status for IAB. If the field is present, the cell supports IAB and the cell is also considered as a candidate for cell (re)selection for IAB-nodes; if the field is absent, the cell does not support IAB and/or the cell is barred for IAB-node. |
| ***gNB-ID-Length***Indicates the length of the gNB ID out of the 36-bit long *cellIdentity*. |
| ***NPN-IdentityInfo***The *NPN-IdentityInfo* contains one or more NPN identities and additional information associated with those NPNs. Only the same type of NPNs (either SNPNs or PNI-NPNs) can be listed in a *NPN-IdentityInfo* element. |
| ***npn-IdentityList***The *npn-IdentityList* contains one or more NPN Identity elements. |
| ***trackingAreaCode***Indicates the Tracking Area Code to which the cell indicated by cellIdentity field belongs.  |
| ***ranac***Indicates the RAN Area Code to which the cell indicated by cellIdentity field belongs.  |
| ***cellReservedForOperatorUse***Indicates whether the cell is reserved for operator use (for the NPN(s) identified in the *npn-IdentityList*) as defined in TS 38.304 [20]. This field is ignored by NPN capable IAB-MT and NPN capable NCR-MT. |

NEXT CHANGE

#### – *PhysicalCellGroupConfig*

The IE *PhysicalCellGroupConfig* is used to configure cell-group specific L1 parameters.

*PhysicalCellGroupConfig* information element

-- ASN1START

-- TAG-PHYSICALCELLGROUPCONFIG-START

PhysicalCellGroupConfig ::= SEQUENCE {

 harq-ACK-SpatialBundlingPUCCH ENUMERATED {true} OPTIONAL, -- Need S

 harq-ACK-SpatialBundlingPUSCH ENUMERATED {true} OPTIONAL, -- Need S

 p-NR-FR1 P-Max OPTIONAL, -- Need R

 pdsch-HARQ-ACK-Codebook ENUMERATED {semiStatic, dynamic},

 tpc-SRS-RNTI RNTI-Value OPTIONAL, -- Need R

 tpc-PUCCH-RNTI RNTI-Value OPTIONAL, -- Need R

 tpc-PUSCH-RNTI RNTI-Value OPTIONAL, -- Need R

 sp-CSI-RNTI RNTI-Value OPTIONAL, -- Need R

 cs-RNTI SetupRelease { RNTI-Value } OPTIONAL, -- Need M

 ...,

 [[

 mcs-C-RNTI RNTI-Value OPTIONAL, -- Need R

 p-UE-FR1 P-Max OPTIONAL -- Cond MCG-Only

 ]],

 [[

 xScale ENUMERATED {dB0, dB6, spare2, spare1} OPTIONAL -- Cond SCG-Only

 ]],

 [[

 pdcch-BlindDetection SetupRelease { PDCCH-BlindDetection } OPTIONAL -- Need M

 ]],

 [[

 dcp-Config-r16 SetupRelease { DCP-Config-r16 } OPTIONAL, -- Need M

 harq-ACK-SpatialBundlingPUCCH-secondaryPUCCHgroup-r16 ENUMERATED {enabled, disabled} OPTIONAL, -- Cond twoPUCCHgroup

 harq-ACK-SpatialBundlingPUSCH-secondaryPUCCHgroup-r16 ENUMERATED {enabled, disabled} OPTIONAL, -- Cond twoPUCCHgroup

 pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup-r16 ENUMERATED {semiStatic, dynamic} OPTIONAL, -- Cond twoPUCCHgroup

 p-NR-FR2-r16 P-Max OPTIONAL, -- Need R

 p-UE-FR2-r16 P-Max OPTIONAL, -- Cond MCG-Only

 nrdc-PCmode-FR1-r16 ENUMERATED {semi-static-mode1, semi-static-mode2, dynamic} OPTIONAL, -- Cond MCG-Only

 nrdc-PCmode-FR2-r16 ENUMERATED {semi-static-mode1, semi-static-mode2, dynamic} OPTIONAL, -- Cond MCG-Only

 pdsch-HARQ-ACK-Codebook-r16 ENUMERATED {enhancedDynamic} OPTIONAL, -- Need R

 nfi-TotalDAI-Included-r16 ENUMERATED {true} OPTIONAL, -- Need R

 ul-TotalDAI-Included-r16 ENUMERATED {true} OPTIONAL, -- Need R

 pdsch-HARQ-ACK-OneShotFeedback-r16 ENUMERATED {true} OPTIONAL, -- Need R

 pdsch-HARQ-ACK-OneShotFeedbackNDI-r16 ENUMERATED {true} OPTIONAL, -- Need R

 pdsch-HARQ-ACK-OneShotFeedbackCBG-r16 ENUMERATED {true} OPTIONAL, -- Need R

 downlinkAssignmentIndexDCI-0-2-r16 ENUMERATED { enabled } OPTIONAL, -- Need S

 downlinkAssignmentIndexDCI-1-2-r16 ENUMERATED {n1, n2, n4} OPTIONAL, -- Need S

 pdsch-HARQ-ACK-CodebookList-r16 SetupRelease {PDSCH-HARQ-ACK-CodebookList-r16} OPTIONAL, -- Need M

 ackNackFeedbackMode-r16 ENUMERATED {joint, separate} OPTIONAL, -- Need R

 pdcch-BlindDetectionCA-CombIndicator-r16 SetupRelease { PDCCH-BlindDetectionCA-CombIndicator-r16 } OPTIONAL, -- Need M

 pdcch-BlindDetection2-r16 SetupRelease { PDCCH-BlindDetection2-r16 } OPTIONAL, -- Need M

 pdcch-BlindDetection3-r16 SetupRelease { PDCCH-BlindDetection3-r16 } OPTIONAL, -- Need M

 bdFactorR-r16 ENUMERATED {n1} OPTIONAL -- Need R

 ]],

 [[

 -- start of enhanced Type3 feedback

 pdsch-HARQ-ACK-EnhType3ToAddModList-r17 SEQUENCE (SIZE(1..maxNrofEnhType3HARQ-ACK-r17)) OF PDSCH-HARQ-ACK-EnhType3-r17

 OPTIONAL, -- Need N

 pdsch-HARQ-ACK-EnhType3ToReleaseList-r17 SEQUENCE (SIZE(1..maxNrofEnhType3HARQ-ACK-r17)) OF PDSCH-HARQ-ACK-EnhType3Index-r17

 OPTIONAL, -- Need N

 pdsch-HARQ-ACK-EnhType3SecondaryToAddModList-r17 SEQUENCE (SIZE(1..maxNrofEnhType3HARQ-ACK-r17)) OF PDSCH-HARQ-ACK-EnhType3-r17

 OPTIONAL, -- Need N

 pdsch-HARQ-ACK-EnhType3SecondaryToReleaseList-r17 SEQUENCE (SIZE(1..maxNrofEnhType3HARQ-ACK-r17)) OF PDSCH-HARQ-ACK-EnhType3Index-r17

 OPTIONAL, -- Need N

 pdsch-HARQ-ACK-EnhType3DCI-FieldSecondaryPUCCHgroup-r17 ENUMERATED {enabled} OPTIONAL, -- Cond twoPUCCHgroup

 pdsch-HARQ-ACK-EnhType3DCI-Field-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 -- end of enhanced Type3 feedback

 -- start of triggering of HARQ-ACK re-transmission on a PUCCH resource

 pdsch-HARQ-ACK-Retx-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 pdsch-HARQ-ACK-RetxSecondaryPUCCHgroup-r17 ENUMERATED {enabled} OPTIONAL, -- Cond twoPUCCHgroup

 -- end of triggering of HARQ-ACK re-transmission on a PUCCH resource

 -- start of PUCCH Cell switching

 pucch-sSCell-r17 SCellIndex OPTIONAL, -- Need R

 pucch-sSCellSecondaryPUCCHgroup-r17 SCellIndex OPTIONAL, -- Cond twoPUCCHgroup

 pucch-sSCellDyn-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 pucch-sSCellDynSecondaryPUCCHgroup-r17 ENUMERATED {enabled} OPTIONAL, -- Cond twoPUCCHgroup

 pucch-sSCellPattern-r17 SEQUENCE (SIZE(1..maxNrofSlots)) OF INTEGER (0..1) OPTIONAL, -- Need R

 pucch-sSCellPatternSecondaryPUCCHgroup-r17 SEQUENCE (SIZE(1..maxNrofSlots)) OF INTEGER (0..1) OPTIONAL, -- Cond twoPUCCHgroup

 -- end of PUCCH Cell switching

 uci-MuxWithDiffPrio-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 uci-MuxWithDiffPrioSecondaryPUCCHgroup-r17 ENUMERATED {enabled} OPTIONAL, -- Cond twoPUCCHgroup

 simultaneousPUCCH-PUSCH-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 simultaneousPUCCH-PUSCH-SecondaryPUCCHgroup-r17 ENUMERATED {enabled} OPTIONAL, -- Cond twoPUCCHgroup

 prioLowDG-HighCG-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 prioHighDG-LowCG-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 twoQCLTypeDforPDCCHRepetition-r17 ENUMERATED {enabled} OPTIONAL, -- Need R

 multicastConfig-r17 SetupRelease { MulticastConfig-r17 } OPTIONAL, -- Need M

 pdcch-BlindDetectionCA-CombIndicator-r17 SetupRelease { PDCCH-BlindDetectionCA-CombIndicator-r17 } OPTIONAL -- Need M

 ]],

 [[

 simultaneousSR-PUSCH-diffPUCCH-Groups-r17 ENUMERATED {enabled} OPTIONAL -- Cond twoPUCCHgroup

 ]],

 [[

 intraBandNC-PRACH-simulTx-r17 ENUMERATED {enabled} OPTIONAL -- Need R

 ]],

 [[

 ncr-RNTI-r18 RNTI-Value OPTIONAL, -- Cond NCR

 ]]

}

PDSCH-HARQ-ACK-EnhType3-r17 ::= SEQUENCE {

 pdsch-HARQ-ACK-EnhType3Index-r17 PDSCH-HARQ-ACK-EnhType3Index-r17,

 applicable-r17 CHOICE {

 perCC SEQUENCE (SIZE (1..maxNrofServingCells)) OF INTEGER (0..1),

 perHARQ SEQUENCE (SIZE (1..maxNrofServingCells)) OF BIT STRING (SIZE (16))

 },

 pdsch-HARQ-ACK-EnhType3NDI-r17 ENUMERATED {true} OPTIONAL, -- Need R

 pdsch-HARQ-ACK-EnhType3CBG-r17 ENUMERATED {true} OPTIONAL, -- Need S

 ...

}

PDSCH-HARQ-ACK-EnhType3Index-r17 ::= INTEGER (0..maxNrofEnhType3HARQ-ACK-1-r17)

PDCCH-BlindDetection ::= INTEGER (1..15)

DCP-Config-r16 ::= SEQUENCE {

 ps-RNTI-r16 RNTI-Value,

 ps-Offset-r16 INTEGER (1..120),

 sizeDCI-2-6-r16 INTEGER (1..maxDCI-2-6-Size-r16),

 ps-PositionDCI-2-6-r16 INTEGER (0..maxDCI-2-6-Size-1-r16),

 ps-WakeUp-r16 ENUMERATED {true} OPTIONAL, -- Need S

 ps-TransmitPeriodicL1-RSRP-r16 ENUMERATED {true} OPTIONAL, -- Need S

 ps-TransmitOtherPeriodicCSI-r16 ENUMERATED {true} OPTIONAL -- Need S

}

PDSCH-HARQ-ACK-CodebookList-r16 ::= SEQUENCE (SIZE (1..2)) OF ENUMERATED {semiStatic, dynamic}

PDCCH-BlindDetectionCA-CombIndicator-r16 ::= SEQUENCE {

 pdcch-BlindDetectionCA1-r16 INTEGER (1..15),

 pdcch-BlindDetectionCA2-r16 INTEGER (1..15)

}

PDCCH-BlindDetection2-r16 ::= INTEGER (1..15)

PDCCH-BlindDetection3-r16 ::= INTEGER (1..15)

MulticastConfig-r17 ::= SEQUENCE {

 pdsch-HARQ-ACK-CodebookListMulticast-r17 SetupRelease { PDSCH-HARQ-ACK-CodebookList-r16} OPTIONAL, -- Need M

 type1CodebookGenerationMode-r17 ENUMERATED { mode1, mode2} OPTIONAL -- Need M

}

PDCCH-BlindDetectionCA-CombIndicator-r17 ::= SEQUENCE {

 pdcch-BlindDetectionCA1-r17 INTEGER (1..15) OPTIONAL, -- Need R

 pdcch-BlindDetectionCA2-r17 INTEGER (1..15) OPTIONAL, -- Need R

 pdcch-BlindDetectionCA3-r17 INTEGER (1..15)

}

-- TAG-PHYSICALCELLGROUPCONFIG-STOP

-- ASN1STOP

|  |
| --- |
| *PhysicalCellGroupConfig* field descriptions |
| ***ackNackFeedbackMode***Indicates which among the joint and separate ACK/NACK feedback modes to use within a slot as specified in TS 38.213 [13] (clause 9). |
| ***bdFactorR***Parameter for determining and distributing the maximum numbers of BD/CCE for mPDCCH based mPDSCH transmission as specified in TS 38.213 [13] Clause 10.1. |
| ***cs-RNTI***RNTI value for downlink SPS (see *SPS-Config*) and uplink configured grant (see *ConfiguredGrantConfig*). |
| ***downlinkAssignmentIndexDCI-0-2***Indicates if "Downlink assignment index" is present or absent in DCI format 0\_2. If the field "*downlinkAssignmentIndexDCI-0-2*" is absent, then 0 bit for "Downlink assignment index" in DCI format 0\_2. If the field "*downlinkAssignmentIndexDCI-0-2*" is present, then the bitwidth of "Downlink assignment index" in DCI format 0\_2 is defined in the same was as that in DCI format 0\_1 (see TS 38.212 [17], clause 7.3.1 and TS 38.213 [13], clause 9.1). |
| ***downlinkAssignmentIndexDCI-1-2***Configures the number of bits for "Downlink assignment index" in DCI format 1\_2. If the field is absent, then 0 bit is applied for "Downlink assignment index" in DCI format 1\_2. Note that 1 bit and 2 bits are applied if only one serving cell is configured in the DL and *pdsch-HARQ-ACK-Codebook* is set to *dynamic*. 4 bits is applied if more than one serving cell are configured in the DL and *pdsch-HARQ-ACK-Codebook* is set to *dynamic* (see TS 38.212 [17], clause 7.3.1 and TS 38.213 [13], clause 9.1). |
| ***harq-ACK-SpatialBundlingPUCCH***Enables spatial bundling of HARQ ACKs. It is configured per cell group (i.e. for all the cells within the cell group) for PUCCH reporting of HARQ-ACK. It is only applicable when more than 4 layers are possible to schedule. When the field is absent, the spatial bundling of PUCCH HARQ ACKs for the primary PUCCH group is disabled (see TS 38.213 [13], clause 9.1.2.1). If the field *harq-ACK SpatialBundlingPUCCH-secondaryPUCCHgroup* is present, *harq-ACK-SpatialBundlingPUCCH* is only applied to primary PUCCH group. Network does not configure for a UE both spatial bundling of HARQ ACKs and *codeBlockGroupTransmission* within the same cell group. |
| ***harq-ACK-SpatialBundlingPUCCH-secondaryPUCCHgroup***Indicates whether spatial bundling of PUCCH HARQ ACKs for the secondary PUCCH group is enabled or disabled. The field is only applicable when more than 4 layers are possible to schedule (see TS 38.213 [13], clause 9.1.2.1). When the field is absent, the use of spatial bundling of PUCCH HARQ ACKs for the secondary PUCCH group is indicated by *harq-ACK-SpatialBundlingPUCCH*. See TS 38.213 [13], clause 9.1.2.1. Network does not configure for a UE both spatial bundling of HARQ ACKs and *codeBlockGroupTransmission* within the same cell group. |
| ***harq-ACK-SpatialBundlingPUSCH***Enables spatial bundling of HARQ ACKs. It is configured per cell group (i.e. for all the cells within the cell group) for PUSCH reporting of HARQ-ACK. It is only applicable when more than 4 layers are possible to schedule. When the field is absent, the spatial bundling of PUSCH HARQ ACKs for the primary PUCCH group is disabled (see TS 38.213 [13], clauses 9.1.2.2 and 9.1.3.2). If the field *harq-ACK SpatialBundlingPUSCH-secondaryPUCCHgroup* is present, *harq-ACK-SpatialBundlingPUSCH* is only applied to primary PUCCH group. Network does not configure for a UE both spatial bundling of HARQ ACKs and *codeBlockGroupTransmission* within the same cell group. |
| ***harq-ACK-SpatialBundlingPUSCH-secondaryPUCCHgroup***Indicates whether spatial bundling of PUSCH HARQ ACKs for the secondary PUCCH group is enabled or disabled. The field is only applicable when more than 4 layers are possible to schedule (see TS 38.213 [13], clauses 9.1.2.2 and 9.1.3.2). When the field is absent, the use of spatial bundling of PUSCH HARQ ACKs for the secondary PUCCH group is indicated by *harq-ACK-SpatialBundlingPUSCH*. See TS 38.213 [13], clauses 9.1.2.2 and 9.1.3.2. Network does not configure for a UE both spatial bundling of HARQ ACKs and *codeBlockGroupTransmission* within the same cell group. |
| ***intraBandNC-PRACH-simulTx***Enables parallel PRACH and SRS/PUCCH/PUSCH transmissions across CCs in intra-band non-contiguous CA (see TS 38.213 [13], clause 8.1 and TS 38.214 [19], clause 6.2.1). This field is absent in the IE *CellGroupConfig* when provided as part of *RRCSetup* message. |
| ***mcs-C-RNTI***RNTI to indicate use of *qam64LowSE* for grant-based transmissions. When the *mcs*-*C-RNTI* is configured, RNTI scrambling of DCI CRC is used to choose the corresponding MCS table. |
| ***ncr-RNTI***RNTI value for NCR-MT, used to scramble the PDCCHs carrying side control information (see TS 38.213 [13], clause [10.1]). |
| ***nfi-TotalDAI-Included***Indicates whether the NFI and total DAI fields of the non-scheduled PDSCH group is included in the non-fallback DL grant DCI (see TS 38.212 [17], clause 7.3.1). The network configures this only when enhanced dynamic codebook is configured (*pdsch-HARQ-ACK-Codebook* is set to *enhancedDynamic*). |
| ***nrdc-PCmode-FR1***Indicates the uplink power sharing mode that the UE uses in NR-DC in frequency range 1 (FR1) (see TS 38.213 [13], clause 7.6). |
| ***nrdc-PCmode-FR2***Indicates the uplink power sharing mode that the UE uses in NR-DC in frequency range 2 (FR2) (see TS 38.213 [13], clause 7.6). |
| ***pdcch-BlindDetection, pdcch-BlindDetection2, pdcch-BlindDetection3***Indicates the reference number of cells for PDCCH blind detection for the CG. Network configures the field for each CG when the UE is in NR DC and sets the value in accordance with the constraints specified in TS 38.213 [13]. The network configures *pdcch-BlindDetection* only if the UE is in NR-DC. The network configures *pdcch-BlindDetection2* only if the UE is in NR-DC with at least one downlink cell using Rel-16 PDCCH monitoring capability. The network configures *pdcch-BlindDetection3* only if the UE is in NR-DC with at least one downlink cell using Rel-15 PDCCH monitoring capability. |
| ***pdcch-BlindDetectionCA-CombIndicator***Configure one combination of *pdcch-BlindDetectionCA1* (for R15) and *pdcch-BlindDetectionCA2* (for R16) for UE to use for scaling PDCCH monitoring capability if the number of serving cells configured to a UE is larger than the reported capability, and if UE reports more than one combination of *pdcch-BlindDetectionCA1* and *pdcch-BlindDetectionCA2* as UE capability. The combination of *pdcch-BlindDetectionCA1* and *pdcch-BlindDetectionCA2* configured by *pdcch-BlindDetectionCA-CombIndicator* is from the more than one combination of *pdcch-BlindDetectionCA1* and *pdcch-BlindDetectionCA2* reported by UE (see TS 38.213 [13], clause 10).*pdcch-BlindDetectionCA-CombIndicator-r17* is used to configure one combination of *pdcch-BlindDetectionCA1* (for R15), *pdcch-BlindDetectionCA2* (for R16) and *pdcch-BlindDetectionCA3* (for R17) for UE to use for scaling PDCCH monitoring capability if the number of serving cells configured to a UE is larger than the reported capability, and if UE reports more than one combination of *pdcch-BlindDetectionCA1*, *pdcch-BlindDetectionCA2* and *pdcch-BlindDetectionCA3* as UE capability. The combination of *pdcch-BlindDetectionCA1*, *pdcch-BlindDetectionCA2* and *pdcch-BlindDetectionCA3* configured by *pdcch-BlindDetectionCA-CombIndicator-r17* is from the more than one combination of *pdcch-BlindDetectionCA1*, *pdcch-BlindDetectionCA2* and *pdcch-BlindDetectionCA3* reported by UE (see TS 38.213 [13], clause 10).*pdcch-BlindDetectionCA-CombIndicator-r16* and *pdcch-BlindDetectionCA-CombIndicator-r17* are not configured simultaneously. |
| ***p-NR-FR1***The maximum total transmit power to be used by the UE in this NR cell group across all serving cells in frequency range 1 (FR1). The maximum transmit power that the UE may use may be additionally limited by *p-Max* (configured in *FrequencyInfoUL*) and by *p-UE-FR1* (configured total for all serving cells operating on FR1). |
| ***p-NR-FR2***The maximum total transmit power to be used by the UE in this NR cell group across all serving cells in frequency range 2 (FR2). The maximum transmit power that the UE may use may be additionally limited by *p-Max* (configured in *FrequencyInfoUL*) and by *p-UE-FR2* (configured total for all serving cells operating on FR2). This field is only used in NR-DC. A UE does not expect to be configured with this parameter in this release of the specification. |
| ***prioLowDG-HighCG***Enable PHY prioritization for the case where low-priority dynamic grant-PUSCH collides with high-priority configured grant-PUSCH on a BWP of a serving cell (see TS 38.213 [13], clause 9), when the UE has generated transport blocks for both DG-PUSCH and CG-PUSCH as described in TS 38.321 [3]. |
| ***prioHighDG-LowCG***Enable PHY prioritization for the case where high-priority dynamic grant PUSCH collides with low-priority configured grant PUSCH on a BWP of a serving cell (see TS 38.213 [13], clause 9), when the UE has generated transport blocks for both DG-PUSCH and CG-PUSCH as described in TS 38.321 [3]. |
| ***ps-RNTI***RNTI value for scrambling CRC of DCI format 2-6 used for power saving (see TS 38.213 [13], clause 10.1). |
| ***ps-Offset***The start of the search-time of DCI format 2-6 with CRC scrambled by PS-RNTI relative to the start of the *drx-onDurationTimer* of Long DRX (see TS 38.213 [13], clause 10.3). Value in multiples of 0.125ms (milliseconds). 1 corresponds to 0.125 ms, 2corresponds to 0.25 ms, 3 corresponds to 0.375 ms and so on. |
| ***ps-WakeUp***Indicates the UE to wake-up if DCI format 2-6 is not detected outside active time (see TS 38.321 [3], clause 5.7). If the field is absent, the UE does not wake-up if DCI format 2-6 is not detected outside active time. |
| ***ps-PositionDCI-2-6***Starting position of UE wakeup and SCell dormancy indication in DCI format 2-6 (see TS 38.213 [13], clause 10.3). |
| ***ps-TransmitPeriodicL1-RSRP***Indicates the UE to transmit periodic L1-RSRP report(s) when the *drx-onDurationTimer* does not start (see TS 38.321 [3], clause 5.7). If the field is absent, the UE does not transmit periodic L1-RSRP report(s) when the *drx-onDurationTimer* does not start. |
| ***ps-TransmitOtherPeriodicCSI***Indicates the UE to transmit periodic CSI report(s) other than L1-RSRP reports when the *drx-onDurationTimer* does not start (see TS 38.321 [3], clause 5.7). If the field is absent, the UE does not transmit periodic CSI report(s) other than L1-RSRP reports when the *drx-onDurationTimer* does not start. |
| ***p-UE-FR1***The maximum total transmit power to be used by the UE across all serving cells in frequency range 1 (FR1) across all cell groups. The maximum transmit power that the UE may use may be additionally limited by *p-Max* (configured in *FrequencyInfoUL*) and by *p-NR-FR1* (configured for the cell group). |
| ***p-UE-FR2***The maximum total transmit power to be used by the UE across all serving cells in frequency range 2 (FR2) across all cell groups. The maximum transmit power that the UE may use may be additionally limited by *p-Max* (configured in *FrequencyInfoUL*) and by p-NR-FR2 (configured for the cell group). A UE does not expect to be configured with this parameter in this release of the specification. |
| ***pdsch-HARQ-ACK-Codebook***The PDSCH HARQ-ACK codebook is either semi-static or dynamic. This is applicable to both CA and non-CA operation (see TS 38.213 [13], clauses 9.1.2 and 9.1.3). If *pdsch-HARQ-ACK-Codebook-r16* is signalled, UE shall ignore the *pdsch-HARQ-ACK-Codebook* (without suffix). For the HARQ-ACK for sidelink, if *pdsch-HARQ-ACK-Codebook-r16* is signalled, the UE uses *pdsch-HARQ-ACK-Codebook* (without suffix) and ignores *pdsch-HARQ-ACK-Codebook-r16*. If the field *pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup* is present, *pdsch-HARQ-ACK-Codebook* is applied to primary PUCCH group. Otherwise, this field is applied to the cell group (i.e. for all the cells within the cell group). For the HARQ-ACK for sidelink, if the field *pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup* is present, *pdsch-HARQ-ACK-Codebook* is applied to primary and secondary PUCCH group and the UE ignores *pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup*. |
| ***pdsch-HARQ-ACK-CodebookList***A list of configurations for one or two HARQ-ACK codebooks. Each configuration in the list is defined in the same way as *pdsch-HARQ-ACK-Codebook* (see TS 38.212 [17], clause 7.3.1.2.2 and TS 38.213 [13], clauses 7.2.1, 9.1.2, 9.1.3 and 9.2.1). If this field is present, the field *pdsch-HARQ-ACK-Codebook* is ignored. If this field is present, the value of this field is applied for primary PUCCH group and for secondary PUCCH group (if configured). For the HARQ-ACK for sidelink, the UE uses *pdsch-HARQ-ACK-Codebook* and ignores *pdsch-HARQ-ACK-CodebookList* if this field is present. |
| ***pdsch-HARQ-ACK-Codebook-secondaryPUCCHgroup***The PDSCH HARQ-ACK codebook is either semi-static or dynamic. This is applicable to CA operation (see TS 38.213 [13], clauses 9.1.2 and 9.1.3). It is configured for secondary PUCCH group*.* |
| ***pdsch-HARQ-ACK-EnhType3DCI-Field, pdsch-HARQ-ACK-EnhType3DCI-FieldSecondaryPUCCHgroup***Indicates the enhanced Type 3 codebook through a new DCI field to indicate the enhanced Type 3 HARQ-ACK codebook in the primary PUCCH group if the more than one enhanced Type 3 HARQ-ACK codebook is configured for the primary PUCCH group, or in the secondary PUCCH group if the more than one enhanced Type 3 HARQ-ACK code is configured for the secondary PUCCH group, respectively. |
| ***pdsch-HARQ-ACK-EnhType3ToAddModList, pdsch-HARQ-ACK-EnhType3SecondaryToAddModList***Configure the list of enhanced Type 3 HARQ-ACK codebooks for the primary PUCCH group and the secondary PUCCH group, respectively. When configured, DCI format 1\_1 can request the UE to report A/N for one of the configured enhanced Type 3 HARQ-ACK codebooks in the corresponding PUCCH group (see TS 38.213 [13], clause 9.1.4). The network can configure *pdsch-HARQ-ACK-EnhType3SecondaryToAddModList* only if secondary PUCCH group is configured. |
| ***pdsch-HARQ-ACK-OneShotFeedback***When configured, the DCI format 1\_1 can request the UE to report A/N for all HARQ processes and all CCs configured in the PUCCH group (see TS 38.212 [17], clause 7.3.1). |
| ***pdsch-HARQ-ACK-OneShotFeedbackCBG***When configured, the DCI format 1\_1 can request the UE to include CBG level A/N for each CC with CBG level transmission configured. When not configured, the UE will report TB level A/N even if CBG level transmission is configured for a CC.The network configures this only when *pdsch-HARQ-ACK-OneShotFeedback* is configured. |
| ***pdsch-HARQ-ACK-OneShotFeedbackNDI***When configured, the DCI format 1\_1 can request the UE to include NDI for each A/N reported.The network configures this only when *pdsch-HARQ-ACK-OneShotFeedback* is configured. |
| ***pdsch-HARQ-ACK-Retx, pdsch-HARQ-ACK-RetxSecondaryPUCCHgroup***When configured, the DCI format 1\_1 can request the UE to perform a HARQ-ACK re-transmission on a PUCCH resource in the primary PUCCH group and the secondary PUCCH group, respectively (see TS 38.213 [13], clause 9.1.5). |
| ***pucch-sSCell, pucch-sSCellSecondaryPUCCHgroup***indictates the alternative PUCCH cells for PUCCH cell switching in the primary and the secondary PUCCH group, respectively. For the primary PUCCH group, it is configured for cells on top of SpCell. For the secondary PUCCH group, it is configured for cell on top of the PUCCH SCell. |
| ***pucch-sSCellDyn, pucch-sSCellDynsecondaryPUCCHgroup***When configured, PUCCH cell switching based on dynamic indication in DCI format 1\_1 is enabled (see TS 38.213 [13], clause 9.A, clause 9.1.5), respectively for the primary PUCCH group and the secondary PUCCH group. |
| ***pucch-sSCellPattern, pucch-sSCellPatternSecondaryPUCCHgroup***When configured, the UE applies the semi-static PUCCH cell switching (see TS 38.213 [13], clause 9.A) using the time domain pattern of applicable PUCCH cells indicated by this field, respectively for the primary PUCCH group and the secondary PUCCH group. |
| ***simultaneousPUCCH-PUSCH, simultaneousPUCCH-PUSCH-SecondaryPUCCHgroup***Enables simultaneous PUCCH and PUSCH transmissions with different priorities for the primary PUCCH group and the secondary PUCCH group, respectively. |
| ***simultaneousSR-PUSCH-diffPUCCH-Groups***Enables simultaneous SR and PUSCH transmissions in different PUCCH groups (see TS 38.321 [3], clause 5.4.1, clause 5.4.4). |
| ***sizeDCI-2-6***Size of DCI format 2-6 (see TS 38.213 [13], clause 10.3). |
| ***sp-CSI-RNTI***RNTI for Semi-Persistent CSI reporting on PUSCH (see *CSI-ReportConfig*) (see TS 38.214 [19], clause 5.2.1.5.2). Network always configures the UE with a value for this field when at least one *CSI-ReportConfig* with *reportConfigType* set to *semiPersistentOnPUSCH* is configured. |
| ***tpc-PUCCH-RNTI***RNTI used for PUCCH TPC commands on DCI (see TS 38.213 [13], clause 10.1). |
| ***tpc-PUSCH-RNTI***RNTI used for PUSCH TPC commands on DCI (see TS 38.213 [13], clause 10.1). |
| ***tpc-SRS-RNTI***RNTI used for SRS TPC commands on DCI (see TS 38.213 [13], clause 10.1). |
| ***twoQCLTypeDforPDCCHRepetition***Indicates whether a UE is expected UE to identify and monitor two QCL-TypeD properties for multiple overlapping CORESETs in the case of PDCCH repetition. |
| ***uci-MuxWithDiffPrio, uci-MuxWithDiffPrio-secondaryPUCCHgroup***When configured, enables multiplexing a high-priority (HP) HARQ-ACK UCI and a low-priority (LP) HARQ-ACK UCI into a PUCCH or PUSCH for the primary PUCCH group and the secondary PUCCH group, respectively. |
| ***ul-TotalDAI-Included***Indicates whether the total DAI fields of the additional PDSCH group is included in the non-fallback UL grant DCI (see TS 38.212 [17], clause 7.3.1). The network configures this only when enhanced dynamic codebook is configured (*pdsch-HARQ-ACK-Codebook* is set to *enhancedDynamic*). |
| ***xScale***The UE is allowed to drop NR only if the power scaling applied to NR results in a difference between scaled and unscaled NR UL of more than *xScale* dB (see TS 38.213 [13]). If the value is not configured for dynamic power sharing, the UE assumes default value of 6 dB. |

|  |
| --- |
| *MulticastConfig* field descriptions |
| ***pdsch-HARQ-ACK-CodebookListMulticast***A list of configurations for one or two HARQ-ACK codebooks for MBS multicast. Each configuration in the list is defined in the same way as *pdsch-HARQ-ACK-Codebook* (see TS 38.212 [17], clause 7.3.1.2.2 and TS 38.213 [13], clauses 7.2.1, 9.1.2, 9.1.3 and 9.2.1). If this field is present, the field *pdsch-HARQ-ACK-Codebook* is ignored. If this field is present, the value of this field is applied for primary PUCCH group and for secondary PUCCH group (if configured). |
| ***type1CodebookGenerationMode***Indicates the mode of Type-1 HARQ-ACK codebook generation, as specified in TS 38.213 [13]. Mode 1 is based on the k1 values that are in the intersection of K1 set for unicast and K1 set for multicast. Mode 2 is based on the k1 values that are in the union of K1 set for unicast and K1 set for multicast. |

|  |
| --- |
| *PDSCH-HARQ-ACK-EnhType3* field descriptions |
| ***pdsch-HARQ-ACK-EnhType3CBG***When configured, the DCI format 1\_1 or DCI format 1\_2 can request the UE to include CBG level A/N for each CC with CBG level transmission configured of the enhanced Type 3 HARQ-ACK codebook. When not configured, the UE will report TB level A/N even if CBG level transmission is configured for a CC. |
| ***pdsch-HARQ-ACK-EnhType3NDI***When configured, the DCI format 1\_1 or DCI format 1\_2 can request the UE to include NDI for each A/N reported of the enhanced Type 3 HARQ-ACK codebook. |
| ***perCC***Configures enhanced Type 3 HARQ-ACK codebook using per CC configuration. |
| ***perHARQ***Configures enhanced Type 3 HARQ-ACK codebook using per HARQ process and CC configuration. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *MCG-Only* | This field is optionally present, Need R, in the *PhysicalCellGroupConfig* of the MCG. It is absent otherwise.  |
| *NCR* | This field is optionally present, Need M for NCR-MT. It is absent otherwise. |
| *SCG-Only* | This field is optionally present, Need S, in the *PhysicalCellGroupConfig* of the SCG in (NG)EN-DC as defined in TS 38.213 [13]. It is absent otherwise. |
| *twoPUCCHgroup* | This field is optionally present, Need R, if secondary PUCCH group is configured. It is absent otherwise, Need R.  |

NEXT CHANGE

#### – *PLMN-IdentityInfoList*

The IE *PLMN-IdentityInfoList* includes a list of PLMN identity information.

*PLMN-IdentityInfoList* information element

-- ASN1START

-- TAG-PLMN-IDENTITYINFOLIST-START

PLMN-IdentityInfoList ::= SEQUENCE (SIZE (1..maxPLMN)) OF PLMN-IdentityInfo

PLMN-IdentityInfo ::= SEQUENCE {

 plmn-IdentityList SEQUENCE (SIZE (1..maxPLMN)) OF PLMN-Identity,

 trackingAreaCode TrackingAreaCode OPTIONAL, -- Need R

 ranac RAN-AreaCode OPTIONAL, -- Need R

 cellIdentity CellIdentity,

 cellReservedForOperatorUse ENUMERATED {reserved, notReserved},

 ...,

 [[

 iab-Support-r16 ENUMERATED {true} OPTIONAL -- Need S

 ]],

 [[

 trackingAreaList-r17 SEQUENCE (SIZE (1..maxTAC-r17)) OF TrackingAreaCode OPTIONAL, -- Need R

 gNB-ID-Length-r17 INTEGER (22..32) OPTIONAL -- Need R

 ]]

}

-- TAG-PLMN-IDENTITYINFOLIST-STOP

-- ASN1STOP

|  |
| --- |
| *PLMN-IdentityInfo* field descriptions |
| ***cellReservedForOperatorUse***Indicates whether the cell is reserved for operator use (per PLMN), as defined in TS 38.304 [20]. This field is ignored by IAB-MT and NCR-MT. |
| ***gNB-ID-Length***Indicates the length of the gNB ID out of the 36-bit long *cellIdentity*. |
| ***iab-Support***This field combines both the support of IAB and the cell status for IAB. If the field is present, the cell supports IAB and the cell is also considered as a candidate for cell (re)selection for IAB-node; if the field is absent, the cell does not support IAB and/or the cell is barred for IAB-node. |
| ***trackingAreaCode***Indicates Tracking Area Code to which the cell indicated by *cellIdentity* field belongs. The absence of the field indicates that the cell only supports PSCell/SCell functionality (per PLMN) or is an NTN cell. |
| ***trackingAreaList***List of Tracking Areas to which the cell indicated by *cellIdentity* field belongs. If this field is present, network does not configure *trackingAreaCode.* Total number of different TACs across different *PLMN-IdentityInfo*s shall not exceed *maxTAC*. This field is only present in an NTN cell. |

NEXT CHANGE

#### – *RadioBearerConfig*

The IE *RadioBearerConfig* is used to add, modify and release signalling, multicast MRBs and/or data radio bearers. Specifically, this IE carries the parameters for PDCP and, if applicable, SDAP entities for the radio bearers.

*RadioBearerConfig* information element

-- ASN1START

-- TAG-RADIOBEARERCONFIG-START

RadioBearerConfig ::= SEQUENCE {

 srb-ToAddModList SRB-ToAddModList OPTIONAL, -- Cond HO-Conn

 srb3-ToRelease ENUMERATED{true} OPTIONAL, -- Need N

 drb-ToAddModList DRB-ToAddModList OPTIONAL, -- Cond HO-toNR

 drb-ToReleaseList DRB-ToReleaseList OPTIONAL, -- Need N

 securityConfig SecurityConfig OPTIONAL, -- Need M

 ...,

 [[

 mrb-ToAddModList-r17 MRB-ToAddModList-r17 OPTIONAL, -- Need N

 mrb-ToReleaseList-r17 MRB-ToReleaseList-r17 OPTIONAL, -- Need N

 srb4-ToAddMod-r17 SRB-ToAddMod OPTIONAL, -- Need N

 srb4-ToRelease-r17 ENUMERATED{true} OPTIONAL -- Need N

 ]]

}

SRB-ToAddModList ::= SEQUENCE (SIZE (1..2)) OF SRB-ToAddMod

SRB-ToAddMod ::= SEQUENCE {

 srb-Identity SRB-Identity,

 reestablishPDCP ENUMERATED{true} OPTIONAL, -- Need N

 discardOnPDCP ENUMERATED{true} OPTIONAL, -- Need N

 pdcp-Config PDCP-Config OPTIONAL, -- Cond PDCP

 ...,

 [[

 srb-Identity-v1700 SRB-Identity-v1700 OPTIONAL -- Need M

 ]]

}

DRB-ToAddModList ::= SEQUENCE (SIZE (1..maxDRB)) OF DRB-ToAddMod

DRB-ToAddMod ::= SEQUENCE {

 cnAssociation CHOICE {

 eps-BearerIdentity INTEGER (0..15),

 sdap-Config SDAP-Config

 } OPTIONAL, -- Cond DRBSetup

 drb-Identity DRB-Identity,

 reestablishPDCP ENUMERATED{true} OPTIONAL, -- Need N

 recoverPDCP ENUMERATED{true} OPTIONAL, -- Need N

 pdcp-Config PDCP-Config OPTIONAL, -- Cond PDCP

 ...,

 [[

 daps-Config-r16 ENUMERATED{true} OPTIONAL -- Cond DAPS

 ]]

}

DRB-ToReleaseList ::= SEQUENCE (SIZE (1..maxDRB)) OF DRB-Identity

SecurityConfig ::= SEQUENCE {

 securityAlgorithmConfig SecurityAlgorithmConfig OPTIONAL, -- Cond RBTermChange1

 keyToUse ENUMERATED{master, secondary} OPTIONAL, -- Cond RBTermChange

 ...

}

MRB-ToAddModList-r17 ::= SEQUENCE (SIZE (1..maxMRB-r17)) OF MRB-ToAddMod-r17

MRB-ToAddMod-r17 ::= SEQUENCE {

 mbs-SessionId-r17 TMGI-r17 OPTIONAL, -- Cond MRBSetup

 mrb-Identity-r17 MRB-Identity-r17,

 mrb-IdentityNew-r17 MRB-Identity-r17 OPTIONAL, -- Need N

 reestablishPDCP-r17 ENUMERATED{true} OPTIONAL, -- Need N

 recoverPDCP-r17 ENUMERATED{true} OPTIONAL, -- Need N

 pdcp-Config-r17 PDCP-Config OPTIONAL, -- Cond PDCP

 ...

}

MRB-ToReleaseList-r17 ::= SEQUENCE (SIZE (1..maxMRB-r17)) OF MRB-Identity-r17

-- TAG-RADIOBEARERCONFIG-STOP

-- ASN1STOP

|  |
| --- |
| *DRB-ToAddMod* and *MRB-ToAddMod* field descriptions |
| ***cnAssociation***Indicates if the bearer is associated with the *eps-bearerIdentity* (when connected to EPC) or *sdap-Config* (when connected to 5GC). |
| ***daps-Config***Indicates that the bearer is configured as DAPS bearer. |
| ***drb-Identity***In case of DC, the DRB identity is unique within the scope of the UE, i.e. an MCG DRB cannot use the same value as a split DRB. For a split DRB the same identity is used for the MCG and SCG parts of the configuration. |
| ***eps-BearerIdentity***The EPS bearer ID determines the EPS bearer. |
| ***mbs-SessionId***Indicates which multicast MBS session the bearer is associated with. |
| ***mrb-Identity***Identification of the multicast MRB. |
| ***mrb-IdentityNew***New identity of the multicast MRB when *mrb-Identity* needs to be changed, e.g. as a result of a handover. |
| ***reestablishPDCP***Indicates that PDCP should be re-established. Network sets this to *true* whenever the security key used for this radio bearer changes. Key change could for example be due to termination point change for the bearer, reconfiguration with sync, resuming an RRC connection, or the first reconfiguration after reestablishment. It is also applicable for LTE procedures when NR PDCP is configured. Network doesn't include this field for DRB if the bearer is configured as DAPS bearer. |
| ***recoverPDCP***Indicates that PDCP should perform recovery according to TS 38.323 [5]. Network doesn't include this field if the bearer is configured as DAPS bearer. |
| ***sdap-Config***The SDAP configuration determines how to map QoS flows to DRBs when NR or E-UTRA connects to the 5GC and presence/absence of UL/DL SDAP headers. |

|  |
| --- |
| *RadioBearerConfig* field descriptions |
| ***securityConfig***Indicates the security algorithm and key to use for the signalling and data radio bearers configured with the list in this IE *RadioBearerConfig*. When the field is not included after AS security has been activated, the UE shall continue to use the currently configured *keyToUse* and security algorithm for the radio bearers reconfigured with the lists in this IE *RadioBearerConfig*. The field is not included when configuring SRB1 before AS security is activated. |
| ***srb3-ToRelease***Release SRB3. SRB3 release can only be done over SRB1 and only at SCG release and reconfiguration with sync. |

|  |
| --- |
| *SecurityConfig* field descriptions |
| ***keyToUse***Indicates if the bearers configured with the list in this IE *RadioBearerConfig* are using the master key or the secondary key for deriving ciphering and/or integrity protection keys. For MR-DC, network should not configure SRB1 and SRB2 with secondary key and SRB3 with the master key. When the field is not included, the UE shall continue to use the currently configured *keyToUse* for the radio bearers reconfigured with the lists in this IE *RadioBearerConfig*. |
| ***securityAlgorithmConfig***Indicates the security algorithm for the signalling and data radio bearers configured with the list in this IE *RadioBearerConfig*. When the field is not included, the UE shall continue to use the currently configured security algorithm for the radio bearers reconfigured with the lists in this IE *RadioBearerConfig*. |

|  |
| --- |
| *SRB-ToAddMod* field descriptions |
| ***discardOnPDCP***Indicates that PDCP should discard stored SDU and PDU according to TS 38.323 [5]. |
| ***reestablishPDCP***Indicates that PDCP should be re-established. Network sets this to *true* whenever the security key used for this radio bearer changes. Key change could for example be due to reconfiguration with sync, for SRB2 when resuming an RRC connection, or at the first reconfiguration after RRC connection reestablishment in NR. For SRB1, when resuming an RRC connection, or at the first reconfiguration after RRC connection reestablishment in NR, the network does not set this field to *true*. For LTE SRBs using NR PDCP, it could be for handover, RRC connection reestablishment or resume. Network doesn't include this field if any DAPS bearer is configured. |
| ***srb-Identity, srb-Identity-v1700***Value 1 is applicable for SRB1 only. Value 2 is applicable for SRB2 only. Value 3 is applicable for SRB3 only. Value 4 is applicable for SRB4 only. If *srb-Identity-v1700* is received for an SRB, the UE shall ignore *srb-Identity* (i.e. without suffix) for this SRB. |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *RBTermChange* | The field is mandatory present in case of:- set up of signalling and data radio bearer,- change of termination point for the radio bearer between MN and SN.It is optionally present otherwise, Need S. |
| *RBTermChange1* | The field is mandatory present in case of:- set up of signalling and data radio bearer,- change of termination point for the radio bearer between MN and SN,- handover from E-UTRA/EPC or E-UTRA/5GC to NR,- handover from NR or E-UTRA/EPC to E-UTRA/5GC if the UE supports NGEN-DC.It is optionally present otherwise, Need S. |
| *PDCP* | The field is mandatory present if the corresponding DRB/multicast MRB is being setup or corresponding DRB/multicast MRB is reconfigured with NR PDCP or corresponding SRB associated with two RLC entities is being setup or if the number of RLC bearers associated with the DRB/multicast MRB or SRB is changed. The field is optionally present, Need S, if the corresponding SRB associated with one RLC entity is being setup or corresponding SRB is reconfigured with NR PDCP; otherwise the field is optionally present, need M. |
| *DRBSetup* | The field is mandatory present if the corresponding DRB is being setup; otherwise the field is optionally present, need M. |
| *HO-Conn* | The field is mandatory present- in case of inter-system handover from E-UTRA/EPC to E-UTRA/5GC or NR,- or when the *fullConfig* is included in the *RRCReconfiguration* message and NE-DC/NR-DC is not configured,- or in case of *RRCSetup*.Otherwise the field is optionally present, need N.Upon *RRCSetup*, only SRB1 can be present. |
| *HO-toNR* | If *mrb-ToAddModList* is not included, the field is mandatory present for UEs other than NCR-MT- in case of inter-system handover from E-UTRA/EPC to E-UTRA/5GC or NR,- or when the *fullConfig* is included in the *RRCReconfiguration* message and NE-DC/NR-DC is not configured.In case of *RRCSetup* and for an NCR-MT, the field is absent; otherwise the field is optionally present, need N. |
| *DAPS* | The field is optionally present, need N, in case masterCellGroup includes ReconfigurationWithSync, SCell(s) and SCG are not configured, multi-DCI/single-DCI based multi-TRP are not configured in any DL BWP, *supplementaryUplink* is not configured, ethernetHeaderCompression is not configured for the DRB, *conditionalReconfiguration* is not configured, and NR sidelink and V2X sidelink are not configured. Otherwise the field is absent. |
| *MRBSetup* | The field is mandatory present if the corresponding multicast MRB is being setup; otherwise the field is optionally present, need M. |

NEXT CHANGE

#### – *SearchSpace*

The IE *SearchSpace* defines how/where to search for PDCCH candidates. Each search space is associated with one *ControlResourceSet*. For a scheduled SCell in the case of cross carrier scheduling, except for *nrofCandidates*, all the optional fields are absent (regardless of their presence conditions). For a scheduled SpCell in the case of the cross carrier scheduling, if the search space is linked to another search space in the scheduling SCell, all the optional fields of this search space in the scheduled SpCell are absent (regardless of their presence conditions) except for *nrofCandidates*.

*SearchSpace* information element

-- ASN1START

-- TAG-SEARCHSPACE-START

SearchSpace ::= SEQUENCE {

 searchSpaceId SearchSpaceId,

 controlResourceSetId ControlResourceSetId OPTIONAL, -- Cond SetupOnly

 monitoringSlotPeriodicityAndOffset CHOICE {

 sl1 NULL,

 sl2 INTEGER (0..1),

 sl4 INTEGER (0..3),

 sl5 INTEGER (0..4),

 sl8 INTEGER (0..7),

 sl10 INTEGER (0..9),

 sl16 INTEGER (0..15),

 sl20 INTEGER (0..19),

 sl40 INTEGER (0..39),

 sl80 INTEGER (0..79),

 sl160 INTEGER (0..159),

 sl320 INTEGER (0..319),

 sl640 INTEGER (0..639),

 sl1280 INTEGER (0..1279),

 sl2560 INTEGER (0..2559)

 } OPTIONAL, -- Cond Setup4

 duration INTEGER (2..2559) OPTIONAL, -- Need S

 monitoringSymbolsWithinSlot BIT STRING (SIZE (14)) OPTIONAL, -- Cond Setup

 nrofCandidates SEQUENCE {

 aggregationLevel1 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8},

 aggregationLevel2 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8},

 aggregationLevel4 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8},

 aggregationLevel8 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8},

 aggregationLevel16 ENUMERATED {n0, n1, n2, n3, n4, n5, n6, n8}

 } OPTIONAL, -- Cond Setup

 searchSpaceType CHOICE {

 common SEQUENCE {

 dci-Format0-0-AndFormat1-0 SEQUENCE {

 ...

 } OPTIONAL, -- Need R

 dci-Format2-0 SEQUENCE {

 nrofCandidates-SFI SEQUENCE {

 aggregationLevel1 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel2 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel4 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel8 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel16 ENUMERATED {n1, n2} OPTIONAL -- Need R

 },

 ...

 } OPTIONAL, -- Need R

 dci-Format2-1 SEQUENCE {

 ...

 } OPTIONAL, -- Need R

 dci-Format2-2 SEQUENCE {

 ...

 } OPTIONAL, -- Need R

 dci-Format2-3 SEQUENCE {

 dummy1 ENUMERATED {sl1, sl2, sl4, sl5, sl8, sl10, sl16, sl20} OPTIONAL, -- Cond Setup

 dummy2 ENUMERATED {n1, n2},

 ...

 } OPTIONAL -- Need R

 },

 ue-Specific SEQUENCE {

 dci-Formats ENUMERATED {formats0-0-And-1-0, formats0-1-And-1-1},

 ...,

 [[

 dci-Formats-MT-r16 ENUMERATED {formats2-5} OPTIONAL, -- Need R

 dci-FormatsSL-r16 ENUMERATED {formats0-0-And-1-0, formats0-1-And-1-1, formats3-0, formats3-1,

 formats3-0-And-3-1} OPTIONAL, -- Need R

 dci-FormatsExt-r16 ENUMERATED {formats0-2-And-1-2, formats0-1-And-1-1And-0-2-And-1-2}

 OPTIONAL -- Need R

 ]],

 [[

 dci-FormatsNCR-r18 ENUMERATED {formats5-0} OPTIONAL, -- Need R

 ]]

 }

 } OPTIONAL -- Cond Setup2

}

SearchSpaceExt-r16 ::= SEQUENCE {

 controlResourceSetId-r16 ControlResourceSetId-r16 OPTIONAL, -- Cond SetupOnly2

 searchSpaceType-r16 SEQUENCE {

 common-r16 SEQUENCE {

 dci-Format2-4-r16 SEQUENCE {

 nrofCandidates-CI-r16 SEQUENCE {

 aggregationLevel1-r16 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel2-r16 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel4-r16 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel8-r16 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel16-r16 ENUMERATED {n1, n2} OPTIONAL -- Need R

 },

 ...

 } OPTIONAL, -- Need R

 dci-Format2-5-r16 SEQUENCE {

 nrofCandidates-IAB-r16 SEQUENCE {

 aggregationLevel1-r16 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel2-r16 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel4-r16 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel8-r16 ENUMERATED {n1, n2} OPTIONAL, -- Need R

 aggregationLevel16-r16 ENUMERATED {n1, n2} OPTIONAL -- Need R

 },

 ...

 } OPTIONAL, -- Need R

 dci-Format2-6-r16 SEQUENCE {

 ...

 } OPTIONAL, -- Need R

 ...

 }

 } OPTIONAL, -- Cond Setup3

 searchSpaceGroupIdList-r16 SEQUENCE (SIZE (1.. 2)) OF INTEGER (0..1) OPTIONAL, -- Need R

 freqMonitorLocations-r16 BIT STRING (SIZE (5)) OPTIONAL -- Need R

}

SearchSpaceExt-v1700 ::= SEQUENCE {

 monitoringSlotPeriodicityAndOffset-v1710 CHOICE {

 sl32 INTEGER (0..31),

 sl64 INTEGER (0..63),

 sl128 INTEGER (0..127),

 sl5120 INTEGER (0..5119),

 sl10240 INTEGER (0..10239),

 sl20480 INTEGER (0..20479)

 } OPTIONAL, -- Cond Setup5

 monitoringSlotsWithinSlotGroup-r17 CHOICE {

 slotGroupLength4-r17 BIT STRING (SIZE (4)),

 slotGroupLength8-r17 BIT STRING (SIZE (8))

 } OPTIONAL, -- Need R

 duration-r17 INTEGER (4..20476) OPTIONAL, -- Need R

 searchSpaceType-r17 SEQUENCE{

 common-r17 SEQUENCE {

 dci-Format4-0-r17 SEQUENCE {

 ...

 } OPTIONAL, -- Need R

 dci-Format4-1-r17 SEQUENCE {

 ...

 } OPTIONAL, -- Need R

 dci-Format4-2-r17 SEQUENCE {

 ...

 } OPTIONAL, -- Need R

 dci-Format4-1-AndFormat4-2-r17 SEQUENCE {

 ...

 } OPTIONAL, -- Need R

 dci-Format2-7-r17 SEQUENCE {

 nrofCandidates-PEI-r17 SEQUENCE {

 aggregationLevel4-r17 ENUMERATED {n0, n1, n2, n3, n4} OPTIONAL, -- Need R

 aggregationLevel8-r17 ENUMERATED {n0, n1, n2} OPTIONAL, -- Need R

 aggregationLevel16-r17 ENUMERATED {n0, n1} OPTIONAL -- Need R

 },

 ...

 } OPTIONAL -- Need R

 }

 } OPTIONAL, -- Need R

 searchSpaceGroupIdList-r17 SEQUENCE (SIZE (1.. 3)) OF INTEGER (0.. maxNrofSearchSpaceGroups-1-r17) OPTIONAL, -- Cond DedicatedOnly

 searchSpaceLinkingId-r17 INTEGER (0..maxNrofSearchSpacesLinks-1-r17) OPTIONAL -- Cond DedicatedOnly

}

-- TAG-SEARCHSPACE-STOP

-- ASN1STOP

|  |
| --- |
| *SearchSpace* field descriptions |
| ***common***Configures this search space as common search space (CSS) and DCI formats to monitor. |
| ***controlResourceSetId***The CORESET applicable for this SearchSpace. Value 0 identifies the common CORESET#0 configured in MIB and in *ServingCellConfigCommon*. Values 1..*maxNrofControlResourceSets-1* identify CORESETs configured in System Information or by dedicated signalling. The CORESETs with *non-zero controlResourceSetId* are configured in the same BWP as this *SearchSpace* except *commonControlResourceSetExt* which is configured by SIB20. If the field *controlResourceSetId-r16* is present, UE shall ignore the *controlResourceSetId* (without suffix). |
| ***dummy1, dummy2***This field is not used in the specification. If received it shall be ignored by the UE. |
| ***dci-Format0-0-AndFormat1-0***If configured, the UE monitors the DCI formats 0\_0 and 1\_0 according to TS 38.213 [13], clause 10.1. |
| ***dci-Format2-0***If configured, UE monitors the DCI format 2\_0 according to TS 38.213 [13], clause 10.1, 11.1.1. |
| ***dci-Format2-1***If configured, UE monitors the DCI format 2\_1 according to TS 38.213 [13], clause 10.1, 11.2. |
| ***dci-Format2-2***If configured, UE monitors the DCI format 2\_2 according to TS 38.213 [13], clause 10.1, 11.3. |
| ***dci-Format2-3***If configured, UE monitors the DCI format 2\_3 according to TS 38.213 [13], clause 10.1, 11.4 |
| ***dci-Format2-4***If configured, UE monitors the DCI format 2\_4 according to TS 38.213 [13], clause 11.2A. |
| ***dci-Format2-5***If configured, IAB-MT monitors the DCI format 2\_5 according to TS 38.213 [13], clause 14. |
| ***dci-Format2-6***If configured, UE monitors the DCI format 2\_6 according to TS 38.213 [13], clause 10.1, 10.3. DCI format 2\_6 can only be configured on the SpCell. |
| ***dci-Format2-7***If configured, UE monitors the DCI format 2\_7 according to TS 38.213 [13], clause 10.1, 10.4A. |
| ***dci-Format4-0***If configured, the UE monitors the DCI format 4\_0 with CRC scrambled by MCCH-RNTI/G-RNTI according to TS 38.213 [13], clause [10.1]. |
| ***dci-Format4-1-AndFormat4-2***If configured, the UE monitors the DCI format 4\_1 and 4\_2 with CRC scrambled by G-RNTI/G-CS-RNTI according to TS 38.213 [13], clause [11.1]. |
| ***dci-Format4-1***If configured, the UE monitors the DCI format 4\_1 with CRC scrambled by G-RNTI/G-CS-RNTI according to TS 38.213 [13], clause [10.1]. |
| ***dci-Format4-2***If configured, the UE monitors the DCI format 4\_2 with CRC scrambled by G-RNTI/G-CS-RNTI according to TS 38.213 [13], clause [10.1]. |
| ***dci-Formats***Indicates whether the UE monitors in this USS for DCI formats 0-0 and 1-0 or for formats 0-1 and 1-1. |
| ***dci-FormatsExt***If this field is present, the field *dci-Formats* is ignored and *dci-FormatsExt* is used instead to indicate whether the UE monitors in this USS for DCI format 0\_2 and 1\_2 or formats 0\_1 and 1\_1 and 0\_2 and 1\_2 (see TS 38.212 [17], clause 7.3.1 and TS 38.213 [13], clause 10.1). This field is not configured for operation with shared spectrum channel access in this release*.* |
| ***dci-Formats-MT***Indicates whether the IAB-MT monitors the DCI formats 2-5 according to TS 38.213 [13], clause 14. |
| ***dci-FormatsNCR***Indicates whether the NCR-MT monitors the DCI formats 5-0 according to TS 38.213 [13], clause TBD. |
| ***dci-FormatsSL***Indicates whether the UE monitors in this USS for DCI formats 0-0 and 1-0 or for formats 0-1 and 1-1 or for format 3-0 or for format 3-1 or for formats 3-0 and 3-1. If this field is present, the field *dci-Formats* is ignored and *dci-FormatsSL* is used. |
| ***duration***Number of consecutive slots that a SearchSpace lasts in every occasion, i.e., upon every period as given in the *periodicityAndOffset*. If the field is absent, the UE applies the value 1 slot, except for DCI format 2\_0. The UE ignores this field for DCI format 2\_0. The maximum valid duration is periodicity-1 (periodicity as given in the *monitoringSlotPeriodicityAndOffset*).For SCS 480 kHz and SCS 960 kHz, duration-r17 is used, and the configured duration is restricted to be an integer multiple of L slots and smaller than periodicity, where L is the configured length of the bitmap *monitoringSlotsWithinSlotGroup-r17*. If *duration-r17* is absent, the UE assumes the duration in slots is equal to L. The maximum valid duration is periodicity-L.For IAB-MT, duration indicates number of consecutive slots that a SearchSpace lasts in every occasion, i.e., upon every period as given in the *periodicityAndOffset*. If the field is absent, the IAB-MT applies the value 1 slot, except for DCI format 2\_0 and DCI format 2\_5. The IAB-MT ignores this field for DCI format 2\_0 and DCI format 2\_5. The maximum valid duration is periodicity-1 (periodicity as given in the *monitoringSlotPeriodicityAndOffset*). |
| ***freqMonitorLocations***Defines an association of the search space to multiple monitoring locations in the frequency domain and indicates whether the pattern configured in the associated CORESET is replicated to a specific RB set, see TS 38.213, clause 10.1. Each bit in the bitmap corresponds to one RB set, and the leftmost (most significant) bit corresponds to RB set 0 in the BWP. A bit set to 1 indicates that a frequency domain resource allocation replicated from the pattern configured in the associated CORESET is mapped to the RB set. |
| ***monitoringSlotPeriodicityAndOffset***Slots for PDCCH Monitoring configured as periodicity and offset.For SCS 15, 30, 60, and 120 kHz and if the UE is configured to monitor:- DCI format 2\_1, only the values 'sl1', 'sl2' or 'sl4' are applicable.- DCI format 2\_0, only the values ′sl1′, ′sl2′, ′sl4′, ′sl5′, ′sl8′, ′sl10′, ′sl16′, and ′sl20′ are applicable (see TS 38.213 [13], clause 10).- DCI format 2\_4, only the values 'sl1', 'sl2', 'sl4', 'sl5', 'sl8' and 'sl10' are applicable.For SCS 480 kHz and if the UE is configured to monitor:- DCI format 2\_0, only the values 'sl4', 'sl8', 'sl16', 'sl20', 'sl32', 'sl40', 'sl64', and 'sl80' are applicable.- DCI format 2\_1, only the values ′sl4′, ′sl8′, and ′sl16′ are applicable.- DCI format 2\_4, only the values 'sl4', 'sl8', 'sl16', 'sl20', 'sl32', 'sl40' are applicable.For SCS 960 kHz and if the UE is configured to monitor:- DCI format 2\_0, only the values 'sl8', 'sl16', 'sl32', 'sl40', 'sl64', 'sl80', 'sl128', and 'sl160' are applicable.- DCI format 2\_1, only the values ′sl8′, ′sl16′, and 'sl32' are applicable.- DCI format 2\_4, only the values 'sl8', 'sl16', 'sl32', 'sl40', 'sl64', 'sl80' are applicable.For SCS 480 kHz and SCS 960 kHz, and the configured periodicity and offset are restricted to be an integer multiple of L slots, where L is the configured length of the bitmap provided by *monitoringSlotsWithinSlotGroup-r17*, i.e. for a given periodicity, the offset has a range of {0, L, 2\*L, …, L\*FLOOR(1/L\*(periodicity-1))}.For IAB-MT, If the IAB-MT is configured to monitor DCI format 2\_1, only the values 'sl1', 'sl2' or 'sl4' are applicable. If the IAB-MT is configured to monitor DCI format 2\_0 or DCI format 2\_5, only the values ′sl1′, ′sl2′, ′sl4′, ′sl5′, ′sl8′, ′sl10′, ′sl16′, and ′sl20′ are applicable (see TS 38.213, clause 10).If *monitoringSlotPeriodicityAndOffset-r17* is present, any previously configured *monitoringSlotPeriodicityAndOffset* is released, and if *monitoringSlotPeriodicityAndOffset* is present, any previously configured *monitoringSlotPeriodicityAndOffset-r17* is released. |
| ***monitoringSlotsWithinSlotGroup***Indicates which slot(s) within a slot group are configured for multi-slot PDCCH monitoring. The first (leftmost, most significant) bit represents the first slot in the slot group, the second bit represents the second slot in the slot group, and so on. A bit set to '1' indicates that the corresponding slot is configured for multi-slot PDCCH monitoring (see TS 38.213 [13], clause 10). The number of slots for multi-slot PDCCH monitoring is configured according to clause 10 in TS 38.213 [13]. |
| ***monitoringSymbolsWithinSlot***The first symbol(s) for PDCCH monitoring in the slots configured for (multi-slot) PDCCH monitoring (see *monitoringSlotPeriodicityAndOffset* and *duration*). The most significant (left) bit represents the first OFDM in a slot, and the second most significant (left) bit represents the second OFDM symbol in a slot and so on. The bit(s) set to one identify the first OFDM symbol(s) of the control resource set within a slot. If the cyclic prefix of the BWP is set to extended CP, the last two bits within the bit string shall be ignored by the UE or IAB-MT.For DCI format 2\_0, the first one symbol applies if the *duration* of CORESET (in the IE *ControlResourceSet*) identified by *controlResourceSetId* indicates 3 symbols, the first two symbols apply if the *duration* of CORESET identified by *controlResourceSetId* indicates 2 symbols, and the first three symbols apply if the *duration* of CORESET identified by *controlResourceSetId* indicates 1 symbol.See TS 38.213 [13], clause 10.For IAB-MT: For DCI format 2\_0 or DCI format 2\_5, the first one symbol applies if the duration of CORESET (in the IE *ControlResourceSet*) identified by *controlResourceSetId* indicates 3 symbols, the first two symbols apply if the *duration* of CORESET identified by *controlResourceSetId* indicates 2 symbols, and the first three symbols apply if the *duration* of CORESET identified by *controlResourceSetId* indicates 1 symbol.See TS 38.213 [13], clause 10. |
| ***nrofCandidates-CI***The number of PDCCH candidates specifically for format 2-4 for the configured aggregation level. If an aggregation level is absent, the UE does not search for any candidates with that aggregation level. The network configures only one aggregationLevel and the corresponding number of candidates (see TS 38.213 [13], clause 10.1). |
| ***nrofCandidates-PEI***The number of PDCCH candidates specifically for format 2-7 for the configured aggregation level. |
| ***nrofCandidates-SFI***The number of PDCCH candidates specifically for format 2-0 for the configured aggregation level. If an aggregation level is absent, the UE does not search for any candidates with that aggregation level. The network configures only one aggregationLevel and the corresponding number of candidates (see TS 38.213 [13], clause 11.1.1). For a search space configured with *freqMonitorLocations-r16*, only value ′n1′ is valid. |
| ***nrofCandidates***Number of PDCCH candidates per aggregation level. The number of candidates and aggregation levels configured here applies to all formats unless a particular value is specified or a format-specific value is provided (see inside *searchSpaceType*). If configured in the *SearchSpace* of a cross carrier scheduled cell, this field determines the number of candidates and aggregation levels to be used on the linked scheduling cell (see TS 38.213 [13], clause 10). |
| ***searchSpaceGroupIdList-r16, searchSpaceGroupIdList-r17***List of search space group IDs which the search space is associated with. The network configures at most 2 search space groups per BWP where the group ID is either 0 or 1 if *searchSpaceGroupIdList-r16* is included. The network configures at most 3 search space groups per BWP where the group ID is either 0, 1 or 2 if *searchSpaceGroupIdList-r17* is included. And if *searchSpaceGroupIdList-r17* is included, *searchSpaceGroupIdList-r16* is ignored. |
| ***searchSpaceId***Identity of the search space. SearchSpaceId = 0 identifies the *searchSpaceZero* configured via PBCH (MIB) or *ServingCellConfigCommon* and may hence not be used in the *SearchSpace* IE. The *searchSpaceId* is unique among the BWPs of a Serving Cell. In case of cross carrier scheduling, search spaces with the same *searchSpaceId* in scheduled cell and scheduling cell are linked to each other. The UE applies the search space for the scheduled cell only if the DL BWPs in which the linked search spaces are configured in scheduling cell and scheduled cell are both active.For an IAB-MT, the search space defines how/where to search for PDCCH candidates for an IAB-MT where each search space is associated with one ControlResearchSet and for a scheduled cell in the case of cross carrier scheduling, except for nrofCandidates, all the optional fields are absent. |
| ***SearchSpaceLinkingId***This parameter is used to link two search spaces of same type in the same BWP. If two search spaces have the same SearchSpaceLinkingId UE assumes these search spaces are linked to PDCCH repetition REF. When PDCCH repetition is monitored in two linked search space (SS) sets, the UE does not expect a third monitored SS set to be linked with any of the two linked SS sets. The two linked SS sets have the same SS set type (USS/CSS). The two linked SS sets have the same DCI formats to monitor. For intra-slot PDCCH repetition: The two SS sets should have the same periodicity and offset (monitoringSlotPeriodicityAndOffset), and the same duration. For linking monitoring occasions across the two SS sets that exist in the same slot: The two SS sets have the same number of monitoring occasions within a slot and n-th monitoring occasion of one SS set is linked to n-th monitoring occasion of the other SS set. The following SS sets cannot be linked with another SS set for PDCCH repetition: SS set 0, *searchSpaceSIB1*, *searchSpaceOtherSystemInformation*, *pagingSearchSpace*, *ra-SearchSpace*, *searchSpaceMCCH*, *searchSpaceMTCH*, *peiSearchSpace*, and *sdt-SearchSpace*. SS set configured by *recoverySearchSpaceId* cannot be linked to another SS set for PDCCH repetition. When a scheduled serving cell is configured to be cross-carrier scheduled by a scheduling serving cell, two PDCCH candidates (with the same AL and candidate index associated with the scheduled serving cell) are linked only if the corresponding two SS sets in the scheduling serving cell are linked and two SS sets in the scheduled serving cell with the same SS set IDs are also linked.This parameter is not applicable to search space configured with *dci-FormatsSL* for monitoring format 3-0 or format 3-1 or for monitoring formats 3-0 and format 3-1. |
| ***searchSpaceType***Indicates whether this is a common search space (present) or a UE specific search space as well as DCI formats to monitor for. |
| ***ue-Specific***Configures this search space as UE specific search space (USS). The UE monitors the DCI format with CRC scrambled by C-RNTI, CS-RNTI (if configured), and SP-CSI-RNTI (if configured) |

|  |  |
| --- | --- |
| Conditional Presence | Explanation |
| *DedicatedOnly* | In PDCCH-Config, the field is optionally present, Need R. Otherwise it is absent, Need R. |
| *Setup* | This field is mandatory present upon creation of a new *SearchSpace*. It is optionally present, Need M, otherwise. |
| *Setup2* | This field is mandatory present when a new *SearchSpace* is set up, if the same *SearchSpace* ID is not included in *searchSpacesToAddModListExt-r16* of the parent IE with the field *searchSpaceType-r16* or *searchSpaceType-r17* included. Otherwise it is optionally present, Need M. |
| *Setup3* | This field is mandatory present when a new *SearchSpace* is set up, if the same *SearchSpace* ID is not included in *searchSpacesToAddModListExt* (without suffix) of the parent IE with the field *searchSpaceType* (without suffix) included. Otherwise it is optionally present, Need M. |
| *Setup4* | This field is mandatory present upon creation of a new *SearchSpace* if *monitoringSlotPeriodicityAndOffset-r17* is not included. It is optionally present, Need M, otherwise. |
| *Setup5* | This field is mandatory present upon creation of a new *SearchSpace* if *monitoringSlotPeriodicityAndOffset* (without suffix) is not included. It is optionally present, Need M, otherwise. |
| *SetupOnly* | This field is mandatory present upon creation of a new *SearchSpace*. It is absent, Need M, otherwise. |
| *SetupOnly2* | In PDCCH-Config, the field is optionally present upon creation of a new SearchSpace and absent, Need M upon reconfiguration of an existing SearchSpace.In PDCCH-ConfigCommon, the field is absent. |

NEXT CHANGE

## 6.4 RRC multiplicity and type constraint values

### – Multiplicity and type constraint definitions

-- ASN1START

-- TAG-MULTIPLICITY-AND-TYPE-CONSTRAINT-DEFINITIONS-START

maxAdditionalRACH-r17 INTEGER ::= 256 -- Maximum number of additional RACH configurations.

maxAI-DCI-PayloadSize-r16 INTEGER ::= 128 --Maximum size of the DCI payload scrambled with ai-RNTI

maxAI-DCI-PayloadSize-1-r16 INTEGER ::= 127 --Maximum size of the DCI payload scrambled with ai-RNTI minus 1

maxBandComb INTEGER ::= 65536 -- Maximum number of DL band combinations

maxBandsUTRA-FDD-r16 INTEGER ::= 64 -- Maximum number of bands listed in UTRA-FDD UE caps

maxBH-RLC-ChannelID-r16 INTEGER ::= 65536 -- Maximum value of BH RLC Channel ID

maxBT-IdReport-r16 INTEGER ::= 32 -- Maximum number of Bluetooth IDs to report

maxBT-Name-r16 INTEGER ::= 4 -- Maximum number of Bluetooth name

maxCAG-Cell-r16 INTEGER ::= 16 -- Maximum number of NR CAG cell ranges in SIB3, SIB4

maxTwoPUCCH-Grp-ConfigList-r16 INTEGER ::= 32 -- Maximum number of supported configuration(s) of {primary PUCCH group

 -- config, secondary PUCCH group config}

maxTwoPUCCH-Grp-ConfigList-r17 INTEGER ::= 16 -- Maximum number of supported configuration(s) of {primary PUCCH group

 -- config, secondary PUCCH group config} for PUCCH cell switching

maxCBR-Config-r16 INTEGER ::= 8 -- Maximum number of CBR range configurations for sidelink communication

 -- congestion control

maxCBR-Config-1-r16 INTEGER ::= 7 -- Maximum number of CBR range configurations for sidelink communication

 -- congestion control minus 1

maxCBR-Level-r16 INTEGER ::= 16 -- Maximum number of CBR levels

maxCBR-Level-1-r16 INTEGER ::= 15 -- Maximum number of CBR levels minus 1

maxCellExcluded INTEGER ::= 16 -- Maximum number of NR exclude-listed cell ranges in SIB3, SIB4

maxCellGroupings-r16 INTEGER ::= 32 -- Maximum number of cell groupings for NR-DC

maxCellHistory-r16 INTEGER ::= 16 -- Maximum number of visited PCells reported

maxPSCellHistory-r17 INTEGER ::= 16 -- Maximum number of visited PSCells across all reported PCells

maxCellInter INTEGER ::= 16 -- Maximum number of inter-Freq cells listed in SIB4

maxCellIntra INTEGER ::= 16 -- Maximum number of intra-Freq cells listed in SIB3

maxCellMeasEUTRA INTEGER ::= 32 -- Maximum number of cells in E-UTRAN

maxCellMeasIdle-r16 INTEGER ::= 8 -- Maximum number of cells per carrier for idle/inactive measurements

maxCellMeasUTRA-FDD-r16 INTEGER ::= 32 -- Maximum number of cells in FDD UTRAN

maxCellNTN-r17 INTEGER ::= 4 -- Maximum number of NTN neighbour cells for which assistance information is

 -- provided

maxCarrierTypePairList-r16 INTEGER ::= 16 -- Maximum number of supported carrier type pair of (carrier type on which

 -- CSI measurement is performed, carrier type on which CSI reporting is

 -- performed) for CSI reporting cross PUCCH group

maxCellAllowed INTEGER ::= 16 -- Maximum number of NR allow-listed cell ranges in SIB3, SIB4

maxEARFCN INTEGER ::= 262143 -- Maximum value of E-UTRA carrier frequency

maxEUTRA-CellExcluded INTEGER ::= 16 -- Maximum number of E-UTRA exclude-listed physical cell identity ranges

 -- in SIB5

maxEUTRA-NS-Pmax INTEGER ::= 8 -- Maximum number of NS and P-Max values per band

maxFeatureCombPreamblesPerRACHResource-r17 INTEGER ::= 256 -- Maximum number of feature combination preambles.

maxLogMeasReport-r16 INTEGER ::= 520 -- Maximum number of entries for logged measurements

maxMultiBands INTEGER ::= 8 -- Maximum number of additional frequency bands that a cell belongs to

maxNARFCN INTEGER ::= 3279165 -- Maximum value of NR carrier frequency

maxNR-NS-Pmax INTEGER ::= 8 -- Maximum number of NS and P-Max values per band

maxFreqIdle-r16 INTEGER ::= 8 -- Maximum number of carrier frequencies for idle/inactive measurements

maxNrofServingCells INTEGER ::= 32 -- Max number of serving cells (SpCells + SCells)

maxNrofServingCells-1 INTEGER ::= 31 -- Max number of serving cells (SpCells + SCells) minus 1

maxNrofAggregatedCellsPerCellGroup INTEGER ::= 16

maxNrofAggregatedCellsPerCellGroupMinus4-r16 INTEGER ::= 12

maxNrofAperiodicFwdTimeResource-r18 INTEGER ::= 112 -- Max number of aperiodic fowarding time resources for NCR

maxNrofAperiodicFwdTimeResource-1-r18 INTEGER ::= 111 -- Max number of aperiodic fowarding time resources for NCR minus 1

maxNrofDUCells-r16 INTEGER ::= 512 -- Max number of cells configured on the collocated IAB-DU

maxNrofAppLayerMeas-r17 INTEGER ::= 16 -- Max number of simultaneous application layer measurements

maxNrofAppLayerMeas-1-r17 INTEGER ::= 15 -- Max number of simultaneous application layer measurements minus 1

maxNrofAvailabilityCombinationsPerSet-r16 INTEGER ::= 512 -- Max number of AvailabilityCombinationId used in the DCI format 2\_5

maxNrofAvailabilityCombinationsPerSet-1-r16 INTEGER ::= 511 -- Max number of AvailabilityCombinationId used in the DCI format 2\_5 minus 1

maxNrofIABResourceConfig-r17 INTEGER ::= 65536 -- Max number of IAB-ResourceConfigID used in MAC CE

maxNrofIABResourceConfig-1-r17 INTEGER ::= 65535 -- Max number of IAB-ResourceConfigID used in MAC CE minus 1

maxNrofPeriodicFwdResourceSet-r18 INTEGER ::= 32 -- Max number of periodic fowarding resource sets for NCR

maxNrofPeriodicFwdResourceSet-1-r18 INTEGER ::= 31 -- Max number of periodic fowarding resource sets for NCR minus 1

maxNrofPeriodicFwdResource-r18 INTEGER ::= 1024 -- Max number of periodic fowarding resources for NCR

maxNrofPeriodicFwdResource-1-r18 INTEGER ::= 1023 -- Max number of periodic fowarding resources for NCR minus 1

maxNrofSemiPersistentFwdResourceSet-r18 INTEGER ::= 32 -- Max number of semi-persistent fowarding resource sets for NCR

maxNrofSemiPersistentFwdResourceSet-1-r18 INTEGER ::= 31 -- Max number of semi-persistent fowarding resource sets for NCR minus 1

maxNrofSemiPersistentFwdResource-r18 INTEGER ::= 128 -- Max number of semi-persistent fowarding resources for NCR

maxNrofSemiPersistentFwdResource-1-r18 INTEGER ::= 127 -- Max number of semi-persistent fowarding resources for NCR minus 1

maxNrofSCellActRS-r17 INTEGER ::= 255 -- Max number of RS configurations per SCell for SCell activation

maxNrofSCells INTEGER ::= 31 -- Max number of secondary serving cells per cell group

maxNrofCellMeas INTEGER ::= 32 -- Maximum number of entries in each of the cell lists in a measurement object

maxNrofCRS-IM-InterfCell-r17 INTEGER ::= 8 -- Maximum number of LTE interference cells for CRS-IM per UE

maxNrofRelayMeas-r17 INTEGER ::= 32 -- Maximum number of L2 U2N Relay UEs to measure for each measurement object

 -- on sidelink frequency

maxNrofCG-SL-r16 INTEGER ::= 8 -- Max number of sidelink configured grant

maxNrofCG-SL-1-r16 INTEGER ::= 7 -- Max number of sidelink configured grant minus 1

maxSL-GC-BC-DRX-QoS-r17 INTEGER ::= 16 -- Max number of sidelink DRX configurations for NR

 -- sidelink groupcast/broadcast communication

maxNrofSL-RxInfoSet-r17 INTEGER ::= 4 -- Max number of sidelink DRX configuration sets in sidelink DRX assistant

 -- information

maxNrofSS-BlocksToAverage INTEGER ::= 16 -- Max number for the (max) number of SS blocks to average to determine cell measurement

maxNrofCondCells-r16 INTEGER ::= 8 -- Max number of conditional candidate SpCells

maxNrofCondCells-1-r17 INTEGER ::= 7 -- Max number of conditional candidate SpCells minus 1

maxNrofCSI-RS-ResourcesToAverage INTEGER ::= 16 -- Max number for the (max) number of CSI-RS to average to determine cell measurement

maxNrofDL-Allocations INTEGER ::= 16 -- Maximum number of PDSCH time domain resource allocations

maxNrofDL-AllocationsExt-r17 INTEGER ::= 64 -- Maximum number of PDSCH time domain resource allocations for multi-PDSCH

 -- scheduling

maxNrofPDU-Sessions-r17 INTEGER ::= 256 -- Maximum number of PDU Sessions

maxNrofSR-ConfigPerCellGroup INTEGER ::= 8 -- Maximum number of SR configurations per cell group

maxLCG-ID INTEGER ::= 7 -- Maximum value of LCG ID

maxLCG-ID-IAB-r17 INTEGER ::= 255 -- Maximum value of LCG ID for IAB-MT

maxLC-ID INTEGER ::= 32 -- Maximum value of Logical Channel ID

maxLC-ID-Iab-r16 INTEGER ::= 65855 -- Maximum value of BH Logical Channel ID extension

maxLTE-CRS-Patterns-r16 INTEGER ::= 3 -- Maximum number of additional LTE CRS rate matching patterns

maxNrofTAGs INTEGER ::= 4 -- Maximum number of Timing Advance Groups

maxNrofTAGs-1 INTEGER ::= 3 -- Maximum number of Timing Advance Groups minus 1

maxNrofBWPs INTEGER ::= 4 -- Maximum number of BWPs per serving cell

maxNrofCombIDC INTEGER ::= 128 -- Maximum number of reported MR-DC combinations for IDC

maxNrofSymbols-1 INTEGER ::= 13 -- Maximum index identifying a symbol within a slot (14 symbols, indexed from 0..13)

maxNrofSlots INTEGER ::= 320 -- Maximum number of slots in a 10 ms period

maxNrofSlots-1 INTEGER ::= 319 -- Maximum number of slots in a 10 ms period minus 1

maxNrofPhysicalResourceBlocks INTEGER ::= 275 -- Maximum number of PRBs

maxNrofPhysicalResourceBlocks-1 INTEGER ::= 274 -- Maximum number of PRBs minus 1

maxNrofPhysicalResourceBlocksPlus1 INTEGER ::= 276 -- Maximum number of PRBs plus 1

maxNrofControlResourceSets INTEGER ::= 12 -- Max number of CoReSets configurable on a serving cell

maxNrofControlResourceSets-1 INTEGER ::= 11 -- Max number of CoReSets configurable on a serving cell minus 1

maxNrofControlResourceSets-1-r16 INTEGER ::= 15 -- Max number of CoReSets configurable on a serving cell extended in minus 1

maxNrofCoresetPools-r16 INTEGER ::= 2 -- Maximum number of CORESET pools

maxCoReSetDuration INTEGER ::= 3 -- Max number of OFDM symbols in a control resource set

maxNrofSearchSpaces-1 INTEGER ::= 39 -- Max number of Search Spaces minus 1

maxNrofSearchSpacesLinks-1-r17 INTEGER ::= 39 -- Max number of Search Space links minus 1

maxNrofBFDResourcePerSet-r17 INTEGER ::= 64 -- Max number of reference signal in one BFD set

maxSFI-DCI-PayloadSize INTEGER ::= 128 -- Max number payload of a DCI scrambled with SFI-RNTI

maxSFI-DCI-PayloadSize-1 INTEGER ::= 127 -- Max number payload of a DCI scrambled with SFI-RNTI minus 1

maxIAB-IP-Address-r16 INTEGER ::= 32 -- Max number of assigned IP addresses

maxINT-DCI-PayloadSize INTEGER ::= 126 -- Max number payload of a DCI scrambled with INT-RNTI

maxINT-DCI-PayloadSize-1 INTEGER ::= 125 -- Max number payload of a DCI scrambled with INT-RNTI minus 1

maxNrofRateMatchPatterns INTEGER ::= 4 -- Max number of rate matching patterns that may be configured

maxNrofRateMatchPatterns-1 INTEGER ::= 3 -- Max number of rate matching patterns that may be configured minus 1

maxNrofRateMatchPatternsPerGroup INTEGER ::= 8 -- Max number of rate matching patterns that may be configured in one group

maxNrofCSI-ReportConfigurations INTEGER ::= 48 -- Maximum number of report configurations

maxNrofCSI-ReportConfigurations-1 INTEGER ::= 47 -- Maximum number of report configurations minus 1

maxNrofCSI-ResourceConfigurations INTEGER ::= 112 -- Maximum number of resource configurations

maxNrofCSI-ResourceConfigurations-1 INTEGER ::= 111 -- Maximum number of resource configurations minus 1

maxNrofAP-CSI-RS-ResourcesPerSet INTEGER ::= 16

maxNrOfCSI-AperiodicTriggers INTEGER ::= 128 -- Maximum number of triggers for aperiodic CSI reporting

maxNrofReportConfigPerAperiodicTrigger INTEGER ::= 16 -- Maximum number of report configurations per trigger state for aperiodic reporting

maxNrofNZP-CSI-RS-Resources INTEGER ::= 192 -- Maximum number of Non-Zero-Power (NZP) CSI-RS resources

maxNrofNZP-CSI-RS-Resources-1 INTEGER ::= 191 -- Maximum number of Non-Zero-Power (NZP) CSI-RS resources minus 1

maxNrofNZP-CSI-RS-ResourcesPerSet INTEGER ::= 64 -- Maximum number of NZP CSI-RS resources per resource set

maxNrofNZP-CSI-RS-ResourceSets INTEGER ::= 64 -- Maximum number of NZP CSI-RS resource sets per cell

maxNrofNZP-CSI-RS-ResourceSets-1 INTEGER ::= 63 -- Maximum number of NZP CSI-RS resource sets per cell minus 1

maxNrofNZP-CSI-RS-ResourceSetsPerConfig INTEGER ::= 16 -- Maximum number of resource sets per resource configuration

maxNrofNZP-CSI-RS-ResourcesPerConfig INTEGER ::= 128 -- Maximum number of resources per resource configuration

maxNrofZP-CSI-RS-Resources INTEGER ::= 32 -- Maximum number of Zero-Power (ZP) CSI-RS resources

maxNrofZP-CSI-RS-Resources-1 INTEGER ::= 31 -- Maximum number of Zero-Power (ZP) CSI-RS resources minus 1

maxNrofZP-CSI-RS-ResourceSets-1 INTEGER ::= 15

maxNrofZP-CSI-RS-ResourcesPerSet INTEGER ::= 16

maxNrofZP-CSI-RS-ResourceSets INTEGER ::= 16

maxNrofCSI-IM-Resources INTEGER ::= 32 -- Maximum number of CSI-IM resources

maxNrofCSI-IM-Resources-1 INTEGER ::= 31 -- Maximum number of CSI-IM resources minus 1

maxNrofCSI-IM-ResourcesPerSet INTEGER ::= 8 -- Maximum number of CSI-IM resources per set

maxNrofCSI-IM-ResourceSets INTEGER ::= 64 -- Maximum number of NZP CSI-IM resource sets per cell

maxNrofCSI-IM-ResourceSets-1 INTEGER ::= 63 -- Maximum number of NZP CSI-IM resource sets per cell minus 1

maxNrofCSI-IM-ResourceSetsPerConfig INTEGER ::= 16 -- Maximum number of CSI IM resource sets per resource configuration

maxNrofCSI-SSB-ResourcePerSet INTEGER ::= 64 -- Maximum number of SSB resources in a resource set

maxNrofCSI-SSB-ResourceSets INTEGER ::= 64 -- Maximum number of CSI SSB resource sets per cell

maxNrofCSI-SSB-ResourceSets-1 INTEGER ::= 63 -- Maximum number of CSI SSB resource sets per cell minus 1

maxNrofCSI-SSB-ResourceSetsPerConfig INTEGER ::= 1 -- Maximum number of CSI SSB resource sets per resource configuration

maxNrofCSI-SSB-ResourceSetsPerConfigExt INTEGER ::= 2 -- Maximum number of CSI SSB resource sets per resource configuration

 -- extended

maxNrofFailureDetectionResources INTEGER ::= 10 -- Maximum number of failure detection resources

maxNrofFailureDetectionResources-1 INTEGER ::= 9 -- Maximum number of failure detection resources minus 1

maxNrofFailureDetectionResources-1-r17 INTEGER ::= 63 -- Maximum number of the enhanced failure detection resources minus 1

maxNrofFreqSL-r16 INTEGER ::= 8 -- Maximum number of carrier frequency for NR sidelink communication

maxNrofSL-BWPs-r16 INTEGER ::= 4 -- Maximum number of BWP for NR sidelink communication

maxFreqSL-EUTRA-r16 INTEGER ::= 8 -- Maximum number of EUTRA anchor carrier frequency for NR sidelink communication

maxNrofSL-MeasId-r16 INTEGER ::= 64 -- Maximum number of sidelink measurement identity (RSRP) per destination

maxNrofSL-ObjectId-r16 INTEGER ::= 64 -- Maximum number of sidelink measurement objects (RSRP) per destination

maxNrofSL-ReportConfigId-r16 INTEGER ::= 64 -- Maximum number of sidelink measurement reporting configuration(RSRP) per destination

maxNrofSL-PoolToMeasureNR-r16 INTEGER ::= 8 -- Maximum number of resource pool for NR sidelink measurement to measure for

 -- each measurement object (for CBR)

maxFreqSL-NR-r16 INTEGER ::= 8 -- Maximum number of NR anchor carrier frequency for NR sidelink communication

maxNrofSL-QFIs-r16 INTEGER ::= 2048 -- Maximum number of QoS flow for NR sidelink communication per UE

maxNrofSL-QFIsPerDest-r16 INTEGER ::= 64 -- Maximum number of QoS flow per destination for NR sidelink communication

maxNrofObjectId INTEGER ::= 64 -- Maximum number of measurement objects

maxNrofPageRec INTEGER ::= 32 -- Maximum number of page records

maxNrofPCI-Ranges INTEGER ::= 8 -- Maximum number of PCI ranges

maxPLMN INTEGER ::= 12 -- Maximum number of PLMNs broadcast and reported by UE at establishment

maxTAC-r17 INTEGER ::= 12 -- Maximum number of Tracking Area Codes to which a cell belongs to

maxNrofCSI-RS-ResourcesRRM INTEGER ::= 96 -- Maximum number of CSI-RS resources per cell for an RRM measurement object

maxNrofCSI-RS-ResourcesRRM-1 INTEGER ::= 95 -- Maximum number of CSI-RS resources per cell for an RRM measurement object

 -- minus 1.

maxNrofMeasId INTEGER ::= 64 -- Maximum number of configured measurements

maxNrofQuantityConfig INTEGER ::= 2 -- Maximum number of quantity configurations

maxNrofCSI-RS-CellsRRM INTEGER ::= 96 -- Maximum number of cells with CSI-RS resources for an RRM measurement object

maxNrofSL-Dest-r16 INTEGER ::= 32 -- Maximum number of destination for NR sidelink communication and discovery

maxNrofSL-Dest-1-r16 INTEGER ::= 31 -- Highest index of destination for NR sidelink communication and discovery

maxNrofSLRB-r16 INTEGER ::= 512 -- Maximum number of radio bearer for NR sidelink communication per UE

maxSL-LCID-r16 INTEGER ::= 512 -- Maximum number of RLC bearer for NR sidelink communication per UE

maxSL-SyncConfig-r16 INTEGER ::= 16 -- Maximum number of sidelink Sync configurations

maxNrofRXPool-r16 INTEGER ::= 16 -- Maximum number of Rx resource pool for NR sidelink communication and

 -- discovery

maxNrofTXPool-r16 INTEGER ::= 8 -- Maximum number of Tx resource pool for NR sidelink communication and

 -- discovery

maxNrofPoolID-r16 INTEGER ::= 16 -- Maximum index of resource pool for NR sidelink communication and

 -- discovery

maxNrofSRS-PathlossReferenceRS-r16 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for SRS power control.

maxNrofSRS-PathlossReferenceRS-1-r16 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for SRS power control

 -- minus 1.

maxNrofSRS-ResourceSets INTEGER ::= 16 -- Maximum number of SRS resource sets in a BWP.

maxNrofSRS-ResourceSets-1 INTEGER ::= 15 -- Maximum number of SRS resource sets in a BWP minus 1.

maxNrofSRS-PosResourceSets-r16 INTEGER ::= 16 -- Maximum number of SRS Positioning resource sets in a BWP.

maxNrofSRS-PosResourceSets-1-r16 INTEGER ::= 15 -- Maximum number of SRS Positioning resource sets in a BWP minus 1.

maxNrofSRS-Resources INTEGER ::= 64 -- Maximum number of SRS resources.

maxNrofSRS-Resources-1 INTEGER ::= 63 -- Maximum number of SRS resources minus 1.

maxNrofSRS-PosResources-r16 INTEGER ::= 64 -- Maximum number of SRS Positioning resources.

maxNrofSRS-PosResources-1-r16 INTEGER ::= 63 -- Maximum number of SRS Positioning resources minus 1.

maxNrofSRS-ResourcesPerSet INTEGER ::= 16 -- Maximum number of SRS resources in an SRS resource set

maxNrofSRS-TriggerStates-1 INTEGER ::= 3 -- Maximum number of SRS trigger states minus 1, i.e., the largest code point.

maxNrofSRS-TriggerStates-2 INTEGER ::= 2 -- Maximum number of SRS trigger states minus 2.

maxRAT-CapabilityContainers INTEGER ::= 8 -- Maximum number of interworking RAT containers (incl NR and MRDC)

maxSimultaneousBands INTEGER ::= 32 -- Maximum number of simultaneously aggregated bands

maxULTxSwitchingBandPairs INTEGER ::= 32 -- Maximum number of band pairs supporting dynamic UL Tx switching in a band

 -- combination.

maxNrofSlotFormatCombinationsPerSet INTEGER ::= 512 -- Maximum number of Slot Format Combinations in a SF-Set.

maxNrofSlotFormatCombinationsPerSet-1 INTEGER ::= 511 -- Maximum number of Slot Format Combinations in a SF-Set minus 1.

maxNrofTrafficPattern-r16 INTEGER ::= 8 -- Maximum number of Traffic Pattern for NR sidelink communication.

maxNrofPUCCH-Resources INTEGER ::= 128

maxNrofPUCCH-Resources-1 INTEGER ::= 127

maxNrofPUCCH-ResourceSets INTEGER ::= 4 -- Maximum number of PUCCH Resource Sets

maxNrofPUCCH-ResourceSets-1 INTEGER ::= 3 -- Maximum number of PUCCH Resource Sets minus 1.

maxNrofPUCCH-ResourcesPerSet INTEGER ::= 32 -- Maximum number of PUCCH Resources per PUCCH-ResourceSet

maxNrofPUCCH-P0-PerSet INTEGER ::= 8 -- Maximum number of P0-pucch present in a p0-pucch set

maxNrofPUCCH-PathlossReferenceRSs INTEGER ::= 4 -- Maximum number of RSs used as pathloss reference for PUCCH power control.

maxNrofPUCCH-PathlossReferenceRSs-1 INTEGER ::= 3 -- Maximum number of RSs used as pathloss reference for PUCCH power control

 -- minus 1.

maxNrofPUCCH-PathlossReferenceRSs-r16 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for PUCCH power control

 -- extended.

maxNrofPUCCH-PathlossReferenceRSs-1-r16 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for PUCCH power control

 -- minus 1 extended.

maxNrofPUCCH-PathlossReferenceRSs-1-r17 INTEGER ::= 7 -- Maximum number of RSs used as pathloss reference for PUCCH power control

 -- minus 1.

maxNrofPUCCH-PathlossReferenceRSsDiff-r16 INTEGER ::= 60 -- Difference between the extended maximum and the non-extended maximum

maxNrofPUCCH-ResourceGroups-r16 INTEGER ::= 4 -- Maximum number of PUCCH resources groups.

maxNrofPUCCH-ResourcesPerGroup-r16 INTEGER ::= 128 -- Maximum number of PUCCH resources in a PUCCH group.

maxNrofPowerControlSetInfos-r17 INTEGER ::= 8 -- Maximum number of PUCCH power control set infos

maxNrofMultiplePUSCHs-r16 INTEGER ::= 8 -- Maximum number of multiple PUSCHs in PUSCH TDRA list

maxNrofP0-PUSCH-AlphaSets INTEGER ::= 30 -- Maximum number of P0-pusch-alpha-sets (see TS 38.213 [13], clause 7.1)

maxNrofP0-PUSCH-AlphaSets-1 INTEGER ::= 29 -- Maximum number of P0-pusch-alpha-sets minus 1 (see TS 38.213 [13], clause 7.1)

maxNrofPUSCH-PathlossReferenceRSs INTEGER ::= 4 -- Maximum number of RSs used as pathloss reference for PUSCH power control.

maxNrofPUSCH-PathlossReferenceRSs-1 INTEGER ::= 3 -- Maximum number of RSs used as pathloss reference for PUSCH power control

 -- minus 1.

maxNrofPUSCH-PathlossReferenceRSs-r16 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for PUSCH power control

 -- extended

maxNrofPUSCH-PathlossReferenceRSs-1-r16 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for PUSCH power control

 -- extended minus 1

maxNrofPUSCH-PathlossReferenceRSsDiff-r16 INTEGER ::= 60 -- Difference between maxNrofPUSCH-PathlossReferenceRSs-r16 and

 -- maxNrofPUSCH-PathlossReferenceRSs

maxNrofPathlossReferenceRSs-r17 INTEGER ::= 64 -- Maximum number of RSs used as pathloss reference for PUSCH, PUCCH, SRS

 -- power control for unified TCI state operation

maxNrofPathlossReferenceRSs-1-r17 INTEGER ::= 63 -- Maximum number of RSs used as pathloss reference for PUSCH, PUCCH, SRS

 -- power control for unified TCI state operation minus 1

maxNrofNAICS-Entries INTEGER ::= 8 -- Maximum number of supported NAICS capability set

maxBands INTEGER ::= 1024 -- Maximum number of supported bands in UE capability.

maxBandsMRDC INTEGER ::= 1280

maxBandsEUTRA INTEGER ::= 256

maxCellReport INTEGER ::= 8

maxDRB INTEGER ::= 29 -- Maximum number of DRBs (that can be added in DRB-ToAddModList).

maxFreq INTEGER ::= 8 -- Max number of frequencies.

maxFreqLayers INTEGER ::= 4 -- Max number of frequency layers.

maxFreqPlus1 INTEGER ::= 9 -- Max number of frequencies for Slicing.

maxFreqIDC-r16 INTEGER ::= 128 -- Max number of frequencies for IDC indication.

maxCombIDC-r16 INTEGER ::= 128 -- Max number of reported UL CA for IDC indication.

maxFreqIDC-MRDC INTEGER ::= 32 -- Maximum number of candidate NR frequencies for MR-DC IDC indication

maxNrofCandidateBeams INTEGER ::= 16 -- Max number of PRACH-ResourceDedicatedBFR in BFR config.

maxNrofCandidateBeams-r16 INTEGER ::= 64 -- Max number of candidate beam resources in BFR config.

maxNrofCandidateBeamsExt-r16 INTEGER ::= 48 -- Max number of PRACH-ResourceDedicatedBFR in the CandidateBeamRSListExt

maxNrofPCIsPerSMTC INTEGER ::= 64 -- Maximum number of PCIs per SMTC.

maxNrofQFIs INTEGER ::= 64

maxNrofResourceAvailabilityPerCombination-r16 INTEGER ::= 256

maxNrOfSemiPersistentPUSCH-Triggers INTEGER ::= 64 -- Maximum number of triggers for semi persistent reporting on PUSCH

maxNrofSR-Resources INTEGER ::= 8 -- Maximum number of SR resources per BWP in a cell.

maxNrofSlotFormatsPerCombination INTEGER ::= 256

maxNrofSpatialRelationInfos INTEGER ::= 8

maxNrofSpatialRelationInfos-plus-1 INTEGER ::= 9

maxNrofSpatialRelationInfos-r16 INTEGER ::= 64

maxNrofSpatialRelationInfosDiff-r16 INTEGER ::= 56 -- Difference between maxNrofSpatialRelationInfos-r16 and maxNrofSpatialRelationInfos

maxNrofIndexesToReport INTEGER ::= 32

maxNrofIndexesToReport2 INTEGER ::= 64

maxNrofSSBs-r16 INTEGER ::= 64 -- Maximum number of SSB resources in a resource set.

maxNrofSSBs-1 INTEGER ::= 63 -- Maximum number of SSB resources in a resource set minus 1.

maxNrofS-NSSAI INTEGER ::= 8 -- Maximum number of S-NSSAI.

maxNrofTCI-StatesPDCCH INTEGER ::= 64

maxNrofTCI-States INTEGER ::= 128 -- Maximum number of TCI states.

maxNrofTCI-States-1 INTEGER ::= 127 -- Maximum number of TCI states minus 1.

maxUL-TCI-r17 INTEGER ::= 64 -- Maximum number of TCI states.

maxUL-TCI-1-r17 INTEGER ::= 63 -- Maximum number of TCI states minus 1.

maxNrofAdditionalPCI-r17 INTEGER ::= 7 -- Maximum number of additional PCI

maxMPE-Resources-r17 INTEGER ::= 64 -- Maximum number of pooled MPE resources

maxNrofUL-Allocations INTEGER ::= 16 -- Maximum number of PUSCH time domain resource allocations.

maxQFI INTEGER ::= 63

maxRA-CSIRS-Resources INTEGER ::= 96

maxRA-OccasionsPerCSIRS INTEGER ::= 64 -- Maximum number of RA occasions for one CSI-RS

maxRA-Occasions-1 INTEGER ::= 511 -- Maximum number of RA occasions in the system

maxRA-SSB-Resources INTEGER ::= 64

maxSCSs INTEGER ::= 5

maxSecondaryCellGroups INTEGER ::= 3

maxNrofServingCellsEUTRA INTEGER ::= 32

maxMBSFN-Allocations INTEGER ::= 8

maxNrofMultiBands INTEGER ::= 8

maxCellSFTD INTEGER ::= 3 -- Maximum number of cells for SFTD reporting

maxReportConfigId INTEGER ::= 64

maxNrofCodebooks INTEGER ::= 16 -- Maximum number of codebooks supported by the UE

maxNrofCSI-RS-ResourcesExt-r16 INTEGER ::= 16 -- Maximum number of codebook resources supported by the UE for eType2/Codebook combo

maxNrofCSI-RS-ResourcesExt-r17 INTEGER ::= 8 -- Maximum number of codebook resources for fetype2R1 and fetype2R2

maxNrofCSI-RS-Resources INTEGER ::= 7 -- Maximum number of codebook resources supported by the UE

maxNrofCSI-RS-ResourcesAlt-r16 INTEGER ::= 512 -- Maximum number of alternative codebook resources supported by the UE

maxNrofCSI-RS-ResourcesAlt-1-r16 INTEGER ::= 511 -- Maximum number of alternative codebook resources supported by the UE minus 1

maxNrofSRI-PUSCH-Mappings INTEGER ::= 16

maxNrofSRI-PUSCH-Mappings-1 INTEGER ::= 15

maxSIB INTEGER::= 32 -- Maximum number of SIBs

maxSI-Message INTEGER::= 32 -- Maximum number of SI messages

maxSIB-MessagePlus1-r17 INTEGER::= 33 -- Maximum number of SIB messages plus 1

maxPO-perPF INTEGER ::= 4 -- Maximum number of paging occasion per paging frame

maxPEI-perPF-r17 INTEGER ::= 4 -- Maximum number of PEI occasion per paging frame

maxAccessCat-1 INTEGER ::= 63 -- Maximum number of Access Categories minus 1

maxBarringInfoSet INTEGER ::= 8 -- Maximum number of access control parameter sets

maxCellEUTRA INTEGER ::= 8 -- Maximum number of E-UTRA cells in SIB list

maxEUTRA-Carrier INTEGER ::= 8 -- Maximum number of E-UTRA carriers in SIB list

maxPLMNIdentities INTEGER ::= 8 -- Maximum number of PLMN identities in RAN area configurations

maxDownlinkFeatureSets INTEGER ::= 1024 -- (for NR DL) Total number of FeatureSets (size of the pool)

maxUplinkFeatureSets INTEGER ::= 1024 -- (for NR UL) Total number of FeatureSets (size of the pool)

maxEUTRA-DL-FeatureSets INTEGER ::= 256 -- (for E-UTRA) Total number of FeatureSets (size of the pool)

maxEUTRA-UL-FeatureSets INTEGER ::= 256 -- (for E-UTRA) Total number of FeatureSets (size of the pool)

maxFeatureSetsPerBand INTEGER ::= 128 -- (for NR) The number of feature sets associated with one band.

maxPerCC-FeatureSets INTEGER ::= 1024 -- (for NR) Total number of CC-specific FeatureSets (size of the pool)

maxFeatureSetCombinations INTEGER ::= 1024 -- (for MR-DC/NR)Total number of Feature set combinations (size of the pool)

maxInterRAT-RSTD-Freq INTEGER ::= 3

maxGIN-r17 INTEGER ::= 24 -- Maximum number of broadcast GINs

maxHRNN-Len-r16 INTEGER ::= 48 -- Maximum length of HRNNs

maxNPN-r16 INTEGER ::= 12 -- Maximum number of NPNs broadcast and reported by UE at establishment

maxNrOfMinSchedulingOffsetValues-r16 INTEGER ::= 2 -- Maximum number of min. scheduling offset (K0/K2) configurations

maxK0-SchedulingOffset-r16 INTEGER ::= 16 -- Maximum number of slots configured as min. scheduling offset (K0)

maxK2-SchedulingOffset-r16 INTEGER ::= 16 -- Maximum number of slots configured as min. scheduling offset (K2)

maxK0-SchedulingOffset-r17 INTEGER ::= 64 -- Maximum number of slots configured as min. scheduling offset (K0)

maxK2-SchedulingOffset-r17 INTEGER ::= 64 -- Maximum number of slots configured as min. scheduling offset (K2)

maxDCI-2-6-Size-r16 INTEGER ::= 140 -- Maximum size of DCI format 2-6

maxDCI-2-7-Size-r17 INTEGER ::= 43 -- Maximum size of DCI format 2-7

maxDCI-2-6-Size-1-r16 INTEGER ::= 139 -- Maximum DCI format 2-6 size minus 1

maxNrofUL-Allocations-r16 INTEGER ::= 64 -- Maximum number of PUSCH time domain resource allocations

maxNrofP0-PUSCH-Set-r16 INTEGER ::= 2 -- Maximum number of P0 PUSCH set(s)

maxOnDemandSIB-r16 INTEGER ::= 8 -- Maximum number of SIB(s) that can be requested on-demand

maxOnDemandPosSIB-r16 INTEGER ::= 32 -- Maximum number of posSIB(s) that can be requested on-demand

maxCI-DCI-PayloadSize-r16 INTEGER ::= 126 -- Maximum number of the DCI size for CI

maxCI-DCI-PayloadSize-1-r16 INTEGER ::= 125 -- Maximum number of the DCI size for CI minus 1

maxUu-RelayRLC-ChannelID-r17 INTEGER ::= 32 -- Maximum value of Uu Relay RLC channel ID

maxWLAN-Id-Report-r16 INTEGER ::= 32 -- Maximum number of WLAN IDs to report

maxWLAN-Name-r16 INTEGER ::= 4 -- Maximum number of WLAN name

maxRAReport-r16 INTEGER ::= 8 -- Maximum number of RA procedures information to be included in the RA report

maxTxConfig-r16 INTEGER ::= 64 -- Maximum number of sidelink transmission parameters configurations

maxTxConfig-1-r16 INTEGER ::= 63 -- Maximum number of sidelink transmission parameters configurations minus 1

maxPSSCH-TxConfig-r16 INTEGER ::= 16 -- Maximum number of PSSCH TX configurations

maxNrofCLI-RSSI-Resources-r16 INTEGER ::= 64 -- Maximum number of CLI-RSSI resources for UE

maxNrofCLI-RSSI-Resources-1-r16 INTEGER ::= 63 -- Maximum number of CLI-RSSI resources for UE minus 1

maxNrofCLI-SRS-Resources-r16 INTEGER ::= 32 -- Maximum number of SRS resources for CLI measurement for UE

maxCLI-Report-r16 INTEGER ::= 8

maxNrofCC-Group-r17 INTEGER ::= 16 -- Maximum number of CC groups for DC location report

maxNrofConfiguredGrantConfig-r16 INTEGER ::= 12 -- Maximum number of configured grant configurations per BWP

maxNrofConfiguredGrantConfig-1-r16 INTEGER ::= 11 -- Maximum number of configured grant configurations per BWP minus 1

maxNrofCG-Type2DeactivationState INTEGER ::= 16 -- Maximum number of deactivation state for type 2 configured grants per BWP

maxNrofConfiguredGrantConfigMAC-1-r16 INTEGER ::= 31 -- Maximum number of configured grant configurations per MAC entity minus 1

maxNrofSPS-Config-r16 INTEGER ::= 8 -- Maximum number of SPS configurations per BWP

maxNrofSPS-Config-1-r16 INTEGER ::= 7 -- Maximum number of SPS configurations per BWP minus 1

maxNrofSPS-DeactivationState INTEGER ::= 16 -- Maximum number of deactivation state for SPS per BWP

maxNrofPPW-Config-r17 INTEGER ::= 4 -- Maximum number of Preconfigured PRS processing windows per DL BWP

maxNrofPPW-ID-1-r17 INTEGER ::= 15 -- Maximum number of Preconfigured PRS processing windows minus 1

maxNrOfTxTEGReport-r17 INTEGER ::= 256 -- Maximum number of UE Tx Timing Error Group Report

maxNrOfTxTEG-ID-1-r17 INTEGER ::= 7 -- Maximum number of UE Tx Timing Error Group ID minus 1

maxNrofPagingSubgroups-r17 INTEGER ::= 8 -- Maximum number of paging subgroups per paging occasion

maxNrofPUCCH-ResourceGroups-1-r16 INTEGER ::= 3

maxNrofReqComDC-Location-r17 INTEGER ::= 128 -- Maximum number of requested carriers/BWPs combinations for DC location

 -- report

maxNrofServingCellsTCI-r16 INTEGER ::= 32 -- Maximum number of serving cells in simultaneousTCI-UpdateList

maxNrofTxDC-TwoCarrier-r16 INTEGER ::= 64 -- Maximum number of UL Tx DC locations reported by the UE for 2CC uplink CA

maxNrofRB-SetGroups-r17 INTEGER ::= 8 -- Maximum number of RB set groups

maxNrofRB-Sets-r17 INTEGER ::= 8 -- Maximum number of RB sets

maxNrofEnhType3HARQ-ACK-r17 INTEGER ::= 8 -- Maximum number of enhanced type 3 HARQ-ACK codebook

maxNrofEnhType3HARQ-ACK-1-r17 INTEGER ::= 7 -- Maximum number of enhanced type 3 HARQ-ACK codebook minus 1

maxNrofPRS-ResourcesPerSet-r17 INTEGER ::= 64 -- Maximum number of PRS resources for one set

maxNrofPRS-ResourcesPerSet-1-r17 INTEGER ::= 63 -- Maximum number of PRS resources for one set minus 1

maxNrofPRS-ResourceOffsetValue-1-r17 INTEGER ::= 511

maxNrofGapId-r17 INTEGER ::= 8 -- Maximum number of measurement gap ID is FFS

maxNrofPreConfigPosGapId-r17 INTEGER ::= 16 -- Maximum number of preconfigured positioning measurement gap

maxNrOfGapPri-r17 INTEGER ::= 16 -- Maximum number of gap priority level

maxCEFReport-r17 INTEGER ::= 4 -- Maximum number of CEF reports by the UE

maxNrofMultiplePDSCHs-r17 INTEGER ::= 8 -- Maximum number of PDSCHs in PDSCH TDRA list

maxSliceInfo-r17 INTEGER ::= 8 -- Maximum number of NSAGs

maxCellSlice-r17 INTEGER ::= 16 -- Maximum number of cells supporting the NSAG

maxNrofTRS-ResourceSets-r17 INTEGER ::= 64 -- Maximum number of TRS resource sets

maxNrofSearchSpaceGroups-1-r17 INTEGER ::= 2 -- Maximum number of search space groups minus 1

maxNrofRemoteUE-r17 INTEGER ::= 32 -- Maximum number of connected L2 U2N Remote UEs

maxDCI-4-2-Size-r17 INTEGER ::= 140 -- Maximum size of DCI format 4-2

maxFreqMBS-r17 INTEGER ::= 16 -- Maximum number of MBS frequencies reported in MBSInterestIndication

maxNrofDRX-ConfigPTM-r17 INTEGER ::= 64 -- Max number of DRX configuration for PTM provided in MBS broadcast in a

 -- cell

maxNrofDRX-ConfigPTM-1-r17 INTEGER ::= 63 -- Max number of DRX configuration for PTM provided in MBS broadcast in a

 -- cell minus 1

maxNrofMBS-ServiceListPerUE-r17 INTEGER ::= 16 -- Maximum number of services which the UE can include in the MBS interest

 -- indication

maxNrofMBS-Session-r17 INTEGER ::= 1024 -- Maximum number of MBS sessions provided in MBS broadcast in a cell

maxNrofMTCH-SSB-MappingWindow-r17 INTEGER ::= 16 -- Maximum number of MTCH to SSB beam mapping pattern

maxNrofMTCH-SSB-MappingWindow-1-r17 INTEGER ::= 15 -- Maximum number of MTCH to SSB beam mapping pattern minus 1

maxNrofMRB-Broadcast-r17 INTEGER ::= 4 -- Maximum number of broadcast MRBs configured for one MBS broadcast service

maxNrofPageGroup-r17 INTEGER ::= 32 -- Maximum number of paging groups in a paging message

maxNrofPDSCH-ConfigPTM-r17 INTEGER ::= 16 -- Maximum number of PDSCH configuration groups for PTM

maxNrofPDSCH-ConfigPTM-1-r17 INTEGER ::= 15 -- Maximum number of PDSCH configuration groups for PTM minus 1

maxG-RNTI-r17 INTEGER ::= 16 -- Maximum number of G-RNTI that can be configured for a UE.

maxG-RNTI-1-r17 INTEGER ::= 15 -- Maximum number of G-RNTI that can be configured for a UE minus 1.

maxG-CS-RNTI-r17 INTEGER ::= 8 -- Maximum number of G-CS-RNTI that can be configured for a UE.

maxG-CS-RNTI-1-r17 INTEGER ::= 7 -- Maximum number of G-CS-RNTI that can be configured for a UE minus 1.

maxMRB-r17 INTEGER ::= 32 -- Maximum number of multicast MRBs (that can be added in MRB-ToAddModLIst)

maxFSAI-MBS-r17 INTEGER ::= 64 -- Maximum number of MBS frequency selection area identities

maxNeighCellMBS-r17 INTEGER ::= 8 -- Maximum number of MBS broadcast neighbour cells

maxNrofPdcch-BlindDetectionMixed-1-r16 INTEGER ::= 7 -- Maximum number of combinations of mixed Rel-16 and Rel-15 PDCCH

 -- monitoring capabilities minus 1

maxNrofPdcch-BlindDetection-r17 INTEGER ::= 16 -- Maximum number of combinations of PDCCH blind detection monitoring

 -- capabilities

-- TAG-MULTIPLICITY-AND-TYPE-CONSTRAINT-DEFINITIONS-STOP

-- ASN1STOP

Editor's note: *maxK0-SchedulingOffset* and *maxK0-SchedulingOffset* need confirmation by RAN1.

# Annex (not part of the specification): RAN2 Agreements

This Annex contains the RAN2 agreements on Rel-18 WI for “Network-controlled repeaters (NCR)”. The agreements are provided verbatim for reference.This annex shall be removed once the WI is completed.

RAN2#119bis-e

|  |
| --- |
| Agreement:RAN2 confirms to use RRC signalling to configure NCR-MT to receive side control information. How the side control information itself is transmitted (i.e. via RRC or DCI or MAC CE) is up to RAN1 (RAN2 may discussion the initial RAN1 decision and revisit if needed). |

|  |
| --- |
| Agreement:NCR-MT supports RRC\_CONNECTED and RRC\_IDLE states, FFS on RRC\_INACTIVE state (e.g. optional support or not support). |

|  |
| --- |
| AgreementNCR-MT supports SRB0/1/2 and DRB is optional. FFS on maximum number of DRBs. |

|  |
| --- |
| AgreementsRRM functions supported by NCR-MR:* Cell selection is mandatory
* Cell reselection, RLM, BFD, BFR are FFS
 |

RAN2#120

* Introduce an NCR-support indication in SIB1 per PLMN; whether it is also per NPN is FFS
* WA: RRC\_INACTIVE is optionally supported without any specific enhancements

|  |
| --- |
| AgreementsgNB cell that NCR-Fwd is forwarding is the same cell the NCT-MT is connected to. Whether the NCR-Fwd can forward other cells is up to implementationNCR-MT indicates the maximum number of supported DRB in UE capability, values {1, 16}. If absent, the NCR-MT does not support DRB.SRB2 is mandatory feature for NCR-MT.On NCR-Fwd ON/OFF:* When NCR-MT is in RRC\_CONNECTED mode, the NCR-Fwd can be ON or OFF following the side control information received from the gNB.
* After NCR-MT enters RRC\_INACTIVE mode, the NCR-Fwd can be ON or OFF following the last configuration received from the gNB.
* Release to RRC-IDLE is FFS.

On NCR-MT RLF:* After RLF is declared by NCR-MT, NCR-MT performs cell selection and trigger RRC re-establishment;
* If NCR-MT enters RRC\_IDLE due to no suitable cell is find, NCR-Fwd is OFF;
* During RRC re-establishment procedure, NCR-Fwd is OFF.

NCR-MT mandatorily support cell reselection and RRM measurements in RRC\_IDLE and RRC\_INACTIVE.In Rel-18, NCR-MT does not support handover and RRM measurements in RRC\_CONNECTED.For reporting the capabilities of NCR-MT, the existing *UECapabilityEnquiry* and *UECapabilityInformation* messages are reused.In NCR-MT capability discussion, to focus on mandatory features that are required for NCR-MT.All existing optional features are considered as applicable to NCR-MT unless explicitly excluded (Same as IAB-MT). FFS on taking IAB specified features as a baseline for future discussion.NPN capable NCR-MT should consider *cellReservedForOtherUse* for determination of an NPN-only cell.  |

RAN2#121

* RAN2 will support RAN3 areement to include NCR indication in msg5
* RRC\_INACTIVE is optionally supported without any specific enhancements.

|  |
| --- |
| * Side control configuration for the NCR-Fwd is provided in CellGroupconfig.
* (A)periodic beam and semi-persistent configurations may be added, modified, or removed.
* One NCR-support indication is included in SIB1 which is applied for all PLMNs/NPNs. (revert previous agreement).
* The NCR-FWD is switched OFF if the NCR-MT in RRC\_INACTIVE state reselects a different cell than the last serving cell on which side control configuration was received.
* After cell reselection, the NCR-MT to resume so that it can receive side-control configuration from the new gNB (can be done by network configuration using existing specifications). The case when a NCR-MT selects/reselects to an acceptable cell or when no cell is found and comes back is FFS.
* The side control information is introduced in CellGroupConfig in RRCReconfiguration and RRCResume
* Whenever side control configuration is removed forwarding will be off. This does not preclude any solutions coming from RAN1.
* The network should be able to send NCR-MT to RRC\_IDLE
 |

|  |
| --- |
| * Separate MAC CEs for UL and DL
 |

RAN2#121bis-e

|  |
| --- |
| Agreements:RAN2 confirms that the NCR Access Link Beam Indication MAC CE can optionally provide the updated beam indexes for semi-persistent beam indication, and if not provided, the UE applies the beam indication configuration provided by RRC.To keep the C-field in NCR Access Link Beam Indication MAC CE.RAN2 confirms that the name to be used for a new dedicated RNTI value for NCR-MT is NCR-RNTI.RAN2 confirms that NCR-RNTI is used to scramble the PDCCHs that carrying side control information and C-RNTI is used to scramble the PDSCHs that carrying side control information via RRC and MAC CE.RAN2 will not support update of partial beam indexes in NCR Access Link Beam Indication MAC CE.RAN2 confirms that the one-octet eLCID space should be used for the new NCR MAC CEs, as per R2-2303445. RAN2 understands that the final values chosen from this space may differ from the ones in the final version of the NCR MAC CatB CR, due to potential alignment across different Rel-18 W |

|  |
| --- |
| NCR-Fwd is OFF when NCR-MT is in RRC\_IDLE state |

|  |
| --- |
| Agreements:Below features are conditional mandatory supported by NCR-MT:- “Timer based SDU discard” in “1-0 Basic PDCP procedures”- “SDU discard” in “2-0 Basic RLC procedures”- “counter check” in “9-2 RRC processing time”Other handover related features, e.g. CHO, DAPS, CPAC, etc, are not supported by NCR-MT.Long SN bit (i.e. PDCP 18bit SN length and RLC AM 18bit SN length) is optional for NCR-MT.CA, MR-DC are not supported by NCR-MT, at least in R18.SDAP related features, and other layer 2 and layer 3 mandatory features in TS 38.822 are optional for NCR-MT. |

RAN1#112

note: only list the agreements that related to RRC value range

**Agreement**

For periodic and semi-persistent beam indication,

* The maximum number of periodic beam indication is 32.
* The maximum supported number of beam is 64 (to determine the value range of beam index).
* The maximum number of duration of time resource is 112 symbols.

For periodic beam indication,

The maximum number of forwarding resources in one periodic beam indication is 1024.

**Agreement**

For aperiodic beam indication,

* The value range of slot offset of time resource is (0…14)
* The maximum number of time resource is 112.
* The maximum bitwidth of beam index field in DCI is 6.