**3GPP TSG-RAN WG2 Meeting #121bisR2-2304341**

**Electronic April 2023**

**Title:** **DRAFT** LS on 2TA operation for Rel-18 MIMO

**Response to: -**

**Release:** Rel-18

**Work Item:** NR\_MIMO\_evo\_DL\_UL-Core

**Source:** Ericsson (to be replaced with 3GPP TSG-RAN WG2)

**To:** 3GPP TSG-RAN WG1

**Contact Person:**

Name: Helka-Liina Määttänen

Email Address: Helka-liina.maattanen@ericsson.com

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:** None

1. **2TA operation:**

RAN2 has discussed the 2TA aspects including per TRP UE initiated RACH procedure, configuring more than one TAG per serving cell and configuring additional RACH configs based on RAN1 input and RAN2 contributions.

For per TRP UE initiated RACH procedure RAN2 agreed the following:

* From RAN2 perspective, per TRP UE-initiated RACH procedure is not supported.

For configuring more than one TAG per serving cell and configuring additional RACH configs RAN2 agreed the following:

* We will send LS to R1 asking questions. Offline drafting the LS, including the following aspects

**- the possible groupings and related operation for 2TAs**

**- other aspects based on offline comments/company contributions**

1. **TAG groups**

RAN2 discussed how the cells/TRPs configured for the UE, are to be grouped if UE is configured with two TAG groups per serving cell.

For example, if UE is configured with three serving cells, named here as A,B,C, and each as two active TRPs. First TRP of cell A is marked as A1 and second TRP of cell A is marked as A2 and so on. Group1 denotes cells/TRPs that follow the first UL timing and hence first time alignment timer and Group2 denotes cells/TRPs that follow the second UL timing and hence second time alignment timer.

There can be different ways to allow this grouping. For example, the allowed grouping is such that both groups need to contain the same cells although it may be optional which TRP is included. If the reference timing is for first group cell A, then the same cell is also reference timing for group 2. Two example groupings could be:

Example 1

Group 1: **A1**, B1, C1

Group2: **A2**, B2, C2

Or example 2:

Group 1: A1, **B2**, C1

Group2: A2, **B1**, C2

The operation according to the above example 1 could be that if TA in A1 of group 1 is lost, it is considered to be lost for A1, B1 and C1 but A2, B2 and C2 would still be running.

Another possibility is that this per TRP TA operation is local to a serving cell, at least for the second time alignment timer.

Example 3

Group 1: A1, **B1**, C1, D1

Group2: A2

Group3: B2

Group4: C2

With this example 3, in Group 1, there is one reference timing which follows the TRP1 of cell B and the first TRPs of cell A, C and D follow the TAT of that. Then, each cell has second group with it’s own TAT.

RAN2 would like to receive RAN1 feedback on the intended grouping and related operation

**Question 1 on grouping and reference timing**

**Q1a:** For the TAG groups configured for the UE, what are the rules for grouping serving cells and their TRPs according to RAN1 understanding?

**Q1b:** What are the rules for the reference timing cell/TRP selection. E.g. If A1 is the reference timing of group 1, is then A2 a reference timing for group 2 or can another cell/TRP of group 2 be chosen as reference timing?

**Question 2 on operation**

**Q2a:** When both timers associated to one serving cell expire, can legacy procedures on time alignment timer be assumed?

**Q2b:** When one of the timers associated to one serving cell expires, is it according to RAN1 view that UL towards that TRP the timer is associated (e.g. UL transmissions associated to UL TCI state, PUCCH and SRS resources of that TRP) are impacted but UL towards the another TRP can remain in operation?

**Q2c:** Can there be a case that if one of the timers associated to one serving cell expires, the legacy procedures would apply which means that all UL for all serving cells belonging to that group are impacted? For example, in case this timer is related to PTAG.

1. **Additional RACH configs:**

RAN2 discussed the additional RACH configs and would like to understand better the configuration details. Currently, the serving cells of one TAG share one common RACH configuration between two TRPs and that configuration is applied in the UL BWP in which the RACH is performed.

**Question 3 on RACH**

**Q3a:** Is there a difference in the preamble or resource configuration(or some other aspect) depending on which additional PCI is active for the second TRP?

**Q3b:** Is there a difference in the preamble or resource configuration(or some other aspect) between first and second TRP?

**4. Actions:**

**To RAN1 group:**

**ACTION:** RAN2 respectfully asks RAN1 to provide responses to above questions.

**5. Date of Next TSG-RAN WG2 Meetings:**

TSG-RAN WG2 Meeting #122 May 2023 Incheon

TSG-RAN WG2 Meeting #123 August 2023 Toulouse