{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["Cover","Parameters","PRACH FR2-1 1T2R"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":10,"n_cols":10,"rows_kept":10,"cut":false,"hidden":false,"merged":[]}
[]
[null,"3GPP TSG-RAN WG4 Meeting #112",null,null,null,null,null,null,null,"R4-2411181"]
[null,"Maastricht , NL, Aug 19-23, 2024"]
[]
[null,"Source: China Telecom"]
[null,"Title: Summary of simulation results for Rel-18 NR coverage enhancements BS demodulation requirements"]
[null,"Agenda: 5.21.2"]
[]
[null,"Reference: R4-2406137 WF on NR_cov_enh2_demod, China Telecom"]
[null,null,"R4-2410018 WF on NR_cov_enh2_demod, China Telecom"]

{"sheet":"Parameters","index":1,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[1,2,1,4],[6,2,6,4],[7,2,7,4]]}
[]
[null,null,"Parameters for deriving performance requirements"]
[null,null,"Ideal Span Threshold",2,"dB"]
[null,null,"Impairment Span Threshold",4,"dB"]
[]
[]
[null,"Notes","1. Call function DerivingPerfReq()"]
[null,null,"2. If the ruls does not apply, or fails, -100dB or less will be returned"]
[null,null,null,-100,"Not enough input"]
[null,null,null,-101,"Input should be pairs"]
[null,null,null,-102,"Too large span for impairment"]
[null,null,null,-103,"After removal iteration, not enough input"]

{"sheet":"PRACH FR2-1 1T2R","index":2,"n_rows":8,"n_cols":25,"rows_kept":8,"cut":false,"hidden":false,"merged":[[0,0,1,1],[4,0,5,0],[2,1,7,1],[0,2,1,2],[2,0,3,0],[6,0,7,0],[0,17,0,18],[0,19,0,20],[0,21,0,22],[0,23,0,24],[0,3,1,3],[0,7,0,8],[0,9,0,10],[0,11,0,12],[0,13,0,14],[0,15,0,16],[0,4,1,4],[0,5,1,5],[0,6,1,6]]}
[" PRACH FR2-1 1T2R",null,"Propagation condition","Frequency offset (Hz)","Repetition Interval","38.104 req","38.141 req","Nokia (R4-2407140)",null,"Ericsson (R4-2412316)",null,"Huawei (R4-2412770)",null,"ZTE (R4-2412789)",null,"Samsung (R4-2413441)",null,"Company 6",null,"Company 7",null,"SPAN",null,"AVERAGE"]
[null,null,null,null,null,null,null,"Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment","Ideal","Impairment"]
["Format A2","120kHz","AWGN",0,"N/A","N/A","N/A",-18.8,-16.100000000000001,-17.8,-15.1,-17.3,-14.8,-18.600000000000001,-16.100000000000001,-16.7,-14.7,null,null,null,null,{"$f":"MAX(H3,J3,L3,N3,P3,R3,T3)-MIN(H3,J3,L3,N3,P3,R3,T3)","v":2.1000000000000014},{"$f":"MAX(I3,K3,M3,O3,Q3,S3,U3)-MIN(I3,K3,M3,O3,Q3,S3,U3)","v":1.4000000000000021},{"$f":"AVERAGE(H3,J3,L3,N3,P3,R3,T3)","v":-17.84},{"$f":"AVERAGE(I3,K3,M3,O3,Q3,S3,U3)","v":-15.36}]
[null,null,"TDLA30-300 Low",4000,"Repetition within 1 slot",{"$f":"DerivingPerfReq(H4:U4)","v":-100},{"$f":"IF(F4>-100,F4+0.6,F4)","v":-100},null,null,-10.4,null,-9.1999999999999993,-6.7,-11.2,null,-11.81,-9.81,null,null,null,null,{"$f":"MAX(H4,J4,L4,N4,P4,R4,T4)-MIN(H4,J4,L4,N4,P4,R4,T4)","v":2.6100000000000012},3.1100000000000003,{"$f":"AVERAGE(H4,J4,L4,N4,P4,R4,T4)","v":-10.6525},-8.2550000000000008]
["Format B4",null,"AWGN",0,"N/A","N/A","N/A",-23.5,-20.8,-22.2,-19.5,-19.5,-17,-21.7,-19.2,-20.9,-18.899999999999999,null,null,null,null,{"$f":"MAX(H5,J5,L5,N5,P5,R5,T5)-MIN(H5,J5,L5,N5,P5,R5,T5)","v":4},3.8000000000000007,{"$f":"AVERAGE(H5,J5,L5,N5,P5,R5,T5)","v":-21.560000000000002},-19.080000000000002]
[null,null,"TDLA30-300 Low",4000,"10 slots",{"$f":"DerivingPerfReq(H6:U6)","v":-12.3},{"$f":"IF(F6>-100,F6+0.6,F6)","v":-11.700000000000001},-14.8,-12.1,-15,-12.3,-11.2,-8.6999999999999993,-14,-11.5,-15.45,-13.45,null,null,null,null,4.25,4.75,-14.09,-11.61]
["Format C2",null,"AWGN",0,"N/A","N/A","N/A",-18.8,-16.100000000000001,-17.8,-15.1,-17.399999999999999,-14.9,-18.600000000000001,-16.100000000000001,-16.61,-14.61,null,null,null,null,2.1900000000000013,1.490000000000002,-17.841999999999999,-15.362]
[null,null,"TDLA30-300 Low",4000,"Repetition within 1 slot",{"$f":"DerivingPerfReq(H8:U8)","v":-100},{"$f":"IF(F8>-100,F8+0.6,F8)","v":-100},null,null,-10.5,null,-9.1999999999999993,-6.7,-11.1,null,-11.69,-9.69,null,null,null,null,{"$f":"MAX(H8,J8,L8,N8,P8,R8,T8)-MIN(H8,J8,L8,N8,P8,R8,T8)","v":2.4900000000000002},{"$f":"MAX(I8,K8,M8,O8,Q8,S8,U8)-MIN(I8,K8,M8,O8,Q8,S8,U8)","v":2.9899999999999993},{"$f":"AVERAGE(H8,J8,L8,N8,P8,R8,T8)","v":-10.622499999999999},{"$f":"AVERAGE(I8,K8,M8,O8,Q8,S8,U8)","v":-8.1950000000000003}]