**3GPP TSG-RAN WG4 Meeting # 98-bis-e R4-210XXXX**

**Electronic Meeting, 12th – 20th April, 2021**

**Agenda item:** 8.16

**Source:** Moderator (Huawei, HiSilicon)

**Title:** Email discussion summary for [98-bis-e][140] NR\_cov\_enh

**Document for:** Information

# Introduction

This email thread discusses the phase continuity and power consistency across PUSCH/PUCCH repetition for NR coverage enhancements WI in AI 8.16, including the following sub-topics:

* Sub-topic 1-1: Conditions to keep phase continuity and power consistency
* Sub-topic 1-2: Phase continuity tolerance

Note: R4-2104702 submitted to AI 12.1 is also discussed in this thread.

List of candidate target of email discussion for 1st round and 2nd round:

* 1st round: Invite companies to review the recommended WF and provide comments directly under each issue in section 1.2.1 and 1.2.2.
* 2nd round: prepare the WF and additional reply LS to RAN1.

# Topic #1: Phase continuity and power consistency for PUSCH and PUCCH repetition

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| [R4-2104580](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2104580.zip) | MediaTek inc. | Observation 1. In order to maintain phase continuity during those unscheduled symbols between UL repetition, UE power consumption would get higher and the OFF power requirement cannot be met.Proposal 1: RAN4 to deprioritize the non-back-2-back UL repetition scenario.Observation 2: SRS typically has very different settings on antenna port, occupied PRBs and UL power to PUCCH and PUSCH. It is an extreme corner case to see all these settings are exactly the same between SRS and PUSCH/PUCCH.Proposal 2: RAN4 does not consider the scenario of other physical signals/channels in-between PUCCH or PUSCH repetitions in later study on phase continuity and power consistency.Observation 3: The use case to remain phase continuity and power consistency for UL repetition is not clear under CA scenario. Proposal 3: RAN4 to further check the use case and the necessity to consider phase continuity and power consistency for UL repetition under CA scenario.Proposal 4: RAN4 to further check the use case and the necessity to consider phase continuity and power consistency for UL repetition under DC scenario. |
| [R4-2104955](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2104955.zip) | China Telecom | Observation 1: Potential use cases for joint channel estimation with non-zero gap in-between adjacent transmissions have been identified in RAN1.Observation 2: Non-back-to-back PUSCH transmissions within one slot or across slots can happen in several practical scenarios.Observation 3: Based on LTE experience, it is feasible to consider non-zero gap between uplink transmissions with joint channel estimation.Proposal: RAN4 to confirm the feasibility to keep phase continuity and power consistency (with certain tolerance level) for scenario with non-zero gap in-between the PUSCH or PUCCH repetition, and further discuss the possible number of OFDM symbols for the gap. |
| [R4-2106918](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2106918.zip) | InterDigital Communications | Observation 1: The PT-RS may help mitigate the phase continuity during non-contiguous repetitions and UE based phase drifting.Observation 2: The DM-RS symbol can be delayed during the repetition’s slots allowing for phase shift evaluation against the first repetition that contain the phase reference PT-RS.Observation 3: The DM-RS symbol can be delayed during the repetition’s slots allowing for phase shift evaluation against the first repetition that contain the phase reference PT-RS.Proposal: Study the phase continuity for non-contiguous and contiguous transmissions and implementation phase drift issues in the context of mitigations methods like PT-RS insertion for FR1 and FR2. |
| [R4-2107273](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2107273.zip) | Huawei,HiSilicon | Proposal 1 : For case that un-scheduled UL symbols between 2 UL transmissions, phase continuity can be maintained, which requires for off power exception on the unscheduled symbol(s).Proposal 2: if there is one slot un-scheduled between 2 UL tranmission, phase continuity cannot be maintained. |
| [R4-2107284](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2107284.zip) | Qualcomm Incorporated | withdrawn |
| [R4-2107366](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2107366.zip) | Qualcomm Incorporated | We discussed the two cases left open in the LS: Case of un scheduled symbols between repetitions and the case of other UL channels between repetitions and made three proposals.Proposal 1: The gap when there is no other channel band in between two repetition can be up to 14 symbols. Proposal 2: In the case of different channel in between two repetitions, a guard period before returning to the repetitions is defined. Length of guard period is Y is FFS. Proposal 3: The length including the guard period of the other channel in between two repetitions is less than 14 symbols. We also discussed about the amount of phase shift when phase can be contiguous and since receiver evalautionm was excluded in the work, we made one proposal:Proposal 4: The amount of phase change allowed for the UE when phase between two repetitions is considered to be contiguous shall be less than 160 degrees |
| [R4-2104702](https://www.3gpp.org/ftp/TSG_RAN/WG4_Radio/TSGR4_98bis_e/Docs/R4-2104702.zip) | Sony | In this contribution we have discussed phase continuity for PUCCH and PUSCH repetition and UE configuration for enhanced Joint Channel Estimation in TDD. The following observations and proposal are made:Observation 1 It is important to have non-zero X un-scheduled UL OFDM symbols in-between the PUSCH and PUCCH repetition to make the JCE more useful in practical scenarios.Observation 2 Phase continuity can be maintained if off power is not required on the un-scheduled symbols by remaining the Tx chain state unchanged.Observation 3 For UEs with cross switch, i.e. UEs that have multiple Rx/Tx chains, it is possible to use different antennas for UL and DL traffic during the JCE window.Observation 4 For FR2 a UE needs to be able to request an alternative beam for DL.Observation 5 Companies are encouraged to estimate the required tolerance of the phase continuity and amplitude consistency needed for JCE.Proposal 1 Companies are encouraged to investigate the additional power needed to keep the PA biased during the DL periods.Proposal 2 Companies are encouraged to investigate the required isolation between the antenna ports to avoid desensitization from PA noise leakage.Proposal 3 Companies are encouraged to investigate the risk of having too weak signal at the second antenna.Proposal 4 UE capability of supporting JCE and signaling that JCE is not applicable is needed. |

## Open issues summary

### Sub-topic 1-1: Conditions to keep phase continuity and power consistency

**Issue 1-1-1: Non-zero un-scheduled gap**

Issue description: Whether it is feasible to keep phase continuity and power consistency when there is non-zero un-scheduled UL OFDM symbols in-between the PUSCH and PUCCH repetition:

* Proposals
	+ Option 1: Feasible (China Telecom, Huawei, Qualcomm, Sony)
		- Huawei: PLL, RFIC and PA do not switch off, and off power exception on the unscheduled symbol(s).
		- Qualcomm: UE can leave the transmitter in to ON state and only ramp down the signal chain
		- Sony: Phase continuity can be maintained if off power is not required on the un-scheduled symbols by remaining the Tx chain state unchanged.
		- China Telecom: Potential use cases have been identified in RAN1 and seen in practical scenario; feasible to consider non-zero gap based on LTE experience.
	+ Option 2: Deprioritize non-zero gap scenario (MediaTek)
		- MediaTek: UE power consumption would get higher and the OFF power requirement cannot be met.
* Recommended WF
	+ Based on majority’s view, is it possible to firstly confirm the feasibility in general, and further discuss the exact number of OFDM symbols in Issue 1-1-1A?

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |

**Issue 1-1-1A: Length of un-scheduled gap for Issue 1-1-1**

* Proposals
	+ Option 1: Less than 14 OFDM symbols (Huawei)
	+ Option 2: Up to 14 OFDM symbols (Qualcomm)
* Recommended WF
	+ It seems the only difference between the two options is whether 14 OFDM symbols can be considered. Further discussion and views from more companies are encouraged.

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |

**Issue 1-1-2: Non-zero gap with other signals/channels for the UE**

Issue description: Whether it is feasible to keep phase continuity and power consistency for scenarios of other physical signals/channels in-between PUCCH or PUSCH repetitions from the UE perspective, e.g., SRS or PUCCH transmission in-between the PUSCH repetition for the UE.

* Proposals
	+ Option 1: Not consider these scenarios (MediaTek)
		- MediaTek: SRS typically has very different settings on antenna port, occupied PRBs and UL power to PUCCH and PUSCH.
	+ Option 2: A guard period before returning to the repetitions should be defined, and the length including the guard period of the other channel in between two repetitions is less than 14 symbols. (Qualcomm)
* Recommended WF
	+ Encourage more inputs

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |

**Issue 1-1-3: PUCCH/PUSCH repetition under CA and DC scenarios**

Agreements related to CA/DC in RAN4 #98e (Approved reply LS in R4-2103393):

* *Question 1: Under what conditions UE can keep phase continuity cross PUCCH or PUSCH repetitions*
* *RAN4 Answer for question 1: If the following conditions are met*
	+ *…*
	+ *No change on transmission power level of its own CC, i.e., no change on the power control parameters specified in TS 38.213, and also when own CC is not impacted by other concurrent CC(s) that are configured for inter-band CA or DC for same UE with dynamic power sharing and no change in any configured CC s that are part of configured intra-band uplink CA or DC.*
	+ *…*
* Proposals
	+ Option 1: RAN4 to further check the use case and the necessity to consider phase continuity and power consistency for UL repetition under CA and DC scenarios. (MediaTek)
* Recommended WF
	+ Keep the RAN4 agreements in the reply LS approved in the last meeting, and leave the decision on the applicable use cases to RAN1.

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |

**Issue 1-1-4: Phase drift mitigation methods like PT-RS insertion for FR1 and FR2**

* Proposals
	+ Option 1: Study the phase continuity for non-contiguous and contiguous transmissions and implementation phase drift issues in the context of mitigations methods like PT-RS insertion for FR1 and FR2. (InterDigital)
		- Observation 1: The PT-RS may help mitigate the phase continuity during non-contiguous repetitions and UE based phase drifting.
		- Observation 2: The DM-RS symbol can be delayed during the repetition’s slots allowing for phase shift evaluation against the first repetition that contain the phase reference PT-RS.
		- Observation 3: The DM-RS symbol can be delayed during the repetition’s slots allowing for phase shift evaluation against the first repetition that contain the phase reference PT-RS.
* Recommended WF
	+ Encourage feedback

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |

**Issue 1-1-5: DL slot(s) in-between repetition**

Issue description: Whether it is feasible to keep phase continuity and power consistency for scenarios with DL slot(s) in-between PUCCH or PUSCH repetition in the same band for TDD case

* Proposals
	+ Option 1: Use different antennas/panels for UL and DL traffic during the JCE window (Sony)
		- Separate UL / DL antennas in FR1
			* Companies are encouraged to investigate the additional power needed to keep the PA biased during the DL periods.
			* Companies are encouraged to investigate the required isolation between the antenna ports to avoid desensitization from PA noise leakage.
			* Companies are encouraged to investigate the risk of having too weak signal at the second antenna.
			* UE capability of supporting JCE and signaling that JCE is not applicable is needed.
		- Separate UL/DL panels in FR2
			* For FR2 a UE needs to be able to request an alternative beam for DL.
* Recommended WF
	+ Encourage feedback

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |

### Sub-topic 1-2: Phase continuity tolerance

**Issue 1-2-1: Amount of phase change from UE implementation aspect**

* Proposals
	+ Option 1 (Qualcomm):The amount of phase change allowed for the UE when phase between two repetitions is considered to be contiguous shall be less than 160 degrees.
		- Repetitions are assumed to be for coverage enhancement and lowest MCS is assumed to be use
		- The number may seem excessive but from UE design point of view without know what matters to the receiver, this is what is desirable with the current knowledge.
		- If the feature is applicable for MIMO, TX switching, CA should be discussed separately after baseline is consensus is achieved for one TX cases.
* Recommended WF
	+ Encourage more inputs

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |
|  |  |

**Issue 1-2-2: Quantification of the acceptable/required tolerance**

* Proposals
	+ Option 1: To estimate the required tolerance of the phase continuity and amplitude consistency from link performance perspective (Sony, [QC])
		- Sony: It is important to clarify the scenario for the UL JCE so that RAN4 (and RAN1) can quantify the acceptable tolerance of phase continuity and amplitude consistency.
		- QC: The intent is to enable phase continuity in the receiver or the repeated transmissions. RAN4 can further discuss further tightening of the phase change value but so far there is no knowledge why that would be needed.
* Recommended WF
	+ Encourage more feedback

|  |  |
| --- | --- |
| **Company** | **Comments** |
|  |  |
|  |  |

## Companies views’ collection for 1st round

*Provided under each issue in section 1.2*

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary**  |
| **Sub-topic#1** | *Tentative agreements:**Candidate options:**Recommendations for 2nd round:* |

## Discussion on 2nd round

1. Recommendations for Tdocs
	1. 1st round

**New tdocs**

|  |  |  |
| --- | --- | --- |
| **Title** | **Source** | **Comments** |
| WF on … | YYY |  |
| LS on … | ZZZ | To: RAN\_X; Cc: RAN\_Y |
|  |  |  |

**Existing tdocs**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Tdoc number** | **Title** | **Source** | **Recommendation**  | **Comments** |
| R4-210xxxx | CR on … | XXX | Agreeable, Revised, Merged, Postponed, Not Pursued |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

Notes:

1. Please include the summary of recommendations for all tdocs across all sub-topics incl. existing and new tdocs.
2. For the Recommendation column please include one of the following:
	1. CRs/TPs: Agreeable, Revised, Merged, Postponed, Not Pursued
	2. Other documents: Agreeable, Revised, Noted
3. For new LS documents, please include information on To/Cc WGs in the comments column
4. Do not include hyper-links in the documents
	1. 2nd round

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Tdoc number** | **Title** | **Source** | **Recommendation**  | **Comments** |
| R4-210xxxx | CR on … | XXX | Agreeable, Revised, Merged, Postponed, Not Pursued |  |
| R4-210xxxx | WF on … | YYY | Agreeable, Revised, Noted |  |
| R4-210xxxx | LS on … | ZZZ | Agreeable, Revised, Noted |  |
|  |  |  |  |  |

Notes:

1. Please include the summary of recommendations for all tdocs across all sub-topics.
2. For the Recommendation column please include one of the following:
	1. CRs/TPs: Agreeable, Revised, Merged, Postponed, Not Pursued
	2. Other documents: Agreeable, Revised, Noted
3. Do not include hyper-links in the documents