3GPP TSG-RAN WG4 Meeting # 98-bis-e R4-2106969

Electronic Meeting, Apr. 12-20, 2021

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.1* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **38.133** | **CR** | **Draft** | **rev** |  | **Current version:** | **16.7.0** |  |
|  | | | | | | | | |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** | Draft CR on CSSF for NR-U | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | Huawei, HiSilicon | | | | | | | | | |
| ***Source to TSG:*** | R4 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | NR\_unlic-Core | | | | |  | ***Date:*** | | | 2021-03-01 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **B** |  | | | | | ***Release:*** | | | Rel-16 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-15 (Release 15) Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | The CSSF for NR-U is not defined | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add the CSSF for NR-U according to previous agreements. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | The requirements are not correct. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | |  | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | |  | | | | | | | | |

### <Start of Change 1>

### 9.1.5 Carrier-specific scaling factor

This clause specifies the derivation of carrier-specific scaling factor (CSSF) values, which scales the measurement delay requirements given in clause 9.2, 9.2A, 9.3, 9.3A, 9.4, and NR PRS-based positioning measurements in clause 9.9 and CSI-RS based L3 measurement in clause 9.10 when UE is configured to monitor multiple measurement objects. The CSSF values are categorized into CSSFoutside\_gap,i andCSSFwithin\_gap,i, for the measurements conducted outside measurement gaps and within measurement gaps, respectively.

#### 9.1.5.1 Monitoring of multiple layers outside gaps

The carrier-specific scaling factor CSSFoutside\_gap,i for measurement object *i* derived in this chapter is applied to following measurement types:

- SSB-based intra-frequency measurement with no measurement gap in clause 9.2.5 and 9.2A.5, when none of the SMTC occasions of this intra-frequency measurement object are overlapped by the measurement gap.

- SSB-based intra-frequency measurement with no measurement gap in clause 9.2.5 and 9.2A.5, when part of the SMTC occasions of this intra-frequency measurement object are overlapped by the measurement gap.

- CSI-RS based intra-frequency measurement in clause xxx, when none of CSI-RS resources for L3 measurement of this intra-frequency measurement object are overlapped by the measurement gap.

- CSI-RS based intra-frequency measurement in clause xxx, when all CSI-RS resources for L3 measurement of this intra-frequency measurement object are partially overlapped by the measurement gap.- SSB-based inter-frequency measurement with no measurement gap in clause 9.3.9, when none of the SMTC occasions of this inter-frequency measurement object are overlapped by the measurement gap, if UE supports *interFrequencyMeas-NoGap-r16* and the flag *interFrequencyConfig-NoGap-r16* is configured by the Network.

- SSB-based inter-frequency measurement with no measurement gap in clause 9.3.9, when part of the SMTC occasions of this inter-frequency measurement object are overlapped by the measurement gap, if UE supports *interFrequencyMeas-NoGap-r16* and the flag *interFrequencyConfig-NoGap-r16* is configured by the Network.

- Intra-frequency RSSI and channel occupancy measurement with no measurement gap on a carrier subject to CCA when SMTC and RMTC are overlapping and RMTCs are not fully overlapped with measurement gap.

UE is expected to conduct the measurement of this measurement object *i* only outside the measurement gaps.

The number of frequency layers for SSB measurements shall include the total number of MOs with

- *ssb-ConfigMobility* configured, or

- *ssb-ConfigMobility* not configured but *csi-rs-ResourceConfigMobility* configured with *associatedSSB*.

If *ssbfrequency, smtc1, smtc2* and *ssbSubcarrierSpacing* are same in multiple MOs, the multiple MOs are counted as one SSB frequency layer.

If the higher layer signaling in TS 38.331 [2] of *smtc2* is present and *smtc1* is fully overlapping with measurement gaps and *smtc2* is partially overlapping with measurement gaps, CSSFoutside\_gap,i and requirements derived from CSSFoutside\_gap,i are not specified.

The UE cell identification and measurement periods derived based on CSSFoutside\_gap,i in clauses 9.2.5.1, 9.2.5.2 and 9.10.2 may be extended for measurement objects of which the cell identification and measurement periods are overlapped with Tmeasure\_SFTD1 specified in clause 9.3.8 when no measurement gaps are provided.

The requirements in this clause apply provided that

- There are only SCCs in FR2, or

- The SMTC on all CCs in FR2 have the same offset, and one of following conditions is met

- If *smtc2* is configured on any FR2 CC,

- All CCs have the same configuration for *smtc1*, and

- All CCs configured with *smtc2* have the same configuration for *smtc2*

- If *smtc2* is not configured on any FR2 CC,

- The total number of different SMTC periodicities on all serving CCs does not exceed 4

- All CSI-RS resources in the same MO are configured within a periodic 5ms window.

Note: Longer delays for cell identification and measurement periods derived based on CSSFoutside\_gap,i in clauses 9.2.5.1, 9.2.5.2, can be expected, if the UE is configured with more than 4 different SMTC periodicities on FR2 serving carriers. The longer delay applies for the FR2 intra-frequency measurement objects with the longest SMTC periodicity/periodicities.

##### 9.1.5.1.1 EN-DC mode: carrier-specific scaling factor for SSB-based,CSI-RS based L3 measurements and RSSI and channel occupancy measurements performed outside gaps

For UE configured with the E-UTRA-NR dual connectivity operation, the carrier-specific scaling factor CSSFoutside\_gap,i for intra-frequency SSB-based measurements, inter-frequency SSB-based measurements performed outside measurements gaps, intra-frequency CSI-RS L3 measurement and RSSI/channel occupancy measurement with no measurement gap on a carrier subject to CCA when SMTC and RMTC are overlapping will be as specified in Table 9.1.5.1.1-1.

Table 9.1.5.1.1-1: CSSFoutside\_gap,i scaling factor for EN-DC mode

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Scenario | *CSSF*outside\_gap,i for FR1 PSCC | *CSSF*outside\_gap,i for FR1 SCC | *CSSF*outside\_gap,i for FR2 PSCC | *CSSF*outside\_gap,i for FR2 SCC where neighbour cell measurement is required Note 2 | *CSSF*outside\_gap,i for FR2 SCC where neighbour cell measurement is not required | *CSSF*outside\_gap,i for inter-frequency MO with no measurement gp |
| **EN-DC with FR1 only CA** | 1+NPSCC\_CSIRS+NPSCC\_CCA\_RSSI/CO | NSCC\_SSB +Y+2x NSCC\_CSIRS + NSCC\_CCA\_RSSI/CO | N/A | N/A | N/A | NSCC\_SSB +Y+2x NSCC\_CSIRS |
| **EN-DC with**  **FR2 only intra band CA** | N/A | N/A | 1+NPSCC\_CSIRS | N/A | NSCC\_SSB +Y+2x NSCC\_CSIRS | NSCC\_SSB +Y+2x NSCC\_CSIRS |
| **EN-DC with**  **FR2 only inter band CA** | N/A | N/A | 1+NPSCC\_CSIRS | 2x(1+ NSCC\_CSIRS\_FR2\_NCM) Note 3,5 | 2×( NSCC\_SSB +Y+2x NSCC\_CSIRS -1-NSCC\_CSIRS\_NCM) | 2×( NSCC\_SSB +Y+2x NSCC\_CSIRS -1-NSCC\_CSIRS\_NCM) |
| **EN-DC with**  **FR1 +FR2 CA (FR1 PSCell) Note 1** | 1+NPSCC\_CSIRS | 2×( NSCC\_SSB +Y+2xNSCC\_CSIRS -1-NSCC\_CSIRS\_NCM) | N/A | 2x(1+NSCC\_CSIRS\_FR2\_NCM) Note 3 | 2×( NSCC\_SSB +Y+2x NSCC\_CSIRS -1-NSCC\_CSIRS\_NCM) | 2×( NSCC\_SSB +Y+2x NSCC\_CSIRS -1-NSCC\_CSIRS\_NCM) |
| **EN-DC with**  **FR1 +FR2 CA (FR2 PSCell) Note 1** | N/A | NSCC\_SSB +Y+2x NSCC\_CSIRS | 1+NPSCC\_CSIRS | N/A | NSCC\_SSB+Y+2x NSCC\_CSIRS | NSCC\_SSB+Y+2x NSCC\_CSIRS |
| Note 1: Only one NR FR1 operating band and one NR FR2 operating band are included for FR1+FR2 inter-band EN-DC.  Note 2: Selection of FR2 SCC where neighbour cell measurement is required follows clause 9.2.3.2.  Note 3: CSSFoutside\_gap,i =1 if only one SCell is configured and no inter-frequency MO without gap.  Note 4: Y is the number of configured inter-frequency MOs without MG that are being measured outside of MG  Note 5: Only two NR FR2 operating band are included for EN-DC with FR2 only inter-band CA  Note 6: NPSCC\_CSIRS=1 if PSCC is with either both SSB and CSI-RS based L3 configured or only CSI-RS based L3 measurement configured; otherwise, NPSCC =0.  Note 7: NSCC\_CSIRS=Number of configured SCell(s) with either both SSB and CSI-RS based L3 measurement configured or only CSI-RS based L3 measurement configured  Note 8: NSCC\_CSIRS\_FR2\_NCM=1 if FR2 SCC, where neighbour cell measurement is required, is with either both SSB and CSI-RS configured or only CSI-RS measurement configured; otherwise, NSCC\_CSIRS\_FR2\_NCM=0.  Note 9: NSCC\_SSB=Number of configured SCell(s) with only SSB based L3 measurement configured  Note 10: NPSCC\_CCA\_RSSI/CO= 1 if PSCC is configured with RSSI/CO measurements without MG when RMTC and SMTC are overlapping; NSCC\_CCA\_RSSI/CO = Number of MOs for SCell(s) configured with RSSI/CO measurements without MG when RMTC and SMTC are overlapping. | | | | | | |

##### 9.1.5.1.2 SA mode: carrier-specific scaling factor for SSB-based, CSI-RS based L3 measurements and RSSI and channel occupancy measurements performed outside gaps

For UE in SA operation mode, the carrier-specific scaling factor CSSFoutside\_gap,i for intra-frequency SSB-based measurements performed outside measurements gaps and RSSI/channel occupancy measurement with no measurement gap on a carrier subject to CCA when SMTC and RMTC are overlapping will be as specified in Table 9.1.5.1.2-1, which shall also be applied for a UE configured with NE-DC operation.

Table 9.1.5.1.2-1: CSSFoutside\_gap,i scaling factor for SA mode

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| Scenario | *CSSF*outside\_gap,i for FR1 PCC | *CSSF*outside\_gap,i for FR1 SCC | *CSSF*outside\_gap,i for FR2 PCC | *CSSF*outside\_gap,i for FR2 SCC where neighbour cell measurement is required | *CSSF* outside\_gap,i for FR2 SCC where neighbour cell measurement is not required | *CSSF*outside\_gap,i for inter-frequency MO with no measurement gap |
| **FR1 only CA** | 1+NPCC\_CSIRS + NPCC\_CCA\_RSSI/CO | NSCC\_SSB +Y+2x NSCC\_CSIRS + NSCC\_CCA\_RSSI/CO | N/A | N/A | N/A | NSCC\_SSB +Y+2x NSCC\_CSIRS |
| **FR2 only intra band CA** | N/A | N/A | 1+NPCC\_CSIRS | N/A | NSCC\_SSB +Y+2x NSCC\_CSIRS | NSCC\_SSB +Y+2x NSCC\_CSIRS |
| **FR2 only inter band CA** | N/A | N/A | 1 | 2\*(1+ NSCC\_CSIRS\_FR2\_NCM) Note 3,5 | 2×( NSCC\_SSB +Y+2x NSCC\_CSIRS -1-NSCC\_CSIRS\_NCM) | 2×( NSCC\_SSB +Y+2x NSCC\_CSIRS -1-NSCC\_CSIRS\_NCM) |
| **FR1 +FR2 CA (FR1 PCell) Note 1** | 1+NPCC\_CSIRS | 2×( NSCC\_SSB +Y+2\* NSCC\_CSIRS -1-NSCC\_CSIRS\_NCM) | N/A | 2x(1+ NSCC\_CSIRS\_FR2\_NCM) Note 3,5 | 2×( NSCC\_SSB +Y+2x NSCC\_CSIRS -1-NSCC\_CSIRS\_NCM) | 2×( NSCC\_SSB +Y+2x NSCC\_CSIRS -1-NSCC\_CSIRS\_NCM) |
| Note 1: Only one FR1 operating band and one FR2 operating band are included for FR1+FR2 inter-band CA.  Note 2: Selection of FR2 SCC where neighbour cell measurement is required follows clause 9.2.3.2.  Note 3: CSSFoutside\_gap,i =1 if only one SCell is configured and no inter-frequency MO without gap.  Note 4: Y is the number of configured inter-frequency MOs without MG that are being measured outside of MG.  Note 5: Only two NR FR2 operating bands are included for FR2 inter-band CA.  Note 6: NPCC\_CSIRS=1 if PCC is with either both SSB and CSI-RS based L3 configured or only CSI-RS based L3 measurement configured; otherwise, NPSCC =0.  Note 7: NSCC\_CSIRS=Number of configured SCell(s) with either both SSB and CSI-RS based L3 measurement configured or only CSI-RS based L3 measurement configured  Note 8: NSCC\_CSIRS\_FR2\_NCM=1 if FR2 SCC, where neighbour cell measurement is required, is with either both SSB and CSI-RS configured or only CSI-RS measurement configured; otherwise, NSCC\_CSIRS\_FR2\_NCM=0.  Note 9: NSCC\_SSB=Number of configured SCell(s) with only SSB based L3 measurement configured  Note 10: NPCC\_CCA\_RSSI/CO= 1 if PSCC is configured with RSSI/CO measurements without MG when RMTC and SMTC are overlapping; NSCC\_CCA\_RSSI/CO = Number of MOs for SCell(s) configured with RSSI/CO measurements without MG when RMTC and SMTC are overlapping. | | | | | | |

### <End of Change 1>

### <Start of Change 2>

#### 9.1.5.2 Monitoring of multiple layers within gaps

The carrier-specific scaling factor CSSFwithin\_gap,i for a measurement object *i* derived in this chapter is applied to following measurement types:

- SSB-based intra-frequency measurement object with no measurement gap in clause 9.2.5 and 9.2A.5, when all of the SMTC occasions of this intra-frequency measurement object are overlapped by the measurement gap.

- SSB-based intra-frequency measurement object with measurement gap in clause 9.2.6 and 9.2A.6.

-- CSI-RS based inter-frequency measurement in clause xxx, when CSI-RS resources for L3 measurement of this inter-frequency measurement object are overlapped by the measurement gap.

- CSI-RS based inter-frequency measurement in clause xxx, when CSI-RS resources for L3 measurement of this inter-frequency measurement object are partially overlapped by the measurement gap.

- SSB-based inter-frequency measurement object with measurement gap in clause 9.3.4.

- Including inter-frequency measurement with no measurement gap, when all of the SMTC occasions of this inter-frequency measurement object are overlapped by the measurement gap, if UE supports *interFrequencyMeas-NoGap-r16*.

- Intra-frequency RSSI/CO measurement with measurement gap in clause 9.2A.7.

- Intra-frequency RSSI/CO measurement with no measurement gap in clause 9.2A.7 when all of the RMTC occasions of this intra-frequency RSSI/CO measurement are overlapped by the measurement gap

- Inter-frequency RSSI/CO measurement in clause 9.3A.8 and 9.3A.9.

- E-UTRA Inter-RAT measurement object in clauses 9.4.2 and 9.4.3.

- NR PRS-based measurements for positioning in clause 9.9.

- E-UTRA Inter-RAT RSTD and E-CID measurements in clauses 9.4.4 and 9.4.5.

- NR Inter-RAT measurement object configured by the E-UTRAN PCell (TS 36.133 [15] clause 8.17.4).

- E-UTRAN Inter-frequency measurement object configured by the E-UTRAN PCell (TS 36.133 [15] clause 8.17.3) and by the E-UTRAN PSCell (TS 36.133 [15] clause 8.19.3).

- E-UTRAN Inter-frequency RSTD measurement configured by the E-UTRAN PCell (TS 36.133 [15] clause 8.17.15).

- UTRA Inter-RAT measurement object configured by the E-UTRAN PCell (TS 36.133 [15] clauses 8.17.5 to 8.17.12).

- GSM Inter-RAT measurements configured by the E-UTRAN PCell (TS 36.133 [15] clauses 8.17.13 and 8.17.14).

UE is expected to conduct the measurement of this measurement object *i* only within the measurement gaps.

If the higher layer signaling in TS 38.331 [2] of *smtc2* is present and *smtc1* is fully overlapping with measurement gaps and *smtc2* is partially overlapping with measurement gaps, CSSFwithin\_gap,i and requirements derived from CSSFoutside\_gap,i are not specified.

Number of SSB layers should include SSB for mobility and that as associated SSB for CSI-RS mobility. the ssbfrequency is counted only once if the ssbfrequency for mobility and associated SSB are the same, or ssbfrequency and smtc in multiple MOs are the same.

Editor’s note: FFS how to add the layer corresponding to the associated SSB for a MO with only CSI-RS measurement configured

##### 9.1.5.2.1 EN-DC mode: carrier-specific scaling factor for SSB, CSI-RS-based L3 measurements and RSSI and channel occupancy measurements performed within gaps

The scaling value CSSFwithin\_gap,i below has been derived without considering GSM inter-RAT carriers.

When one or more measurement objects are monitored within measurement gaps, the carrier specific scaling factor for a target measurement object with index *i* is designated as CSSFwithin\_gap,i and is derived as described in this clause.

If measurement object *i* refers to an RSTD measurement with periodicity Tprs>160ms or with periodicity Tprs=160ms but *prs-MutingInfo-r9* is configured, CSSFwithin\_gap,i=1. Otherwise, the CSSFwithin\_gap,i for other measurement objects (including RSTD measurement with periodicity Tprs=160ms) participate in the gap competition are derived as below.

For each measurement gap *j* not used for an RSTD measurement with periodicity Tprs>160ms or with periodicity Tprs=160ms but *prs-MutingInfo-r9* is configured within an arbitrary 160ms period, count the total number of intra-frequency measurement objects and inter-frequency/inter-RAT measurement objects which are candidates to be measured within the gap *j*.

- An NR measurement object with SSB measurement configured is a candidate to be measured in a gap if its SMTC duration is fully covered by the MGL excluding RF switching time. For intra-frequency NR carriers, if the higher layer in TS 38.331 [2] signaling of *smtc2* is configured, the assumed periodicity of SMTC occasions corresponds to the value of higher layer parameter *smtc2*; otherwise the assumed periodicity of SMTC occasions corresponds to the value of higher layer parameter *smtc1*.

- An NR measurement object with CSI-RS measurement configured is a candidate to be measured in a gap if the window confining all CSI-RS resources are fully covered by the MGL excluding RF switching time. -

- An NR measurement object with RSSI and channel occupancy measurement is a candidate to be measurement in a gap if the RMTC duration is fully covered by MGL excluding RF switching time

- An inter-RAT UTRA measurement object configured by E-UTRA PCell [15] is a candidate to be measured in all measurement gaps.

- An inter-frequency E-UTRA measurement object configured by E-UTRA PCell [15] is a candidate to be measured in all measurement gaps.

- For UEs which support and are configured with per FR gaps, the counting is done on a per FR basis, and for UEs which are configured with per UE gaps the counting is done on a per UE basis.

- Mintra,i,j: Number of intra-frequency measurement objects, including both SSB, CSI-RS based and RSSI/CO measurement, which are candidates to be measured in gap *j* where the measurement object *i* is also a candidate. Otherwise Mintra,i,j equals 0.

- Minter,i,j : Number of NR inter-frequency layers or NR inter-RAT frequency layer, including both SSB,CSI-RS based and RSSI/CO measurement, configured by E-UTRA PCell, EUTRA inter-frequency measurement objects configured by E-UTRA PCell, UTRA inter-RAT measurement objects configured by E-UTRA PCell which are candidates to be measured in gap *j* where the measurement object *i* is also a candidate. Otherwise Minter,i,j equals 0.

- A measurement object *i* in Mintra,i,j and in Minter,i,j is counted twice if the measurement object is configured with both RMTC and SMTC which are candidates to be measured in gap *j* where the measurement object *i* is also a candidate

- Mtot,i,j = Mintra,i,j + Minter,i,j : Total number of intra-frequency, inter-frequency and inter-RAT frequency layers which are candidates to be measured in gap *j* where the measurement object *i* is also a candidate. Otherwise Mtot,i,j equals 0.

For each measurement gap *j* used for an RSTD measurement with periodicity Tprs>160ms or with periodicity Tprs=160ms but *prs-MutingInfo-r9* is configured within an arbitrary 160ms period, Mintra,i,j = Minter,i,j = Mtot,i,j =0.

The carrier specific scaling factor CSSFwithin\_gap,i is given by:

If *measGapSharingScheme* is equal sharing, CSSFwithin\_gap,i= max(ceil(Ri×Mtot,i,j)), where *j*=0…(160/MGRP)-1

If *measGapSharingScheme* is not equal sharing and

- measurement object *i* is an intra-frequency measurement object, CSSFwithin\_gap,i is the maximum among

- ceil(Ri×Kintra×Mintra,i,j) in gaps where Minter,i,j≠0, where *j*=0…(160/MGRP)-1

- ceil(Ri×Mintra,i,j) in gaps where Minter,i,j=0, where *j*=0…(160/MGRP)-1

- measurement object *i* is an inter-frequency or inter-RAT measurement object, CSSFwithin\_gap,i is the maximum among

- ceil(Ri×Kinter×Minter,i,j) in gaps where Mintra,i,j ≠0, where *j*=0…(160/MGRP)-1

- ceil(Ri×Minter,i,j)in gaps where Mintra,i,j=0, where *j*=0…(160/MGRP)-1

Where Ri is the maximal ratio of the number of measurement gap where measurement object *i* is a candidate to be measured over the number of measurement gap where measurement object *i* is a candidate and not used for RSTD measurement with periodicity Tprs>160ms or with periodicity Tprs=160ms but *prs-MutingInfo-r9* is configured within an arbitrary 1280ms period.

##### 9.1.5.2.2 SA mode: carrier-specific scaling factor for SSB, CSI-RS-based L3 measurements and RSSI and channel occupancy measurements performed within gaps

When one or more measurement objects are monitored within measurement gaps, the carrier specific scaling factor for a target measurement object with index *i* is designated as CSSFwithin\_gap,i and is derived as described in this clause.

If measurement object *i* refers to a long-periodicity measurement which is any of:

- an E-UTRA RSTD measurement with periodicity Tprs>160ms or with periodicity Tprs=160ms but *prs-MutingInfo-r9* is configured, or

- an NR measurement for positioning based on PRS configurations in Table 9.1.5.2.2-1

then CSSFwithin\_gap,i=1. Otherwise, the CSSFwithin\_gap,i for other measurement objects (including E-UTRA RSTD measurement with periodicity Tprs=160ms) participate in the gap competition and the CSSFwithin\_gap,i are derived as below.

Table 9.1.5.2.2-1: PRS configurations for long-periodicity NR measurements for positioning

|  |  |
| --- | --- |
| [PRS periodicity] (ms) | DL-PRS-MutingPattern configuration |
| 320, 640, … ,10240 | [With or without muting] |
| Other values (≤ 160) | FFS |

For each measurement gap *j* not used for a long-periodicity measurement defined above, count the total number of intra-frequency measurement objects and inter-frequency/inter-RAT measurement objects and [TBD for NR positioning measurements] which are candidates to be measured within the gap *j*.

- An NR measurement object with SSB measurement configured is a candidate to be measured in a gap if its SMTC duration is fully covered by the MGL excluding RF switching time. For intra-frequency NR measurement objects, if the higher layer in TS 38.331 [2] signaling of *smtc2* is configured, the assumed periodicity of SMTC occasions corresponds to the value of higher layer parameter *smtc2*; otherwise the assumed periodicity of SMTC occasions corresponds to the value of higher layer parameter *smtc1*.

- An NR measurement object with CSI-RS measurement configured is a candidate to be measured in a gap if the window confining all CSI-RS resources are fully covered by the MGL excluding RF switching time.

- An NR measurement object with RSSI and channel occupancy measurement is a candidate to be measurement in a gap if the RMTC duration is fully covered by MGL excluding RF switching time

- An inter-frequency SFTD measurement object, if to be measured with measurement gaps, is a candidate to be measured in all measurement gaps.

- For UEs which support and are configured with per FR gaps, the counting is done on a per FR basis, and for UEs which are configured with per UE gaps the counting is done on a per UE basis. For UEs which support and are configured with per FR gaps, the CSSF requirements do not apply when NR PRS measurement in one FR gap collides with SSB/CSI-RS/PRS measurements in the other FR gap in time domain.

- Mintra,i,j: Number of intra-frequency measurement objects, including both SSB,CSI-RS based and RSSI/CO measurements, which are candidates to be measured in gap *j* where the measurement object *i* is also a candidate. Otherwise Mintra,i,j equals 0.

- Minter,i,j : Number of NR inter-frequency, EUTRA inter-RAT and UTRA inter-RAT frequency layers, including both SSB, CSI-RS based and RSSI/CO measurements, which are candidates to be measured in gap *j* where the measurement object *i* is also a candidate. Otherwise Minter,i,j equals 0.

- A measurement object *i* in Mintra,i,j and in Minter,i,j is counted twice if the measurement object is configured with both RMTC and SMTC which are candidates to be measured in gap *j* where the measurement object *i* is also a candidate

- Mtot,i,j = Mintra,i,j + Minter,i,j : Total number of intra-frequency, inter-frequency and inter-RAT frequncy layers and [TBD for NR positioning measurements] which are candidates to be measured in gap *j* where the measurement object *i* is also a candidate. Otherwise Mtot,i,j equals 0.

For each measurement gap *j* used for a long-periodicity measurement defined above, Mintra,i,j = Minter,i,j = Mtot,i,j =0. The carrier specific scaling factor CSSFwithin\_gap,i is given by:

If *measGapSharingScheme* is equal sharing, CSSFwithin\_gap,i= max(ceil(Ri×Mtot,i,j)), where *j*=0…(160/MGRP)-1

If *measGapSharingScheme* is not equal sharing and

- measurement object *i* is an intra-frequency measurement object, CSSFwithin\_gap,i is the maximum among

- ceil(Ri×Kintra×Mintra,i,j) in gaps where Minter,i,j≠0, where *j*=0…(160/MGRP)-1

- ceil(Ri×Mintra,i,j) in gaps where Minter,i,j=0, where *j*=0…(160/MGRP)-1

- measurement object *i* is an inter-frequency or inter-RAT measurement object or [TBD for NR positioning measurements], CSSFwithin\_gap,i is the maximum among

- ceil(Ri×Kinter×Minter,i,j) in gaps where Mintra,i,j ≠0, where *j*=0…(160/MGRP)-1

- ceil(Ri×Minter,i,j)in gaps where Mintra,i,j=0, where *j*=0…(160/MGRP)-1

Where Ri is the maximal ratio of the number of measurement gap where measurement object *i* is a candidate to be measured over the number of measurement gap where measurement object *i* is a candidate and not used for a long-periodicity measurement defined above.

CSSFwithin\_gap,k=1 during TDetect, E-UTRAN FDD specified in clause 9.4.4.1.2.2 and TDetect, E-UTRAN TDD specified in clause 9.4.4.2.2.2, where k is the carrier frequency where the UE is performing cell detection of the inter-RAT E-UTRA OTDOA assistance data reference cell when acquiring the subframe and slot timing of the cell according to clause 9.4.4. In this case, the UE cell identification and measurement periods derived based on CSSFwithin\_gap,i in clauses 9.2.5.1, 9.2.5.2, 9.2.6.2, 9.2.6.3, 9.3.4, 9.3.5, 9.4.2.2, 9.4.2.3 and 9.10.2 may be extended for measurement objects of which the cell identification and measurement periods are overlapped with TDetect, E-UTRAN FDD and TDetect, E-UTRAN TDD.

### <End of Change 2>