**3GPP TSG-RAN WG4 Meeting # 98-bis-e R4-2105682**

**Electronic Meeting, 12th – 20th April, 2021**

**Agenda item:** 5.7.1, 5.7.2.1, 5.7.2.2

**Source:** Moderator (CATT)

**Title:** Email discussion summary for [98-bis-e][212] NR\_CSIRS\_L3meas\_1

**Document for:** Information

# Introduction

The documents in agenda items 5.7.1, 5.7.2.1 and 5.7.2.2 contain the following 2 main topics:

* Topic #1: CSI-RS RRM core requirements maintenance
* Topic #2: CSI-RS RRM performance requirements.
  + Topic #2.1 CSI-RSRP requirements
  + Topic #2.2 CSI-RSRQ requirements
  + Topic #2.3 CSI-SINR requirements

# Topic #1: CSI-RS RRM core requirements maintenance

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2104692 | Xiaomi | **Proposal 1: When UE performs CSI-RS intra-frequency measurements in a TDD band, UE is not expected to transmit on data OFDM symbols overlapped by CSI-RS resource symbols to be measured, and 1 OFDM symbols before and after each consecutive CSI-RS symbols, where the serving cell is taken as the symbol level timing reference.**  **Observation: If different CSI-RS resources in the same MO fall in different window occasions, the throughput performance degradation is expected from network point of view.**  **Proposal 2: All CSI-RS resources in the same MO are configured in the same 5ms window.** |
| R4-2104733 | CATT | **Proposal 1: When UE performs CSI-RS intra-frequency measurements in a TDD band, UE is not expected to transmit PUCCH/PUSCH/SRS on CSI-RS resource symbols to be measured, and on 1 OFDM symbol before and after each consecutive CSI-RS symbols to be measured.**  **Proposal 2: For the applicability of CSI-RS L3 measurement on the CSI-RS configuration, one of the following options can be accepted:**   * **Option 1: All CSI-RS resources in the same MO are configured in the same 5ms window.** * **Option 2: The CSI-RS resources can be configured as**   **where and are time offsets (in millisecond) of CSI-RS resource i and j respectively.**  **Proposal 3: There is no need to define the starting point of the 5ms time window.** |
| R4-2104734 | CATT | **Draft CR** |
| R4-2104836 | Apple | **Proposal 1a: for CSI-RS based L3 intra-frequency measurement, the starting point of the 5ms window is the slot boundary of the serving cell, where the corresponding slot contains the first configured L3 CSI-RS resource of the serving cell in the intra-frequency MO.**  **Proposal 1a: for CSI-RS based L3 intra-frequency measurement, the starting point of the 5ms window is the boundary of slot N in the serving cell, where the following slot, i.e. slot N+1, contains the first configured L3 CSI-RS resource of the serving cell in the intra-frequency MO.**  **Proposal 2: Single periodicity and frequency offset is defined for all CSI-RS resources in the same MO. Consequently, all CSI-RS resources in the same MO should be configured in the same 5ms window.** |
| R4-2106410 | Nokia, Nokia Shanghai Bell | **Proposal1: We propose using the same way as in SSB-based measurements to define the scheduling restriction for CSI-RS based measurement, i.e. Option 2 is preferred:**   * **When UE performs CSI-RS intra-frequency measurements in a TDD band, UE is not expected to transmit PUCCH/PUSCH/SRS on CSI-RS resource symbols to be measured, and on 1 OFDM symbol before and after each consecutive CSI-RS symbols to be measured.**   **Proposal2: Different CSI-RS resources in the same MO may fall in different 5ms window.**  **Proposal3: It is unnecessary to specify the starting point as the location of the 5ms window is up to network configuration.**  **Proposal4: In Rel16, the UE is not required to measure the CSI-RS resource if the timing difference exceeds a threshold.** |
| R4-2106459 | Intel Corporation | **Proposal 1: All CSI-RS resources in the same MO are configured in the same 5ms window.**  **Proposal 2: It’s better that NW can order these timing offset of CSI-RS resources and make sure that the first configured L3 CSI-RS resource corresponding to the smallest offset.**  **Proposal 3: For CSI-RSRP, the upper bound of timing offset for case 1 is 1CP.** |
| R4-2106525 | OPPO | **Proposal 1: Requirement are defined for the cases where all CSI-RS resources in the same MO are configured in the same 5ms window.**  **Proposal 2: Define the starting point of the 5ms window as the slot boundary of the first configured L3 CSI-RS resource is located.**  **Proposal 3: Support option 1 that UE is not expected to transmit on data OFDM symbols overlapped by CSI-RS resource symbols to be measured, and 1 OFDM symbols before and after each consecutive CSI-RS symbol.** |
| R4-2106614 | vivo | ***Proposal 1a: All CSI-RS resources in the same MO are configured in the same 5ms window. Or***  ***Proposal 1b: All CSI-RS resources in the same MO are configured in the same 5ms window for inter frequency measurement, and measurement requirements should allow all CSI-RS resources in the same MO are configured in two separated 5ms windows during one CSI-RS resource period for intra frequency measurement.***  ***Proposal 2: Define the starting point of the 5ms window as the slot boundary where the first configured L3 CSI-RS resource during one CSI-RS periodicity is located.***  ***Proposal 3: When UE performs CSI-RS intra-frequency measurements in a TDD band, UE is not expected to transmit PUCCH/PUSCH/SRS on CSI-RS resource symbols, and on 1 OFDM symbol after the consecutive CSI-RS symbols.*** |
| R4-2106620 | vivo | **Draft CR** |
| R4-2106926 | Huawei, HiSilicon | **Proposal 1: as there are some possible understanding of uplink scheduling restriction, there are two options of defining uplink scheduling restrictions in TDD band in FR1:**  **- Option 1: If we regard the guard period before UL symbols as the scheduling restriction, the uplink scheduling restriction is: CSI-RS resource symbols to be measured, and 1 OFDM symbol (for 15kHz/30kHz SCS) or 2 OFDM symbols (for 60kHz) before CSI-RS resource symbols to be measured,** **and 1 OFDM symbol after CSI-RS resource symbols to be measured.**  **- Option 2: without considering GP, the uplink scheduling restriction is: CSI-RS resource symbols to be measured, and 1 OFDM symbol before and after CSI-RS resource symbols to be measured.**  **Proposal 2: Support the case where different CSI-RS resources in the same MO fall in different 5ms windows.**  **Proposal 3: RAN4 to further discuss the following options for defining CSI-RS measurement window.**   * **Based on configured CSI-RS resources, which requires SFN level sync from NW** * **Based on measured CSI-RS resources, which leads to the sliding window** |
| R4-2106927 | Huawei, HiSilicon | **Draft CR** |
| R4-2106928 | Huawei, HiSilicon | **Draft CR** |
| R4-2106929 | Huawei, HiSilicon | **Draft CR** |
| R4-2107218 | Qualcomm CDMA Technologies | **Observation1: further discussions are needed for distributing CSI-RS resources into multiple windows but RAN4 has limited time remained for this work item.**  **Proposal1: RAN4 may consider option2(multiple windows per resource period) in the future release if needed.**  **Proposal2: For a CSI-RS layer, the slot boundary of the resource with the smallest (slot) offset can be treated as the starting point of the 5ms window.**  **Proposal2.1: in other words, option2 can be clarified as defining the starting point of 5-ms window as the slot boundary of the resource with smallest offset for a CSI-RS frequency layer.**  **Proposal3: When UE performs CSI-RS intra-frequency measurements in a TDD band, UE is not expected to transmit PUCCH/PUSCH/SRS on CSI-RS resource symbols to be measured, and on 1 OFDM symbol before and after each consecutive configured CSI-RS.**  **Proposal3.1: restricted CSI-RS symbols are corresponding to the CSI-RS resources configured by the network.** |
| R4-2107365 | Qualcomm CDMA Technologies | **Observation1: further discussions are needed for distributing CSI-RS resources into multiple windows but RAN4 has limited time remained for this work item.**  **Proposal1: RAN4 may consider option2(multiple windows per resource period) in the future release if needed.**  **Proposal2: For a CSI-RS layer, the slot boundary of the resource with the smallest (slot) offset can be treated as the starting point of the 5ms window.**  **Proposal2.1: in other words, option2 can be clarified as defining the starting point of 5-ms window as the slot boundary of the resource with smallest offset for a CSI-RS frequency layer.**  **Proposal3: When UE performs CSI-RS intra-frequency measurements in a TDD band, UE is not expected to transmit PUCCH/PUSCH/SRS on CSI-RS resource symbols to be measured, and on 1 OFDM symbol before and after each consecutive configured CSI-RS.**  **Proposal3.1: restricted CSI-RS symbols are corresponding to the CSI-RS resources configured by the network.** |

## Open issues summary

### Sub-topic 1-1 Scheduling restriction for intra-f CSI-RS measurement in TDD band

* Proposals
  + Option 1: (Xiaomi, OPPO)
    - When UE performs CSI-RS intra-frequency measurements in a TDD band, UE is not expected to transmit on data OFDM symbols overlapped by CSI-RS resource symbols to be measured, and 1 OFDM symbols before and after each consecutive CSI-RS symbols, where the serving cell is taken as the symbol level timing reference
  + Option 2: (CATT, Nokia, Huawei)
    - When UE performs CSI-RS intra-frequency measurements in a TDD band, UE is not expected to transmit PUCCH/PUSCH/SRS on CSI-RS resource symbols to be measured, and on 1 OFDM symbol before and after each consecutive CSI-RS symbols to be measured.
  + Option 2a: (Qualcomm)
    - When UE performs CSI-RS intra-frequency measurements in a TDD band, UE is not expected to transmit PUCCH/PUSCH/SRS on configured CSI-RS resource symbols, and on 1 OFDM symbol before and after each consecutively configured CSI-RS symbols.
  + Option 3: (vivo)
    - When UE performs CSI-RS intra-frequency measurements in a TDD band, UE is not expected to transmit PUCCH/PUSCH/SRS on CSI-RS resource symbols, and on 1 OFDM symbol after the consecutive CSI-RS symbols
* Recommended WF
  + *Need more discussion*

|  |  |
| --- | --- |
| Sub-topic 1-1 Scheduling restriction for intra-f CSI-RS measurement in TDD band | |
| **Company** | **Comments** |
| Qualcomm | Option2a is supported.  Note the option aims to be precise about symbols that are configured because symbols to be measured are up for UE to determine and can be dynamic which may not be aware to the network. |
| MTK | Support Option 2a.  Option 1 is technically correct. But as other companies mentioned, the problem (also in other options) is that NW has no idea about UE’s absolute timing advance value. Therefore, we can compromise to Option 2 or 2a in which more margin is provided.  Option 2a additionally helps to resolve the issue that network does not have the knowledge about which CSI-RS UE will measure, which is determined by UE’s SSB detection results. |
|  |  |

### Sub-topic 1-2 Time domain restriction for CSI-RS configuration

**Issue 1-2: Whether the CSI-RS resources in the same MO can be configured in the different 5ms window?**

* Proposals
  + Option 1: (Xiaomi, CATT, Apple, Intel, OPPO, vivo, Qualcomm)
    - No. All CSI-RS resources in the same MO are configured in the same 5ms window.
  + Option 2a: (Nokia, Huawei)
    - Yes. Different CSI-RS resources in the same MO may fall in different 5ms window
  + Option 3a: (CATT)
    - The CSI-RS resources can be configured as

where and are time offsets (in millisecond) of CSI-RS resource i and j respectively.

* + Option 3b: (vivo)
    - All CSI-RS resources in the same MO are configured in the same 5ms window for inter frequency measurement, and measurement requirements should allow all CSI-RS resources in the same MO are configured in two separated 5ms windows during one CSI-RS resource period for intra frequency measurement.
* Recommended WF
  + *Need more discussion*

|  |  |
| --- | --- |
| Sub-topic 1-2 Time domain restriction for CSI-RS configuration | |
| **Company** | **Comments** |
| Qualcomm | Option1 is supported as it shouldnot result in any functional issue even without the enhancement. |
| MTK | Support Option 1.  Other options will create different gap overlapping status for CSI-RS resources in the same MO, e.g., some are overlapped by gap and some are not. We do not prefer RAN4 to open up this discussion in this very late Rel-16 stage. |
|  |  |

### Sub-topic 1-3 Starting point of 5ms time window

* Proposals
  + Option 1: (CATT, Nokia)
    - No need to define the starting point of the 5ms time window
  + Option 2a: (Apple)
    - For CSI-RS based L3 intra-frequency measurement, the starting point of the 5ms window is the slot boundary of the serving cell, where the corresponding slot contains the first configured L3 CSI-RS resource of the serving cell in the intra-frequency MO.
  + Option 2b: (Apple)
    - For CSI-RS based L3 intra-frequency measurement, the starting point of the 5ms window is the boundary of slot N in the serving cell, where the following slot, i.e. slot N+1, contains the first configured L3 CSI-RS resource of the serving cell in the intra-frequency MO.
  + Option 3: (Qualcomm)
    - Define the starting point of 5-ms window as the slot boundary of the resource with smallest offset for a CSI-RS frequency layer
  + Option 4: (OPPO, vivo)
    - Define the starting point of the 5ms window as the slot boundary where the first configured L3 CSI-RS resource during one CSI-RS periodicity is located
  + Option 5: (Intel)
    - NW can order these timing offset of CSI-RS resources and make sure that the first configured L3 CSI-RS resource corresponding to the smallest offset.
  + Option 6: (Huawei)
    - RAN4 to further discuss the following options for defining CSI-RS measurement window.
      * Based on configured CSI-RS resources, which requires SFN level sync from NW
      * Based on measured CSI-RS resources, which leads to the sliding window
* Recommended WF
  + *Need more discussion*

|  |  |
| --- | --- |
| Sub-topic 1-3 Starting point of 5ms time window | |
| **Company** | **Comments** |
| Qualcomm | Option3 is supported as it intends to base on the configured resource with the earliest offset, the slot boundary of which is regarded as the starting point. |
| MTK | Support Option 1 or Option 2a.  Slot index, boundary and SFN may not be the same between serving and neighboring cells. Therefore, Options 3, 4, 5 do not work. The second bullet of Option 6 is essentially the same as Option1 in our view. |
|  |  |

### Sub-topic 1-4 UE behavior when the timing offset exceeds the threshold

* Proposals
  + Option 1: (Nokia)
    - In Rel16, the UE is not required to measure the CSI-RS resource if the timing difference exceeds a threshold.
* Recommended WF
  + *Need more discussion*

|  |  |
| --- | --- |
| Sub-topic 1-4 UE behavior when the timing offset exceeds the threshold | |
| **Company** | **Comments** |
| Qualcomm | We feel it is up to the UE implementation and there can be other options. For examples, UE may not report. Or, NW may not use. |
| MTK | Fine with Option 1, but this should be limited to intra-frequency case with serving cell and neighboring cell CSI-RS aligned in the same OFDM symbol. |
|  |  |

### Sub-topic 1-5 Time validity of the detected associatedSSB

* Proposals
  + Option 1: (Huawei)
    - Adding the definition of detected associatedSSB in 9.10.2.5 section: The associatedSSB is detected if it has been meeting the relevant cell identification requirement during the last 5 seconds.
* Recommended WF
  + *Need more discussion*

|  |  |
| --- | --- |
| Sub-topic 1-5 Time validity of the detected associatedSSB | |
| **Company** | **Comments** |
| Qualcomm | Option1 is agreeable. |
| MTK | Ok with Option 1 |
|  |  |

## Companies views’ collection for 1st round

### Open issues

### CRs/TPs comments collection

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2104734 (CATT) | MTK: Section 9.10.2.5 was already modified by agreed CR R4-2103633. On top of 3633, we are not sure if the additional change “Note: TSSB\_time\_index\_intra is not defined for FR2 in 9.2.5.1.” is needed. |
| Company B |
|  |
| R4-2106620 (vivo) | Company A |
| Company B |
|  |
| R4-2106927 (Huawei) |  |
|  |
|  |
| R4-2106928 (Huawei) | MTK: pending on conclusion in open issue discussion. |
|  |
|  |
| R4-2106929 (Huawei) |  |
|  |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
| **Sub-topic #1** | *Tentative agreements:*  *Candidate options:*  *Recommendations for 2nd round:* |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provides recommendation on CRs/TPs Status update*

*Note: The tdoc decisions shall be provided in Section 3 and this table is optional in case moderators would like to provide additional information.*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation** |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

# Topic #2: CSI-RS RRM performance requirements

*Main technical topic overview. The structure can be done based on sub-agenda basis.*

## Companies’ contributions summary

|  |  |  |
| --- | --- | --- |
| **T-doc number** | **Company** | **Proposals / Observations** |
| R4-2104577 | MediaTek Inc. | **Proposal 1: Specify CSI-RSRP accuracy requirement with the absolute timing offset between UE’s FFT window and the target CSI-RS no larger than CP.** |
| R4-2104578 | MediaTek Inc. | **Proposal 1: Specify CSI-SINR accuracy requirement based on one of the following 2 options on timing offset (TΔ) and Es/Iot side condition**   * **Option 1: |TΔ |≤ CP/2 with Es/Iot ≤ 25dB** * **Option 2: |TΔ |≤ CP with Es/Iot ≤ 0 dB** |
| R4-2104735 | CATT | **Observation 1: The measurement accuracy for the timing offset CP and –CP has some small difference, but there is no significant performance gap between them.**  **Proposal 1: Specify CSI-RSRP measurement accuracy requirement when the timing offset between target CSI-RS and reference timing is smaller than or equal to CP.** |
| R4-2104736 | CATT | **Observation 1: The measurement accuracy for the timing offset CP and –CP has some small difference, but there is no significant performance gap between the results.**  **Proposal 1: Specify CSI-SINR measurement accuracy requirement when the timing offset between target CSI-RS and reference timing is smaller than or equal to CP, together with the side condition Es/Iot ≤ 15dB.** |
| R4-2104737 | CATT | **Draft CR for CSI-RSRP** |
| R4-2104738 | CATT | **Draft CR for CSI-RSRQ** |
| R4-2104739 | CATT | **Draft CR for CSI-SINR** |
| R4-2104937 | CMCC | **Simulation results for CSI-RSRP** |
| R4-2104938 | CMCC | **Simulation results for CSI-RSRQ** |
| R4-2104940 | CMCC | **Proposal 1: for CSI-RSRP, the upper bound of timing offset is proposed to be CP.** |
| R4-2104941 | CMCC | **Proposal 1: for CSI-RSRQ, the upper bound of timing offset is proposed to be CP.** |
| R4-2104942 | CMCC | **Proposal 1: for the specification of CSI-SINR measurement accuracy requirements, both Es/Iot ≤ [10] dB with timing offset within CP and Es/Iot ≤ [18] dB with timing offset within CP/2 are applied. For the test case, we can choose only one timing offset to design the test case.** |
| R4-2106411 | Nokia, Nokia Shanghai Bell | **Proposal1: The CSI-RS based measurement performance shall be defined when the timing offset is within one CP length.** |
| R4-2106412 | Nokia, Nokia Shanghai Bell | **Draft CR for CSI-RSRP** |
| R4-2106459 | Intel Corporation | **Proposal 1: All CSI-RS resources in the same MO are configured in the same 5ms window.**  **Proposal 2: It’s better that NW can order these timing offset of CSI-RS resources and make sure that the first configured L3 CSI-RS resource corresponding to the smallest offset.**  **Proposal 3: For CSI-RSRP, the upper bound of timing offset for case 1 is 1CP.** |
| R4-2106526 | OPPO | **Observation 1: The absolute measurement error of CSI-RS RSRP with negative timing offset is worse than that of CSI-RS RSRP with positive timing offset.**  **Observation 2: The absolute measurement error of CSI-RS RSRP can be within ±2.0dB for timing offset within [-0.5\*CP, +0.5\*CP], and ±3.0dB for timing offset within [-CP, +CP].**  **Observation 3: The relative measurement error of CSI-RS RSRP can be within ±1.5dB for timing offset within [-0.5\*CP, +0.5\*CP], and ±2.0dB for timing offset within [-CP, +CP].** |
| R4-2106527 | OPPO | **Observation 1: The absolute measurement error of CSI-RS RSRQ with negative timing offset is worse than that of CSI-RS RSRQ with positive timing offset.**  **Observation 2: The absolute measurement error of CSI-RS RSRQ can be within ±2.0dB for timing offset within [-0.5\*CP, +0.5\*CP], and ±3.0dB for timing offset within [-CP, +CP].**  **Observation 3: The relative measurement error of CSI-RS RSRQ can be within ±1.5dB for timing offset within [-0.5\*CP, +0.5\*CP], and ±2.0dB for timing offset within [-CP, +CP].** |
| R4-2106528 | OPPO | **Observation 1: The absolute accuracy performance of CSI-RS SINR can be found:**   * **For AWGN channel at FR1, ±4.0dB for timing offset within [-CP, +CP]** * **For TDL-A channel at FR2 ±6.0dB for timing offset within [-CP, +CP].**   **Observation 2: The relative accuracy performance of CSI-RS SINR can be found:**   * **For AWGN channel at FR1, ±2.0dB for timing offset within [-CP, +CP]** * **For TDL-A channel at FR2 ±5.50dB for timing offset within [-CP, +CP].**   **Observation 3: The absolute accuracy performance of CSI-RS SINR with negative timing offset is worse than that of CSI-RS SINR with positive timing offset.**  **Proposal 1: To ensure the absolute and relative accuracy performance of CSI-RS SINR can be reused as those of SSB’s, the upper bound of timing offset can be set within 0.9 CP.**  **Proposal 2: Option 3 as compromise for the upper limit of Es/Iot for CSI-SINR measurement with timing offset(T△):**   * **Option 3: Es/Iot ≤ [12] dB for the case that timing offset is within 0.9\*CP.** |
| R4-2106615 | vivo | **Proposal 1: The CSI-RSRP/CSI-RSRQ/CSI-SINR accuracy requirements are applicable when timing offset is within CP.** |
| R4-2106616 | vivo | *Observation 1.* If timining delay between two cells is smaller than CP, the absolute accuary of CSI-RSRP measurement with 5 samples is within ±2 dB in both FR1 and FR2.  *Observation 2.* The CSI-RSRP accuracy is comparable between timing offset of CP and 0.9CP.  *Observation 3.* The CSI-RSRP accuracy is comparable between corresponding positive timing offset and negative timing offset. |
| R4-2106617 | vivo | *Observation 1.* If timining delay between two cells is smaller than CP, the absolute accuary of CSI-RSRQ measurement with 5 samples is within ±2 dB in both FR1 and FR2.  *Observation 2.* The CSI-RSRQ accuracy is comparable between timing offset of CP and 0.9CP.  *Observation 3.* The CSI-RSRQ accuracy is comparable between corresponding positive timing offset and negative timing offset. |
| R4-2106618 | vivo | *Observation 1.* If timining delay between two cells is smaller than CP, the absolute accuary of CSI-SINR measurement with 5 samples is within ±2 dB in both FR1 and FR2.  *Observation 2.* The CSI-SINR accuracy is comparable between timing offset of CP and 0.9CP.  *Observation 3.* The CSI-SINR accuracy is comparable between corresponding positive timing offset and negative timing offset. |
| R4-2106619 | vivo | **Proposal 1a: The upper limit of Ês/Iot for CSI-SINR accuracy can be set as 15dB under the condition of timing offset is within CP/2.**  **Proposal 1b: The upper limit of Ês/Iot for CSI-SINR accuracy can be set as 25dB under the condition of timing offset is within CP/2 and for AWGN channel only.** |
| R4-2107023 | Huawei, HiSilicon | **Proposal: For CSI-RSRP and CSI-RSRQ the upper bound of timing offset for case 1 is 1\*CP.** |
| R4-2107024 | Huawei, HiSilicon | **Proposal: Define the CSI-SINR accuracy based on timing offset condition 0.9\*CP and the upper bound Es/Iot 6dB.** |
| R4-2107025 | Huawei, HiSilicon | **Draft CR for CSI-SINR** |
| R4-2107214 | Qualcomm CDMA Technologies | **Observation1: trivial degradation of the measurement error for 1CP relative to 0.9CP.**  **Observation2: simulated accuracy is the baseband accuracy only.**  **Proposal1: Same accuracy requirements as SSB based measurements can be resused for CSI-RSRP.**  **Proposal1.1: Cell timing offset of 1CP or 0.9 CP can be supported as the side condition.** |
| R4-2107215 | Qualcomm CDMA Technologies | **Es/Iot≤20dB with certain margin.**  **Proposal1: Support to reuse the accuracy requirements of SS-SINR measurement with the side condition of Es/Iot ≤ [18] dB for the case that timing offset is within CP/2** |

## Open issues summary

### Sub-topic 2-1 CSI-RSRP measurement accuracy requirements

**Issue 2-1: Timing offset for specifying CSI-RSRP measurement accuracy requirements**

* Proposals
  + Option 1: (MTK, CATT, CMCC, Nokia, Intel, vivo, Huawei, Qualcomm)
    - Specify CSI-RSRP accuracy requirement with the absolute timing offset between the reference measurement timing and the target CSI-RS in one layer no larger than CP
* Recommended WF
  + *Agree on option 1.*

|  |  |
| --- | --- |
| Sub-topic 2-1 Timing offset for specifying CSI-RSRP measurement accuracy requirements | |
| **Company** | **Comments** |
| Qualcomm | Option1 is supported |
| MTK | Support Option 1 |
|  |  |

### Sub-topic 2-2 CSI-RSRQ measurement accuracy requirements

**Issue 2-2: Timing offset for specifying CSI-RSRQ measurement accuracy requirements**

* Proposals
  + Option 1: (CMCC, vivo, Huawei)
    - Specify CSI-RSRQ accuracy requirement with the absolute timing offset between the reference measurement timing and the target CSI-RS in one layer no larger than CP
* Recommended WF
  + *Agree on option 1.*

|  |  |
| --- | --- |
| Sub-topic 2-2 CSI-RSRQ measurement accuracy requirements | |
| **Company** | **Comments** |
| Qualcomm | Option1 is supported |
| MTK | Support Option 1 |
|  |  |

### Sub-topic 2-3 CSI-SINR measurement accuracy requirements

**Issue 2-3: Timing offset and upper limit of side condition for specifying CSI-SINR measurement accuracy requirements**

* Proposals
  + Specify CSI-SINR accuracy requirement based on one of the following options on timing offset between the reference measurement timing and the target CSI-RS (TΔ) and Es/Iot side condition
    - When |TΔ |≤ CP/2
      * Option 1: (MTK, vivo)
        + Es/Iot ≤ 25 dB for AWGN only
      * Option 2: (Qualcomm)
        + Es/Iot ≤ [18]dB
    - When |TΔ |≤ CP
      * Option 3: (MTK)
        + Es/Iot ≤ 0 dB
      * Option 4: (CATT)
        + Es/Iot ≤ 15 dB
    - When |TΔ |≤ 0.9\*CP
      * Option 5: (OPPO)
        + Es/Iot ≤ [12] dB
      * Option 6: (Huawei)
        + Es/Iot ≤ 6dB
    - Option 7: (CMCC)
      * Both |TΔ |≤ CP with Es/Iot ≤ [10] dB and |TΔ |≤ CP/2 with Es/Iot ≤ [18] dB are applied. But choose one to design the test cases.
* Recommended WF
  + *Need more discussion.*

|  |  |
| --- | --- |
| Sub-topic 2-3 CSI-SINR measurement accuracy requirements | |
| **Company** | **Comments** |
| Qualcomm | Option2 is supported.  Option1 is also agreeable to us for AWGN only.  We also notice some options were not in line with the recommended WF.. for example, we are open to discuss option6 if companies are open for including 0.9CP. |
| MTK | Support Option 1 and Option 2.  To us, it is fine to slightly limit the timing offset in order to achieve good measurement accuracy in higher Es/Iot region. |
|  |  |

## Companies views’ collection for 1st round

### Open issues

### CRs/TPs comments collection

*Major close to finalize WIs and Rel-15 maintenance, comments collections can be arranged for TPs and CRs. For Rel-16 on-going WIs, suggest to focus on open issues discussion on 1st round.*

|  |  |
| --- | --- |
| **CR/TP number** | **Comments collection** |
| R4-2104737 (CATT) | Company A |
| Company B |
|  |
| R4-2104738 (CATT) | Company A |
| Company B |
|  |
| R4-2104739 (CATT) |  |
|  |
|  |
| R4-2106412 (Nokia) |  |
|  |
|  |
| R4-2107025 (Huawei) | MTK: pending on the conclusion in open issue. |
|  |
|  |

## Summary for 1st round

### Open issues

*Moderator tries to summarize discussion status for 1st round, list all the identified open issues and tentative agreements or candidate options and suggestion for 2nd round i.e. WF assignment.*

|  |  |
| --- | --- |
|  | **Status summary** |
| **Sub-topic#1** | *Tentative agreements:*  *Candidate options:*  *Recommendations for 2nd round:* |

### CRs/TPs

*Moderator tries to summarize discussion status for 1st round and provided recommendation on CRs/TPs Status update suggestion*

|  |  |
| --- | --- |
| **CR/TP number** | **CRs/TPs Status update recommendation** |
| XXX | *Based on 1st round of comments collection, moderator can recommend the next steps such as “agreeable”, “to be revised”* |

## Discussion on 2nd round (if applicable)

*Moderator can provide summary of 2nd round here. Note that recommended decisions on tdocs should be provided in the section titled ”Recommendations for Tdocs”.*

# Recommendations for Tdocs

## 1st round

**New tdocs**

|  |  |  |
| --- | --- | --- |
| **Title** | **Source** | **Comments** |
| WF on … | YYY |  |
| LS on … | ZZZ | To: RAN\_X; Cc: RAN\_Y |
|  |  |  |

**Existing tdocs**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Tdoc number** | **Title** | **Source** | **Recommendation** | **Comments** |
| R4-210xxxx | CR on … | XXX | Agreeable, Revised, Merged, Postponed, Not Pursued |  |
| R4-2104734 | draft CR on CSI-RS based L3 measurement | CATT |  |  |
| R4-2106620 | Draft CR to 38.133 Correction on core requirements for CSI-RS based measurement | vivo |  |  |
| R4-2106927 | CR on CSI-RS based intra-frequency scheduling restriction | Huawei |  |  |
| R4-2106928 | CR on CSI-RS measurement window and intra-frequency measurements | Huawei |  |  |
| R4-2106929 | Adding intra-frequency CSI-RS measurement in CSSF | Huawei |  |  |
| R4-2104737 | draft CR on performance requirement for CSI-RSRP | CATT |  |  |
| R4-2104738 | draft CR on performance requirement for CSI-RSRQ | CATT |  |  |
| R4-2104739 | draft CR on performance requirement for CSI-SINR | CATT |  |  |
| R4-2106412 | 38.133 draftCR on the CSI-RSRP accuracy requirements | Nokia |  |  |
| R4-2107025 | draftCR on CSI-SINR accuracy requirements | Huawei |  |  |

Notes:

1. Please include the summary of recommendations for all tdocs across all sub-topics incl. existing and new tdocs.
2. For the Recommendation column please include one of the following:
   1. CRs/TPs: Agreeable, Revised, Merged, Postponed, Not Pursued
   2. Other documents: Agreeable, Revised, Noted
3. For new LS documents, please include information on To/Cc WGs in the comments column
4. Do not include hyper-links in the documents

## 2nd round

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Tdoc number** | **Title** | **Source** | **Recommendation** | **Comments** |
| R4-210xxxx | CR on … | XXX | Agreeable, Revised, Merged, Postponed, Not Pursued |  |
| R4-210xxxx | WF on … | YYY | Agreeable, Revised, Noted |  |
| R4-210xxxx | LS on … | ZZZ | Agreeable, Revised, Noted |  |
|  |  |  |  |  |

Notes:

1. Please include the summary of recommendations for all tdocs across all sub-topics.
2. For the Recommendation column please include one of the following:
   1. CRs/TPs: Agreeable, Revised, Merged, Postponed, Not Pursued
   2. Other documents: Agreeable, Revised, Noted
3. Do not include hyper-links in the documents