**3GPP TSG-RAN WG4 Meeting #98-bis-e *R4-2106419***

**E-meeting, 12th April – 20th April 2021**

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **38.101-4** | **CR** | **-** | **rev** | **-** | **Current version:** | **16.4.0** |  |
|  |
| *For* [***HELP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME | **X** | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** | Intel Corporation |
| ***Source to TSG:*** | RAN4 |
|  |  |
| ***Work item code:*** | 5G\_V2X\_NRSL-Perf |  | ***Date:*** | 2021-04-02 |
|  |  |  |  |  |
| ***Category:*** | **B** |  | ***Release:*** | Rel-16 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | Definition of NR V2X Single Link PSCCH requirements |
|  |  |
| ***Summary of change:*** | Changes in comparison to R4-2103976* Update of PSSCH RMC
* Remove of communication resource pool configuration from test description
* SNR point for requirements
 |
|  |  |
| ***Consequences if not approved:*** | NR V2X Single Link PSCCH requirements are not defined |
|  |  |
| ***Clauses affected:*** | 11.1.3 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  |  |
| ***affected:*** | **X** |  |  Test specifications | TS 38.521-4  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications |  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

**START OF CHANGE**

11.1.3 PSCCH demodulation requirements

#### 11.1.3.1 2Rx requirements

##### 11.1.3.1.1 Minimum requirements

The purpose of the requirements in this subclause is to verify the PSCCH for V2X demodulation performance with a single active PSSCH link.

The minimum requirements are specified in Table 11.1.3.1.1-2 with the test parameters specified in Table 11.1.3.1.1-1. In this test scenario, GNSS or GNSS-equivalent synchronization source is used and Sidelink UE 1 transmits PSCCH and PSSCH.

Table 11.1.3.1.1-1: Test Parameters

|  |  |  |
| --- | --- | --- |
| Parameter | Unit | Test 1 |
|  |  |  |
| Active cell(s) |  | None |
| Sidelink UE 1 | Sidelink Transmissions |  | PSCCH+PSSCH |
| Timing offset (Note 1) |  | CP/2-12\*64\*Tc |
| Frequency offset (Note 2) | Hz | +600 |
| Synchronization |  | GNSS or GNSS-equivalent |
| Antenna configuration |  | 1x2 Low |
| PSSCH RMC |  | R.PSSCH.2-1.1 |
| NOTE 1: Time offset of Sidelink UE receive signal with respect to GNSS reference timing.NOTE 2: Frequency offset of Sidelink UE with respect to GNSS reference frequency.NOTE 3: OCC index i for PSCCH DMRS is randomly selected from {0, 1, 2} for each PSCCH transmission. |

Table 11.1.3.1.1-2: Minimum performance

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Test number | PSCCH Reference channel | Bandwidth (MHz) / Subcarrier spacing (kHz) | Propagation condition | Reference value |
| Probability of missed PSCCH (%) | SNR (dB) of PSCCH |
| 1 | R.PSCCH.2-1.1 | 20 / 30 | TDLA30-1400 | 1 | [4.6] |

**END OF CHANGE**