**3GPP TSG-SA WG2 Meeting #141E S2-200xxxx**

**Elbonia, 12 – 23 Oct. 2020, Electronic meeting**

**Title: LS on Enhancement of RAN Slicing**

**Response to: S2-200xxxx/R3-205802**

**Release:** **Rel-17**

**Work Item: FS\_eNS\_Ph2**

**Source:** SA2

**To:** RAN3

**Cc:** RAN2

**Contact Person:**

#### **Name:** Tricci So

**Tel. Number:**

E-mail Address: TSO@ZTETX.COM

**Send any reply LS to: 3GPP Liaisons Coordinator,** [**mailto:3GPPLiaison@etsi.org**](mailto:3GPPLiaison@etsi.org)

**Attachments:**

**1. Overall Description:**

SA2 thanks RAN3 for sharing the use cases for studying the RAN part of slicing service continuity support.

According to TS 23.501, Table 5.6.1-1: Attributes of a PDU Session, it has been identified in NOTE 4 that the S-NSSAI value of the Serving PLMN associated to a PDU Session can change whenever the UE moves to a different PLMNs while handing over the PDU Session. Hence, SA2 would agree with RAN3 that the change of S-NSSAI for a given PDU session within the serving PLMN could also happen.

SA2 will wait for RAN3’s conclusions on the study for these scenarios before examining the impacts to SA2 specifications in order to support RAN3’s decision for the appropriate solution.

**2. Actions:**

**To RAN3:**

**ACTION:**

SA2 requests RAN3 to keep us informed on the outcome of your study.

**3. Date of Next TSG-SA2 Meetings:**

3GPP TSG SA2#142E 16th – 20th November 2020 eMeeting