**3GPP TSG-WG SA2 Meeting #161 *S2-2403403***

**Athens, Greece, Feb 26 – Mar 1, 2024 (revision of S2-2402723)**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  | **23.304** | **CR** | **0432** | **rev** | **1** | **Current version:** | **18.4.0** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Clarification on multi-path communication via Uu and via 5G ProSe UE-to-Network Relay |
|  |  |
| ***Source to WG:*** | Huawei, HiSilicon |
| ***Source to TSG:*** | SA2 |
|  |  |
| ***Work item code:*** | 5G\_ProSe\_Ph2 |  | ***Date:*** | 2024-02-27 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-18 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | Path management of the 5G ProSe Layer-2 Remote UE is defined in 38.300 RAN specifcation, and SA2 needs to correlates to it. |
|  |  |
| ***Summary of change:*** | Path management of Remote UE is controlled by gNB, as specified in clause 16.21 of TS 38.300 |
|  |  |
| ***Consequences if not approved:*** | Incomplete spec. |
|  |  |
| ***Clauses affected:*** | 5.17.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\* \* \* \* First change \* \* \* \*

### 6.9.3 Multi-path communication via direct Uu path and via 5G ProSe Layer-2 UE-to-Network Relay

Procedures for Multi-path communication via direct Uu path and via 5G ProSe Layer-2 UE-to-Network Relay is specified in TS 38.300 [12].

ath management of the 5G ProSe Layer-2 Remote UE is specified in clause 16.21 of TS 38.300 [12].

\* \* \* \* End of changes \* \* \* \*