3GPP TSG SA WG 3 Meeting SA3#104e S3-213170-r1

Electronic meeting, Online, 16 - 27 August 2021

**Title:** [Draft] LS on Home Network triggered re-authentication

**Release:** Release-17

**Work Item:** TEI17

**Source:** SA3

**To:** **SA2, CT1,** CT4

**Cc:** -

**Contact person:** Rajavelsamy Rajadurai

 Rajvel@]Samsung.com

**Send any reply LS to: 3GPP Liaisons Coordinator, mailto:3GPPLiaison@etsi.org**

**Attachments:** None

# 1 Overall description

SA3 has been discussing to specify a procedure, which allows the home network (particularly UDM and/or AUSF) to trigger re-authentication procedure, whenever the home network needs to refresh the key KAUSF.

Key KAUSF that is shared between the UE and the home network, is refreshed when primary authentication procedure is performed successfully. It is SA3 understanding that, while the UE can refresh the key KAUSF by sending the ngKSI with value "111" to the AMF, but the UDM/AUSF doesn't have a procedure of triggering re-authentication of the UE to refresh KAUSF.

SA3 is aware of the application error *(REAUTHENTICATION\_REQUIRED)* specified in TS 29.503, where the error response returned by the UDM services to the AMF indicates that the UE needs to be re-authenticated. SA3 understanding is that this application error is provided in response to a request from the AMF and it is not provided by the UDM without a request from the AMF.

SA3 would like to ask SA2, CT1 and CT4:

1) Is it possible for the UDM to send the application error *(REAUTHENTICATION\_REQUIRED)* to the AMF without a request from the AMF.

2) Whether SA2 and CT4 has already specified any procedure that allows the home network (particularly UDM and/or AUSF) to trigger re-authentication procedure.

3) If the answer to Q2 is yes. Whether the trigger of setting the ngKSI with value “111” by the UE has been defined in CT1.

# 2 Actions

**To SA2, CT1 and CT4**

**ACTION:** SA3 kindly asks SA2, CT1 and CT4:

**Q1**. Is it possible for the UDM to send the application error (REAUTHENTICATION\_REQUIRED) to the AMF without a request from the AMF.

**Q2**. To inform whether SA2 and CT4 has already specified any procedure that allows the home network (particularly UDM and/or AUSF) to trigger re-authentication.

Q3. If the answer to Q2 is yes. Whether the trigger of setting the ngKSI with value “111” by the UE has been defined in CT1

# 3 Dates of next TSG SA WG 3 meetings

Please see the SA3 link from the 3GPP calendar page at [https://portal.3gpp.org/Home.aspx?tbid=386&SubTB=386#/](https://portal.3gpp.org/Home.aspx?tbid=386&SubTB=386" \l "/)