**3GPP TSG-SA3 Meeting #106-e  *draft\_S3-220225-r1***

e-meeting, 14 - 25 February 2022

|  |
| --- |
| *CR-Form-v12.1* |
| **CHANGE REQUEST** |
|  |
|  | **33.501** | **CR** | **1294** | **rev** | **1** | **Current version:** | **17.4.2** |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network |  |

|  |
| --- |
|  |
| ***Title:***  | Clarification on AS security aspect in 5MBS |
|  |  |
| ***Source to WG:*** | LG Electronics |
| ***Source to TSG:*** | S3 |
|  |  |
| ***Work item code:*** | 5MBS |  | ***Date:*** | 2022-02-23 |
|  |  |  |  |  |
| ***Category:*** | **F** |  | ***Release:*** | Rel-17 |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-15 (Release 15)Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)* |
|  |  |
| ***Reason for change:*** | In W.4.1.1, there is a sentence mentioning about AS security aspect in regards to MBS traffic as brought below * The multicast security policy between UE and RAN shall be not needed to avoid redundant protection.

In the above sentence, the definition of the multicast security policy is unclear, and the meaning of the sentence is somewhat misleading. * This sentence should be modified to clearly indicate that the user plane security between UE and RAN shall be deactivated as the MBS traffic is already protected in service layer.
* It also needs to be clarified which type of MBS traffic delivery the above sentence is applied for.
 |
|  |  |
| ***Summary of change:*** | It is proposed to update the sentence to be more clear and accurate. |
|  |  |
| ***Consequences if not approved:*** | The above mentioned sentence would remain misleading and unclear.  |
|  |  |
| ***Clauses affected:*** | W.4.1.1 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

\*\*\* 1st CHANGE \*\*\*

# W.4 Security mechanisms for MBS traffic transmission

## W.4.1 Key derivation, management and distribution

### W.4.1.1 General

For security protection of MBS traffic, control-plane procedure and user-plane procedure are optionally supported in service layer. The user plane security between UE and RAN shall be deactivated when 5GC shared MBS traffic delivery method for MBS data transmission is used to avoid redundant protection.

\*\*\* END OF CHANGES \*\*\*