**3GPP TSG-SA3 Meeting #86-LI-e-a *s3i220333***

**Online, , 13th Jul 2022 - 15th Jul 2022**

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| *CR-Form-v12.2* | | | | | | | | |
| **CHANGE REQUEST** | | | | | | | | |
|  | | | | | | | | |
|  | **33.128** | **CR** | **0370** | **rev** | **1** | **Current version:** | **18.0.0** |  |
|  | | | | | | | | |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* | | | | | | | | |
|  | | | | | | | | |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | | | | |
| ***Title:*** |  | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Source to WG:*** | SA3-LI (OTD) | | | | | | | | | |
| ***Source to TSG:*** | SA3 | | | | | | | | | |
|  |  | | | | | | | | | |
| ***Work item code:*** | LI17 | | | | |  | ***Date:*** | | | 2022-07-13 |
|  |  | | | |  | |  | | |  |
| ***Category:*** | **A** |  | | | | | ***Release:*** | | | Rel-18 |
|  | *Use one of the following categories:* ***F*** *(correction)* ***A*** *(mirror corresponding to a change in an earlier release)* ***B*** *(addition of feature),* ***C*** *(functional modification of feature)* ***D*** *(editorial modification)*  Detailed explanations of the above categories can be found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | | | | | | | | *Use one of the following releases: Rel-8 (Release 8) Rel-9 (Release 9) Rel-10 (Release 10) Rel-11 (Release 11) … Rel-16 (Release 16) Rel-17 (Release 17) Rel-18 (Release 18) Rel-19 (Release 19)* | |
|  |  | | | | | | | | | |
| ***Reason for change:*** | | EUI64 was added to ETSI TS 103 221-1 but the updates were not put in TS 33.128. This CR adds EUI64 as a target identifier format and also adds the paging restriction indicator to the AMFRegistration record. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Summary of change:*** | | Add EUI64 to target identifier formats. Add paging restriction indicator to the AMFRegistration record. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Consequences if not approved:*** | | Specification will not be aligned to ETSI TS 103 221-1. Paging restriction indicator (R17 feature) will not be singalled to LEAs. | | | | | | | | |
|  | |  | | | | | | | | |
| ***Clauses affected:*** | | 6.2.2, 6.2.2.2, Annex A | | | | | | | | |
|  | |  | | | | | | | | |
|  | | **Y** | **N** |  | | | |  | | |
| ***Other specs*** | |  | **X** | Other core specifications | | | | TS/TR ... CR ... | | |
| ***affected:*** | |  | **X** | Test specifications | | | | TS/TR ... CR ... | | |
| ***(show related CRs)*** | |  | **X** | O&M Specifications | | | | TS/TR ... CR ... | | |
|  | |  | | | | | | | | |
| ***Other comments:*** | | This CR is the R18 mirror for CR 0369.  ASN.1 for this CR can be found in Forge:  <https://forge.3gpp.org/rep/sa3/li/-/merge_requests/59/diffs?commit_id=71a437d9bd6be9b531f25ba07c84b9402b5faaa9>  Commit hash: [71a437d9bd6be9b531f25ba07c84b9402b5faaa9](https://forge.3gpp.org/rep/sa3/li/-/commit/71a437d9bd6be9b531f25ba07c84b9402b5faaa9) | | | | | | | | |
|  | |  | | | | | | | | |
| ***This CR's revision history:*** | | s3i22033 | | | | | | | | |

START OF CHANGES

START OF FIRST CHANGE

##### 6.2.2.2.2 Registration

The IRI-POI in the AMF shall generate an xIRI containing an AMFRegistration record when the IRI-POI present in the AMF detects that a UE matching one of the target identifiers provided via LI\_X1 has successfully registered to the 5GS via 3GPP NG-RAN or non-3GPP access. Accordingly, the IRI-POI in the AMF generates the xIRI when the following event is detected:

- AMF sends a N1: REGISTRATION ACCEPT message to the target UE and the UE 5G Mobility Management (5GMM) state for the access type (3GPP NG-RAN or non-3GPP access) within the AMF is changed to 5GMM-REGISTERED.

Table 6.2.2-1: Payload for AMFRegistration record

|  |  |  |
| --- | --- | --- |
| Field name | Description | M/C/O |
| registrationType | Specifies the type of registration, see TS 24.501 [13] clause 9.11.3.7. This is derived from the information received from the UE in the REGISTRATION REQUEST message. | M |
| registrationResult | Specifies the result of registration, see TS 24.501 [13] clause 9.11.3.6. | M |
| slice | Provide, if available, one or more of the following:  - allowed NSSAI (see TS 24.501 [13] clause 9.11.3.37).  - configured NSSAI (see TS 24.501 [13] clause 9.11.3.37).  - rejected NSSAI (see TS 24.501 [13] clause 9.11.3.46).  This is derived from the information sent to the UE in the REGISTRATION ACCEPT message. | C |
| sUPI | SUPI associated with the registration (see clause 6.2.2.4). | M |
| sUCI | SUCI used in the registration, if available. | C |
| pEI | PEI provided by the UE during the registration, if available. | C |
| gPSI | GPSI obtained in the registration, if available as part of the subscription profile. | C |
| gUTI | 5G-GUTI provided as outcome of initial registration or used in other cases, see TS 24.501 [13] clause 5.5.1.2.2. | M |
| location | Location information determined by the network during the registration, if available.  Encoded as a *userLocation* parameter (*location>locationInfo>userLocation*) and, when Dual Connectivity is activated, as an *additionalCellIDs* parameter (*location>locationInfo>additionalCellIDs*), see Annex A. | C |
| non3GPPAccessEndpoint | UE's local IP address used to reach the N3IWF, TNGF or TWIF, if available. IP addresses are given as 4 octets (for IPv4) or 16 octets (for IPv6) with the most significant octet first (network byte order). | C |
| fiveGSTAIList | List of tracking areas associated with the registration area within which the UE is current registered, see TS 24.501 [13] clause 9.11.3.9 (see NOTE) | C |
| sMSoverNASIndicator | Indicates whether SMS over NAS is supported. Provide, if included in registrationResult, see TS 24.501 [13] clause 9.11.3.6. | C |
| oldGUTI | GUTI or 5G-GUTI, if provided in the REGISTRATION REQUEST message, see TS 24.501 [13] clause 5.5.1.2.2. | C |
| eMM5GRegStatus | UE Status, if provided in the REGISTRATION REQUEST message, see TS 24.501 [13] clause 9.11.3.56. | C |
| nonIMEISVPEI | MACAddress or EUI-64 used as UE equipment identity if IMEI or IMEISV based PEI is not available. Provide if known, see TS 24.501 [13] clause 8.2.26.4. | C |
| mACRestIndicator | Indicates whether the non-IMEISV PEI MACAddress can be used as an equipment identifier. Required if non-IMEISVPEI is used, see TS 24.501 [13] clause 9.11.3.4. | C |
| pagingRestrictionIndicator | Indicates if paging is restricted and the type of paging allowed, Shall include the IEI and length octets. Include if sent in the REGISTRATION REQUEST message. See TS 24.501 [13] clause 9.11.3.77.2 for encoding. | C |
| NOTE: List shall be included each time there is a change to the registration area. | | |

END OF FIRST CHANGE

START OF SECOND CHANGE

Annex A (normative):  
ASN.1 Schema for the Internal and External Interfaces

TS33128Payloads

{itu-t(0) identified-organization(4) etsi(0) securityDomain(2) lawfulIntercept(2) threeGPP(4) ts33128(19) r18(18) version0(0)}

DEFINITIONS IMPLICIT TAGS EXTENSIBILITY IMPLIED ::=

BEGIN

-- =============

-- Relative OIDs

-- =============

tS33128PayloadsOID RELATIVE-OID ::= {threeGPP(4) ts33128(19) r18(18) version0(0)}

xIRIPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID xIRI(1)}

xCCPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID xCC(2)}

iRIPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID iRI(3)}

cCPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID cC(4)}

lINotificationPayloadOID RELATIVE-OID ::= {tS33128PayloadsOID lINotification(5)}

-- ===============

-- X2 xIRI payload

-- ===============

XIRIPayload ::= SEQUENCE

{

xIRIPayloadOID [1] RELATIVE-OID,

event [2] XIRIEvent

}

XIRIEvent ::= CHOICE

{

-- Access and mobility related events, see clause 6.2.2

registration [1] AMFRegistration,

deregistration [2] AMFDeregistration,

locationUpdate [3] AMFLocationUpdate,

startOfInterceptionWithRegisteredUE [4] AMFStartOfInterceptionWithRegisteredUE,

unsuccessfulAMProcedure [5] AMFUnsuccessfulProcedure,

-- PDU session-related events, see clause 6.2.3

pDUSessionEstablishment [6] SMFPDUSessionEstablishment,

pDUSessionModification [7] SMFPDUSessionModification,

pDUSessionRelease [8] SMFPDUSessionRelease,

startOfInterceptionWithEstablishedPDUSession [9] SMFStartOfInterceptionWithEstablishedPDUSession,

unsuccessfulSMProcedure [10] SMFUnsuccessfulProcedure,

-- Subscriber-management related events, see clause 7.2.2

servingSystemMessage [11] UDMServingSystemMessage,

-- SMS-related events, see clause 6.2.5, see also sMSReport ([56] below)

sMSMessage [12] SMSMessage,

-- LALS-related events, see clause 7.3.1

lALSReport [13] LALSReport,

-- PDHR/PDSR-related events, see clause 6.2.3.4.1

pDHeaderReport [14] PDHeaderReport,

pDSummaryReport [15] PDSummaryReport,

-- tag 16 is reserved because there is no equivalent mDFCellSiteReport in XIRIEvent

-- MMS-related events, see clause 7.4.2

mMSSend [17] MMSSend,

mMSSendByNonLocalTarget [18] MMSSendByNonLocalTarget,

mMSNotification [19] MMSNotification,

mMSSendToNonLocalTarget [20] MMSSendToNonLocalTarget,

mMSNotificationResponse [21] MMSNotificationResponse,

mMSRetrieval [22] MMSRetrieval,

mMSDeliveryAck [23] MMSDeliveryAck,

mMSForward [24] MMSForward,

mMSDeleteFromRelay [25] MMSDeleteFromRelay,

mMSDeliveryReport [26] MMSDeliveryReport,

mMSDeliveryReportNonLocalTarget [27] MMSDeliveryReportNonLocalTarget,

mMSReadReport [28] MMSReadReport,

mMSReadReportNonLocalTarget [29] MMSReadReportNonLocalTarget,

mMSCancel [30] MMSCancel,

mMSMBoxStore [31] MMSMBoxStore,

mMSMBoxUpload [32] MMSMBoxUpload,

mMSMBoxDelete [33] MMSMBoxDelete,

mMSMBoxViewRequest [34] MMSMBoxViewRequest,

mMSMBoxViewResponse [35] MMSMBoxViewResponse,

-- PTC-related events, see clause 7.5.2

pTCRegistration [36] PTCRegistration,

pTCSessionInitiation [37] PTCSessionInitiation,

pTCSessionAbandon [38] PTCSessionAbandon,

pTCSessionStart [39] PTCSessionStart,

pTCSessionEnd [40] PTCSessionEnd,

pTCStartOfInterception [41] PTCStartOfInterception,

pTCPreEstablishedSession [42] PTCPreEstablishedSession,

pTCInstantPersonalAlert [43] PTCInstantPersonalAlert,

pTCPartyJoin [44] PTCPartyJoin,

pTCPartyDrop [45] PTCPartyDrop,

pTCPartyHold [46] PTCPartyHold,

pTCMediaModification [47] PTCMediaModification,

pTCGroupAdvertisement [48] PTCGroupAdvertisement,

pTCFloorControl [49] PTCFloorControl,

pTCTargetPresence [50] PTCTargetPresence,

pTCParticipantPresence [51] PTCParticipantPresence,

pTCListManagement [52] PTCListManagement,

pTCAccessPolicy [53] PTCAccessPolicy,

-- More Subscriber-management related events, see clause 7.2.2

subscriberRecordChangeMessage [54] UDMSubscriberRecordChangeMessage,

cancelLocationMessage [55] UDMCancelLocationMessage,

-- SMS-related events continued from choice 12

sMSReport [56] SMSReport,

-- MA PDU session-related events, see clause 6.2.3.2.7

sMFMAPDUSessionEstablishment [57] SMFMAPDUSessionEstablishment,

sMFMAPDUSessionModification [58] SMFMAPDUSessionModification,

sMFMAPDUSessionRelease [59] SMFMAPDUSessionRelease,

startOfInterceptionWithEstablishedMAPDUSession [60] SMFStartOfInterceptionWithEstablishedMAPDUSession,

unsuccessfulMASMProcedure [61] SMFMAUnsuccessfulProcedure,

-- Identifier Association events, see clauses 6.2.2.2.7 and 6.3.2.2.2

aMFIdentifierAssociation [62] AMFIdentifierAssociation,

mMEIdentifierAssociation [63] MMEIdentifierAssociation,

-- PDU to MA PDU session-related events, see clause 6.2.3.2.8

sMFPDUtoMAPDUSessionModification [64] SMFPDUtoMAPDUSessionModification,

-- NEF services related events, see clause 7.7.2

nEFPDUSessionEstablishment [65] NEFPDUSessionEstablishment,

nEFPDUSessionModification [66] NEFPDUSessionModification,

nEFPDUSessionRelease [67] NEFPDUSessionRelease,

nEFUnsuccessfulProcedure [68] NEFUnsuccessfulProcedure,

nEFStartOfInterceptionWithEstablishedPDUSession [69] NEFStartOfInterceptionWithEstablishedPDUSession,

nEFdeviceTrigger [70] NEFDeviceTrigger,

nEFdeviceTriggerReplace [71] NEFDeviceTriggerReplace,

nEFdeviceTriggerCancellation [72] NEFDeviceTriggerCancellation,

nEFdeviceTriggerReportNotify [73] NEFDeviceTriggerReportNotify,

nEFMSISDNLessMOSMS [74] NEFMSISDNLessMOSMS,

nEFExpectedUEBehaviourUpdate [75] NEFExpectedUEBehaviourUpdate,

-- SCEF services related events, see clause 7.8.2

sCEFPDNConnectionEstablishment [76] SCEFPDNConnectionEstablishment,

sCEFPDNConnectionUpdate [77] SCEFPDNConnectionUpdate,

sCEFPDNConnectionRelease [78] SCEFPDNConnectionRelease,

sCEFUnsuccessfulProcedure [79] SCEFUnsuccessfulProcedure,

sCEFStartOfInterceptionWithEstablishedPDNConnection [80] SCEFStartOfInterceptionWithEstablishedPDNConnection,

sCEFdeviceTrigger [81] SCEFDeviceTrigger,

sCEFdeviceTriggerReplace [82] SCEFDeviceTriggerReplace,

sCEFdeviceTriggerCancellation [83] SCEFDeviceTriggerCancellation,

sCEFdeviceTriggerReportNotify [84] SCEFDeviceTriggerReportNotify,

sCEFMSISDNLessMOSMS [85] SCEFMSISDNLessMOSMS,

sCEFCommunicationPatternUpdate [86] SCEFCommunicationPatternUpdate,

-- EPS Events, see clause 6.3

-- MME Events, see clause 6.3.2.2

mMEAttach [87] MMEAttach,

mMEDetach [88] MMEDetach,

mMELocationUpdate [89] MMELocationUpdate,

mMEStartOfInterceptionWithEPSAttachedUE [90] MMEStartOfInterceptionWithEPSAttachedUE,

mMEUnsuccessfulProcedure [91] MMEUnsuccessfulProcedure,

-- AKMA key management events, see clause 7.9.1

aAnFAnchorKeyRegister [92] AAnFAnchorKeyRegister,

aAnFKAKMAApplicationKeyGet [93] AAnFKAKMAApplicationKeyGet,

aAnFStartOfInterceptWithEstablishedAKMAKeyMaterial [94] AAnFStartOfInterceptWithEstablishedAKMAKeyMaterial,

aAnFAKMAContextRemovalRecord [95] AAnFAKMAContextRemovalRecord,

aFAKMAApplicationKeyRefresh [96] AFAKMAApplicationKeyRefresh,

aFStartOfInterceptWithEstablishedAKMAApplicationKey [97] AFStartOfInterceptWithEstablishedAKMAApplicationKey,

aFAuxiliarySecurityParameterEstablishment [98] AFAuxiliarySecurityParameterEstablishment,

aFApplicationKeyRemoval [99] AFApplicationKeyRemoval,

-- HR LI Events, see clause 7.10.3.3

n9HRPDUSessionInfo [100] N9HRPDUSessionInfo,

s8HRBearerInfo [101] S8HRBearerInfo,

-- Separated Location Reporting, see clause 7.3.4

separatedLocationReporting [102] SeparatedLocationReporting,

-- STIR SHAKEN and RCD/eCNAM Events, see clause 7.11.2

sTIRSHAKENSignatureGeneration [103] STIRSHAKENSignatureGeneration,

sTIRSHAKENSignatureValidation [104] STIRSHAKENSignatureValidation,

-- IMS events, see clause 7.12.4.2

iMSMessage [105] IMSMessage,

startOfInterceptionForActiveIMSSession [106] StartOfInterceptionForActiveIMSSession,

iMSCCUnavailable [107] IMSCCUnavailable,

-- UDM events, see clause 7.2.2

uDMLocationInformationResult [108] UDMLocationInformationResult,

uDMUEInformationResponse [109] UDMUEInformationResponse,

uDMUEAuthenticationResponse [110] UDMUEAuthenticationResponse,

-- AMF events, see 6.2.2.2.8

positioningInfoTransfer [111] AMFPositioningInfoTransfer,

-- MME Events, see clause 6.3.2.2.8

mMEPositioningInfoTransfer [112] MMEPositioningInfoTransfer,

-- AMF events, see 6.2.2.2.9 continued from choice 5

aMFRANHandoverCommand [113] AMFRANHandoverCommand,

aMFRANHandoverRequest [114] AMFRANHandoverRequest

}

-- ==============

-- X3 xCC payload

-- ==============

-- No additional xCC payload definitions required in the present document.

-- ===============

-- HI2 IRI payload

-- ===============

IRIPayload ::= SEQUENCE

{

iRIPayloadOID [1] RELATIVE-OID,

event [2] IRIEvent,

targetIdentifiers [3] SEQUENCE OF IRITargetIdentifier OPTIONAL

}

IRIEvent ::= CHOICE

{

-- Registration-related events, see clause 6.2.2

registration [1] AMFRegistration,

deregistration [2] AMFDeregistration,

locationUpdate [3] AMFLocationUpdate,

startOfInterceptionWithRegisteredUE [4] AMFStartOfInterceptionWithRegisteredUE,

unsuccessfulRegistrationProcedure [5] AMFUnsuccessfulProcedure,

-- PDU session-related events, see clause 6.2.3

pDUSessionEstablishment [6] SMFPDUSessionEstablishment,

pDUSessionModification [7] SMFPDUSessionModification,

pDUSessionRelease [8] SMFPDUSessionRelease,

startOfInterceptionWithEstablishedPDUSession [9] SMFStartOfInterceptionWithEstablishedPDUSession,

unsuccessfulSessionProcedure [10] SMFUnsuccessfulProcedure,

-- Subscriber-management related events, see clause 7.2.2

servingSystemMessage [11] UDMServingSystemMessage,

-- SMS-related events, see clause 6.2.5, see also sMSReport ([56] below)

sMSMessage [12] SMSMessage,

-- LALS-related events, see clause 7.3.1

lALSReport [13] LALSReport,

-- PDHR/PDSR-related events, see clause 6.2.3.4.1

pDHeaderReport [14] PDHeaderReport,

pDSummaryReport [15] PDSummaryReport,

-- MDF-related events, see clause 7.3.2

mDFCellSiteReport [16] MDFCellSiteReport,

-- MMS-related events, see clause 7.4.2

mMSSend [17] MMSSend,

mMSSendByNonLocalTarget [18] MMSSendByNonLocalTarget,

mMSNotification [19] MMSNotification,

mMSSendToNonLocalTarget [20] MMSSendToNonLocalTarget,

mMSNotificationResponse [21] MMSNotificationResponse,

mMSRetrieval [22] MMSRetrieval,

mMSDeliveryAck [23] MMSDeliveryAck,

mMSForward [24] MMSForward,

mMSDeleteFromRelay [25] MMSDeleteFromRelay,

mMSDeliveryReport [26] MMSDeliveryReport,

mMSDeliveryReportNonLocalTarget [27] MMSDeliveryReportNonLocalTarget,

mMSReadReport [28] MMSReadReport,

mMSReadReportNonLocalTarget [29] MMSReadReportNonLocalTarget,

mMSCancel [30] MMSCancel,

mMSMBoxStore [31] MMSMBoxStore,

mMSMBoxUpload [32] MMSMBoxUpload,

mMSMBoxDelete [33] MMSMBoxDelete,

mMSMBoxViewRequest [34] MMSMBoxViewRequest,

mMSMBoxViewResponse [35] MMSMBoxViewResponse,

-- PTC-related events, see clause 7.5.2

pTCRegistration [36] PTCRegistration,

pTCSessionInitiation [37] PTCSessionInitiation,

pTCSessionAbandon [38] PTCSessionAbandon,

pTCSessionStart [39] PTCSessionStart,

pTCSessionEnd [40] PTCSessionEnd,

pTCStartOfInterception [41] PTCStartOfInterception,

pTCPreEstablishedSession [42] PTCPreEstablishedSession,

pTCInstantPersonalAlert [43] PTCInstantPersonalAlert,

pTCPartyJoin [44] PTCPartyJoin,

pTCPartyDrop [45] PTCPartyDrop,

pTCPartyHold [46] PTCPartyHold,

pTCMediaModification [47] PTCMediaModification,

pTCGroupAdvertisement [48] PTCGroupAdvertisement,

pTCFloorControl [49] PTCFloorControl,

pTCTargetPresence [50] PTCTargetPresence,

pTCParticipantPresence [51] PTCParticipantPresence,

pTCListManagement [52] PTCListManagement,

pTCAccessPolicy [53] PTCAccessPolicy,

-- More Subscriber-management related events, see clause 7.2.2

subscriberRecordChangeMessage [54] UDMSubscriberRecordChangeMessage,

cancelLocationMessage [55] UDMCancelLocationMessage,

-- SMS-related events, continued from choice 12

sMSReport [56] SMSReport,

-- MA PDU session-related events, see clause 6.2.3.2.7

sMFMAPDUSessionEstablishment [57] SMFMAPDUSessionEstablishment,

sMFMAPDUSessionModification [58] SMFMAPDUSessionModification,

sMFMAPDUSessionRelease [59] SMFMAPDUSessionRelease,

startOfInterceptionWithEstablishedMAPDUSession [60] SMFStartOfInterceptionWithEstablishedMAPDUSession,

unsuccessfulMASMProcedure [61] SMFMAUnsuccessfulProcedure,

-- Identifier Association events, see clauses 6.2.2.2.7 and 6.3.2.2.2

aMFIdentifierAssociation [62] AMFIdentifierAssociation,

mMEIdentifierAssociation [63] MMEIdentifierAssociation,

-- PDU to MA PDU session-related events, see clause 6.2.3.2.8

sMFPDUtoMAPDUSessionModification [64] SMFPDUtoMAPDUSessionModification,

-- NEF services related events, see clause 7.7.2,

nEFPDUSessionEstablishment [65] NEFPDUSessionEstablishment,

nEFPDUSessionModification [66] NEFPDUSessionModification,

nEFPDUSessionRelease [67] NEFPDUSessionRelease,

nEFUnsuccessfulProcedure [68] NEFUnsuccessfulProcedure,

nEFStartOfInterceptionWithEstablishedPDUSession [69] NEFStartOfInterceptionWithEstablishedPDUSession,

nEFdeviceTrigger [70] NEFDeviceTrigger,

nEFdeviceTriggerReplace [71] NEFDeviceTriggerReplace,

nEFdeviceTriggerCancellation [72] NEFDeviceTriggerCancellation,

nEFdeviceTriggerReportNotify [73] NEFDeviceTriggerReportNotify,

nEFMSISDNLessMOSMS [74] NEFMSISDNLessMOSMS,

nEFExpectedUEBehaviourUpdate [75] NEFExpectedUEBehaviourUpdate,

-- SCEF services related events, see clause 7.8.2

sCEFPDNConnectionEstablishment [76] SCEFPDNConnectionEstablishment,

sCEFPDNConnectionUpdate [77] SCEFPDNConnectionUpdate,

sCEFPDNConnectionRelease [78] SCEFPDNConnectionRelease,

sCEFUnsuccessfulProcedure [79] SCEFUnsuccessfulProcedure,

sCEFStartOfInterceptionWithEstablishedPDNConnection [80] SCEFStartOfInterceptionWithEstablishedPDNConnection,

sCEFdeviceTrigger [81] SCEFDeviceTrigger,

sCEFdeviceTriggerReplace [82] SCEFDeviceTriggerReplace,

sCEFdeviceTriggerCancellation [83] SCEFDeviceTriggerCancellation,

sCEFdeviceTriggerReportNotify [84] SCEFDeviceTriggerReportNotify,

sCEFMSISDNLessMOSMS [85] SCEFMSISDNLessMOSMS,

sCEFCommunicationPatternUpdate [86] SCEFCommunicationPatternUpdate,

-- EPS Events, see clause 6.3

-- MME Events, see clause 6.3.2.2

mMEAttach [87] MMEAttach,

mMEDetach [88] MMEDetach,

mMELocationUpdate [89] MMELocationUpdate,

mMEStartOfInterceptionWithEPSAttachedUE [90] MMEStartOfInterceptionWithEPSAttachedUE,

mMEUnsuccessfulProcedure [91] MMEUnsuccessfulProcedure,

-- AKMA key management events, see clause 7.9.1

aAnFAnchorKeyRegister [92] AAnFAnchorKeyRegister,

aAnFKAKMAApplicationKeyGet [93] AAnFKAKMAApplicationKeyGet,

aAnFStartOfInterceptWithEstablishedAKMAKeyMaterial [94] AAnFStartOfInterceptWithEstablishedAKMAKeyMaterial,

aAnFAKMAContextRemovalRecord [95] AAnFAKMAContextRemovalRecord,

aFAKMAApplicationKeyRefresh [96] AFAKMAApplicationKeyRefresh,

aFStartOfInterceptWithEstablishedAKMAApplicationKey [97] AFStartOfInterceptWithEstablishedAKMAApplicationKey,

aFAuxiliarySecurityParameterEstablishment [98] AFAuxiliarySecurityParameterEstablishment,

aFApplicationKeyRemoval [99] AFApplicationKeyRemoval,

-- tag 100 is reserved because there is no equivalent n9HRPDUSessionInfo in IRIEvent.

-- tag 101 is reserved because there is no equivalent S8HRBearerInfo in IRIEvent.

-- Separated Location Reporting, see clause 7.3.4

separatedLocationReporting [102] SeparatedLocationReporting,

-- STIR SHAKEN and RCD/eCNAM Events, see clause 7.11.3

sTIRSHAKENSignatureGeneration [103] STIRSHAKENSignatureGeneration,

sTIRSHAKENSignatureValidation [104] STIRSHAKENSignatureValidation,

-- IMS events, see clause 7.11.4.2

iMSMessage [105] IMSMessage,

startOfInterceptionForActiveIMSSession [106] StartOfInterceptionForActiveIMSSession,

iMSCCUnavailable [107] IMSCCUnavailable,

-- UDM events, see clause 7.2.2

uDMLocationInformationResultRecord [108] UDMLocationInformationResult,

uDMUEInformationResponse [109] UDMUEInformationResponse,

uDMUEAuthenticationResponse [110] UDMUEAuthenticationResponse,

-- AMF events, see 6.2.2.2.8

positioningInfoTransfer [111] AMFPositioningInfoTransfer,

-- MME Events, see clause 6.3.2.2.8

mMEPositioningInfoTransfer [112] MMEPositioningInfoTransfer,

-- AMF events, see 6.2.2.2.9 continued from choice 5

aMFRANHandoverCommand [113] AMFRANHandoverCommand,

aMFRANHandoverRequest [114] AMFRANHandoverRequest

}

IRITargetIdentifier ::= SEQUENCE

{

identifier [1] TargetIdentifier,

provenance [2] TargetIdentifierProvenance OPTIONAL

}

-- ==============

-- HI3 CC payload

-- ==============

CCPayload ::= SEQUENCE

{

cCPayloadOID [1] RELATIVE-OID,

pDU [2] CCPDU

}

CCPDU ::= CHOICE

{

uPFCCPDU [1] UPFCCPDU,

extendedUPFCCPDU [2] ExtendedUPFCCPDU,

mMSCCPDU [3] MMSCCPDU,

nIDDCCPDU [4] NIDDCCPDU,

pTCCCPDU [5] PTCCCPDU,

iMSCCPDU [6] IMSCCPDU

}

-- ===========================

-- HI4 LI notification payload

-- ===========================

LINotificationPayload ::= SEQUENCE

{

lINotificationPayloadOID [1] RELATIVE-OID,

notification [2] LINotificationMessage

}

LINotificationMessage ::= CHOICE

{

lINotification [1] LINotification

}

-- =================

-- HR LI definitions

-- =================

N9HRPDUSessionInfo ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

pDUSessionID [3] PDUSessionID,

location [4] Location OPTIONAL,

sNSSAI [5] SNSSAI OPTIONAL,

dNN [6] DNN OPTIONAL,

messageCause [7] N9HRMessageCause

}

S8HRBearerInfo ::= SEQUENCE

{

iMSI [1] IMSI,

iMEI [2] IMEI OPTIONAL,

bearerID [3] EPSBearerID,

linkedBearerID [4] EPSBearerID OPTIONAL,

location [5] Location OPTIONAL,

aPN [6] APN OPTIONAL,

sGWIPAddress [7] IPAddress OPTIONAL,

messageCause [8] S8HRMessageCause

}

-- ================

-- HR LI parameters

-- ================

N9HRMessageCause ::= ENUMERATED

{

pDUSessionEstablished(1),

pDUSessionModified(2),

pDUSessionReleased(3),

updatedLocationAvailable(4),

sMFChanged(5),

other(6),

hRLIEnabled(7)

}

S8HRMessageCause ::= ENUMERATED

{

bearerActivated(1),

bearerModified(2),

bearerDeleted(3),

pDNDisconnected(4),

updatedLocationAvailable(5),

sGWChanged(6),

other(7),

hRLIEnabled(8)

}

-- ==================

-- 5G NEF definitions

-- ==================

-- See clause 7.7.2.1.2 for details of this structure

NEFPDUSessionEstablishment ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

pDUSessionID [3] PDUSessionID,

sNSSAI [4] SNSSAI,

nEFID [5] NEFID,

dNN [6] DNN,

rDSSupport [7] RDSSupport,

sMFID [8] SMFID,

aFID [9] AFID

}

-- See clause 7.7.2.1.3 for details of this structure

NEFPDUSessionModification ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

sNSSAI [3] SNSSAI,

initiator [4] Initiator,

rDSSourcePortNumber [5] RDSPortNumber OPTIONAL,

rDSDestinationPortNumber [6] RDSPortNumber OPTIONAL,

applicationID [7] ApplicationID OPTIONAL,

aFID [8] AFID OPTIONAL,

rDSAction [9] RDSAction OPTIONAL,

serializationFormat [10] SerializationFormat OPTIONAL

}

-- See clause 7.7.2.1.4 for details of this structure

NEFPDUSessionRelease ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

pDUSessionID [3] PDUSessionID,

timeOfFirstPacket [4] Timestamp OPTIONAL,

timeOfLastPacket [5] Timestamp OPTIONAL,

uplinkVolume [6] INTEGER OPTIONAL,

downlinkVolume [7] INTEGER OPTIONAL,

releaseCause [8] NEFReleaseCause

}

-- See clause 7.7.2.1.5 for details of this structure

NEFUnsuccessfulProcedure ::= SEQUENCE

{

failureCause [1] NEFFailureCause,

sUPI [2] SUPI,

gPSI [3] GPSI OPTIONAL,

pDUSessionID [4] PDUSessionID,

dNN [5] DNN OPTIONAL,

sNSSAI [6] SNSSAI OPTIONAL,

rDSDestinationPortNumber [7] RDSPortNumber,

applicationID [8] ApplicationID,

aFID [9] AFID

}

-- See clause 7.7.2.1.6 for details of this structure

NEFStartOfInterceptionWithEstablishedPDUSession ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

pDUSessionID [3] PDUSessionID,

dNN [4] DNN,

sNSSAI [5] SNSSAI,

nEFID [6] NEFID,

rDSSupport [7] RDSSupport,

sMFID [8] SMFID,

aFID [9] AFID

}

-- See clause 7.7.3.1.1 for details of this structure

NEFDeviceTrigger ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

triggerId [3] TriggerID,

aFID [4] AFID,

triggerPayload [5] TriggerPayload OPTIONAL,

validityPeriod [6] INTEGER OPTIONAL,

priorityDT [7] PriorityDT OPTIONAL,

sourcePortId [8] PortNumber OPTIONAL,

destinationPortId [9] PortNumber OPTIONAL

}

-- See clause 7.7.3.1.2 for details of this structure

NEFDeviceTriggerReplace ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

triggerId [3] TriggerID,

aFID [4] AFID,

triggerPayload [5] TriggerPayload OPTIONAL,

validityPeriod [6] INTEGER OPTIONAL,

priorityDT [7] PriorityDT OPTIONAL,

sourcePortId [8] PortNumber OPTIONAL,

destinationPortId [9] PortNumber OPTIONAL

}

-- See clause 7.7.3.1.3 for details of this structure

NEFDeviceTriggerCancellation ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

triggerId [3] TriggerID

}

-- See clause 7.7.3.1.4 for details of this structure

NEFDeviceTriggerReportNotify ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

triggerId [3] TriggerID,

deviceTriggerDeliveryResult [4] DeviceTriggerDeliveryResult

}

-- See clause 7.7.4.1.1 for details of this structure

NEFMSISDNLessMOSMS ::= SEQUENCE

{

sUPI [1] SUPI,

gPSI [2] GPSI,

terminatingSMSParty [3] AFID,

sMS [4] SMSTPDUData OPTIONAL,

sourcePort [5] PortNumber OPTIONAL,

destinationPort [6] PortNumber OPTIONAL

}

-- See clause 7.7.5.1.1 for details of this structure

NEFExpectedUEBehaviourUpdate ::= SEQUENCE

{

gPSI [1] GPSI,

expectedUEMovingTrajectory [2] SEQUENCE OF UMTLocationArea5G OPTIONAL,

stationaryIndication [3] StationaryIndication OPTIONAL,

communicationDurationTime [4] INTEGER OPTIONAL,

periodicTime [5] INTEGER OPTIONAL,

scheduledCommunicationTime [6] ScheduledCommunicationTime OPTIONAL,

scheduledCommunicationType [7] ScheduledCommunicationType OPTIONAL,

batteryIndication [8] BatteryIndication OPTIONAL,

trafficProfile [9] TrafficProfile OPTIONAL,

expectedTimeAndDayOfWeekInTrajectory [10] SEQUENCE OF UMTLocationArea5G OPTIONAL,

aFID [11] AFID,

validityTime [12] Timestamp OPTIONAL

}

-- ==========================

-- Common SCEF/NEF parameters

-- ==========================

RDSSupport ::= BOOLEAN

RDSPortNumber ::= INTEGER (0..15)

RDSAction ::= ENUMERATED

{

reservePort(1),

releasePort(2)

}

SerializationFormat ::= ENUMERATED

{

xml(1),

json(2),

cbor(3)

}

ApplicationID ::= OCTET STRING

NIDDCCPDU ::= OCTET STRING

TriggerID ::= UTF8String

PriorityDT ::= ENUMERATED

{

noPriority(1),

priority(2)

}

TriggerPayload ::= OCTET STRING

DeviceTriggerDeliveryResult ::= ENUMERATED

{

success(1),

unknown(2),

failure(3),

triggered(4),

expired(5),

unconfirmed(6),

replaced(7),

terminate(8)

}

StationaryIndication ::= ENUMERATED

{

stationary(1),

mobile(2)

}

BatteryIndication ::= ENUMERATED

{

batteryRecharge(1),

batteryReplace(2),

batteryNoRecharge(3),

batteryNoReplace(4),

noBattery(5)

}

ScheduledCommunicationTime ::= SEQUENCE

{

days [1] SEQUENCE OF Daytime

}

UMTLocationArea5G ::= SEQUENCE

{

timeOfDay [1] Daytime,

durationSec [2] INTEGER,

location [3] NRLocation

}

Daytime ::= SEQUENCE

{

daysOfWeek [1] Day OPTIONAL,

timeOfDayStart [2] Timestamp OPTIONAL,

timeOfDayEnd [3] Timestamp OPTIONAL

}

Day ::= ENUMERATED

{

monday(1),

tuesday(2),

wednesday(3),

thursday(4),

friday(5),

saturday(6),

sunday(7)

}

TrafficProfile ::= ENUMERATED

{

singleTransUL(1),

singleTransDL(2),

dualTransULFirst(3),

dualTransDLFirst(4),

multiTrans(5)

}

ScheduledCommunicationType ::= ENUMERATED

{

downlinkOnly(1),

uplinkOnly(2),

bidirectional(3)

}

-- =================

-- 5G NEF parameters

-- =================

NEFFailureCause ::= ENUMERATED

{

userUnknown(1),

niddConfigurationNotAvailable(2),

contextNotFound(3),

portNotFree(4),

portNotAssociatedWithSpecifiedApplication(5)

}

NEFReleaseCause ::= ENUMERATED

{

sMFRelease(1),

dNRelease(2),

uDMRelease(3),

cHFRelease(4),

localConfigurationPolicy(5),

unknownCause(6)

}

AFID ::= UTF8String

NEFID ::= UTF8String

-- ==================

-- SCEF definitions

-- ==================

-- See clause 7.8.2.1.2 for details of this structure

SCEFPDNConnectionEstablishment ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

iMEI [4] IMEI OPTIONAL,

ePSBearerID [5] EPSBearerID,

sCEFID [6] SCEFID,

aPN [7] APN,

rDSSupport [8] RDSSupport,

sCSASID [9] SCSASID

}

-- See clause 7.8.2.1.3 for details of this structure

SCEFPDNConnectionUpdate ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

initiator [4] Initiator,

rDSSourcePortNumber [5] RDSPortNumber OPTIONAL,

rDSDestinationPortNumber [6] RDSPortNumber OPTIONAL,

applicationID [7] ApplicationID OPTIONAL,

sCSASID [8] SCSASID OPTIONAL,

rDSAction [9] RDSAction OPTIONAL,

serializationFormat [10] SerializationFormat OPTIONAL

}

-- See clause 7.8.2.1.4 for details of this structure

SCEFPDNConnectionRelease ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

ePSBearerID [4] EPSBearerID,

timeOfFirstPacket [5] Timestamp OPTIONAL,

timeOfLastPacket [6] Timestamp OPTIONAL,

uplinkVolume [7] INTEGER OPTIONAL,

downlinkVolume [8] INTEGER OPTIONAL,

releaseCause [9] SCEFReleaseCause

}

-- See clause 7.8.2.1.5 for details of this structure

SCEFUnsuccessfulProcedure ::= SEQUENCE

{

failureCause [1] SCEFFailureCause,

iMSI [2] IMSI OPTIONAL,

mSISDN [3] MSISDN OPTIONAL,

externalIdentifier [4] NAI OPTIONAL,

ePSBearerID [5] EPSBearerID,

aPN [6] APN,

rDSDestinationPortNumber [7] RDSPortNumber OPTIONAL,

applicationID [8] ApplicationID OPTIONAL,

sCSASID [9] SCSASID

}

-- See clause 7.8.2.1.6 for details of this structure

SCEFStartOfInterceptionWithEstablishedPDNConnection ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

iMEI [4] IMEI OPTIONAL,

ePSBearerID [5] EPSBearerID,

sCEFID [6] SCEFID,

aPN [7] APN,

rDSSupport [8] RDSSupport,

sCSASID [9] SCSASID

}

-- See clause 7.8.3.1.1 for details of this structure

SCEFDeviceTrigger ::= SEQUENCE

{

iMSI [1] IMSI,

mSISDN [2] MSISDN,

externalIdentifier [3] NAI,

triggerId [4] TriggerID,

sCSASID [5] SCSASID OPTIONAL,

triggerPayload [6] TriggerPayload OPTIONAL,

validityPeriod [7] INTEGER OPTIONAL,

priorityDT [8] PriorityDT OPTIONAL,

sourcePortId [9] PortNumber OPTIONAL,

destinationPortId [10] PortNumber OPTIONAL

}

-- See clause 7.8.3.1.2 for details of this structure

SCEFDeviceTriggerReplace ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

triggerId [4] TriggerID,

sCSASID [5] SCSASID OPTIONAL,

triggerPayload [6] TriggerPayload OPTIONAL,

validityPeriod [7] INTEGER OPTIONAL,

priorityDT [8] PriorityDT OPTIONAL,

sourcePortId [9] PortNumber OPTIONAL,

destinationPortId [10] PortNumber OPTIONAL

}

-- See clause 7.8.3.1.3 for details of this structure

SCEFDeviceTriggerCancellation ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

triggerId [4] TriggerID

}

-- See clause 7.8.3.1.4 for details of this structure

SCEFDeviceTriggerReportNotify ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifier [3] NAI OPTIONAL,

triggerId [4] TriggerID,

deviceTriggerDeliveryResult [5] DeviceTriggerDeliveryResult

}

-- See clause 7.8.4.1.1 for details of this structure

SCEFMSISDNLessMOSMS ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

externalIdentifie [3] NAI OPTIONAL,

terminatingSMSParty [4] SCSASID,

sMS [5] SMSTPDUData OPTIONAL,

sourcePort [6] PortNumber OPTIONAL,

destinationPort [7] PortNumber OPTIONAL

}

-- See clause 7.8.5.1.1 for details of this structure

SCEFCommunicationPatternUpdate ::= SEQUENCE

{

mSISDN [1] MSISDN OPTIONAL,

externalIdentifier [2] NAI OPTIONAL,

periodicCommunicationIndicator [3] PeriodicCommunicationIndicator OPTIONAL,

communicationDurationTime [4] INTEGER OPTIONAL,

periodicTime [5] INTEGER OPTIONAL,

scheduledCommunicationTime [6] ScheduledCommunicationTime OPTIONAL,

scheduledCommunicationType [7] ScheduledCommunicationType OPTIONAL,

stationaryIndication [8] StationaryIndication OPTIONAL,

batteryIndication [9] BatteryIndication OPTIONAL,

trafficProfile [10] TrafficProfile OPTIONAL,

expectedUEMovingTrajectory [11] SEQUENCE OF UMTLocationArea5G OPTIONAL,

sCSASID [13] SCSASID,

validityTime [14] Timestamp OPTIONAL

}

-- =================

-- SCEF parameters

-- =================

SCEFFailureCause ::= ENUMERATED

{

userUnknown(1),

niddConfigurationNotAvailable(2),

invalidEPSBearer(3),

operationNotAllowed(4),

portNotFree(5),

portNotAssociatedWithSpecifiedApplication(6)

}

SCEFReleaseCause ::= ENUMERATED

{

mMERelease(1),

dNRelease(2),

hSSRelease(3),

localConfigurationPolicy(4),

unknownCause(5)

}

SCSASID ::= UTF8String

SCEFID ::= UTF8String

PeriodicCommunicationIndicator ::= ENUMERATED

{

periodic(1),

nonPeriodic(2)

}

EPSBearerID ::= INTEGER (0..255)

APN ::= UTF8String

-- =======================

-- AKMA AAnF definitions

-- =======================

AAnFAnchorKeyRegister ::= SEQUENCE

{

aKID [1] NAI,

sUPI [2] SUPI,

kAKMA [3] KAKMA OPTIONAL

}

AAnFKAKMAApplicationKeyGet ::= SEQUENCE

{

type [1] KeyGetType,

aKID [2] NAI,

keyInfo [3] AFKeyInfo

}

AAnFStartOfInterceptWithEstablishedAKMAKeyMaterial ::= SEQUENCE

{

aKID [1] NAI,

kAKMA [2] KAKMA OPTIONAL,

aFKeyList [3] SEQUENCE OF AFKeyInfo OPTIONAL

}

AAnFAKMAContextRemovalRecord ::= SEQUENCE

{

aKID [1] NAI,

nFID [2] NFID

}

-- ======================

-- AKMA common parameters

-- ======================

FQDN ::= UTF8String

NFID ::= UTF8String

UAProtocolID ::= OCTET STRING (SIZE(5))

AKMAAFID ::= SEQUENCE

{

aFFQDN [1] FQDN,

uaProtocolID [2] UAProtocolID

}

UAStarParams ::= CHOICE

{

tls12 [1] TLS12UAStarParams,

generic [2] GenericUAStarParams

}

GenericUAStarParams ::= SEQUENCE

{

genericClientParams [1] OCTET STRING,

genericServerParams [2] OCTET STRING

}

-- ===========================================

-- Specific UaStarParmas for TLS 1.2 (RFC5246)

-- ===========================================

TLSCipherType ::= ENUMERATED

{

stream(1),

block(2),

aead(3)

}

TLSCompressionAlgorithm ::= ENUMERATED

{

null(1),

deflate(2)

}

TLSPRFAlgorithm ::= ENUMERATED

{

rfc5246(1)

}

TLSCipherSuite ::= SEQUENCE (SIZE(2)) OF INTEGER (0..255)

TLS12UAStarParams ::= SEQUENCE

{

preMasterSecret [1] OCTET STRING (SIZE(6)) OPTIONAL,

masterSecret [2] OCTET STRING (SIZE(6)),

pRFAlgorithm [3] TLSPRFAlgorithm,

cipherSuite [4] TLSCipherSuite,

cipherType [5] TLSCipherType,

encKeyLength [6] INTEGER (0..255),

blockLength [7] INTEGER (0..255),

fixedIVLength [8] INTEGER (0..255),

recordIVLength [9] INTEGER (0..255),

macLength [10] INTEGER (0..255),

macKeyLength [11] INTEGER (0..255),

compressionAlgorithm [12] TLSCompressionAlgorithm,

clientRandom [13] OCTET STRING (SIZE(4)),

serverRandom [14] OCTET STRING (SIZE(4)),

clientSequenceNumber [15] INTEGER,

serverSequenceNumber [16] INTEGER,

sessionID [17] OCTET STRING (SIZE(0..32)),

tLSExtensions [18] OCTET STRING (SIZE(0..65535))

}

KAF ::= OCTET STRING

KAKMA ::= OCTET STRING

-- ====================

-- AKMA AAnF parameters

-- ====================

KeyGetType ::= ENUMERATED

{

internal(1),

external(2)

}

AFKeyInfo ::= SEQUENCE

{

aFID [1] AKMAAFID,

kAF [2] KAF,

kAFExpTime [3] KAFExpiryTime

}

-- =======================

-- AKMA AF definitions

-- =======================

AFAKMAApplicationKeyRefresh ::= SEQUENCE

{

aFID [1] AFID,

aKID [2] NAI,

kAF [3] KAF,

uaStarParams [4] UAStarParams OPTIONAL

}

AFStartOfInterceptWithEstablishedAKMAApplicationKey ::= SEQUENCE

{

aFID [1] FQDN,

aKID [2] NAI,

kAFParamList [3] SEQUENCE OF AFSecurityParams

}

AFAuxiliarySecurityParameterEstablishment ::= SEQUENCE

{

aFSecurityParams [1] AFSecurityParams

}

AFSecurityParams ::= SEQUENCE

{

aFID [1] AFID,

aKID [2] NAI,

kAF [3] KAF,

uaStarParams [4] UAStarParams

}

AFApplicationKeyRemoval ::= SEQUENCE

{

aFID [1] AFID,

aKID [2] NAI,

removalCause [3] AFKeyRemovalCause

}

-- ===================

-- AKMA AF parameters

-- ===================

KAFParams ::= SEQUENCE

{

aKID [1] NAI,

kAF [2] KAF,

kAFExpTime [3] KAFExpiryTime,

uaStarParams [4] UAStarParams

}

KAFExpiryTime ::= GeneralizedTime

AFKeyRemovalCause ::= ENUMERATED

{

unknown(1),

keyExpiry(2),

applicationSpecific(3)

}

-- ==================

-- 5G AMF definitions

-- ==================

-- See clause 6.2.2.2.2 for details of this structure

AMFRegistration ::= SEQUENCE

{

registrationType [1] AMFRegistrationType,

registrationResult [2] AMFRegistrationResult,

slice [3] Slice OPTIONAL,

sUPI [4] SUPI,

sUCI [5] SUCI OPTIONAL,

pEI [6] PEI OPTIONAL,

gPSI [7] GPSI OPTIONAL,

gUTI [8] FiveGGUTI,

location [9] Location OPTIONAL,

non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

fiveGSTAIList [11] TAIList OPTIONAL,

sMSOverNasIndicator [12] SMSOverNASIndicator OPTIONAL,

oldGUTI [13] EPS5GGUTI OPTIONAL,

eMM5GRegStatus [14] EMM5GMMStatus OPTIONAL,

nonIMEISVPEI [15] NonIMEISVPEI OPTIONAL,

mACRestIndicator [16] MACRestrictionIndicator OPTIONAL,

pagingRestrictionIndicator [17] PagingRestrictionIndicator OPTIONAL

}

-- See clause 6.2.2.2.3 for details of this structure

AMFDeregistration ::= SEQUENCE

{

deregistrationDirection [1] AMFDirection,

accessType [2] AccessType,

sUPI [3] SUPI OPTIONAL,

sUCI [4] SUCI OPTIONAL,

pEI [5] PEI OPTIONAL,

gPSI [6] GPSI OPTIONAL,

gUTI [7] FiveGGUTI OPTIONAL,

cause [8] FiveGMMCause OPTIONAL,

location [9] Location OPTIONAL,

switchOffIndicator [10] SwitchOffIndicator OPTIONAL,

reRegRequiredIndicator [11] ReRegRequiredIndicator OPTIONAL

}

-- See clause 6.2.2.2.4 for details of this structure

AMFLocationUpdate ::= SEQUENCE

{

sUPI [1] SUPI,

sUCI [2] SUCI OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

gUTI [5] FiveGGUTI OPTIONAL,

location [6] Location,

sMSOverNASIndicator [7] SMSOverNASIndicator OPTIONAL,

oldGUTI [8] EPS5GGUTI OPTIONAL

}

-- See clause 6.2.2.2.5 for details of this structure

AMFStartOfInterceptionWithRegisteredUE ::= SEQUENCE

{

registrationResult [1] AMFRegistrationResult,

registrationType [2] AMFRegistrationType OPTIONAL,

slice [3] Slice OPTIONAL,

sUPI [4] SUPI,

sUCI [5] SUCI OPTIONAL,

pEI [6] PEI OPTIONAL,

gPSI [7] GPSI OPTIONAL,

gUTI [8] FiveGGUTI,

location [9] Location OPTIONAL,

non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

timeOfRegistration [11] Timestamp OPTIONAL,

fiveGSTAIList [12] TAIList OPTIONAL,

sMSOverNASIndicator [13] SMSOverNASIndicator OPTIONAL,

oldGUTI [14] EPS5GGUTI OPTIONAL,

eMM5GRegStatus [15] EMM5GMMStatus OPTIONAL

}

-- See clause 6.2.2.2.6 for details of this structure

AMFUnsuccessfulProcedure ::= SEQUENCE

{

failedProcedureType [1] AMFFailedProcedureType,

failureCause [2] AMFFailureCause,

requestedSlice [3] NSSAI OPTIONAL,

sUPI [4] SUPI OPTIONAL,

sUCI [5] SUCI OPTIONAL,

pEI [6] PEI OPTIONAL,

gPSI [7] GPSI OPTIONAL,

gUTI [8] FiveGGUTI OPTIONAL,

location [9] Location OPTIONAL

}

-- See clause 6.2.2.2.8 on for details of this structure

AMFPositioningInfoTransfer ::= SEQUENCE

{

sUPI [1] SUPI,

sUCI [2] SUCI OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

gUTI [5] FiveGGUTI OPTIONAL,

nRPPaMessage [6] OCTET STRING OPTIONAL,

lPPMessage [7] OCTET STRING OPTIONAL,

lcsCorrelationId [8] UTF8String (SIZE(1..255))

}

-- See clause 6.2.2.2.9.2 for details of this structure

AMFRANHandoverCommand ::= SEQUENCE

{

userIdentifiers [1] UserIdentifiers,

aMFUENGAPID [2] AMFUENGAPID,

rANUENGAPID [3] RANUENGAPID,

handoverType [4] HandoverType,

targetToSourceContainer [5] RANTargetToSourceContainer

}

-- See clause 6.2.2.2.9.3 for details of this structure

AMFRANHandoverRequest ::= SEQUENCE

{

userIdentifiers [1] UserIdentifiers,

aMFUENGAPID [2] AMFUENGAPID,

rANUENGAPID [3] RANUENGAPID,

handoverType [4] HandoverType,

handoverCause [5] HandoverCause,

pDUSessionResourceInformation [6] PDUSessionResourceInformation,

mobilityRestrictionList [7] MobilityRestrictionList OPTIONAL,

locationReportingRequestType [8] LocationReportingRequestType OPTIONAL,

targetToSourceContainer [9] RANTargetToSourceContainer,

nPNAccessInformation [10] NPNAccessInformation OPTIONAL,

sourceToTargetContainer [11] RANSourceToTargetContainer

}

-- =================

-- 5G AMF parameters

-- =================

AMFID ::= SEQUENCE

{

aMFRegionID [1] AMFRegionID,

aMFSetID [2] AMFSetID,

aMFPointer [3] AMFPointer

}

AMFDirection ::= ENUMERATED

{

networkInitiated(1),

uEInitiated(2)

}

AMFFailedProcedureType ::= ENUMERATED

{

registration(1),

sMS(2),

pDUSessionEstablishment(3)

}

AMFFailureCause ::= CHOICE

{

fiveGMMCause [1] FiveGMMCause,

fiveGSMCause [2] FiveGSMCause

}

AMFPointer ::= INTEGER (0..63)

AMFRegistrationResult ::= ENUMERATED

{

threeGPPAccess(1),

nonThreeGPPAccess(2),

threeGPPAndNonThreeGPPAccess(3)

}

AMFRegionID ::= INTEGER (0..255)

AMFRegistrationType ::= ENUMERATED

{

initial(1),

mobility(2),

periodic(3),

emergency(4)

}

AMFSetID ::= INTEGER (0..1023)

AMFUENGAPID ::= INTEGER (0..1099511627775)

-- ==================

-- 5G SMF definitions

-- ==================

-- See clause 6.2.3.2.2 for details of this structure

SMFPDUSessionEstablishment ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

pDUSessionID [5] PDUSessionID,

gTPTunnelID [6] FTEID,

pDUSessionType [7] PDUSessionType,

sNSSAI [8] SNSSAI OPTIONAL,

uEEndpoint [9] SEQUENCE OF UEEndpointAddress OPTIONAL,

non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

location [11] Location OPTIONAL,

dNN [12] DNN,

aMFID [13] AMFID OPTIONAL,

hSMFURI [14] HSMFURI OPTIONAL,

requestType [15] FiveGSMRequestType,

accessType [16] AccessType OPTIONAL,

rATType [17] RATType OPTIONAL,

sMPDUDNRequest [18] SMPDUDNRequest OPTIONAL,

uEEPSPDNConnection [19] UEEPSPDNConnection OPTIONAL,

ePS5GSComboInfo [20] EPS5GSComboInfo OPTIONAL,

selectedDNN [21] DNN OPTIONAL,

servingNetwork [22] SMFServingNetwork OPTIONAL,

oldPDUSessionID [23] PDUSessionID OPTIONAL,

handoverState [24] HandoverState OPTIONAL,

gTPTunnelInfo [25] GTPTunnelInfo OPTIONAL,

pCCRules [26] PCCRuleSet OPTIONAL

}

-- See clause 6.2.3.2.3 for details of this structure

SMFPDUSessionModification ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

sNSSAI [5] SNSSAI OPTIONAL,

non3GPPAccessEndpoint [6] UEEndpointAddress OPTIONAL,

location [7] Location OPTIONAL,

requestType [8] FiveGSMRequestType,

accessType [9] AccessType OPTIONAL,

rATType [10] RATType OPTIONAL,

pDUSessionID [11] PDUSessionID OPTIONAL,

ePS5GSComboInfo [12] EPS5GSComboInfo OPTIONAL,

uEEndpoint [13] UEEndpointAddress OPTIONAL,

servingNetwork [14] SMFServingNetwork OPTIONAL,

handoverState [15] HandoverState OPTIONAL,

gTPTunnelInfo [16] GTPTunnelInfo OPTIONAL,

pCCRules [17] PCCRuleSet OPTIONAL

}

-- See clause 6.2.3.2.4 for details of this structure

SMFPDUSessionRelease ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

pDUSessionID [4] PDUSessionID,

timeOfFirstPacket [5] Timestamp OPTIONAL,

timeOfLastPacket [6] Timestamp OPTIONAL,

uplinkVolume [7] INTEGER OPTIONAL,

downlinkVolume [8] INTEGER OPTIONAL,

location [9] Location OPTIONAL,

cause [10] SMFErrorCodes OPTIONAL,

ePS5GSComboInfo [11] EPS5GSComboInfo OPTIONAL,

nGAPCause [12] NGAPCauseInt OPTIONAL,

fiveGMMCause [13] FiveGMMCause OPTIONAL,

pCCRuleIDs [14] PCCRuleIDSet OPTIONAL

}

-- See clause 6.2.3.2.5 for details of this structure

SMFStartOfInterceptionWithEstablishedPDUSession ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

pDUSessionID [5] PDUSessionID,

gTPTunnelID [6] FTEID,

pDUSessionType [7] PDUSessionType,

sNSSAI [8] SNSSAI OPTIONAL,

uEEndpoint [9] SEQUENCE OF UEEndpointAddress,

non3GPPAccessEndpoint [10] UEEndpointAddress OPTIONAL,

location [11] Location OPTIONAL,

dNN [12] DNN,

aMFID [13] AMFID OPTIONAL,

hSMFURI [14] HSMFURI OPTIONAL,

requestType [15] FiveGSMRequestType,

accessType [16] AccessType OPTIONAL,

rATType [17] RATType OPTIONAL,

sMPDUDNRequest [18] SMPDUDNRequest OPTIONAL,

timeOfSessionEstablishment [19] Timestamp OPTIONAL,

ePS5GSComboInfo [20] EPS5GSComboInfo OPTIONAL,

uEEPSPDNConnection [21] UEEPSPDNConnection OPTIONAL,

servingNetwork [22] SMFServingNetwork OPTIONAL,

gTPTunnelInfo [23] GTPTunnelInfo OPTIONAL,

pCCRules [24] PCCRuleSet OPTIONAL

}

-- See clause 6.2.3.2.6 for details of this structure

SMFUnsuccessfulProcedure ::= SEQUENCE

{

failedProcedureType [1] SMFFailedProcedureType,

failureCause [2] FiveGSMCause,

initiator [3] Initiator,

requestedSlice [4] NSSAI OPTIONAL,

sUPI [5] SUPI OPTIONAL,

sUPIUnauthenticated [6] SUPIUnauthenticatedIndication OPTIONAL,

pEI [7] PEI OPTIONAL,

gPSI [8] GPSI OPTIONAL,

pDUSessionID [9] PDUSessionID OPTIONAL,

uEEndpoint [10] SEQUENCE OF UEEndpointAddress OPTIONAL,

non3GPPAccessEndpoint [11] UEEndpointAddress OPTIONAL,

dNN [12] DNN OPTIONAL,

aMFID [13] AMFID OPTIONAL,

hSMFURI [14] HSMFURI OPTIONAL,

requestType [15] FiveGSMRequestType OPTIONAL,

accessType [16] AccessType OPTIONAL,

rATType [17] RATType OPTIONAL,

sMPDUDNRequest [18] SMPDUDNRequest OPTIONAL,

location [19] Location OPTIONAL

}

-- See clause 6.2.3.2.8 for details of this structure

SMFPDUtoMAPDUSessionModification ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

sNSSAI [5] SNSSAI OPTIONAL,

non3GPPAccessEndpoint [6] UEEndpointAddress OPTIONAL,

location [7] Location OPTIONAL,

requestType [8] FiveGSMRequestType,

accessType [9] AccessType OPTIONAL,

rATType [10] RATType OPTIONAL,

pDUSessionID [11] PDUSessionID,

requestIndication [12] RequestIndication,

aTSSSContainer [13] ATSSSContainer,

uEEndpoint [14] UEEndpointAddress OPTIONAL,

servingNetwork [15] SMFServingNetwork OPTIONAL,

handoverState [16] HandoverState OPTIONAL,

gTPTunnelInfo [17] GTPTunnelInfo OPTIONAL

}

-- See clause 6.2.3.2.7.1 for details of this structure

SMFMAPDUSessionEstablishment ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

pDUSessionID [5] PDUSessionID,

pDUSessionType [6] PDUSessionType,

accessInfo [7] SEQUENCE OF AccessInfo,

sNSSAI [8] SNSSAI OPTIONAL,

uEEndpoint [9] SEQUENCE OF UEEndpointAddress OPTIONAL,

location [10] Location OPTIONAL,

dNN [11] DNN,

aMFID [12] AMFID OPTIONAL,

hSMFURI [13] HSMFURI OPTIONAL,

requestType [14] FiveGSMRequestType,

sMPDUDNRequest [15] SMPDUDNRequest OPTIONAL,

servingNetwork [16] SMFServingNetwork,

oldPDUSessionID [17] PDUSessionID OPTIONAL,

mAUpgradeIndication [18] SMFMAUpgradeIndication OPTIONAL,

ePSPDNCnxInfo [19] SMFEPSPDNCnxInfo OPTIONAL,

mAAcceptedIndication [20] SMFMAAcceptedIndication,

aTSSSContainer [21] ATSSSContainer OPTIONAL,

uEEPSPDNConnection [22] UEEPSPDNConnection OPTIONAL,

ePS5GSComboInfo [23] EPS5GSComboInfo OPTIONAL,

selectedDNN [24] DNN OPTIONAL,

handoverState [25] HandoverState OPTIONAL,

pCCRules [26] PCCRuleSet OPTIONAL

}

-- See clause 6.2.3.2.7.2 for details of this structure

SMFMAPDUSessionModification ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

pDUSessionID [5] PDUSessionID,

accessInfo [6] SEQUENCE OF AccessInfo OPTIONAL,

sNSSAI [7] SNSSAI OPTIONAL,

location [8] Location OPTIONAL,

requestType [9] FiveGSMRequestType OPTIONAL,

servingNetwork [10] SMFServingNetwork,

oldPDUSessionID [11] PDUSessionID OPTIONAL,

mAUpgradeIndication [12] SMFMAUpgradeIndication OPTIONAL,

ePSPDNCnxInfo [13] SMFEPSPDNCnxInfo OPTIONAL,

mAAcceptedIndication [14] SMFMAAcceptedIndication,

aTSSSContainer [15] ATSSSContainer OPTIONAL,

uEEPSPDNConnection [16] UEEPSPDNConnection OPTIONAL,

ePS5GSComboInfo [17] EPS5GSComboInfo OPTIONAL,

handoverState [18] HandoverState OPTIONAL,

pCCRules [19] PCCRuleSet OPTIONAL

}

-- See clause 6.2.3.2.7.3 for details of this structure

SMFMAPDUSessionRelease ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

pDUSessionID [4] PDUSessionID,

timeOfFirstPacket [5] Timestamp OPTIONAL,

timeOfLastPacket [6] Timestamp OPTIONAL,

uplinkVolume [7] INTEGER OPTIONAL,

downlinkVolume [8] INTEGER OPTIONAL,

location [9] Location OPTIONAL,

cause [10] SMFErrorCodes OPTIONAL,

nGAPCause [11] NGAPCauseInt OPTIONAL,

fiveGMMCause [12] FiveGMMCause OPTIONAL,

pCCRuleIDs [13] PCCRuleIDSet OPTIONAL

}

-- See clause 6.2.3.2.7.4 for details of this structure

SMFStartOfInterceptionWithEstablishedMAPDUSession ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

sUPIUnauthenticated [2] SUPIUnauthenticatedIndication OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

pDUSessionID [5] PDUSessionID,

pDUSessionType [6] PDUSessionType,

accessInfo [7] SEQUENCE OF AccessInfo,

sNSSAI [8] SNSSAI OPTIONAL,

uEEndpoint [9] SEQUENCE OF UEEndpointAddress OPTIONAL,

location [10] Location OPTIONAL,

dNN [11] DNN,

aMFID [12] AMFID OPTIONAL,

hSMFURI [13] HSMFURI OPTIONAL,

requestType [14] FiveGSMRequestType OPTIONAL,

sMPDUDNRequest [15] SMPDUDNRequest OPTIONAL,

servingNetwork [16] SMFServingNetwork,

oldPDUSessionID [17] PDUSessionID OPTIONAL,

mAUpgradeIndication [18] SMFMAUpgradeIndication OPTIONAL,

ePSPDNCnxInfo [19] SMFEPSPDNCnxInfo OPTIONAL,

mAAcceptedIndication [20] SMFMAAcceptedIndication,

aTSSSContainer [21] ATSSSContainer OPTIONAL,

ePS5GSComboInfo [22] EPS5GSComboInfo OPTIONAL,

uEEPSPDNConnection [23] UEEPSPDNConnection OPTIONAL,

pCCRules [24] PCCRuleSet OPTIONAL

}

-- See clause 6.2.3.2.7.5 for details of this structure

SMFMAUnsuccessfulProcedure ::= SEQUENCE

{

failedProcedureType [1] SMFFailedProcedureType,

failureCause [2] FiveGSMCause,

requestedSlice [3] NSSAI OPTIONAL,

initiator [4] Initiator,

sUPI [5] SUPI OPTIONAL,

sUPIUnauthenticated [6] SUPIUnauthenticatedIndication OPTIONAL,

pEI [7] PEI OPTIONAL,

gPSI [8] GPSI OPTIONAL,

pDUSessionID [9] PDUSessionID OPTIONAL,

accessInfo [10] SEQUENCE OF AccessInfo,

uEEndpoint [11] SEQUENCE OF UEEndpointAddress OPTIONAL,

location [12] Location OPTIONAL,

dNN [13] DNN OPTIONAL,

aMFID [14] AMFID OPTIONAL,

hSMFURI [15] HSMFURI OPTIONAL,

requestType [16] FiveGSMRequestType OPTIONAL,

sMPDUDNRequest [17] SMPDUDNRequest OPTIONAL

}

-- =================

-- 5G SMF parameters

-- =================

SMFID ::= UTF8String

SMFFailedProcedureType ::= ENUMERATED

{

pDUSessionEstablishment(1),

pDUSessionModification(2),

pDUSessionRelease(3)

}

SMFServingNetwork ::= SEQUENCE

{

pLMNID [1] PLMNID,

nID [2] NID OPTIONAL

}

AccessInfo ::= SEQUENCE

{

accessType [1] AccessType,

rATType [2] RATType OPTIONAL,

gTPTunnelID [3] FTEID,

non3GPPAccessEndpoint [4] UEEndpointAddress OPTIONAL,

establishmentStatus [5] EstablishmentStatus,

aNTypeToReactivate [6] AccessType OPTIONAL,

gTPTunnelInfo [7] GTPTunnelInfo OPTIONAL

}

-- see Clause 6.1.2 of TS 24.193[44] for the details of the ATSSS container contents.

ATSSSContainer ::= OCTET STRING

DLRANTunnelInformation ::= SEQUENCE

{

dLQOSFlowTunnelInformation [1] QOSFlowTunnelInformation OPTIONAL,

additionalDLQOSFlowTunnelInformation [2] QOSFlowTunnelInformationList OPTIONAL,

redundantDLQOSFlowTunnelInformation [3] QOSFlowTunnelInformationList OPTIONAL,

additionalredundantDLQOSFlowTunnelInformation [4] QOSFlowTunnelInformationList OPTIONAL

}

EstablishmentStatus ::= ENUMERATED

{

established(0),

released(1)

}

FiveGSGTPTunnels ::= SEQUENCE

{

uLNGUUPTunnelInformation [1] FTEID OPTIONAL,

additionalULNGUUPTunnelInformation [2] FTEIDList OPTIONAL,

dLRANTunnelInformation [3] DLRANTunnelInformation OPTIONAL

}

FiveQI ::= INTEGER (0..255)

HandoverState ::= ENUMERATED

{

none(1),

preparing(2),

prepared(3),

completed(4),

cancelled(5)

}

NGAPCauseInt ::= SEQUENCE

{

group [1] NGAPCauseGroupInt,

value [2] NGAPCauseValueInt

}

-- Derived as described in TS 29.571 [17] clause 5.4.4.12

NGAPCauseGroupInt ::= INTEGER

NGAPCauseValueInt ::= INTEGER

SMFMAUpgradeIndication ::= BOOLEAN

-- Given in YAML encoding as defined in clause 6.1.6.2.31 of TS 29.502[16]

SMFEPSPDNCnxInfo ::= UTF8String

SMFMAAcceptedIndication ::= BOOLEAN

-- see Clause 6.1.6.3.8 of TS 29.502[16] for the details of this structure.

SMFErrorCodes ::= UTF8String

-- see Clause 6.1.6.3.2 of TS 29.502[16] for details of this structure.

UEEPSPDNConnection ::= OCTET STRING

-- see Clause 6.1.6.3.6 of TS 29.502[16] for the details of this structure.

RequestIndication ::= ENUMERATED

{

uEREQPDUSESMOD(0),

uEREQPDUSESREL(1),

pDUSESMOB(2),

nWREQPDUSESAUTH(3),

nWREQPDUSESMOD(4),

nWREQPDUSESREL(5),

eBIASSIGNMENTREQ(6),

rELDUETO5GANREQUEST(7)

}

QOSFlowTunnelInformation ::= SEQUENCE

{

uPTunnelInformation [1] FTEID,

associatedQOSFlowList [2] QOSFlowLists

}

QOSFlowTunnelInformationList ::= SEQUENCE OF QOSFlowTunnelInformation

QOSFlowDescription ::= OCTET STRING

QOSFlowLists ::= SEQUENCE OF QOSFlowList

QOSFlowList ::= SEQUENCE

{

qFI [1] QFI,

qOSRules [2] QOSRules OPTIONAL,

eBI [3] EPSBearerID OPTIONAL,

qOSFlowDescription [4] QOSFlowDescription OPTIONAL,

qOSFlowProfile [5] QOSFlowProfile OPTIONAL,

associatedANType [6] AccessType OPTIONAL,

defaultQOSRuleIndication [7] BOOLEAN OPTIONAL

}

QOSFlowProfile ::= SEQUENCE

{

fiveQI [1] FiveQI

}

QOSRules ::= OCTET STRING

-- See clauses 5.6.2.6-1 and 5.6.2.9-1 of TS 29.512 [89], clause table 5.6.2.5-1 of TS 29.508 [90] for the details of this structure

PCCRule ::= SEQUENCE

{

pCCRuleID [1] PCCRuleID OPTIONAL,

appId [2] UTF8String OPTIONAL,

flowInfos [3] FlowInformationSet OPTIONAL,

appReloc [4] BOOLEAN OPTIONAL,

simConnInd [5] BOOLEAN OPTIONAL,

simConnTerm [6] INTEGER OPTIONAL,

maxAllowedUpLat [7] INTEGER OPTIONAL,

trafficRoutes [8] RouteToLocationSet,

trafficSteeringPolIdDl [9] UTF8String OPTIONAL,

trafficSteeringPolIdUl [10] UTF8String OPTIONAL,

sourceDNAI [11] DNAI OPTIONAL,

targetDNAI [12] DNAI OPTIONAL,

dNAIChangeType [13] DNAIChangeType OPTIONAL,

sourceUEIPAddr [14] IPAddress OPTIONAL,

targetUEIPAddr [15] IPAddress OPTIONAL,

sourceTrafficRouting [16] RouteToLocation OPTIONAL,

targetTrafficRouting [17] RouteToLocation OPTIONAL,

eASIPReplaceInfos [18] EASIPReplaceInfos OPTIONAL

}

-- See table 5.6.2.14-1 of TS 29.512 [89]

PCCRuleID ::= UTF8String

PCCRuleSet ::= SET OF PCCRule

PCCRuleIDSet ::= SET OF PCCRuleID

FlowInformationSet ::= SET OF FlowInformation

RouteToLocationSet ::= SET OF RouteToLocation

-- See table 5.6.2.14 of TS 29.512 [89]

FlowInformation ::= SEQUENCE

{

flowDescription [1] FlowDescription OPTIONAL,

ethFlowDescription [2] EthFlowDescription OPTIONAL,

tosTrafficClass [3] OCTET STRING (SIZE(2)) OPTIONAL,

spi [4] OCTET STRING (SIZE(4)) OPTIONAL,

flowLabel [5] OCTET STRING (SIZE(3)) OPTIONAL,

flowDirection [6] FlowDirection OPTIONAL

}

-- See table 5.6.2.14 of TS 29.512 [89]

FlowDescription ::= SEQUENCE

{

sourceIPAddress [1] IPAddressOrRangeOrAny,

destinationIPAddress [2] IPAddressOrRangeOrAny,

sourcePortNumber [3] PortNumber OPTIONAL,

destinationPortNumber [4] PortNumber OPTIONAL,

protocol [5] NextLayerProtocolOrAny

}

IPAddressOrRangeOrAny ::= CHOICE

{

iPAddress [1] IPAddress,

ipAddressRange [2] IPMask,

anyIPAddress [3] AnyIPAddress

}

IPMask ::= SEQUENCE

{

fromIPAddress [1] IPAddress,

toIPAddress [2] IPAddress

}

AnyIPAddress ::= ENUMERATED

{

any(1)

}

NextLayerProtocolOrAny ::= CHOICE

{

nextLayerProtocol [1] NextLayerProtocol,

anyNextLayerProtocol [2] AnyNextLayerProtocol

}

AnyNextLayerProtocol ::= ENUMERATED

{

ip(1)

}

-- See table 5.6.2.17-1 of TS 29.514 [91]

EthFlowDescription ::= SEQUENCE

{

destMacAddress [1] MACAddress OPTIONAL,

ethType [2] OCTET STRING (SIZE(2)),

fDesc [3] FlowDescription OPTIONAL,

fDir [4] FDir OPTIONAL,

sourceMacAddress [5] MACAddress OPTIONAL,

vlanTags [6] SET OF VLANTag,

srcMacAddrEnd [7] MACAddress OPTIONAL,

destMacAddrEnd [8] MACAddress OPTIONAL

}

-- See table 5.6.2.17-1 of TS 29.514 [91]

FDir ::= ENUMERATED

{

downlink(1)

}

-- See table 5.6.2.17-1 of TS 29.514 [91]

VLANTag ::= SEQUENCE

{

priority [1] BIT STRING (SIZE(3)),

cFI [2] BIT STRING (SIZE(1)),

vLANID [3] BIT STRING (SIZE(12))

}

-- See table 5.6.2.14 of TS 29.512 [89]

FlowDirection ::= ENUMERATED

{

downlinkOnly(1),

uplinkOnly(2),

dowlinkAndUplink(3)

}

-- See table 5.4.2.1 of TS 29.571 [17]

DNAIChangeType ::= ENUMERATED

{

early(1),

earlyAndLate(2),

late(3)

}

-- See table 5.6.2.15 of TS 29.571 [17]

RouteToLocation ::= SEQUENCE

{

dNAI [1] DNAI,

routeInfo [2] RouteInfo

}

-- See table 5.4.2.1 of TS 29.571 [17]

DNAI ::= UTF8String

-- See table 5.4.4.16 of TS 29.571 [17]

RouteInfo ::= SEQUENCE

{

iPAddressTunnelEndpoint [1] IPAddress,

uDPPortNumberTunnelEndpoint [2] PortNumber

}

-- See clause 4.1.4.2 of TS 29.512 [89]

EASIPReplaceInfos ::= SEQUENCE

{

sourceEASAddress [1] EASServerAddress,

targetEASAddress [2] EASServerAddress

}

-- See clause 4.1.4.2 of TS 29.512 [89]

EASServerAddress ::= SEQUENCE

{

iPAddress [1] IPAddress,

port [2] PortNumber

}

-- ======================

-- PGW-C + SMF Parameters

-- ======================

EPS5GSComboInfo ::= SEQUENCE

{

ePSInterworkingIndication [1] EPSInterworkingIndication,

ePSSubscriberIDs [2] EPSSubscriberIDs,

ePSPDNCnxInfo [3] EPSPDNCnxInfo OPTIONAL,

ePSBearerInfo [4] EPSBearerInfo OPTIONAL

}

EPSInterworkingIndication ::= ENUMERATED

{

none(1),

withN26(2),

withoutN26(3),

iwkNon3GPP(4)

}

EPSSubscriberIDs ::= SEQUENCE

{

iMSI [1] IMSI OPTIONAL,

mSISDN [2] MSISDN OPTIONAL,

iMEI [3] IMEI OPTIONAL

}

EPSPDNCnxInfo ::= SEQUENCE

{

pGWS8ControlPlaneFTEID [1] FTEID,

linkedBearerID [2] EPSBearerID OPTIONAL

}

EPSBearerInfo ::= SEQUENCE OF EPSBearers

EPSBearers ::= SEQUENCE

{

ePSBearerID [1] EPSBearerID,

pGWS8UserPlaneFTEID [2] FTEID,

qCI [3] QCI

}

QCI ::= INTEGER (0..255)

GTPTunnelInfo ::= SEQUENCE

{

fiveGSGTPTunnels [1] FiveGSGTPTunnels OPTIONAL

}

-- ==================

-- 5G UPF definitions

-- ==================

UPFCCPDU ::= OCTET STRING

-- See clause 6.2.3.8 for the details of this structure

ExtendedUPFCCPDU ::= SEQUENCE

{

payload [1] UPFCCPDUPayload,

qFI [2] QFI OPTIONAL

}

-- =================

-- 5G UPF parameters

-- =================

UPFCCPDUPayload ::= CHOICE

{

uPFIPCC [1] OCTET STRING,

uPFEthernetCC [2] OCTET STRING,

uPFUnstructuredCC [3] OCTET STRING

}

QFI ::= INTEGER (0..63)

-- ==================

-- 5G UDM definitions

-- ==================

UDMServingSystemMessage ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

gUAMI [4] GUAMI OPTIONAL,

gUMMEI [5] GUMMEI OPTIONAL,

pLMNID [6] PLMNID OPTIONAL,

servingSystemMethod [7] UDMServingSystemMethod,

serviceID [8] ServiceID OPTIONAL

}

UDMSubscriberRecordChangeMessage ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

oldPEI [4] PEI OPTIONAL,

oldSUPI [5] SUPI OPTIONAL,

oldGPSI [6] GPSI OPTIONAL,

oldserviceID [7] ServiceID OPTIONAL,

subscriberRecordChangeMethod [8] UDMSubscriberRecordChangeMethod,

serviceID [9] ServiceID OPTIONAL

}

UDMCancelLocationMessage ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

gUAMI [4] GUAMI OPTIONAL,

pLMNID [5] PLMNID OPTIONAL,

cancelLocationMethod [6] UDMCancelLocationMethod

}

UDMLocationInformationResult ::= SEQUENCE

{

sUPI [1] SUPI,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

locationInfoRequest [4] UDMLocationInfoRequest,

vPLMNID [5] PLMNID OPTIONAL,

currentLocationIndicator [6] BOOLEAN OPTIONAL,

aMFInstanceID [7] NFID OPTIONAL,

sMSFInstanceID [8] NFID OPTIONAL,

location [9] Location OPTIONAL,

rATType [10] RATType OPTIONAL,

problemDetails [11] UDMProblemDetails OPTIONAL

}

UDMUEInformationResponse ::= SEQUENCE

{

sUPI [1] SUPI,

tADSInfo [2] UEContextInfo OPTIONAL,

fiveGSUserStateInfo [3] FiveGSUserStateInfo OPTIONAL,

fiveGSRVCCInfo [4] FiveGSRVCCInfo OPTIONAL,

problemDetails [5] UDMProblemDetails OPTIONAL

}

UDMUEAuthenticationResponse ::= SEQUENCE

{

sUPI [1] SUPI,

authenticationInfoRequest [2] UDMAuthenticationInfoRequest,

aKMAIndicator [3] BOOLEAN OPTIONAL,

problemDetails [4] UDMProblemDetails OPTIONAL

}

-- =================

-- 5G UDM parameters

-- =================

UDMServingSystemMethod ::= ENUMERATED

{

amf3GPPAccessRegistration(0),

amfNon3GPPAccessRegistration(1),

unknown(2)

}

UDMSubscriberRecordChangeMethod ::= ENUMERATED

{

pEIChange(1),

sUPIChange(2),

gPSIChange(3),

uEDeprovisioning(4),

unknown(5),

serviceIDChange(6)

}

UDMCancelLocationMethod ::= ENUMERATED

{

aMF3GPPAccessDeregistration(1),

aMFNon3GPPAccessDeregistration(2),

uDMDeregistration(3),

unknown(4)

}

ServiceID ::= SEQUENCE

{

nSSAI [1] NSSAI OPTIONAL,

cAGID [2] SEQUENCE OF CAGID OPTIONAL

}

CAGID ::= UTF8String

UDMAuthenticationInfoRequest ::= SEQUENCE

{

infoRequestType [1] UDMInfoRequestType,

rGAuthCtx [2] SEQUENCE SIZE(1..MAX) OF SubscriberIdentifier,

authType [3] PrimaryAuthenticationType,

servingNetworkName [4] PLMNID,

aUSFInstanceID [5] NFID OPTIONAL,

cellCAGInfo [6] CAGID OPTIONAL,

n5GCIndicator [7] BOOLEAN OPTIONAL

}

UDMLocationInfoRequest ::= SEQUENCE

{

requested5GSLocation [1] BOOLEAN OPTIONAL,

requestedCurrentLocation [2] BOOLEAN OPTIONAL,

requestedRATType [3] BOOLEAN OPTIONAL,

requestedTimeZone [4] BOOLEAN OPTIONAL,

requestedServingNode [5] BOOLEAN OPTIONAL

}

UDMProblemDetails ::= SEQUENCE

{

cause [1] UDMProblemDetailsCause OPTIONAL

}

UDMProblemDetailsCause ::= CHOICE

{

uDMDefinedCause [1] UDMDefinedCause,

otherCause [2] UDMProblemDetailsOtherCause

}

UDMDefinedCause ::= ENUMERATED

{

userNotFound(1),

dataNotFound(2),

contextNotFound(3),

subscriptionNotFound(4),

other(5)

}

UDMInfoRequestType ::= ENUMERATED

{

hSS(1),

aUSF(2),

other(3)

}

UDMProblemDetailsOtherCause ::= SEQUENCE

{

problemDetailsType [1] UTF8String OPTIONAL,

title [2] UTF8String OPTIONAL,

status [3] INTEGER OPTIONAL,

detail [4] UTF8String OPTIONAL,

instance [5] UTF8String OPTIONAL,

cause [6] UTF8String OPTIONAL,

uDMInvalidParameters [7] UDMInvalidParameters,

uDMSupportedFeatures [8] UTF8String

}

UDMInvalidParameters ::= SEQUENCE

{

parameter [1] UTF8String OPTIONAL,

reason [2] UTF8String OPTIONAL

}

-- ===================

-- 5G SMSF definitions

-- ===================

-- See clause 6.2.5.3 for details of this structure

SMSMessage ::= SEQUENCE

{

originatingSMSParty [1] SMSParty,

terminatingSMSParty [2] SMSParty,

direction [3] Direction,

linkTransferStatus [4] SMSTransferStatus,

otherMessage [5] SMSOtherMessageIndication OPTIONAL,

location [6] Location OPTIONAL,

peerNFAddress [7] SMSNFAddress OPTIONAL,

peerNFType [8] SMSNFType OPTIONAL,

sMSTPDUData [9] SMSTPDUData OPTIONAL,

messageType [10] SMSMessageType OPTIONAL,

rPMessageReference [11] SMSRPMessageReference OPTIONAL

}

SMSReport ::= SEQUENCE

{

location [1] Location OPTIONAL,

sMSTPDUData [2] SMSTPDUData,

messageType [3] SMSMessageType,

rPMessageReference [4] SMSRPMessageReference

}

-- ==================

-- 5G SMSF parameters

-- ==================

SMSAddress ::= OCTET STRING(SIZE(2..12))

SMSMessageType ::= ENUMERATED

{

deliver(1),

deliverReportAck(2),

deliverReportError(3),

statusReport(4),

command(5),

submit(6),

submitReportAck(7),

submitReportError(8),

reserved(9)

}

SMSParty ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

pEI [2] PEI OPTIONAL,

gPSI [3] GPSI OPTIONAL,

sMSAddress [4] SMSAddress OPTIONAL

}

SMSTransferStatus ::= ENUMERATED

{

transferSucceeded(1),

transferFailed(2),

undefined(3)

}

SMSOtherMessageIndication ::= BOOLEAN

SMSNFAddress ::= CHOICE

{

iPAddress [1] IPAddress,

e164Number [2] E164Number

}

SMSNFType ::= ENUMERATED

{

sMSGMSC(1),

iWMSC(2),

sMSRouter(3)

}

SMSRPMessageReference ::= INTEGER (0..255)

SMSTPDUData ::= CHOICE

{

sMSTPDU [1] SMSTPDU,

truncatedSMSTPDU [2] TruncatedSMSTPDU

}

SMSTPDU ::= OCTET STRING (SIZE(1..270))

TruncatedSMSTPDU ::= OCTET STRING (SIZE(1..130))

-- ===============

-- MMS definitions

-- ===============

MMSSend ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

dateTime [3] Timestamp,

originatingMMSParty [4] MMSParty,

terminatingMMSParty [5] SEQUENCE OF MMSParty OPTIONAL,

cCRecipients [6] SEQUENCE OF MMSParty OPTIONAL,

bCCRecipients [7] SEQUENCE OF MMSParty OPTIONAL,

direction [8] MMSDirection,

subject [9] MMSSubject OPTIONAL,

messageClass [10] MMSMessageClass OPTIONAL,

expiry [11] MMSExpiry,

desiredDeliveryTime [12] Timestamp OPTIONAL,

priority [13] MMSPriority OPTIONAL,

senderVisibility [14] BOOLEAN OPTIONAL,

deliveryReport [15] BOOLEAN OPTIONAL,

readReport [16] BOOLEAN OPTIONAL,

store [17] BOOLEAN OPTIONAL,

state [18] MMState OPTIONAL,

flags [19] MMFlags OPTIONAL,

replyCharging [20] MMSReplyCharging OPTIONAL,

applicID [21] UTF8String OPTIONAL,

replyApplicID [22] UTF8String OPTIONAL,

auxApplicInfo [23] UTF8String OPTIONAL,

contentClass [24] MMSContentClass OPTIONAL,

dRMContent [25] BOOLEAN OPTIONAL,

adaptationAllowed [26] MMSAdaptation OPTIONAL,

contentType [27] MMSContentType,

responseStatus [28] MMSResponseStatus,

responseStatusText [29] UTF8String OPTIONAL,

messageID [30] UTF8String

}

MMSSendByNonLocalTarget ::= SEQUENCE

{

version [1] MMSVersion,

transactionID [2] UTF8String,

messageID [3] UTF8String,

terminatingMMSParty [4] SEQUENCE OF MMSParty,

originatingMMSParty [5] MMSParty,

direction [6] MMSDirection,

contentType [7] MMSContentType,

messageClass [8] MMSMessageClass OPTIONAL,

dateTime [9] Timestamp,

expiry [10] MMSExpiry OPTIONAL,

deliveryReport [11] BOOLEAN OPTIONAL,

priority [12] MMSPriority OPTIONAL,

senderVisibility [13] BOOLEAN OPTIONAL,

readReport [14] BOOLEAN OPTIONAL,

subject [15] MMSSubject OPTIONAL,

forwardCount [16] INTEGER OPTIONAL,

previouslySentBy [17] MMSPreviouslySentBy OPTIONAL,

prevSentByDateTime [18] Timestamp OPTIONAL,

applicID [19] UTF8String OPTIONAL,

replyApplicID [20] UTF8String OPTIONAL,

auxApplicInfo [21] UTF8String OPTIONAL,

contentClass [22] MMSContentClass OPTIONAL,

dRMContent [23] BOOLEAN OPTIONAL,

adaptationAllowed [24] MMSAdaptation OPTIONAL

}

MMSNotification ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

originatingMMSParty [3] MMSParty OPTIONAL,

direction [4] MMSDirection,

subject [5] MMSSubject OPTIONAL,

deliveryReportRequested [6] BOOLEAN OPTIONAL,

stored [7] BOOLEAN OPTIONAL,

messageClass [8] MMSMessageClass,

priority [9] MMSPriority OPTIONAL,

messageSize [10] INTEGER,

expiry [11] MMSExpiry,

replyCharging [12] MMSReplyCharging OPTIONAL

}

MMSSendToNonLocalTarget ::= SEQUENCE

{

version [1] MMSVersion,

transactionID [2] UTF8String,

messageID [3] UTF8String,

terminatingMMSParty [4] SEQUENCE OF MMSParty,

originatingMMSParty [5] MMSParty,

direction [6] MMSDirection,

contentType [7] MMSContentType,

messageClass [8] MMSMessageClass OPTIONAL,

dateTime [9] Timestamp,

expiry [10] MMSExpiry OPTIONAL,

deliveryReport [11] BOOLEAN OPTIONAL,

priority [12] MMSPriority OPTIONAL,

senderVisibility [13] BOOLEAN OPTIONAL,

readReport [14] BOOLEAN OPTIONAL,

subject [15] MMSSubject OPTIONAL,

forwardCount [16] INTEGER OPTIONAL,

previouslySentBy [17] MMSPreviouslySentBy OPTIONAL,

prevSentByDateTime [18] Timestamp OPTIONAL,

applicID [19] UTF8String OPTIONAL,

replyApplicID [20] UTF8String OPTIONAL,

auxApplicInfo [21] UTF8String OPTIONAL,

contentClass [22] MMSContentClass OPTIONAL,

dRMContent [23] BOOLEAN OPTIONAL,

adaptationAllowed [24] MMSAdaptation OPTIONAL

}

MMSNotificationResponse ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

direction [3] MMSDirection,

status [4] MMStatus,

reportAllowed [5] BOOLEAN OPTIONAL

}

MMSRetrieval ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

messageID [3] UTF8String,

dateTime [4] Timestamp,

originatingMMSParty [5] MMSParty OPTIONAL,

previouslySentBy [6] MMSPreviouslySentBy OPTIONAL,

prevSentByDateTime [7] Timestamp OPTIONAL,

terminatingMMSParty [8] SEQUENCE OF MMSParty OPTIONAL,

cCRecipients [9] SEQUENCE OF MMSParty OPTIONAL,

direction [10] MMSDirection,

subject [11] MMSSubject OPTIONAL,

state [12] MMState OPTIONAL,

flags [13] MMFlags OPTIONAL,

messageClass [14] MMSMessageClass OPTIONAL,

priority [15] MMSPriority,

deliveryReport [16] BOOLEAN OPTIONAL,

readReport [17] BOOLEAN OPTIONAL,

replyCharging [18] MMSReplyCharging OPTIONAL,

retrieveStatus [19] MMSRetrieveStatus OPTIONAL,

retrieveStatusText [20] UTF8String OPTIONAL,

applicID [21] UTF8String OPTIONAL,

replyApplicID [22] UTF8String OPTIONAL,

auxApplicInfo [23] UTF8String OPTIONAL,

contentClass [24] MMSContentClass OPTIONAL,

dRMContent [25] BOOLEAN OPTIONAL,

replaceID [26] UTF8String OPTIONAL,

contentType [27] UTF8String OPTIONAL

}

MMSDeliveryAck ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

reportAllowed [3] BOOLEAN OPTIONAL,

status [4] MMStatus,

direction [5] MMSDirection

}

MMSForward ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

dateTime [3] Timestamp OPTIONAL,

originatingMMSParty [4] MMSParty,

terminatingMMSParty [5] SEQUENCE OF MMSParty OPTIONAL,

cCRecipients [6] SEQUENCE OF MMSParty OPTIONAL,

bCCRecipients [7] SEQUENCE OF MMSParty OPTIONAL,

direction [8] MMSDirection,

expiry [9] MMSExpiry OPTIONAL,

desiredDeliveryTime [10] Timestamp OPTIONAL,

deliveryReportAllowed [11] BOOLEAN OPTIONAL,

deliveryReport [12] BOOLEAN OPTIONAL,

store [13] BOOLEAN OPTIONAL,

state [14] MMState OPTIONAL,

flags [15] MMFlags OPTIONAL,

contentLocationReq [16] UTF8String,

replyCharging [17] MMSReplyCharging OPTIONAL,

responseStatus [18] MMSResponseStatus,

responseStatusText [19] UTF8String OPTIONAL,

messageID [20] UTF8String OPTIONAL,

contentLocationConf [21] UTF8String OPTIONAL,

storeStatus [22] MMSStoreStatus OPTIONAL,

storeStatusText [23] UTF8String OPTIONAL

}

MMSDeleteFromRelay ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

direction [3] MMSDirection,

contentLocationReq [4] SEQUENCE OF UTF8String,

contentLocationConf [5] SEQUENCE OF UTF8String,

deleteResponseStatus [6] MMSDeleteResponseStatus,

deleteResponseText [7] SEQUENCE OF UTF8String

}

MMSMBoxStore ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

direction [3] MMSDirection,

contentLocationReq [4] UTF8String,

state [5] MMState OPTIONAL,

flags [6] MMFlags OPTIONAL,

contentLocationConf [7] UTF8String OPTIONAL,

storeStatus [8] MMSStoreStatus,

storeStatusText [9] UTF8String OPTIONAL

}

MMSMBoxUpload ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

direction [3] MMSDirection,

state [4] MMState OPTIONAL,

flags [5] MMFlags OPTIONAL,

contentType [6] UTF8String,

contentLocation [7] UTF8String OPTIONAL,

storeStatus [8] MMSStoreStatus,

storeStatusText [9] UTF8String OPTIONAL,

mMessages [10] SEQUENCE OF MMBoxDescription

}

MMSMBoxDelete ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

direction [3] MMSDirection,

contentLocationReq [4] SEQUENCE OF UTF8String,

contentLocationConf [5] SEQUENCE OF UTF8String OPTIONAL,

responseStatus [6] MMSDeleteResponseStatus,

responseStatusText [7] UTF8String OPTIONAL

}

MMSDeliveryReport ::= SEQUENCE

{

version [1] MMSVersion,

messageID [2] UTF8String,

terminatingMMSParty [3] SEQUENCE OF MMSParty,

mMSDateTime [4] Timestamp,

responseStatus [5] MMSResponseStatus,

responseStatusText [6] UTF8String OPTIONAL,

applicID [7] UTF8String OPTIONAL,

replyApplicID [8] UTF8String OPTIONAL,

auxApplicInfo [9] UTF8String OPTIONAL

}

MMSDeliveryReportNonLocalTarget ::= SEQUENCE

{

version [1] MMSVersion,

transactionID [2] UTF8String,

messageID [3] UTF8String,

terminatingMMSParty [4] SEQUENCE OF MMSParty,

originatingMMSParty [5] MMSParty,

direction [6] MMSDirection,

mMSDateTime [7] Timestamp,

forwardToOriginator [8] BOOLEAN OPTIONAL,

status [9] MMStatus,

statusExtension [10] MMStatusExtension,

statusText [11] MMStatusText,

applicID [12] UTF8String OPTIONAL,

replyApplicID [13] UTF8String OPTIONAL,

auxApplicInfo [14] UTF8String OPTIONAL

}

MMSReadReport ::= SEQUENCE

{

version [1] MMSVersion,

messageID [2] UTF8String,

terminatingMMSParty [3] SEQUENCE OF MMSParty,

originatingMMSParty [4] SEQUENCE OF MMSParty,

direction [5] MMSDirection,

mMSDateTime [6] Timestamp,

readStatus [7] MMSReadStatus,

applicID [8] UTF8String OPTIONAL,

replyApplicID [9] UTF8String OPTIONAL,

auxApplicInfo [10] UTF8String OPTIONAL

}

MMSReadReportNonLocalTarget ::= SEQUENCE

{

version [1] MMSVersion,

transactionID [2] UTF8String,

terminatingMMSParty [3] SEQUENCE OF MMSParty,

originatingMMSParty [4] SEQUENCE OF MMSParty,

direction [5] MMSDirection,

messageID [6] UTF8String,

mMSDateTime [7] Timestamp,

readStatus [8] MMSReadStatus,

readStatusText [9] MMSReadStatusText OPTIONAL,

applicID [10] UTF8String OPTIONAL,

replyApplicID [11] UTF8String OPTIONAL,

auxApplicInfo [12] UTF8String OPTIONAL

}

MMSCancel ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

cancelID [3] UTF8String,

direction [4] MMSDirection

}

MMSMBoxViewRequest ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

contentLocation [3] UTF8String OPTIONAL,

state [4] SEQUENCE OF MMState OPTIONAL,

flags [5] SEQUENCE OF MMFlags OPTIONAL,

start [6] INTEGER OPTIONAL,

limit [7] INTEGER OPTIONAL,

attributes [8] SEQUENCE OF UTF8String OPTIONAL,

totals [9] INTEGER OPTIONAL,

quotas [10] MMSQuota OPTIONAL

}

MMSMBoxViewResponse ::= SEQUENCE

{

transactionID [1] UTF8String,

version [2] MMSVersion,

contentLocation [3] UTF8String OPTIONAL,

state [4] SEQUENCE OF MMState OPTIONAL,

flags [5] SEQUENCE OF MMFlags OPTIONAL,

start [6] INTEGER OPTIONAL,

limit [7] INTEGER OPTIONAL,

attributes [8] SEQUENCE OF UTF8String OPTIONAL,

mMSTotals [9] BOOLEAN OPTIONAL,

mMSQuotas [10] BOOLEAN OPTIONAL,

mMessages [11] SEQUENCE OF MMBoxDescription

}

MMBoxDescription ::= SEQUENCE

{

contentLocation [1] UTF8String OPTIONAL,

messageID [2] UTF8String OPTIONAL,

state [3] MMState OPTIONAL,

flags [4] SEQUENCE OF MMFlags OPTIONAL,

dateTime [5] Timestamp OPTIONAL,

originatingMMSParty [6] MMSParty OPTIONAL,

terminatingMMSParty [7] SEQUENCE OF MMSParty OPTIONAL,

cCRecipients [8] SEQUENCE OF MMSParty OPTIONAL,

bCCRecipients [9] SEQUENCE OF MMSParty OPTIONAL,

messageClass [10] MMSMessageClass OPTIONAL,

subject [11] MMSSubject OPTIONAL,

priority [12] MMSPriority OPTIONAL,

deliveryTime [13] Timestamp OPTIONAL,

readReport [14] BOOLEAN OPTIONAL,

messageSize [15] INTEGER OPTIONAL,

replyCharging [16] MMSReplyCharging OPTIONAL,

previouslySentBy [17] MMSPreviouslySentBy OPTIONAL,

previouslySentByDateTime [18] Timestamp OPTIONAL,

contentType [19] UTF8String OPTIONAL

}

-- =========

-- MMS CCPDU

-- =========

MMSCCPDU ::= SEQUENCE

{

version [1] MMSVersion,

transactionID [2] UTF8String,

mMSContent [3] OCTET STRING

}

-- ==============

-- MMS parameters

-- ==============

MMSAdaptation ::= SEQUENCE

{

allowed [1] BOOLEAN,

overriden [2] BOOLEAN

}

MMSCancelStatus ::= ENUMERATED

{

cancelRequestSuccessfullyReceived(1),

cancelRequestCorrupted(2)

}

MMSContentClass ::= ENUMERATED

{

text(1),

imageBasic(2),

imageRich(3),

videoBasic(4),

videoRich(5),

megaPixel(6),

contentBasic(7),

contentRich(8)

}

MMSContentType ::= UTF8String

MMSDeleteResponseStatus ::= ENUMERATED

{

ok(1),

errorUnspecified(2),

errorServiceDenied(3),

errorMessageFormatCorrupt(4),

errorSendingAddressUnresolved(5),

errorMessageNotFound(6),

errorNetworkProblem(7),

errorContentNotAccepted(8),

errorUnsupportedMessage(9),

errorTransientFailure(10),

errorTransientSendingAddressUnresolved(11),

errorTransientMessageNotFound(12),

errorTransientNetworkProblem(13),

errorTransientPartialSuccess(14),

errorPermanentFailure(15),

errorPermanentServiceDenied(16),

errorPermanentMessageFormatCorrupt(17),

errorPermanentSendingAddressUnresolved(18),

errorPermanentMessageNotFound(19),

errorPermanentContentNotAccepted(20),

errorPermanentReplyChargingLimitationsNotMet(21),

errorPermanentReplyChargingRequestNotAccepted(22),

errorPermanentReplyChargingForwardingDenied(23),

errorPermanentReplyChargingNotSupported(24),

errorPermanentAddressHidingNotSupported(25),

errorPermanentLackOfPrepaid(26)

}

MMSDirection ::= ENUMERATED

{

fromTarget(0),

toTarget(1)

}

MMSElementDescriptor ::= SEQUENCE

{

reference [1] UTF8String,

parameter [2] UTF8String OPTIONAL,

value [3] UTF8String OPTIONAL

}

MMSExpiry ::= SEQUENCE

{

expiryPeriod [1] INTEGER,

periodFormat [2] MMSPeriodFormat

}

MMFlags ::= SEQUENCE

{

length [1] INTEGER,

flag [2] MMStateFlag,

flagString [3] UTF8String

}

MMSMessageClass ::= ENUMERATED

{

personal(1),

advertisement(2),

informational(3),

auto(4)

}

MMSParty ::= SEQUENCE

{

mMSPartyIDs [1] SEQUENCE OF MMSPartyID,

nonLocalID [2] NonLocalID

}

MMSPartyID ::= CHOICE

{

e164Number [1] E164Number,

emailAddress [2] EmailAddress,

iMSI [3] IMSI,

iMPU [4] IMPU,

iMPI [5] IMPI,

sUPI [6] SUPI,

gPSI [7] GPSI

}

MMSPeriodFormat ::= ENUMERATED

{

absolute(1),

relative(2)

}

MMSPreviouslySent ::= SEQUENCE

{

previouslySentByParty [1] MMSParty,

sequenceNumber [2] INTEGER,

previousSendDateTime [3] Timestamp

}

MMSPreviouslySentBy ::= SEQUENCE OF MMSPreviouslySent

MMSPriority ::= ENUMERATED

{

low(1),

normal(2),

high(3)

}

MMSQuota ::= SEQUENCE

{

quota [1] INTEGER,

quotaUnit [2] MMSQuotaUnit

}

MMSQuotaUnit ::= ENUMERATED

{

numMessages(1),

bytes(2)

}

MMSReadStatus ::= ENUMERATED

{

read(1),

deletedWithoutBeingRead(2)

}

MMSReadStatusText ::= UTF8String

MMSReplyCharging ::= ENUMERATED

{

requested(0),

requestedTextOnly(1),

accepted(2),

acceptedTextOnly(3)

}

MMSResponseStatus ::= ENUMERATED

{

ok(1),

errorUnspecified(2),

errorServiceDenied(3),

errorMessageFormatCorrupt(4),

errorSendingAddressUnresolved(5),

errorMessageNotFound(6),

errorNetworkProblem(7),

errorContentNotAccepted(8),

errorUnsupportedMessage(9),

errorTransientFailure(10),

errorTransientSendingAddressUnresolved(11),

errorTransientMessageNotFound(12),

errorTransientNetworkProblem(13),

errorTransientPartialSuccess(14),

errorPermanentFailure(15),

errorPermanentServiceDenied(16),

errorPermanentMessageFormatCorrupt(17),

errorPermanentSendingAddressUnresolved(18),

errorPermanentMessageNotFound(19),

errorPermanentContentNotAccepted(20),

errorPermanentReplyChargingLimitationsNotMet(21),

errorPermanentReplyChargingRequestNotAccepted(22),

errorPermanentReplyChargingForwardingDenied(23),

errorPermanentReplyChargingNotSupported(24),

errorPermanentAddressHidingNotSupported(25),

errorPermanentLackOfPrepaid(26)

}

MMSRetrieveStatus ::= ENUMERATED

{

success(1),

errorTransientFailure(2),

errorTransientMessageNotFound(3),

errorTransientNetworkProblem(4),

errorPermanentFailure(5),

errorPermanentServiceDenied(6),

errorPermanentMessageNotFound(7),

errorPermanentContentUnsupported(8)

}

MMSStoreStatus ::= ENUMERATED

{

success(1),

errorTransientFailure(2),

errorTransientNetworkProblem(3),

errorPermanentFailure(4),

errorPermanentServiceDenied(5),

errorPermanentMessageFormatCorrupt(6),

errorPermanentMessageNotFound(7),

errorMMBoxFull(8)

}

MMState ::= ENUMERATED

{

draft(1),

sent(2),

new(3),

retrieved(4),

forwarded(5)

}

MMStateFlag ::= ENUMERATED

{

add(1),

remove(2),

filter(3)

}

MMStatus ::= ENUMERATED

{

expired(1),

retrieved(2),

rejected(3),

deferred(4),

unrecognized(5),

indeterminate(6),

forwarded(7),

unreachable(8)

}

MMStatusExtension ::= ENUMERATED

{

rejectionByMMSRecipient(0),

rejectionByOtherRS(1)

}

MMStatusText ::= UTF8String

MMSSubject ::= UTF8String

MMSVersion ::= SEQUENCE

{

majorVersion [1] INTEGER,

minorVersion [2] INTEGER

}

-- ==================

-- 5G PTC definitions

-- ==================

PTCRegistration ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCServerURI [2] UTF8String,

pTCRegistrationRequest [3] PTCRegistrationRequest,

pTCRegistrationOutcome [4] PTCRegistrationOutcome

}

PTCSessionInitiation ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCServerURI [3] UTF8String,

pTCSessionInfo [4] PTCSessionInfo,

pTCOriginatingID [5] PTCTargetInformation,

pTCParticipants [6] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCParticipantPresenceStatus [7] MultipleParticipantPresenceStatus OPTIONAL,

location [8] Location OPTIONAL,

pTCBearerCapability [9] UTF8String OPTIONAL,

pTCHost [10] PTCTargetInformation OPTIONAL

}

PTCSessionAbandon ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessionInfo [3] PTCSessionInfo,

location [4] Location OPTIONAL,

pTCAbandonCause [5] INTEGER

}

PTCSessionStart ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCServerURI [3] UTF8String,

pTCSessionInfo [4] PTCSessionInfo,

pTCOriginatingID [5] PTCTargetInformation,

pTCParticipants [6] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCParticipantPresenceStatus [7] MultipleParticipantPresenceStatus OPTIONAL,

location [8] Location OPTIONAL,

pTCHost [9] PTCTargetInformation OPTIONAL,

pTCBearerCapability [10] UTF8String OPTIONAL

}

PTCSessionEnd ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCServerURI [3] UTF8String,

pTCSessionInfo [4] PTCSessionInfo,

pTCParticipants [5] SEQUENCE OF PTCTargetInformation OPTIONAL,

location [6] Location OPTIONAL,

pTCSessionEndCause [7] PTCSessionEndCause

}

PTCStartOfInterception ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

preEstSessionID [3] PTCSessionInfo OPTIONAL,

pTCOriginatingID [4] PTCTargetInformation,

pTCSessionInfo [5] PTCSessionInfo OPTIONAL,

pTCHost [6] PTCTargetInformation OPTIONAL,

pTCParticipants [7] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCMediaStreamAvail [8] BOOLEAN OPTIONAL,

pTCBearerCapability [9] UTF8String OPTIONAL

}

PTCPreEstablishedSession ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCServerURI [2] UTF8String,

rTPSetting [3] RTPSetting,

pTCMediaCapability [4] UTF8String,

pTCPreEstSessionID [5] PTCSessionInfo,

pTCPreEstStatus [6] PTCPreEstStatus,

pTCMediaStreamAvail [7] BOOLEAN OPTIONAL,

location [8] Location OPTIONAL,

pTCFailureCode [9] PTCFailureCode OPTIONAL

}

PTCInstantPersonalAlert ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCIPAPartyID [2] PTCTargetInformation,

pTCIPADirection [3] Direction

}

PTCPartyJoin ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessionInfo [3] PTCSessionInfo,

pTCParticipants [4] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCParticipantPresenceStatus [5] MultipleParticipantPresenceStatus OPTIONAL,

pTCMediaStreamAvail [6] BOOLEAN OPTIONAL,

pTCBearerCapability [7] UTF8String OPTIONAL

}

PTCPartyDrop ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessionInfo [3] PTCSessionInfo,

pTCPartyDrop [4] PTCTargetInformation,

pTCParticipantPresenceStatus [5] PTCParticipantPresenceStatus OPTIONAL

}

PTCPartyHold ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessionInfo [3] PTCSessionInfo,

pTCParticipants [4] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCHoldID [5] SEQUENCE OF PTCTargetInformation,

pTCHoldRetrieveInd [6] BOOLEAN

}

PTCMediaModification ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessionInfo [3] PTCSessionInfo,

pTCMediaStreamAvail [4] BOOLEAN OPTIONAL,

pTCBearerCapability [5] UTF8String

}

PTCGroupAdvertisement ::=SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCIDList [3] SEQUENCE OF PTCTargetInformation OPTIONAL,

pTCGroupAuthRule [4] PTCGroupAuthRule OPTIONAL,

pTCGroupAdSender [5] PTCTargetInformation,

pTCGroupNickname [6] UTF8String OPTIONAL

}

PTCFloorControl ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCSessioninfo [3] PTCSessionInfo,

pTCFloorActivity [4] SEQUENCE OF PTCFloorActivity,

pTCFloorSpeakerID [5] PTCTargetInformation OPTIONAL,

pTCMaxTBTime [6] INTEGER OPTIONAL,

pTCQueuedFloorControl [7] BOOLEAN OPTIONAL,

pTCQueuedPosition [8] INTEGER OPTIONAL,

pTCTalkBurstPriority [9] PTCTBPriorityLevel OPTIONAL,

pTCTalkBurstReason [10] PTCTBReasonCode OPTIONAL

}

PTCTargetPresence ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCTargetPresenceStatus [2] PTCParticipantPresenceStatus

}

PTCParticipantPresence ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCParticipantPresenceStatus [2] PTCParticipantPresenceStatus

}

PTCListManagement ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCListManagementType [3] PTCListManagementType OPTIONAL,

pTCListManagementAction [4] PTCListManagementAction OPTIONAL,

pTCListManagementFailure [5] PTCListManagementFailure OPTIONAL,

pTCContactID [6] PTCTargetInformation OPTIONAL,

pTCIDList [7] SEQUENCE OF PTCIDList OPTIONAL,

pTCHost [8] PTCTargetInformation OPTIONAL

}

PTCAccessPolicy ::= SEQUENCE

{

pTCTargetInformation [1] PTCTargetInformation,

pTCDirection [2] Direction,

pTCAccessPolicyType [3] PTCAccessPolicyType OPTIONAL,

pTCUserAccessPolicy [4] PTCUserAccessPolicy OPTIONAL,

pTCGroupAuthRule [5] PTCGroupAuthRule OPTIONAL,

pTCContactID [6] PTCTargetInformation OPTIONAL,

pTCAccessPolicyFailure [7] PTCAccessPolicyFailure OPTIONAL

}

-- =========

-- PTC CCPDU

-- =========

PTCCCPDU ::= OCTET STRING

-- =================

-- 5G PTC parameters

-- =================

PTCRegistrationRequest ::= ENUMERATED

{

register(1),

reRegister(2),

deRegister(3)

}

PTCRegistrationOutcome ::= ENUMERATED

{

success(1),

failure(2)

}

PTCSessionEndCause ::= ENUMERATED

{

initiaterLeavesSession(1),

definedParticipantLeaves(2),

numberOfParticipants(3),

sessionTimerExpired(4),

pTCSpeechInactive(5),

allMediaTypesInactive(6)

}

PTCTargetInformation ::= SEQUENCE

{

identifiers [1] SEQUENCE SIZE(1..MAX) OF PTCIdentifiers

}

PTCIdentifiers ::= CHOICE

{

mCPTTID [1] UTF8String,

instanceIdentifierURN [2] UTF8String,

pTCChatGroupID [3] PTCChatGroupID,

iMPU [4] IMPU,

iMPI [5] IMPI

}

PTCSessionInfo ::= SEQUENCE

{

pTCSessionURI [1] UTF8String,

pTCSessionType [2] PTCSessionType

}

PTCSessionType ::= ENUMERATED

{

ondemand(1),

preEstablished(2),

adhoc(3),

prearranged(4),

groupSession(5)

}

MultipleParticipantPresenceStatus ::= SEQUENCE OF PTCParticipantPresenceStatus

PTCParticipantPresenceStatus ::= SEQUENCE

{

presenceID [1] PTCTargetInformation,

presenceType [2] PTCPresenceType,

presenceStatus [3] BOOLEAN

}

PTCPresenceType ::= ENUMERATED

{

pTCClient(1),

pTCGroup(2)

}

PTCPreEstStatus ::= ENUMERATED

{

established(1),

modified(2),

released(3)

}

RTPSetting ::= SEQUENCE

{

iPAddress [1] IPAddress,

portNumber [2] PortNumber

}

PTCIDList ::= SEQUENCE

{

pTCPartyID [1] PTCTargetInformation,

pTCChatGroupID [2] PTCChatGroupID

}

PTCChatGroupID ::= SEQUENCE

{

groupIdentity [1] UTF8String

}

PTCFloorActivity ::= ENUMERATED

{

tBCPRequest(1),

tBCPGranted(2),

tBCPDeny(3),

tBCPIdle(4),

tBCPTaken(5),

tBCPRevoke(6),

tBCPQueued(7),

tBCPRelease(8)

}

PTCTBPriorityLevel ::= ENUMERATED

{

preEmptive(1),

highPriority(2),

normalPriority(3),

listenOnly(4)

}

PTCTBReasonCode ::= ENUMERATED

{

noQueuingAllowed(1),

oneParticipantSession(2),

listenOnly(3),

exceededMaxDuration(4),

tBPrevented(5)

}

PTCListManagementType ::= ENUMERATED

{

contactListManagementAttempt(1),

groupListManagementAttempt(2),

contactListManagementResult(3),

groupListManagementResult(4),

requestUnsuccessful(5)

}

PTCListManagementAction ::= ENUMERATED

{

create(1),

modify(2),

retrieve(3),

delete(4),

notify(5)

}

PTCAccessPolicyType ::= ENUMERATED

{

pTCUserAccessPolicyAttempt(1),

groupAuthorizationRulesAttempt(2),

pTCUserAccessPolicyQuery(3),

groupAuthorizationRulesQuery(4),

pTCUserAccessPolicyResult(5),

groupAuthorizationRulesResult(6),

requestUnsuccessful(7)

}

PTCUserAccessPolicy ::= ENUMERATED

{

allowIncomingPTCSessionRequest(1),

blockIncomingPTCSessionRequest(2),

allowAutoAnswerMode(3),

allowOverrideManualAnswerMode(4)

}

PTCGroupAuthRule ::= ENUMERATED

{

allowInitiatingPTCSession(1),

blockInitiatingPTCSession(2),

allowJoiningPTCSession(3),

blockJoiningPTCSession(4),

allowAddParticipants(5),

blockAddParticipants(6),

allowSubscriptionPTCSessionState(7),

blockSubscriptionPTCSessionState(8),

allowAnonymity(9),

forbidAnonymity(10)

}

PTCFailureCode ::= ENUMERATED

{

sessionCannotBeEstablished(1),

sessionCannotBeModified(2)

}

PTCListManagementFailure ::= ENUMERATED

{

requestUnsuccessful(1),

requestUnknown(2)

}

PTCAccessPolicyFailure ::= ENUMERATED

{

requestUnsuccessful(1),

requestUnknown(2)

}

-- ===============

-- IMS definitions

-- ===============

-- See clause 7.12.4.2.1 for details of this structure

IMSMessage ::= SEQUENCE

{

payload [1] IMSPayload,

sessionDirection [2] SessionDirection,

voIPRoamingIndication [3] VoIPRoamingIndication OPTIONAL,

location [6] Location OPTIONAL

}

-- See clause 7.12.4.2.2 for details of this structure

StartOfInterceptionForActiveIMSSession ::= SEQUENCE

{

originatingId [1] SEQUENCE OF IMPU,

terminatingId [2] IMPU,

sDPState [3] SEQUENCE OF OCTET STRING OPTIONAL,

diversionIdentity [4] IMPU OPTIONAL,

voIPRoamingIndication [5] VoIPRoamingIndication OPTIONAL,

location [7] Location OPTIONAL

}

-- See clause 7.12.4.2.3 for the details.

IMSCCUnavailable ::= SEQUENCE

{

cCUnavailableReason [1] UTF8String,

sDPState [2] OCTET STRING OPTIONAL

}

-- =========

-- IMS CCPDU

-- =========

IMSCCPDU ::= SEQUENCE

{

payload [1] IMSCCPDUPayload,

sDPInfo [2] OCTET STRING OPTIONAL

}

IMSCCPDUPayload ::= OCTET STRING

-- ==============

-- IMS parameters

-- ==============

IMSPayload ::= CHOICE

{

encapsulatedSIPMessage [1] SIPMessage

}

SIPMessage ::= SEQUENCE

{

iPSourceAddress [1] IPAddress,

iPDestinationAddress [2] IPAddress,

sIPContent [3] OCTET STRING

}

VoIPRoamingIndication ::= ENUMERATED

{

roamingLBO(1),

roamingS8HR(2),

roamingN9HR(3)

}

SessionDirection ::= ENUMERATED

{

fromTarget(1),

toTarget(2),

combined(3),

indeterminate(4)

}

HeaderOnlyIndication ::= BOOLEAN

-- =================================

-- STIR/SHAKEN/RCD/eCNAM definitions

-- =================================

-- See clause 7.11.2.1.2 for details of this structure

STIRSHAKENSignatureGeneration ::= SEQUENCE

{

pASSporTs [1] SEQUENCE OF PASSporT,

encapsulatedSIPMessage [2] SIPMessage OPTIONAL

}

-- See clause 7.11.2.1.3 for details of this structure

STIRSHAKENSignatureValidation ::= SEQUENCE

{

pASSporTs [1] SEQUENCE OF PASSporT OPTIONAL,

rCDTerminalDisplayInfo [2] RCDDisplayInfo OPTIONAL,

eCNAMTerminalDisplayInfo [3] ECNAMDisplayInfo OPTIONAL,

sHAKENValidationResult [4] SHAKENValidationResult,

sHAKENFailureStatusCode [5] SHAKENFailureStatusCode OPTIONAL,

encapsulatedSIPMessage [6] SIPMessage OPTIONAL

}

-- ================================

-- STIR/SHAKEN/RCD/eCNAM parameters

-- ================================

PASSporT ::= SEQUENCE

{

pASSporTHeader [1] PASSporTHeader,

pASSporTPayload [2] PASSporTPayload,

pASSporTSignature [3] OCTET STRING

}

PASSporTHeader ::= SEQUENCE

{

type [1] JWSTokenType,

algorithm [2] UTF8String,

ppt [3] UTF8String OPTIONAL,

x5u [4] UTF8String

}

JWSTokenType ::= ENUMERATED

{

passport(1)

}

PASSporTPayload ::= SEQUENCE

{

issuedAtTime [1] GeneralizedTime,

originator [2] STIRSHAKENOriginator,

destination [3] STIRSHAKENDestinations,

attestation [4] Attestation,

origId [5] UTF8String,

diversion [6] STIRSHAKENDestination

}

STIRSHAKENOriginator ::= CHOICE

{

telephoneNumber [1] STIRSHAKENTN,

sTIRSHAKENURI [2] UTF8String

}

STIRSHAKENDestinations ::= SEQUENCE OF STIRSHAKENDestination

STIRSHAKENDestination ::= CHOICE

{

telephoneNumber [1] STIRSHAKENTN,

sTIRSHAKENURI [2] UTF8String

}

STIRSHAKENTN ::= CHOICE

{

mSISDN [1] MSISDN

}

Attestation ::= ENUMERATED

{

attestationA(1),

attestationB(2),

attestationC(3)

}

SHAKENValidationResult ::= ENUMERATED

{

tNValidationPassed(1),

tNValidationFailed(2),

noTNValidation(3)

}

SHAKENFailureStatusCode ::= INTEGER

ECNAMDisplayInfo ::= SEQUENCE

{

name [1] UTF8String,

additionalInfo [2] OCTET STRING OPTIONAL

}

RCDDisplayInfo ::= SEQUENCE

{

name [1] UTF8String,

jcd [2] OCTET STRING OPTIONAL,

jcl [3] OCTET STRING OPTIONAL

}

-- ===================

-- 5G LALS definitions

-- ===================

LALSReport ::= SEQUENCE

{

sUPI [1] SUPI OPTIONAL,

-- pEI [2] PEI OPTIONAL, deprecated in Release-16, do not re-use this tag number

gPSI [3] GPSI OPTIONAL,

location [4] Location OPTIONAL,

iMPU [5] IMPU OPTIONAL,

iMSI [7] IMSI OPTIONAL,

mSISDN [8] MSISDN OPTIONAL

}

-- =====================

-- PDHR/PDSR definitions

-- =====================

PDHeaderReport ::= SEQUENCE

{

pDUSessionID [1] PDUSessionID,

sourceIPAddress [2] IPAddress,

sourcePort [3] PortNumber OPTIONAL,

destinationIPAddress [4] IPAddress,

destinationPort [5] PortNumber OPTIONAL,

nextLayerProtocol [6] NextLayerProtocol,

iPv6flowLabel [7] IPv6FlowLabel OPTIONAL,

direction [8] Direction,

packetSize [9] INTEGER

}

PDSummaryReport ::= SEQUENCE

{

pDUSessionID [1] PDUSessionID,

sourceIPAddress [2] IPAddress,

sourcePort [3] PortNumber OPTIONAL,

destinationIPAddress [4] IPAddress,

destinationPort [5] PortNumber OPTIONAL,

nextLayerProtocol [6] NextLayerProtocol,

iPv6flowLabel [7] IPv6FlowLabel OPTIONAL,

direction [8] Direction,

pDSRSummaryTrigger [9] PDSRSummaryTrigger,

firstPacketTimestamp [10] Timestamp,

lastPacketTimestamp [11] Timestamp,

packetCount [12] INTEGER,

byteCount [13] INTEGER

}

-- ====================

-- PDHR/PDSR parameters

-- ====================

PDSRSummaryTrigger ::= ENUMERATED

{

timerExpiry(1),

packetCount(2),

byteCount(3),

startOfFlow(4),

endOfFlow(5)

}

-- ==================================

-- Identifier Association definitions

-- ==================================

AMFIdentifierAssociation ::= SEQUENCE

{

sUPI [1] SUPI,

sUCI [2] SUCI OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

gUTI [5] FiveGGUTI,

location [6] Location,

fiveGSTAIList [7] TAIList OPTIONAL

}

MMEIdentifierAssociation ::= SEQUENCE

{

iMSI [1] IMSI,

iMEI [2] IMEI OPTIONAL,

mSISDN [3] MSISDN OPTIONAL,

gUTI [4] GUTI,

location [5] Location,

tAIList [6] TAIList OPTIONAL

}

-- =================================

-- Identifier Association parameters

-- =================================

MMEGroupID ::= OCTET STRING (SIZE(2))

MMECode ::= OCTET STRING (SIZE(1))

TMSI ::= OCTET STRING (SIZE(4))

-- ===================

-- EPS MME definitions

-- ===================

MMEAttach ::= SEQUENCE

{

attachType [1] EPSAttachType,

attachResult [2] EPSAttachResult,

iMSI [3] IMSI,

iMEI [4] IMEI OPTIONAL,

mSISDN [5] MSISDN OPTIONAL,

gUTI [6] GUTI OPTIONAL,

location [7] Location OPTIONAL,

ePSTAIList [8] TAIList OPTIONAL,

sMSServiceStatus [9] EPSSMSServiceStatus OPTIONAL,

oldGUTI [10] GUTI OPTIONAL,

eMM5GRegStatus [11] EMM5GMMStatus OPTIONAL

}

MMEDetach ::= SEQUENCE

{

detachDirection [1] MMEDirection,

detachType [2] EPSDetachType,

iMSI [3] IMSI,

iMEI [4] IMEI OPTIONAL,

mSISDN [5] MSISDN OPTIONAL,

gUTI [6] GUTI OPTIONAL,

cause [7] EMMCause OPTIONAL,

location [8] Location OPTIONAL,

switchOffIndicator [9] SwitchOffIndicator OPTIONAL

}

MMELocationUpdate ::= SEQUENCE

{

iMSI [1] IMSI,

iMEI [2] IMEI OPTIONAL,

mSISDN [3] MSISDN OPTIONAL,

gUTI [4] GUTI OPTIONAL,

location [5] Location OPTIONAL,

oldGUTI [6] GUTI OPTIONAL,

sMSServiceStatus [7] EPSSMSServiceStatus OPTIONAL

}

MMEStartOfInterceptionWithEPSAttachedUE ::= SEQUENCE

{

attachType [1] EPSAttachType,

attachResult [2] EPSAttachResult,

iMSI [3] IMSI,

iMEI [4] IMEI OPTIONAL,

mSISDN [5] MSISDN OPTIONAL,

gUTI [6] GUTI OPTIONAL,

location [7] Location OPTIONAL,

ePSTAIList [9] TAIList OPTIONAL,

sMSServiceStatus [10] EPSSMSServiceStatus OPTIONAL,

eMM5GRegStatus [12] EMM5GMMStatus OPTIONAL

}

MMEUnsuccessfulProcedure ::= SEQUENCE

{

failedProcedureType [1] MMEFailedProcedureType,

failureCause [2] MMEFailureCause,

iMSI [3] IMSI OPTIONAL,

iMEI [4] IMEI OPTIONAL,

mSISDN [5] MSISDN OPTIONAL,

gUTI [6] GUTI OPTIONAL,

location [7] Location OPTIONAL

}

-- See clause 6.3.2.2.8 for details of this structure

MMEPositioningInfoTransfer ::= SEQUENCE

{

iMSI [1] IMSI,

iMEI [2] IMEI OPTIONAL,

mSISDN [3] MSISDN OPTIONAL,

gUTI [4] GUTI OPTIONAL,

lPPaMessage [5] OCTET STRING OPTIONAL,

lPPMessage [6] OCTET STRING OPTIONAL,

mMELCSCorrelationId [7] OCTET STRING (SIZE(4))

}

-- ==================

-- EPS MME parameters

-- ==================

EMMCause ::= INTEGER (0..255)

ESMCause ::= INTEGER (0..255)

EPSAttachType ::= ENUMERATED

{

ePSAttach(1),

combinedEPSIMSIAttach(2),

ePSRLOSAttach(3),

ePSEmergencyAttach(4),

reserved(5)

}

EPSAttachResult ::= ENUMERATED

{

ePSOnly(1),

combinedEPSIMSI(2)

}

EPSDetachType ::= ENUMERATED

{

ePSDetach(1),

iMSIDetach(2),

combinedEPSIMSIDetach(3),

reAttachRequired(4),

reAttachNotRequired(5),

reserved(6)

}

EPSSMSServiceStatus ::= ENUMERATED

{

sMSServicesNotAvailable(1),

sMSServicesNotAvailableInThisPLMN(2),

networkFailure(3),

congestion(4)

}

MMEDirection ::= ENUMERATED

{

networkInitiated(1),

uEInitiated(2)

}

MMEFailedProcedureType ::= ENUMERATED

{

attachReject(1),

authenticationReject(2),

securityModeReject(3),

serviceReject(4),

trackingAreaUpdateReject(5),

activateDedicatedEPSBearerContextReject(6),

activateDefaultEPSBearerContextReject(7),

bearerResourceAllocationReject(8),

bearerResourceModificationReject(9),

modifyEPSBearerContectReject(10),

pDNConnectivityReject(11),

pDNDisconnectReject(12)

}

MMEFailureCause ::= CHOICE

{

eMMCause [1] EMMCause,

eSMCause [2] ESMCause

}

-- ===========================

-- LI Notification definitions

-- ===========================

LINotification ::= SEQUENCE

{

notificationType [1] LINotificationType,

appliedTargetID [2] TargetIdentifier OPTIONAL,

appliedDeliveryInformation [3] SEQUENCE OF LIAppliedDeliveryInformation OPTIONAL,

appliedStartTime [4] Timestamp OPTIONAL,

appliedEndTime [5] Timestamp OPTIONAL

}

-- ==========================

-- LI Notification parameters

-- ==========================

LINotificationType ::= ENUMERATED

{

activation(1),

deactivation(2),

modification(3)

}

LIAppliedDeliveryInformation ::= SEQUENCE

{

hI2DeliveryIPAddress [1] IPAddress OPTIONAL,

hI2DeliveryPortNumber [2] PortNumber OPTIONAL,

hI3DeliveryIPAddress [3] IPAddress OPTIONAL,

hI3DeliveryPortNumber [4] PortNumber OPTIONAL

}

-- ===============

-- MDF definitions

-- ===============

MDFCellSiteReport ::= SEQUENCE OF CellInformation

-- ==============================

-- 5G EPS Interworking Parameters

-- ==============================

EMM5GMMStatus ::= SEQUENCE

{

eMMRegStatus [1] EMMRegStatus OPTIONAL,

fiveGMMStatus [2] FiveGMMStatus OPTIONAL

}

EPS5GGUTI ::= CHOICE

{

gUTI [1] GUTI,

fiveGGUTI [2] FiveGGUTI

}

EMMRegStatus ::= ENUMERATED

{

uEEMMRegistered(1),

uENotEMMRegistered(2)

}

FiveGMMStatus ::= ENUMERATED

{

uE5GMMRegistered(1),

uENot5GMMRegistered(2)

}

-- ========================================

-- Separated Location Reporting definitions

-- ========================================

SeparatedLocationReporting ::= SEQUENCE

{

sUPI [1] SUPI,

sUCI [2] SUCI OPTIONAL,

pEI [3] PEI OPTIONAL,

gPSI [4] GPSI OPTIONAL,

gUTI [5] FiveGGUTI OPTIONAL,

location [6] Location,

non3GPPAccessEndpoint [7] UEEndpointAddress OPTIONAL,

rATType [8] RATType OPTIONAL

}

-- =================

-- Common Parameters

-- =================

AccessType ::= ENUMERATED

{

threeGPPAccess(1),

nonThreeGPPAccess(2),

threeGPPandNonThreeGPPAccess(3)

}

AllowedNSSAI ::= SEQUENCE OF NSSAI

AllowedTACs ::= SEQUENCE (SIZE(1..MAX)) OF TAC

AreaOfInterest ::= SEQUENCE

{

areaOfInterestTAIList [1] AreaOfInterestTAIList OPTIONAL,

areaOfInterestCellList [2] AreaOfInterestCellList OPTIONAL,

areaOfInterestRANNodeList [3] AreaOfInterestRANNodeList OPTIONAL

}

AreaOfInterestCellList ::= SEQUENCE (SIZE(1..MAX)) OF NCGI

AreaOfInterestItem ::= SEQUENCE

{

areaOfInterest [1] AreaOfInterest

}

AreaOfInterestRANNodeList ::= SEQUENCE (SIZE(1..MAX)) OF GlobalRANNodeID

AreaOfInterestTAIList ::= SEQUENCE (SIZE(1..MAX)) OF TAI

CellCAGList ::= SEQUENCE (SIZE(1..MAX)) OF CAGID

CauseMisc ::= ENUMERATED

{

controlProcessingOverload(1),

notEnoughUserPlaneProcessingResources(2),

hardwareFailure(3),

oMIntervention(4),

unknownPLMNOrSNPN(5),

unspecified(6)

}

CauseNas ::= ENUMERATED

{

normalRelease(1),

authenticationFailure(2),

deregister(3),

unspecified(4)

}

CauseProtocol ::= ENUMERATED

{

transferSyntaxError(1),

abstractSyntaxError-reject(2),

abstractSyntaxErrorIgnoreAndNotify(3),

messageNotCompatibleWithReceiverState(4),

semanticError(5),

abstractSyntaxErrorFalselyConstructedMessage(6),

unspecified(7)

}

CauseRadioNetwork ::= ENUMERATED

{

unspecified(1),

txnrelocoverallExpiry(2),

successfulHandover(3),

releaseDueToNGRANGeneratedReason(4),

releaseDueTo5gcGeneratedReason(5),

handoverCancelled(6),

partialHandover(7),

hoFailureInTarget5GCNGRANNodeOrTargetSystem(8),

hoTargetNotAllowed(9),

tNGRelocOverallExpiry(10),

tNGRelocPrepExpiry(11),

cellNotAvailable(12),

unknownTargetID(13),

noRadioResourcesAvailableInTargetCell(14),

unknownLocalUENGAPID(15),

inconsistentRemoteUENGAPID(16),

handoverDesirableForRadioReason(17),

timeCriticalHandover(18),

resourceOptimisationHandover(19),

reduceLoadInServingCell(20),

userInactivity(21),

radioConnectionWithUELost(22),

radioResourcesNotAvailable(23),

invalidQoSCombination(24),

failureInRadioInterfaceProcedure(25),

interactionWithOtherProcedure(26),

unknownPDUSessionID(27),

multiplePDUSessionIDInstances(29),

multipleQoSFlowIDInstances(30),

encryptionAndOrIntegrityProtectionAlgorithmsNotSupported(31),

nGIntraSystemHandoverTriggered(32),

nGInterSystemHandoverTriggered(33),

xNHandoverTriggered(34),

notSupported5QIValue(35),

uEContextTransfer(36),

iMSVoiceeEPSFallbackOrRATFallbackTriggered(37),

uPIntegrityProtectioNotPossible(38),

uPConfidentialityProtectionNotPossible(39),

sliceNotSupported(40),

uEInRRCInactiveStateNotReachable(41),

redirection(42),

resourcesNotAvailableForTheSlice(43),

uEMaxIntegrityProtectedDataRateReason(44),

releaseDueToCNDetectedMobility(45),

n26InterfaceNotAvailable(46),

releaseDueToPreemption(47),

multipleLocationReportingReferenceIDInstances(48),

rSNNotAvailableForTheUP(49),

nPMAccessDenied(50),

cAGOnlyAccessDenied(51),

insufficientUECapabilities(52)

}

CauseTransport ::= ENUMERATED

{

transportResourceUnavailable(1),

unspecified(2)

}

Direction ::= ENUMERATED

{

fromTarget(1),

toTarget(2)

}

DNN ::= UTF8String

E164Number ::= NumericString (SIZE(1..15))

EmailAddress ::= UTF8String

EquivalentPLMNs ::= SEQUENCE (SIZE(1..MAX)) OF PLMNID

EUI64 ::= OCTET STRING (SIZE(8))

FiveGGUTI ::= SEQUENCE

{

mCC [1] MCC,

mNC [2] MNC,

aMFRegionID [3] AMFRegionID,

aMFSetID [4] AMFSetID,

aMFPointer [5] AMFPointer,

fiveGTMSI [6] FiveGTMSI

}

FiveGMMCause ::= INTEGER (0..255)

FiveGSSubscriberID ::= CHOICE

{

sUPI [1] SUPI,

sUCI [2] SUCI,

pEI [3] PEI,

gPSI [4] GPSI

}

FiveGSSubscriberIDs ::= SEQUENCE

{

fiveGSSubscriberID [1] SEQUENCE SIZE(1..MAX) OF FiveGSSubscriberID

}

FiveGSMRequestType ::= ENUMERATED

{

initialRequest(1),

existingPDUSession(2),

initialEmergencyRequest(3),

existingEmergencyPDUSession(4),

modificationRequest(5),

reserved(6),

mAPDURequest(7)

}

FiveGSMCause ::= INTEGER (0..255)

FiveGTMSI ::= INTEGER (0..4294967295)

FiveGSRVCCInfo ::= SEQUENCE

{

uE5GSRVCCCapability [1] BOOLEAN,

sessionTransferNumber [2] UTF8String OPTIONAL,

correlationMSISDN [3] MSISDN OPTIONAL

}

FiveGSUserStateInfo ::= SEQUENCE

{

fiveGSUserState [1] FiveGSUserState,

accessType [2] AccessType

}

FiveGSUserState ::= ENUMERATED

{

deregistered(1),

registeredNotReachableForPaging(2),

registeredReachableForPaging(3),

connectedNotReachableForPaging(4),

connectedReachableForPaging(5),

notProvidedFromAMF(6)

}

ForbiddenAreaInformation ::= SEQUENCE

{

pLMNIdentity [1] PLMNID,

forbiddenTACs [2] ForbiddenTACs

}

ForbiddenTACs ::= SEQUENCE (SIZE(1..MAX)) OF TAC

FTEID ::= SEQUENCE

{

tEID [1] INTEGER (0.. 4294967295),

iPv4Address [2] IPv4Address OPTIONAL,

iPv6Address [3] IPv6Address OPTIONAL

}

FTEIDList ::= SEQUENCE OF FTEID

GPSI ::= CHOICE

{

mSISDN [1] MSISDN,

nAI [2] NAI

}

GUAMI ::= SEQUENCE

{

aMFID [1] AMFID,

pLMNID [2] PLMNID

}

GUMMEI ::= SEQUENCE

{

mMEID [1] MMEID,

mCC [2] MCC,

mNC [3] MNC

}

GUTI ::= SEQUENCE

{

mCC [1] MCC,

mNC [2] MNC,

mMEGroupID [3] MMEGroupID,

mMECode [4] MMECode,

mTMSI [5] TMSI

}

HandoverCause ::= CHOICE

{

radioNetwork [1] CauseRadioNetwork,

transport [2] CauseTransport,

nas [3] CauseNas,

protocol [4] CauseProtocol,

misc [5] CauseMisc

}

HandoverType ::= ENUMERATED

{

intra5GS(1),

fiveGStoEPS(2),

ePSto5GS(3),

fiveGStoUTRA(4)

}

HomeNetworkPublicKeyID ::= OCTET STRING

HSMFURI ::= UTF8String

IMEI ::= NumericString (SIZE(14))

IMEISV ::= NumericString (SIZE(16))

IMPI ::= NAI

IMPU ::= CHOICE

{

sIPURI [1] SIPURI,

tELURI [2] TELURI

}

IMSI ::= NumericString (SIZE(6..15))

Initiator ::= ENUMERATED

{

uE(1),

network(2),

unknown(3)

}

IPAddress ::= CHOICE

{

iPv4Address [1] IPv4Address,

iPv6Address [2] IPv6Address

}

IPv4Address ::= OCTET STRING (SIZE(4))

IPv6Address ::= OCTET STRING (SIZE(16))

IPv6FlowLabel ::= INTEGER(0..1048575)

LocationAreaOfInterestList ::= SEQUENCE (SIZE(1..MAX)) OF AreaOfInterestItem

LocationEventType ::= ENUMERATED

{

direct(1),

changeOfServeCell(2),

uEPrescenceInAreaOfInterest(3),

stopChangeOfServeCell(4),

stopUEPresenceInAreaOfInterest(5),

cancelLocationReportingForTheUE(6)

}

LocationReportArea ::= ENUMERATED

{

cell(1)

}

LocationReportingRequestType ::= SEQUENCE

{

eventType [1] LocationEventType,

reportArea [2] LocationReportArea,

areaOfInterestList [3] LocationAreaOfInterestList

}

MACAddress ::= OCTET STRING (SIZE(6))

MACRestrictionIndicator ::= ENUMERATED

{

noResrictions(1),

mACAddressNotUseableAsEquipmentIdentifier(2),

unknown(3)

}

MCC ::= NumericString (SIZE(3))

MNC ::= NumericString (SIZE(2..3))

MMEID ::= SEQUENCE

{

mMEGI [1] MMEGI,

mMEC [2] MMEC

}

MMEC ::= NumericString

MMEGI ::= NumericString

MobilityRestrictionList ::= SEQUENCE

{

servingPLMN [1] PLMNID,

equivalentPLMNs [2] EquivalentPLMNs OPTIONAL,

rATRestrictions [3] RATRestrictions OPTIONAL,

forbiddenAreaInformation [4] ForbiddenAreaInformation OPTIONAL,

serviceAreaInformation [5] ServiceAreaInformation OPTIONAL

}

MSISDN ::= NumericString (SIZE(1..15))

NAI ::= UTF8String

NextLayerProtocol ::= INTEGER(0..255)

NonLocalID ::= ENUMERATED

{

local(1),

nonLocal(2)

}

NonIMEISVPEI ::= CHOICE

{

mACAddress [1] MACAddress,

eUI64 [2] EUI64

}

NPNAccessInformation ::= CHOICE

{

pNINPNAccessInformation [1] CellCAGList

}

NSSAI ::= SEQUENCE OF SNSSAI

PagingRestrictionIndicator ::= OCTET STRING (SIZE(3..35))

PLMNID ::= SEQUENCE

{

mCC [1] MCC,

mNC [2] MNC

}

PLMNList ::= SEQUENCE (SIZE(1..MAX)) OF PLMNID

PDUSessionID ::= INTEGER (0..255)

PDUSessionResourceInformation ::= SEQUENCE

{

pDUSessionID [1] PDUSessionID

}

PDUSessionType ::= ENUMERATED

{

iPv4(1),

iPv6(2),

iPv4v6(3),

unstructured(4),

ethernet(5)

}

PEI ::= CHOICE

{

iMEI [1] IMEI,

iMEISV [2] IMEISV,

mACAddress [3] MACAddress,

eUI64 [4] EUI64

}

PortNumber ::= INTEGER (0..65535)

PrimaryAuthenticationType ::= ENUMERATED

{

eAPAKAPrime(1),

fiveGAKA(2),

eAPTLS(3),

none(4),

ePSAKA(5),

eAPAKA(6),

iMSAKA(7),

gBAAKA(8),

uMTSAKA(9)

}

ProtectionSchemeID ::= INTEGER (0..15)

RANUENGAPID ::= INTEGER (0..4294967295)

-- See clause 9.3.1.20 of TS 38.413 [23] for details

RANSourceToTargetContainer ::= OCTET STRING

-- See clause 9.3.1.21 of TS 38.413 [23] for details

RANTargetToSourceContainer ::= OCTET STRING

RATRestrictions ::= SEQUENCE (SIZE(1..MAX)) OF RATRestrictionItem

RATRestrictionInformation ::= BIT STRING (SIZE(8, ...))

RATRestrictionItem ::= SEQUENCE

{

pLMNIdentity [1] PLMNID,

rATRestrictionInformation [2] RATRestrictionInformation

}

RATType ::= ENUMERATED

{

nR(1),

eUTRA(2),

wLAN(3),

virtual(4),

nBIOT(5),

wireline(6),

wirelineCable(7),

wirelineBBF(8),

lTEM(9),

nRU(10),

eUTRAU(11),

trustedN3GA(12),

trustedWLAN(13),

uTRA(14),

gERA(15),

nRLEO(16),

nRMEO(17),

nRGEO(18),

nROTHERSAT(19),

nRREDCAP(20)

}

RejectedNSSAI ::= SEQUENCE OF RejectedSNSSAI

RejectedSNSSAI ::= SEQUENCE

{

causeValue [1] RejectedSliceCauseValue,

sNSSAI [2] SNSSAI

}

RejectedSliceCauseValue ::= INTEGER (0..255)

ReRegRequiredIndicator ::= ENUMERATED

{

reRegistrationRequired(1),

reRegistrationNotRequired(2)

}

RoutingIndicator ::= INTEGER (0..9999)

SchemeOutput ::= OCTET STRING

ServiceAreaInformation ::= SEQUENCE (SIZE(1..MAX)) OF ServiceAreaInfo

ServiceAreaInfo ::= SEQUENCE

{

pLMNIdentity [1] PLMNID,

allowedTACs [2] AllowedTACs OPTIONAL,

notAllowedTACs [3] ForbiddenTACs OPTIONAL

}

SIPURI ::= UTF8String

Slice ::= SEQUENCE

{

allowedNSSAI [1] NSSAI OPTIONAL,

configuredNSSAI [2] NSSAI OPTIONAL,

rejectedNSSAI [3] RejectedNSSAI OPTIONAL

}

SMPDUDNRequest ::= OCTET STRING

-- TS 24.501 [13], clause 9.11.3.6.1

SMSOverNASIndicator ::= ENUMERATED

{

sMSOverNASNotAllowed(1),

sMSOverNASAllowed(2)

}

SNSSAI ::= SEQUENCE

{

sliceServiceType [1] INTEGER (0..255),

sliceDifferentiator [2] OCTET STRING (SIZE(3)) OPTIONAL

}

SubscriberIdentifier ::= CHOICE

{

sUCI [1] SUCI,

sUPI [2] SUPI

}

SUCI ::= SEQUENCE

{

mCC [1] MCC,

mNC [2] MNC,

routingIndicator [3] RoutingIndicator,

protectionSchemeID [4] ProtectionSchemeID,

homeNetworkPublicKeyID [5] HomeNetworkPublicKeyID,

schemeOutput [6] SchemeOutput,

routingIndicatorLength [7] INTEGER (1..4) OPTIONAL

-- shall be included if different from the number of meaningful digits given

-- in routingIndicator

}

SUPI ::= CHOICE

{

iMSI [1] IMSI,

nAI [2] NAI

}

SUPIUnauthenticatedIndication ::= BOOLEAN

SwitchOffIndicator ::= ENUMERATED

{

normalDetach(1),

switchOff(2)

}

TargetIdentifier ::= CHOICE

{

sUPI [1] SUPI,

iMSI [2] IMSI,

pEI [3] PEI,

iMEI [4] IMEI,

gPSI [5] GPSI,

mSISDN [6] MSISDN,

nAI [7] NAI,

iPv4Address [8] IPv4Address,

iPv6Address [9] IPv6Address,

ethernetAddress [10] MACAddress

}

TargetIdentifierProvenance ::= ENUMERATED

{

lEAProvided(1),

observed(2),

matchedOn(3),

other(4)

}

TELURI ::= UTF8String

Timestamp ::= GeneralizedTime

UEContextInfo ::= SEQUENCE

{

supportVoPS [1] BOOLEAN OPTIONAL,

supportVoPSNon3GPP [2] BOOLEAN OPTIONAL,

lastActiveTime [3] Timestamp OPTIONAL,

accessType [4] AccessType OPTIONAL,

rATType [5] RATType OPTIONAL

}

UEEndpointAddress ::= CHOICE

{

iPv4Address [1] IPv4Address,

iPv6Address [2] IPv6Address,

ethernetAddress [3] MACAddress

}

UserIdentifiers ::= SEQUENCE

{

fiveGSSubscriberIDs [1] FiveGSSubscriberIDs OPTIONAL,

ePSSubscriberIDs [2] EPSSubscriberIDs OPTIONAL

}

-- ===================

-- Location parameters

-- ===================

Location ::= SEQUENCE

{

locationInfo [1] LocationInfo OPTIONAL,

positioningInfo [2] PositioningInfo OPTIONAL,

locationPresenceReport [3] LocationPresenceReport OPTIONAL,

ePSLocationInfo [4] EPSLocationInfo OPTIONAL

}

CellSiteInformation ::= SEQUENCE

{

geographicalCoordinates [1] GeographicalCoordinates,

azimuth [2] INTEGER (0..359) OPTIONAL,

operatorSpecificInformation [3] UTF8String OPTIONAL

}

-- TS 29.518 [22], clause 6.4.6.2.6

LocationInfo ::= SEQUENCE

{

userLocation [1] UserLocation OPTIONAL,

currentLoc [2] BOOLEAN OPTIONAL,

geoInfo [3] GeographicArea OPTIONAL,

rATType [4] RATType OPTIONAL,

timeZone [5] TimeZone OPTIONAL,

additionalCellIDs [6] SEQUENCE OF CellInformation OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.7

UserLocation ::= SEQUENCE

{

eUTRALocation [1] EUTRALocation OPTIONAL,

nRLocation [2] NRLocation OPTIONAL,

n3GALocation [3] N3GALocation OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.8

EUTRALocation ::= SEQUENCE

{

tAI [1] TAI,

eCGI [2] ECGI,

ageOfLocationInfo [3] INTEGER OPTIONAL,

uELocationTimestamp [4] Timestamp OPTIONAL,

geographicalInformation [5] UTF8String OPTIONAL,

geodeticInformation [6] UTF8String OPTIONAL,

globalNGENbID [7] GlobalRANNodeID OPTIONAL,

cellSiteInformation [8] CellSiteInformation OPTIONAL,

globalENbID [9] GlobalRANNodeID OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.9

NRLocation ::= SEQUENCE

{

tAI [1] TAI,

nCGI [2] NCGI,

ageOfLocationInfo [3] INTEGER OPTIONAL,

uELocationTimestamp [4] Timestamp OPTIONAL,

geographicalInformation [5] UTF8String OPTIONAL,

geodeticInformation [6] UTF8String OPTIONAL,

globalGNbID [7] GlobalRANNodeID OPTIONAL,

cellSiteInformation [8] CellSiteInformation OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.10

N3GALocation ::= SEQUENCE

{

tAI [1] TAI OPTIONAL,

n3IWFID [2] N3IWFIDNGAP OPTIONAL,

uEIPAddr [3] IPAddr OPTIONAL,

portNumber [4] INTEGER OPTIONAL,

tNAPID [5] TNAPID OPTIONAL,

tWAPID [6] TWAPID OPTIONAL,

hFCNodeID [7] HFCNodeID OPTIONAL,

gLI [8] GLI OPTIONAL,

w5GBANLineType [9] W5GBANLineType OPTIONAL,

gCI [10] GCI OPTIONAL,

ageOfLocationInfo [11] INTEGER OPTIONAL,

uELocationTimestamp [12] Timestamp OPTIONAL,

protocol [13] TransportProtocol OPTIONAL

}

-- TS 38.413 [23], clause 9.3.2.4

IPAddr ::= SEQUENCE

{

iPv4Addr [1] IPv4Address OPTIONAL,

iPv6Addr [2] IPv6Address OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.28

GlobalRANNodeID ::= SEQUENCE

{

pLMNID [1] PLMNID,

aNNodeID [2] ANNodeID,

nID [3] NID OPTIONAL

}

ANNodeID ::= CHOICE

{

n3IWFID [1] N3IWFIDSBI,

gNbID [2] GNbID,

nGENbID [3] NGENbID,

eNbID [4] ENbID,

wAGFID [5] WAGFID,

tNGFID [6] TNGFID

}

-- TS 38.413 [23], clause 9.3.1.6

GNbID ::= BIT STRING(SIZE(22..32))

-- TS 29.571 [17], clause 5.4.4.4

TAI ::= SEQUENCE

{

pLMNID [1] PLMNID,

tAC [2] TAC,

nID [3] NID OPTIONAL

}

CGI ::= SEQUENCE

{

lAI [1] LAI,

cellID [2] CellID

}

LAI ::= SEQUENCE

{

pLMNID [1] PLMNID,

lAC [2] LAC

}

LAC ::= OCTET STRING (SIZE(2))

CellID ::= OCTET STRING (SIZE(2))

SAI ::= SEQUENCE

{

pLMNID [1] PLMNID,

lAC [2] LAC,

sAC [3] SAC

}

SAC ::= OCTET STRING (SIZE(2))

-- TS 29.571 [17], clause 5.4.4.5

ECGI ::= SEQUENCE

{

pLMNID [1] PLMNID,

eUTRACellID [2] EUTRACellID,

nID [3] NID OPTIONAL

}

TAIList ::= SEQUENCE OF TAI

-- TS 29.571 [17], clause 5.4.4.6

NCGI ::= SEQUENCE

{

pLMNID [1] PLMNID,

nRCellID [2] NRCellID,

nID [3] NID OPTIONAL

}

RANCGI ::= CHOICE

{

eCGI [1] ECGI,

nCGI [2] NCGI

}

CellInformation ::= SEQUENCE

{

rANCGI [1] RANCGI,

cellSiteinformation [2] CellSiteInformation OPTIONAL,

timeOfLocation [3] Timestamp OPTIONAL

}

-- TS 38.413 [23], clause 9.3.1.57

N3IWFIDNGAP ::= BIT STRING (SIZE(16))

-- TS 29.571 [17], clause 5.4.4.28

N3IWFIDSBI ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.28 and table 5.4.2-1

TNGFID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.28 and table 5.4.2-1

WAGFID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.62

TNAPID ::= SEQUENCE

{

sSID [1] SSID OPTIONAL,

bSSID [2] BSSID OPTIONAL,

civicAddress [3] CivicAddressBytes OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.64

TWAPID ::= SEQUENCE

{

sSID [1] SSID OPTIONAL,

bSSID [2] BSSID OPTIONAL,

civicAddress [3] CivicAddressBytes OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.62 and clause 5.4.4.64

SSID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.62 and clause 5.4.4.64

BSSID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.36 and table 5.4.2-1

HFCNodeID ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.10 and table 5.4.2-1

-- Contains the original binary data i.e. value of the YAML field after base64 encoding is removed

GLI ::= OCTET STRING (SIZE(0..150))

-- TS 29.571 [17], clause 5.4.4.10 and table 5.4.2-1

GCI ::= UTF8String

-- TS 29.571 [17], clause 5.4.4.10 and table 5.4.3.38

TransportProtocol ::= ENUMERATED

{

uDP(1),

tCP(2)

}

-- TS 29.571 [17], clause 5.4.4.10 and clause 5.4.3.33

W5GBANLineType ::= ENUMERATED

{

dSL(1),

pON(2)

}

-- TS 29.571 [17], table 5.4.2-1

TAC ::= OCTET STRING (SIZE(2..3))

-- TS 38.413 [23], clause 9.3.1.9

EUTRACellID ::= BIT STRING (SIZE(28))

-- TS 38.413 [23], clause 9.3.1.7

NRCellID ::= BIT STRING (SIZE(36))

-- TS 38.413 [23], clause 9.3.1.8

NGENbID ::= CHOICE

{

macroNGENbID [1] BIT STRING (SIZE(20)),

shortMacroNGENbID [2] BIT STRING (SIZE(18)),

longMacroNGENbID [3] BIT STRING (SIZE(21))

}

-- TS 23.003 [19], clause 12.7.1 encoded as per TS 29.571 [17], clause 5.4.2

NID ::= UTF8String (SIZE(11))

-- TS 36.413 [38], clause 9.2.1.37

ENbID ::= CHOICE

{

macroENbID [1] BIT STRING (SIZE(20)),

homeENbID [2] BIT STRING (SIZE(28)),

shortMacroENbID [3] BIT STRING (SIZE(18)),

longMacroENbID [4] BIT STRING (SIZE(21))

}

-- TS 29.518 [22], clause 6.4.6.2.3

PositioningInfo ::= SEQUENCE

{

positionInfo [1] LocationData OPTIONAL,

rawMLPResponse [2] RawMLPResponse OPTIONAL

}

RawMLPResponse ::= CHOICE

{

-- The following parameter contains a copy of unparsed XML code of the

-- MLP response message, i.e. the entire XML document containing

-- a <slia> (described in OMA-TS-MLP-V3\_5-20181211-C [20], clause 5.2.3.2.2) or

-- a <slirep> (described in OMA-TS-MLP-V3\_5-20181211-C [20], clause 5.2.3.2.3) MLP message.

mLPPositionData [1] UTF8String,

-- OMA MLP result id, defined in OMA-TS-MLP-V3\_5-20181211-C [20], Clause 5.4

mLPErrorCode [2] INTEGER (1..699)

}

-- TS 29.572 [24], clause 6.1.6.2.3

LocationData ::= SEQUENCE

{

locationEstimate [1] GeographicArea,

accuracyFulfilmentIndicator [2] AccuracyFulfilmentIndicator OPTIONAL,

ageOfLocationEstimate [3] AgeOfLocationEstimate OPTIONAL,

velocityEstimate [4] VelocityEstimate OPTIONAL,

civicAddress [5] CivicAddress OPTIONAL,

positioningDataList [6] SET OF PositioningMethodAndUsage OPTIONAL,

gNSSPositioningDataList [7] SET OF GNSSPositioningMethodAndUsage OPTIONAL,

eCGI [8] ECGI OPTIONAL,

nCGI [9] NCGI OPTIONAL,

altitude [10] Altitude OPTIONAL,

barometricPressure [11] BarometricPressure OPTIONAL

}

-- TS 29.172 [53], table 6.2.2-2

EPSLocationInfo ::= SEQUENCE

{

locationData [1] LocationData,

cGI [2] CGI OPTIONAL,

sAI [3] SAI OPTIONAL,

eSMLCCellInfo [4] ESMLCCellInfo OPTIONAL

}

-- TS 29.172 [53], clause 7.4.57

ESMLCCellInfo ::= SEQUENCE

{

eCGI [1] ECGI,

cellPortionID [2] CellPortionID

}

-- TS 29.171 [54], clause 7.4.31

CellPortionID ::= INTEGER (0..4095)

-- TS 29.518 [22], clause 6.2.6.2.5

LocationPresenceReport ::= SEQUENCE

{

type [1] AMFEventType,

timestamp [2] Timestamp,

areaList [3] SET OF AMFEventArea OPTIONAL,

timeZone [4] TimeZone OPTIONAL,

accessTypes [5] SET OF AccessType OPTIONAL,

rMInfoList [6] SET OF RMInfo OPTIONAL,

cMInfoList [7] SET OF CMInfo OPTIONAL,

reachability [8] UEReachability OPTIONAL,

location [9] UserLocation OPTIONAL,

additionalCellIDs [10] SEQUENCE OF CellInformation OPTIONAL

}

-- TS 29.518 [22], clause 6.2.6.3.3

AMFEventType ::= ENUMERATED

{

locationReport(1),

presenceInAOIReport(2)

}

-- TS 29.518 [22], clause 6.2.6.2.16

AMFEventArea ::= SEQUENCE

{

presenceInfo [1] PresenceInfo OPTIONAL,

lADNInfo [2] LADNInfo OPTIONAL

}

-- TS 29.571 [17], clause 5.4.4.27

PresenceInfo ::= SEQUENCE

{

presenceState [1] PresenceState OPTIONAL,

trackingAreaList [2] SET OF TAI OPTIONAL,

eCGIList [3] SET OF ECGI OPTIONAL,

nCGIList [4] SET OF NCGI OPTIONAL,

globalRANNodeIDList [5] SET OF GlobalRANNodeID OPTIONAL,

globalENbIDList [6] SET OF GlobalRANNodeID OPTIONAL

}

-- TS 29.518 [22], clause 6.2.6.2.17

LADNInfo ::= SEQUENCE

{

lADN [1] UTF8String,

presence [2] PresenceState OPTIONAL

}

-- TS 29.571 [17], clause 5.4.3.20

PresenceState ::= ENUMERATED

{

inArea(1),

outOfArea(2),

unknown(3),

inactive(4)

}

-- TS 29.518 [22], clause 6.2.6.2.8

RMInfo ::= SEQUENCE

{

rMState [1] RMState,

accessType [2] AccessType

}

-- TS 29.518 [22], clause 6.2.6.2.9

CMInfo ::= SEQUENCE

{

cMState [1] CMState,

accessType [2] AccessType

}

-- TS 29.518 [22], clause 6.2.6.3.7

UEReachability ::= ENUMERATED

{

unreachable(1),

reachable(2),

regulatoryOnly(3)

}

-- TS 29.518 [22], clause 6.2.6.3.9

RMState ::= ENUMERATED

{

registered(1),

deregistered(2)

}

-- TS 29.518 [22], clause 6.2.6.3.10

CMState ::= ENUMERATED

{

idle(1),

connected(2)

}

-- TS 29.572 [24], clause 6.1.6.2.5

GeographicArea ::= CHOICE

{

point [1] Point,

pointUncertaintyCircle [2] PointUncertaintyCircle,

pointUncertaintyEllipse [3] PointUncertaintyEllipse,

polygon [4] Polygon,

pointAltitude [5] PointAltitude,

pointAltitudeUncertainty [6] PointAltitudeUncertainty,

ellipsoidArc [7] EllipsoidArc

}

-- TS 29.572 [24], clause 6.1.6.3.12

AccuracyFulfilmentIndicator ::= ENUMERATED

{

requestedAccuracyFulfilled(1),

requestedAccuracyNotFulfilled(2)

}

-- TS 29.572 [24], clause 6.1.6.2.17

VelocityEstimate ::= CHOICE

{

horVelocity [1] HorizontalVelocity,

horWithVertVelocity [2] HorizontalWithVerticalVelocity,

horVelocityWithUncertainty [3] HorizontalVelocityWithUncertainty,

horWithVertVelocityAndUncertainty [4] HorizontalWithVerticalVelocityAndUncertainty

}

-- TS 29.572 [24], clause 6.1.6.2.14

CivicAddress ::= SEQUENCE

{

country [1] UTF8String,

a1 [2] UTF8String OPTIONAL,

a2 [3] UTF8String OPTIONAL,

a3 [4] UTF8String OPTIONAL,

a4 [5] UTF8String OPTIONAL,

a5 [6] UTF8String OPTIONAL,

a6 [7] UTF8String OPTIONAL,

prd [8] UTF8String OPTIONAL,

pod [9] UTF8String OPTIONAL,

sts [10] UTF8String OPTIONAL,

hno [11] UTF8String OPTIONAL,

hns [12] UTF8String OPTIONAL,

lmk [13] UTF8String OPTIONAL,

loc [14] UTF8String OPTIONAL,

nam [15] UTF8String OPTIONAL,

pc [16] UTF8String OPTIONAL,

bld [17] UTF8String OPTIONAL,

unit [18] UTF8String OPTIONAL,

flr [19] UTF8String OPTIONAL,

room [20] UTF8String OPTIONAL,

plc [21] UTF8String OPTIONAL,

pcn [22] UTF8String OPTIONAL,

pobox [23] UTF8String OPTIONAL,

addcode [24] UTF8String OPTIONAL,

seat [25] UTF8String OPTIONAL,

rd [26] UTF8String OPTIONAL,

rdsec [27] UTF8String OPTIONAL,

rdbr [28] UTF8String OPTIONAL,

rdsubbr [29] UTF8String OPTIONAL,

prm [30] UTF8String OPTIONAL,

pom [31] UTF8String OPTIONAL

}

-- TS 29.571 [17], clauses 5.4.4.62 and 5.4.4.64

-- Contains the original binary data i.e. value of the YAML field after base64 encoding is removed

CivicAddressBytes ::= OCTET STRING

-- TS 29.572 [24], clause 6.1.6.2.15

PositioningMethodAndUsage ::= SEQUENCE

{

method [1] PositioningMethod,

mode [2] PositioningMode,

usage [3] Usage,

methodCode [4] MethodCode OPTIONAL

}

-- TS 29.572 [24], clause 6.1.6.2.16

GNSSPositioningMethodAndUsage ::= SEQUENCE

{

mode [1] PositioningMode,

gNSS [2] GNSSID,

usage [3] Usage

}

-- TS 29.572 [24], clause 6.1.6.2.6

Point ::= SEQUENCE

{

geographicalCoordinates [1] GeographicalCoordinates

}

-- TS 29.572 [24], clause 6.1.6.2.7

PointUncertaintyCircle ::= SEQUENCE

{

geographicalCoordinates [1] GeographicalCoordinates,

uncertainty [2] Uncertainty

}

-- TS 29.572 [24], clause 6.1.6.2.8

PointUncertaintyEllipse ::= SEQUENCE

{

geographicalCoordinates [1] GeographicalCoordinates,

uncertainty [2] UncertaintyEllipse,

confidence [3] Confidence

}

-- TS 29.572 [24], clause 6.1.6.2.9

Polygon ::= SEQUENCE

{

pointList [1] SET SIZE (3..15) OF GeographicalCoordinates

}

-- TS 29.572 [24], clause 6.1.6.2.10

PointAltitude ::= SEQUENCE

{

point [1] GeographicalCoordinates,

altitude [2] Altitude

}

-- TS 29.572 [24], clause 6.1.6.2.11

PointAltitudeUncertainty ::= SEQUENCE

{

point [1] GeographicalCoordinates,

altitude [2] Altitude,

uncertaintyEllipse [3] UncertaintyEllipse,

uncertaintyAltitude [4] Uncertainty,

confidence [5] Confidence

}

-- TS 29.572 [24], clause 6.1.6.2.12

EllipsoidArc ::= SEQUENCE

{

point [1] GeographicalCoordinates,

innerRadius [2] InnerRadius,

uncertaintyRadius [3] Uncertainty,

offsetAngle [4] Angle,

includedAngle [5] Angle,

confidence [6] Confidence

}

-- TS 29.572 [24], clause 6.1.6.2.4

GeographicalCoordinates ::= SEQUENCE

{

latitude [1] UTF8String,

longitude [2] UTF8String,

mapDatumInformation [3] OGCURN OPTIONAL

}

-- TS 29.572 [24], clause 6.1.6.2.22

UncertaintyEllipse ::= SEQUENCE

{

semiMajor [1] Uncertainty,

semiMinor [2] Uncertainty,

orientationMajor [3] Orientation

}

-- TS 29.572 [24], clause 6.1.6.2.18

HorizontalVelocity ::= SEQUENCE

{

hSpeed [1] HorizontalSpeed,

bearing [2] Angle

}

-- TS 29.572 [24], clause 6.1.6.2.19

HorizontalWithVerticalVelocity ::= SEQUENCE

{

hSpeed [1] HorizontalSpeed,

bearing [2] Angle,

vSpeed [3] VerticalSpeed,

vDirection [4] VerticalDirection

}

-- TS 29.572 [24], clause 6.1.6.2.20

HorizontalVelocityWithUncertainty ::= SEQUENCE

{

hSpeed [1] HorizontalSpeed,

bearing [2] Angle,

uncertainty [3] SpeedUncertainty

}

-- TS 29.572 [24], clause 6.1.6.2.21

HorizontalWithVerticalVelocityAndUncertainty ::= SEQUENCE

{

hSpeed [1] HorizontalSpeed,

bearing [2] Angle,

vSpeed [3] VerticalSpeed,

vDirection [4] VerticalDirection,

hUncertainty [5] SpeedUncertainty,

vUncertainty [6] SpeedUncertainty

}

-- The following types are described in TS 29.572 [24], table 6.1.6.3.2-1

Altitude ::= UTF8String

Angle ::= INTEGER (0..360)

Uncertainty ::= INTEGER (0..127)

Orientation ::= INTEGER (0..180)

Confidence ::= INTEGER (0..100)

InnerRadius ::= INTEGER (0..327675)

AgeOfLocationEstimate ::= INTEGER (0..32767)

HorizontalSpeed ::= UTF8String

VerticalSpeed ::= UTF8String

SpeedUncertainty ::= UTF8String

BarometricPressure ::= INTEGER (30000..115000)

-- TS 29.572 [24], clause 6.1.6.3.13

VerticalDirection ::= ENUMERATED

{

upward(1),

downward(2)

}

-- TS 29.572 [24], clause 6.1.6.3.6

PositioningMethod ::= ENUMERATED

{

cellID(1),

eCID(2),

oTDOA(3),

barometricPressure(4),

wLAN(5),

bluetooth(6),

mBS(7),

motionSensor(8),

dLTDOA(9),

dLAOD(10),

multiRTT(11),

nRECID(12),

uLTDOA(13),

uLAOA(14),

networkSpecific(15)

}

-- TS 29.572 [24], clause 6.1.6.3.7

PositioningMode ::= ENUMERATED

{

uEBased(1),

uEAssisted(2),

conventional(3)

}

-- TS 29.572 [24], clause 6.1.6.3.8

GNSSID ::= ENUMERATED

{

gPS(1),

galileo(2),

sBAS(3),

modernizedGPS(4),

qZSS(5),

gLONASS(6),

bDS(7),

nAVIC(8)

}

-- TS 29.572 [24], clause 6.1.6.3.9

Usage ::= ENUMERATED

{

unsuccess(1),

successResultsNotUsed(2),

successResultsUsedToVerifyLocation(3),

successResultsUsedToGenerateLocation(4),

successMethodNotDetermined(5)

}

-- TS 29.571 [17], table 5.2.2-1

TimeZone ::= UTF8String

-- Open Geospatial Consortium URN [35]

OGCURN ::= UTF8String

-- TS 29.572 [24], clause 6.1.6.2.15

MethodCode ::= INTEGER (16..31)

END

END OF SECOND CHANGE

END OF ALL CHANGES