**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  | Addition of modifiedSIPMessage payload to IMSPayload type |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | There are times when a SIP message may contain information that is not authorized. It is beneficial to reuse the existing SIP structure defined in other documents for reporting the SIP Message, however, the unauthorized information needs to be removed prior to reporting the message over LI\_HI2. This CR provides specifications for what information needs to be removed. |
|  |  |
| ***Summary of change:*** | A new choice is added to the IMSPayload structure to allow for the reporting of modified SIP Payloads. Additionally, details for which information may need to be removed for specific authorizations is added. |
|  |  |
| ***Consequences if not approved:*** | There will be no way to report the authorized portion of IMS records if any of the information in the message is unauthoized.  |
|  |  |
| ***Clauses affected:*** |  |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ... |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** |  |

## \*\*\*\* START OF FIRST CHANGE (MAIN DOCUMENT) \*\*\*

# 2 References

The following documents contain provisions which, through reference in this text, constitute provisions of the present document.

- References are either specific (identified by date of publication, edition number, version number, etc.) or non‑specific.

- For a specific reference, subsequent revisions do not apply.

- For a non-specific reference, the latest version applies. In the case of a reference to a 3GPP document (including a GSM document), a non-specific reference implicitly refers to the latest version of that document *in the same Release as the present document*.

[1] 3GPP TR 21.905: "Vocabulary for 3GPP Specifications".

[2] 3GPP TS 23.501: "System Architecture for the 5G System".

[3] 3GPP TS 33.126: "Lawful Interception Requirements".

[4] 3GPP TS 23.502: "Procedures for the 5G System; Stage 2".

[5] 3GPP TS 33.127: "Lawful Interception (LI) Architecture and Functions".

[6] ETSI TS 103 120: "Lawful Interception (LI); Interface for warrant information".

[7] ETSI TS 103 221-1: "Lawful Interception (LI); Internal Network Interfaces; Part 1: X1".

[8] ETSI TS 103 221-2: "Lawful Interception (LI); Internal Network Interfaces; Part 2: X2/X3".

 [9] ETSI TS 102 232-1: "Lawful Interception (LI); Handover Interface and Service-Specific Details (SSD) for IP delivery; Part 1: Handover specification for IP delivery".

[10] ETSI TS 102 232-7: "Lawful Interception (LI); Handover Interface and Service-Specific Details (SSD) for IP delivery; Part 7: Service-specific details for Mobile Services".

[11] 3GPP TS 33.501: "Security Architecture and Procedures for the 5G System".

[12] 3GPP TS 33.108: "3G security; Handover interface for Lawful Interception (LI)".

[13] 3GPP TS 24.501: "Non-Access-Stratum (NAS) protocol for 5G System (5GS)".

[14] 3GPP TS 24.007: "Mobile radio interface signalling layer 3; General Aspects".

[15] 3GPP TS 29.244: "Interface between the Control Plane and the User Plane nodes".

[16] 3GPP TS 29.502: "5G System; Session Management Services; Stage 3".

[17] 3GPP TS 29.571: "5G System; Common Data Types for Service Based Interfaces; Stage 3".

[18] 3GPP TS 23.040: "Technical realization of the Short Message Service (SMS)".

[19] 3GPP TS 23.003: "Numbering, addressing and identification ".

[20] OMA-TS-MLP-V3\_5-20181211-C: "Open Mobile Alliance; Mobile Location Protocol, Candidate Version 3.5", <https://www.openmobilealliance.org/release/MLS/V1_4-20181211-C/OMA-TS-MLP-V3_5-20181211-C.pdf>.

[21] 3GPP TS 29.540: "5G System; SMS Services; Stage 3".

[22] 3GPP TS 29.518: "5G System; Access and Mobility Management Services; Stage 3".

[23] 3GPP TS 38.413: "NG Application Protocol (NGAP)".

[24] 3GPP TS 29.572: "Location Management Services; Stage 3".

[25] 3GPP TS 29.503: "5G System; Unified Data Management Services".

[26] IETF RFC 815: "IP datagram reassembly algorithms".

[27] IETF RFC 2460: "Internet Protocol, Version 6 (IPv6) Specification".

[28] IETF RFC 793: "Transmission Control Protocol".

[29] IETF RFC 768: "User Datagram Protocol".

[30] IETF RFC 4340: "Datagram Congestion Control Protocol (DCCP)".

[31] IETF RFC 4960: "Stream Control Transmission Protocol".

[32] IANA (www.iana.org): Assigned Internet Protocol Numbers, "Protocol Numbers".

[33] IETF RFC 6437: "IPv6 Flow Label Specification".

[34] IETF RFC 791: "Internet Protocol".

[35] Open Geospatial Consortium OGC 05-010: "URNs of definitions in ogc namespace".

[36] 3GPP TS 33.107: "3G security; Lawful interception architecture and functions".

[37] 3GPP TS 37.340: "Evolved Universal Radio Access (E-UTRA) and NR-Multi-connectivity; Stage 2".

[38] 3GPP TS 36.413: "S1 Application Protocol (S1AP)".

[39] OMA-TS-MMS\_ENC-V1\_3-20110913-A: "Multimedia Messaging Service Encapsulation Protocol".

[40] 3GPP TS 23.140: "Multimedia Messaging Protocol. Functional Description. Stage 2".

[41] 3GPP TS 38.415: "NG-RAN; PDU Session User Plane Protocol".

[42] 3GPP TS 23.273: "5G System (5GS) Location Services (LCS); Stage 2".

[43] IETF RFC 4566: "SDP: Session Description Protocol".

[44] 3GPP TS 24.193: "Stage 3: Access Traffic Steering, Switching and Splitting (ATSSS)".

[45] 3GPP TS 29.509: "5G System; Authentication Server Services; Stage 3".

[46] 3GPP TS 24.011: "Point-to-Point (PP) Short Message Service (SMS) support on mobile radio interface".

[47] 3GPP TS 29.002: "Mobile Application Part (MAP) specification".

[48] 3GPP TS 29.504: "5G System; Unified Data Repository Services; Stage 3".

[49] 3GPP TS 29.505: "5G System; Usage of the Unified Data Repository services for Subscription Data; Stage 3".

[50] 3GPP TS 23.401 "General Packet Radio Service (GPRS) enhancements for Evolved Universal Terrestrial Radio Access Network (E-UTRAN) access".

[51] 3GPP TS 24.301 "Non-Access-Stratum (NAS) protocol for Evolved Packet System (EPS), Stage 3".

[52] 3GPP TS 23.271 "Functional stage 2 description of Location Services (LCS)".

[53] 3GPP TS 29.172 "Evolved Packet Core (EPC) LCS Protocol (ELP) between the Gateway Mobile Location Centre (GMLC) and the Mobile Management Entity (MME); SLg interface".

[54] 3GPP TS 29.171 "LCS Application Protocol (LCS-AP) between the Mobile Management Entity (MME) and Evolved Serving Mobile Location Centre (E-SMLC); SLs interface".

[55] 3GPP TS 24.379: "Mission Critical Push to Talk (MCPTT) call control; protocol specification".

[56] OMA-TS-PoC-System\_Description-V2\_1-20110802-A: "OMA PoC System Description".

[57] 3GPP TS 29.541: "5G System; Network Exposure (NE) function services for Non-IP Data Delivery (NIDD); Stage 3".

[58] 3GPP TS 29.522: "5G System; Network Exposure Function Northbound APIs; Stage 3".

[59] 3GPP TS 29.338: "Diameter based protocols to support Short Message Service (SMS) capable Mobile Management Entities (MMEs); Stage 3".

[60] 3GPP TS 29.337: "Diameter-based T4 interface for communications with packet data networks and applications".

[61] 3GPP TS 24.250: "Protocol for Reliable Data Service; Stage 3".

[62] 3GPP TS 29.128: "Mobility Management Entity (MME) and Serving GPRS Support Node (SGSN) interfaces for interworking with packet data networks and applications".

[63] 3GPP TS 29.122: "T8 reference point for Northbound APIs".

[64] 3GPP TS 29.598: "5G System; Unstructured Data Storage Services; Stage3".

[65] 3GPP TS 33.535: "Authentication and Key Management for Applications (AKMA) based on 3GPP credentials in the 5G System (5GS)".

[66] IETF RFC 5246: "The Transport Layer Security (TLS) Protocol Version 1.2".

[67] GSMA IR.88: "IR.88 LTE and EPC Roaming Guidelines".

[68] GSMA NG.114 "IMS Profile for Voice, Video and Messaging over 5GS".

[69] IETF RFC 8225: "PASSporT: Personal Assertion Token".

[70] IETF RFC 8224: "Authenticated Identity Management in the Session Initiation Protocol (SIP)".

[71] IETF RFC 8588: "Personal Assertion Token (PaSSporT) Extension for Signature-based Handling of Asserted information using toKENs (SHAKEN)".

[72] 3GPP TS 24.196: "Enhanced Calling Name (eCNAM)".

[73] IETF draft-ietf-stir-passport-rcd-17: "PASSporT Extension for Rich Call Data".

NOTE: The above document cannot be formally referenced until it is published as an RFC.

[74] 3GPP TS 24.229: "IP multimedia call control protocol based on Session Initiation Protocol (SIP)and Session Description Protocol (SDP); Stage 3".

[75] IANA Session Initiation Protocol (SIP) Parameters: <https://www.iana.org/assignments/sip-parameters/sip-parameters.xhtml>

[76] IETF RFC 8946: "Personal Assertion Token (PASSporT) Extension for Diverted Calls".

[77] 3GPP TS 23.204: "3rd Generation Partnership Project; Technical Specification Group Services and System Aspects; Support of Short Message Service (SMS) over generic 3GPP Internet Protocol (IP) access; Stage 2".

[78] GSMA RCC.07: "Rich Communication Suite – Advanced Communications Services and Client Specification".

[79] IETF RFC 4975: "The Message Session Relay Protocol (MSRP)".

[80] IETF RFC 3862: "Common Presence and Instant Messaging (CPIM): Message Format".

[81] IETF RFC 5438: "Instant Message Disposition Notification (IMDN)".

[82] OMA-TS-CPM\_System\_Description-V2\_2-20170926-C: "OMA Converged IP Messaging System Description".

[83] IETF RFC 4566: "SDP: Session Description Protocol".

[84] 3GPP TS 36.455: "Evolved Universal Terrestrial Radio Access (E-UTRA); LTE Positioning Protocol A (LPPa) ".

[85] 3GPP TS 37.355: "LTE Positioning Protocol (LPP)".

[86] 3GPP TS 38.455: "NG-RAN; NR Positioning Protocol A (NRPPa)".

[87] 3GPP TS 29.274: "3GPP Evolved Packet System (EPS); Evolved General Packet Radio Service (GPRS) Tunnelling Protocol for Control plane (GTPv2-C); Stage 3".

[88] 3GPP TS 29.513: "5G System; Policy and Charging Control signalling flows and QoS parameter mapping".

[89] 3GPP TS 29.512: "5G System; Session Management Policy Control Service; Stage 3".

[90] 3GPP TS 29.508: "5G System; Session Management Event Exposure Service; Stage 3".

[91] 3GPP TS 29.514: "5G System; Policy Authorization Service; Stage 3".

[92] 3GPP TS 29.214: "Policy and Charging Control over Rx reference point".

[93] 3GPP TS 24.558: "Enabling Edge Applications; Protocol specification".

[94] 3GPP TS 29.558: "Enabling Edge Applications; Application Programming Interface (API) specification".

[95] 3GPP TS 24.008: "Mobile radio interface Layer 3 specification; Core network protocols; Stage 3".

[96] 3GPP TS 29.551: "5G System; Packet Flow Description Management Service; Stage 3".

[97] ETSI TS 103 280: "Lawful Interception (LI); Dictionary for common parameters".

[98] 3GPP TS 26.512: "5G Media Streaming (5GMS); Protocols".

[99] 3GPP TS 26.247: "Transparent end-to-end Packet-switched Streaming Service (PSS); Progressive Download and Dynamic Adaptive Streaming over HTTP (3GP-DASH)".

[100] 3GPP TS 29.563: "5G System; Home Subscriber Server (HSS) services for interworking with Unified Data Management (UDM); Stage 3".

[101] 3GPP TS 29.562: "5G System; Home Subscriber Server (HSS) Services; Stage 3".

[102] 3GPP TS 24.341 "Support of SMS over IP networks, Stage 3".

[103] 3GPP TS 38.473 "NG-RAN;F1 application protocol (F1AP)".

[104] 3GPP TS 23.032: "Universal Geographical Area Description (GAD)".

[105] ITU-T Recommendation Q.763 (1999): "Specifications of Signalling System No.7; Formats and codes".

[106] 3GPP TS 29.272: "Mobility Management Entity (MME) and Serving GPRS Support Node (SGSN) related interfaces based on Diameter protocol".

[107] IETF RFC 6442: "Location Conveyance for the Session Initiation Protocol".

[108] 3GPP TS 29.272 " Mobility Management Entity (MME) and Serving GPRS Support Node (SGSN) related interfaces based on Diameter protocol".

[Re1] IETF RFC 2046: "Multipurpose Internet Mail Extensions (MIME) Part Two: Media Types".

## \*\*\*\* START OF NEXT CHANGE (MAIN DOCUMENT) \*\*\*

##### 7.12.4.2.1 IMS Message

For an intercepted IMS based communication (see clause 7.12.2.8), the IRI-POI present in the IMS Signaling Function shall generate the xIRI IMSMessage from the SIP message used to handle that IMS based communication. All SIP messages use the same xIRI record as shown in table 7.12.4.2-1.

Table 7.12.4.2-1: Payload for IMSMessage record

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Field name | Type | Cardinality | Description | M/C/O |
| payload | IMSPayload | 1 | One of the following payload types (other payload types may be added in future versions of the specification):- encapsulatedSIPMessage shall be chosen when the SIP message does not contain any unauthorized information.  | M |
| sessionDirection | SessionDirection | 1 | Indicates the direction of the SIP session: fromTarget, toTarget, combined (if target calls him/herself) or indeterminate if the direction cannot be determined reliable (see NOTE). | M |
| voIPRoamingIndication | VoIPRoamingIndication | 0..1 | Indicates whether the roaming mode is inbound LBO, S8HR or N9HR when the target is in roaming situation. | C |
| location | Location | 0..1 | Location with timestamp, if available.Shall include all location information for the target UE available at the NF where the POI is located encoded as *location>IMSLocation.* | C |
| accessNetworkInformation | SEQUENCE OF SIPAccessNetworkInformation | 0..MAX | Provides non-location related access network information. Shall be present if available at the NF where the POI is located. One instance of SIPAccessNetworkInformation shall be used for each P-Access-Network-Information header. | C |
| cellularNetworkInformation | SEQUENCE OF SIPCellularNetworkInformation | 0..MAX | Provides non-location related cellular network information. Shall be present if available at the NF where the POI is located. One instance of SIPCellularNetworkInformation shall be used for each Cellular-Network-Info header. | C |
| NOTE: When an incoming call to a target is redirected to another user, the sessionDirection field shall be set to toTarget. When an incoming call from a target non-local ID to an IMS user is redirected to, the sessionDirection field shall be set to fromTarget. |

Table 7.12.4.2-2: Void

The IRI-POI present in the IMS signaling function generating an xIRI containing an IMSMessage record shall set:

- The Payload Direction field in the PDU header to the direction of the signaling message carried in the IRI payload (see ETSI TS 103 221-2 [8] clause 5.2.6). If the signalling message was sent from the target, the Direction Value "3" (sent from the target) shall be used, if the signalling message was sent to the target, the Direction Value "2" (sent to the target) shall be used; if the direction could not be determined reliably, the Direction Value "1" (not known to the POI) shall be used. If the SIP message is sent from and to the target, the Direction Value "4" (more than one direction) shall be used. For the SIP messages generated by the network, the Direction Value "5" (not applicable) shall be used.

- The conditional source IPv4 address or source IPv6 address field in the PDU header to the source IP address of the intercepted SIP message (see ETSI TS 103 221-2 [8] clause 5.3). It shall contain the source address of the packet from the 32-bit "Source Address" field in IPv4, as defined in IETF RFC 791 [34], or from the 128-bit "Source Address" field in IPv6, as defined in IETF RFC 2460 [27].

- The conditional destination IPv4 address or destination IPv6 address field in the PDU header to the destination IP address of the intercepted SIP message (see ETSI TS 103 221-2 [8] clause 5.3). It shall contain the destination address of the packet from the 32-bit "Source Address" field in IPv4, as defined in IETF RFC 791 [34], or from the 128-bit "Source Address" field in IPv6, as defined in IETF RFC 2460 [27].

## \*\*\*\* START OF NEXT CHANGE (MAIN DOCUMENT) \*\*\*

##### 7.12.4.3.1 Type: IMSPayload

Table 7.12.4.3.1-1 contains the details for the IMSPayload type.

Table 7.12.4.3.1-1: Definition of Choices for IMSPayload

|  |  |  |
| --- | --- | --- |
| CHOICE | Type | Description |
| encapsulatedSIPMessage | SIPMessage | Used to report entire SIPMessage when the SIP message contains only authorized information. |

## \*\*\*\* START OF NEXT CHANGE (MAIN DOCUMENT) \*\*\*

### 7.12.X Removal of unauthorised information from IMS record payloads

#### 7.12.X.1 General

If the Content-Type of the SIP message is "multipart" as defined in RFC 2046 [Re1] clause 2.4, each part of the SIP message shall be modified as required.

#### 7.12.X.2 Removal of location information

##### 7.12.X.2.1 General

Depending on the SIP message being reported and the implementation, location information may be present in the SIP Headers, the body of the SIP message, or both. When location is not authorized, all location information shall be removed from the encapsulated SIP message prior to its delivery over LI\_HI2. As such, when location is not authorized, the MDF2 and, optionally, the IRI-POIs in the IMS shall be provisioned with the payload modifications detailed in the subclauses below.

Additionally, if the location present in the SIP message is the location of the non-target party, the location shall be removed.

If an implementation has location information in other portions of the payload, the appropriate modifications shall be made to the encapsulated payload in addition to those specified below prior to the delivery of the message over LI\_HI2.

##### 7.12.X.2.2 P-Access-Network-Info location removal

Each character of each access-info parameter field of the P-Access-Network-Info header shall be over-written with zeros (see TS 24.229 [74] clause 7.2A.4). If multiple P-Access-Network-Info headers are present in the message, each shall be modified.

If the P-Access-Network-Info header contains a UE-local-IP-address parameter field:

- If the parameter field contains an IPv4address, each digit of the address shall be set to zero.

- If the parameter field contains an IPv6address, each hex digit of the address shall be set to zero.

##### 7.12.X.2.3 Cellular-Network-Info location removal

Each character of the access-info portion of the Cellular-Network-Info header shall be over-written with zeros. If multiple Cellular-Network-Info headers are present in the message, each shall be modified.

##### 7.12.X.2.4 Geolocation header location removal

If there is a Geolocation header present in the message and the location object is included in the message, the portion of the body of the SIP message that contains the location object shall be modified as described in clause 7.12.X.2.5.

##### 7.12.X.2.5 Removal of location information from presence information

If the Content-Type of any body part of the SIP message is "application/pidf+xml", if the presence information contains a geopriv element, the character data of each element within each location-info element shall be overwritten with the zero character such that the length of the element does not change.

#### 7.12.X.3 Removal of communications content

##### 7.12.X.3.1 General

In some cases portions of a SIP message body may contain communications content. Unless otherwise specified, all communications content shall be removed from the encapsulated SIP message prior to its delivery over LI\_HI2. As such, the MDF2 and, optionally, the IRI-POIs in the IMS shall be provisioned with the payload modifications detailed in the subclauses below.

If an implementation has location information in other portions of the payload, the appropriate modifications shall be made to the encapsulated payload in addition to those specified below prior to the delivery of the message over LI\_HI2.

##### 7.12.X.3.2 Removal of SMS content

If the Content-Type of any body part of the SIP message is "application/vnd.3gpp.sms", the TP-User-Data (TS 23.040 [18] clause 9.2.3.4) of the SMS TPDU shall be modified to remove any content such that the length of the TPDU remains unchanged.

##### 7.12.X.3.3 Removal of text content

If the Content-Type of the SIP message is "text" or any of the subtypes of "text", the contents of the body shall be overwritten with spaces such that the length of the body remains unchanged.

##### 7.12.X.3.4 Removal of content from the Subject header field.

If the delivery of the Subject header of a SIP message is unauthorized, each character of the field-value of the Subject header shall be replaced with a space.

## \*\*\*\* END OF MAIN DOCUMENTS CHANGES \*\*\*

## \*\*\*\* END OF ALL CHANGES \*\*\*