**3GPP TSG- Meeting #**

**, , -**

|  |
| --- |
| *CR-Form-v12.2* |
| **CHANGE REQUEST** |
|  |
|  |  | **CR** |  | **rev** |  | **Current version:** |  |  |
|  |
| *For* [***HE******LP***](http://www.3gpp.org/3G_Specs/CRs.htm#_blank)*on using this form: comprehensive instructions can be found at* [*http://www.3gpp.org/Change-Requests*](http://www.3gpp.org/Change-Requests)*.* |
|  |

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| ***Proposed change affects:*** | UICC apps |  | ME |  | Radio Access Network |  | Core Network | **X** |

|  |
| --- |
|  |
| ***Title:***  |  |
|  |  |
| ***Source to WG:*** |  |
| ***Source to TSG:*** |  |
|  |  |
| ***Work item code:*** |  |  | ***Date:*** |  |
|  |  |  |  |  |
| ***Category:*** |  |  | ***Release:*** |  |
|  | *Use one of the following categories:****F*** *(correction)****A*** *(mirror corresponding to a change in an earlier release)****B*** *(addition of feature),* ***C*** *(functional modification of feature)****D*** *(editorial modification)*Detailed explanations of the above categories canbe found in 3GPP [TR 21.900](http://www.3gpp.org/ftp/Specs/html-info/21900.htm). | *Use one of the following releases:Rel-8 (Release 8)Rel-9 (Release 9)Rel-10 (Release 10)Rel-11 (Release 11)…Rel-16 (Release 16)Rel-17 (Release 17)Rel-18 (Release 18)Rel-19 (Release 19)* |
|  |  |
| ***Reason for change:*** | The current requirements state that the MDF shall be able to deliver different service types to different LEMFs when multiple service types are applicable due to multiple warrants. The MDF should instead be able to deliver to service specific intercept product to multiple endpoints due to multiple warrants or when a single warrant requires different services be sent to different destinations.This contribution clarifies that RCS falls under messaging. |
|  |  |
| ***Summary of change:*** | Updates the description for the RCS and Messaging service scoping options. |
|  |  |
| ***Consequences if not approved:*** | The inclusion of RCS within the messaging service scoping option will remain ambiguous. |
|  |  |
| ***Clauses affected:*** | 4.4.2 |
|  |  |
|  | **Y** | **N** |  |  |
| ***Other specs*** |  | **X** |  Other core specifications  | TS/TR ... CR ...  |
| ***affected:*** |  | **X** |  Test specifications | TS/TR ... CR ...  |
| ***(show related CRs)*** |  | **X** |  O&M Specifications | TS/TR ... CR ...  |
|  |  |
| ***Other comments:*** |  |
|  |  |
| ***This CR's revision history:*** | s3i240013 |

## \*\*\*\* START OF FIRST CHANGE (MAIN DOCUMENT) \*\*\*\*

### 4.4.2 CSP service type

The LIPF shall be able to provision the POIs, TFs and MDF2/MDF3 according to the requirements of the warrant with the following CSP service type(s):

- Voice.

- Data.

- Messaging.

- Push-to-Talk (including MCPTT).

- LALS (the Target Positioning service, per TS 33.127 [5], clause 7.3.3.2).

- RCS (including all associated services).

When multiple service types are applicable to a target, the MDF2/MDF3 shall be able to deliver interception product for each CSP service type independently to different destinations when required.

When no service type is provisioned, the POIs shall generate and deliver applicable interception product for all services specified for the NF where the POI is located.

When no service type is provisioned, the MDF2/MDF3 shall deliver all interception product it receives from the POIs.

## \*\*\*\* END OF MAIN DOCUMENT CHANGES \*\*\*\*

## \*\*\*\* START OF FIRST CHANGE (ATTACHMENTS) \*\*\*\*

## \*\*\*\* END OF ALL CHANGES \*\*\*\*